;/*****************************************************************************
;*  Copyright Statement:
;*  --------------------
;*  This software is protected by Copyright and the information contained
;*  herein is confidential. The software may not be copied and the information
;*  contained herein may not be used or disclosed except with the written
;*  permission of MediaTek Inc. (C) 2007
;*
;*  BY OPENING THIS FILE, BUYER HEREBY UNEQUIVOCALLY ACKNOWLEDGES AND AGREES
;*  THAT THE SOFTWARE/FIRMWARE AND ITS DOCUMENTATIONS ("MEDIATEK SOFTWARE")
;*  RECEIVED FROM MEDIATEK AND/OR ITS REPRESENTATIVES ARE PROVIDED TO BUYER ON
;*  AN "AS-IS" BASIS ONLY. MEDIATEK EXPRESSLY DISCLAIMS ANY AND ALL WARRANTIES,
;*  EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE IMPLIED WARRANTIES OF
;*  MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE OR NONINFRINGEMENT.
;*  NEITHER DOES MEDIATEK PROVIDE ANY WARRANTY WHATSOEVER WITH RESPECT TO THE
;*  SOFTWARE OF ANY THIRD PARTY WHICH MAY BE USED BY, INCORPORATED IN, OR
;*  SUPPLIED WITH THE MEDIATEK SOFTWARE, AND BUYER AGREES TO LOOK ONLY TO SUCH
;*  THIRD PARTY FOR ANY WARRANTY CLAIM RELATING THERETO. MEDIATEK SHALL ALSO
;*  NOT BE RESPONSIBLE FOR ANY MEDIATEK SOFTWARE RELEASES MADE TO BUYER'S
;*  SPECIFICATION OR TO CONFORM TO A PARTICULAR STANDARD OR OPEN FORUM.
;*
;*  BUYER'S SOLE AND EXCLUSIVE REMEDY AND MEDIATEK'S ENTIRE AND CUMULATIVE
;*  LIABILITY WITH RESPECT TO THE MEDIATEK SOFTWARE RELEASED HEREUNDER WILL BE,
;*  AT MEDIATEK'S OPTION, TO REVISE OR REPLACE THE MEDIATEK SOFTWARE AT ISSUE,
;*  OR REFUND ANY SOFTWARE LICENSE FEES OR SERVICE CHARGE PAID BY BUYER TO
;*  MEDIATEK FOR SUCH MEDIATEK SOFTWARE AT ISSUE.
;*
;*  THE TRANSACTION CONTEMPLATED HEREUNDER SHALL BE CONSTRUED IN ACCORDANCE
;*  WITH THE LAWS OF THE STATE OF CALIFORNIA, USA, EXCLUDING ITS CONFLICT OF
;*  LAWS PRINCIPLES.  ANY DISPUTES, CONTROVERSIES OR CLAIMS ARISING THEREOF AND
;*  RELATED THERETO SHALL BE SETTLED BY ARBITRATION IN SAN FRANCISCO, CA, UNDER
;*  THE RULES OF THE INTERNATIONAL CHAMBER OF COMMERCE (ICC).
;*
;*****************************************************************************/
;
;/*****************************************************************************
; *
; * Filename:
; * ---------
; *   scatJRD53_09B.txt
; *
; * Project:
; * --------
; *   Maui_Software
; *
; * Description:
; * ------------
; *   defines the memory map for the validation board
; *
; * Author:
; * -------
; *   system auto generator v2.39 -> p2.41
; *
; * Auto Generated Date:
; * -------
; *   2010/3/2
; *
; * Revision History:
; * -------
; * $Log: scatJRD53_09B.txt system auto generator v2.39 -> p2.41 $
; * 
; ****************************************************************************/
;
;=========================================================================
; This scatter file is auto-generated and please DO NOT change the content at will
;=========================================================================
;
;--------------------
; SCHEME   : external 18MB flash memory and 8MB SRAM
; PLATFORM : MT6253
; FEATURES : USBDOWNLOAD MULTIBIN SECURE 
;--------------------

BOOTLOADER 0x08000000 0x20000
{
}

ROM 0x08020000 0xF20000
{
    ROM 0x08020000 0x800
    {
         bootarm.obj (C$$code,+First)
    }
    ROM_SECINF0 0x08021000 FIXED ;4KB
    {
         *.obj (SECINFO)
    }
    ROM0_1 0x08021400 FIXED 0x400 ;1KB
    { 
        maincode_version_string.obj (MAINCODE_JUMPTABLE) 
    }
    ROM0_2 +0x0 0x000bec00
    {
         *.obj (LEADING_PART,+First)

         Regioninit_ads.obj (+RO-CODE)
;         *l1_classb_g2.lib (+RO-CODE)
;         *l1_g2.lib (+RO-CODE)
;         *l1_classb_umts.lib (+RO-CODE)
;         *l4_classb.lib (+RO-CODE)
         *l4misc.lib (+RO-CODE)
         *kal.lib (+RO-CODE)
;         *fs.lib (+RO-CODE)
;         *tst.lib (+RO-CODE)
    }
    __KEEP_ROM 0x08100000 FIXED 0x00020000
    {
         *.obj (KEEP_ROM)
    }
    ROM1 0x08120000 FIXED 0x00400000
    {
         *l1_classb_g2.lib (+RO-CODE)
         *l1_g2.lib (+RO-CODE)
         *l1_classb_umts.lib (+RO-CODE)
         *l4_classb.lib (+RO-CODE)
         *lcmmi.lib (+RO-CODE)
         *mmi_framework.lib (+RO-CODE)
         *mmi_app.lib (+RO-CODE)
         *conn_app.lib (+RO-CODE)
         *inet_app.lib (+RO-CODE)
         
         cpp_initialise.o(+RO)
         cpp_finalise.o(+RO)
         * (C$$pi_ctorvec)
         * (C$$pi_dtorvec)
         * (C$$ddtorvec)
         
         divrt_real.o (+RO-CODE)
         *f_t_p.l (+RO-CODE)
         
; moved from ITCM
         tct.obj (+RO)
    }

    CODE_SECURITY +0x0
    {
        bn_add_se.obj (+RO)
        bn_asm_se.obj (+RO)
        bn_blind_se.obj (+RO)
        bn_ctx_se.obj (+RO)
        bn_div_se.obj (+RO)
        bn_exp_se.obj (+RO)
        bn_gcd_se.obj (+RO)
        bn_lib_se.obj (+RO)
        bn_mod_se.obj (+RO)
        bn_mont_se.obj (+RO)
        bn_mul_se.obj (+RO)
        bn_prime_se.obj (+RO)
        bn_rand_se.obj (+RO)
        bn_recp_se.obj (+RO)
        bn_shift_se.obj (+RO)
        bn_sqr_se.obj (+RO)
        bn_word_se.obj (+RO)
        md_rand_se.obj (+RO)
        mem_clr_se.obj (+RO)
        rand_lib_se.obj (+RO)
        rand_unix_se.obj (+RO)
        rsa_eay_se.obj (+RO)
        rsa_gen_se.obj (+RO)
        rsa_lib_se.obj (+RO)
        rsa_pk1_se.obj (+RO)
        sha1dgst_se.obj (+RO)
        sl_A1_Decipher.obj (+RO)
        sl_BackgroundTask.obj (+RO)
        sl_FSM.obj (+RO)
        sl_Key_Common.obj (+RO)
        sl_Key_Generator.obj (+RO)
        sl_MTK_API.obj (+RO)
        sl_OpenSSL.obj (+RO)
        sl_Private_Ciphering.obj (+RO)
        sl_RAM_Functions.obj (+RO)
        sl_Safe_Common.obj (+RO)
        sl_Safe_Core.obj (+RO)
        sl_SML.obj (+RO)
        sl_SML_Update.obj (+RO)
        sl_TLV_Read.obj (+RO)
        sl_Trace_Layer.obj (+RO)
    }
    DATA_SECURITY +0x0 0x1000
    {
        sl_Safe_Data.obj (+RO)
        SST_decrypt.obj (i.INT_IntializeSystemMemory)
    }

    
    ROM2 +0x0 0x00400000
    {
; WAP family
         *wapadp.lib (+RO-CODE)
         *wap.lib (+RO-CODE)
         *wae.lib (+RO-CODE)
         *jataayu.lib (+RO-CODE)
         *jataayuapp.lib (+RO-CODE)
         *wapapp.lib (+RO-CODE)
         *obigo05aadp.lib (+RO-CODE)
         *obigo05alib.lib (+RO-CODE)
         *obigo03capp.lib (+RO-CODE)
         *obigo03cadp.lib (+RO-CODE)
         *obigo03clib.lib (+RO-CODE)
; J2ME family
         *j2me_11.lib (+RO-CODE)
         *j2me_hi.lib (+RO-CODE)
         *jal.lib (+RO-CODE)
         *ijet_adp.lib (+RO-CODE)
         *jblendia.lib (+RO-CODE)
         j2me_custom_*.obj (+RO-CODE)
    }
    ROM3 +0x0 0x00400000
    {
         .ANY (+RO-CODE)
    }
    ROM4 +0x0 0x00400000
    {
         .ANY (+RO-CODE)
    }
    ROM5 +0x0 
    {
         .ANY (+RO-DATA)
    }
    ROM_TAIL +0x0 
    {
         *.obj (SECINFO_TAIL)
    }
    EXTSRAM_LARGEPOOL_NORMAL 0x00000200
    {
; For MT6225 projects, app-based ASM always at first due to Java FBBR
         app_mem.obj (LARGEPOOL_FIRST_ZI)
         ScrMemMgr.obj (LARGEPOOL_ZI)
         j2me_custom_resource.obj (LARGEPOOL_ZI)
         med_main.obj (LARGEPOOL_ZI)
         sl_BackgroundTask.obj (+ZI)
         sl_Safe_Data.obj (+ZI)
    }
    EXTSRAM_SL_INFO2 +0x0
    {
    	sl_BackgroundTask2.obj (+ZI)
    }
    EXTSRAM_SL_CODE +0x0
    { 
    	sl_RAM_Functions.obj (i.sl_RAM_SML_Decrypt)
    	sl_RAM_Functions.obj (i.sl_RAM_SML_Encrypt)
    	sl_RAM_Functions.obj (i.sl_RAM_FSM_Get_File_Name)
    	sl_Key_Generator.obj (i.sl_Key_Generator)
    }

    EXTSRAM_SL_INFO3 +0x0
    {
    	sl_BackgroundTask3.obj (+ZI)
    }
    EXTSRAM +0x00 
    {
         * (+RW, +ZI)
    }
; DSP execution regions cannot be OVERLAY; its size should be specified as 2^N, larger than 4KB, and should align with its start address
    EXTSRAM_DSP_TX 0x00Ffc000 0x2000
    {
         *.obj (EXTRAM_TXDATA)
    }
    EXTSRAM_DSP_RX 0x00Ffe000 0x2000
    {
         *.obj (EXTRAM_RXDATA)
    }
    EMIINIT_CODE 0x40000000 OVERLAY
    {
    	   * (EMIINITCODE, EMIINITCONST, EMIINITZI)
    }
    INTSRAM_CODE 0x40000000 OVERLAY 0x6A70
    {
         * (INTSRAM_ROCODE)
; system-realted CODE , SMALL set
         bootarm.obj (INTERNCODE)
         data_buff_pool.obj (INTERNCODE)
         ctrl_buff_pool.obj (INTERNCODE)
         stack_buff_pool.obj (INTERNCODE)
         stack_ltlcom.obj (INTERNCODE)
         stack_timer.obj (INTERNCODE)
         SST_intrCtrl.obj (INTERNCODE, INTERNCONST)
         cache.obj (INTERNCODE)
; Nucleus-related CODE , SMALL set
         tct.obj (INTERNCODE)
         tcc.obj (INTERNCODE)
         csc.obj (INTERNCODE)
         tmt.obj (+RO)
         smc.obj (INTERNCODE)
         evc.obj (INTERNCODE)
         pmc.obj (INTERNCODE)
         quc.obj (INTERNCODE)
         kal_nucleus_buff_mgr.obj (INTERNCODE)
         kal_nucleus_evshed_buff_mgr.obj (INTERNCODE)
         kal_nucleus_itc.obj (INTERNCODE)
         kal_nucleus_timer.obj (INTERNCODE)
; THREADX-related CODE , SMALL set
         ; UNDER CONSTRUCTION
         tx_thread_interrupt_disable.obj (+RO)
         tx_thread_interrupt_restore.obj (+RO)
         tx_thread_context_save.obj (+RO)
         tx_thread_context_restore.obj (+RO)
         tx_thread_irq_nesting_start.obj (+RO)
         tx_thread_irq_nesting_end.obj (+RO)
         tx_thread_system_return.obj (+RO)
         tx_thread_schedule.obj (+RO)
         tx_thread_resume.obj (+RO)
         tx_thread_system_resume.obj (+RO)
         tx_timer_interrupt.obj (+RO)
         tx_timer_thread_entry.obj (+RO)
         tx_block_allocate.obj (+RO)
         tx_block_release.obj (+RO)
         tx_event_flags_get.obj (+RO)
         tx_event_flags_set.obj (+RO)
         tx_mutex_get.obj (+RO)
         tx_mutex_put.obj (+RO)
         kal_threadx_tasks.obj (INTERNCODE)
         kal_threadx_buff_mgr.obj (INTERNCODE)
         kal_threadx_itc.obj (INTERNCODE)
         kal_threadx_timer.obj (INTERNCODE)
; common used C library
         memset.o (+RO)
         rt_memclr.o (+RO)
         callvia.o (+RO)
         _sprintf.o (+RO)
         rt_memcpy.o (+RO)
         lludiv10.o (+RO)
         rt_udiv.o (+RO)
         uread4.o (+RO)
         uwrite4.o (+RO)
; INTSRAM_CODE_OBJ_others_6253
         m11303.obj (INTERNCODE)
         cam_module.obj (INTERNCODE)
         uart.obj (INTERNCODE)
         gdi_image_direct_gif.obj (INTERNCODE)
         gdi_mutex.obj (INTERNCODE)
         gpt.obj (INTERNCODE)
         custom_EMI.obj(INTERNCODE)
         * (SNORCODE_INT)
         * (SNORCONST_INT)

; Please Do Not Remove
         m12100.obj (INTERNCODE)
         m12110.obj (INTERNCODE)
         m12120.obj (INTERNCODE)
         m12160.obj (INTERNCODE)
         m12170.obj (INTERNCODE)
         m12171.obj (INTERNCODE)
         m12180.obj (INTERNCODE)
    }
    INTSRAM_DATA 0x40006A70 0x6200
    {
         * (INTSRAM_RODATA, INTSRAM_RW, INTSRAM_ZI)
; system-realted data
         bootarm.obj (STACK_POOL_INTSRAM)
         stack_init.obj (INTERNCONST, INTERNRW, INTERNZI)
         ctrl_buff_pool.obj (INTERNCONST, INTERNRW, INTERNZI)
         stack_ltlcom.obj (INTERNCONST, INTERNRW, INTERNZI)
; Nucleus-related data ; Standard set
         tst*.obj (INTERNCONST, INTERNRW, INTERNZI)
         tct.obj (+RW, +ZI)
         tcd.obj (INTERNCONST, INTERNRW, INTERNZI)
         tmd.obj (+RW, +ZI)
         evd.obj (+RW, +ZI)
         pmd.obj (+RW, +ZI)
         qud.obj (+RW, +ZI)
         smd.obj (+RW, +ZI)
; THREADX-related data ; Standard set
         tx_thread_initialize.obj (+RW, +ZI)
         tx_timer_initialize.obj (+RW, +ZI)
; INTSRAM_DATA_OBJ_others_6253
         gdi_image.obj (INTERNCONST, INTERNRW, INTERNZI)
         gdi.obj (INTERNZI)
         interpret.obj (INTERNZI)
         sw_jpeg_decoder.obj (INTERNRW1, INTERNZI1)
         jpeg_encoder.obj (INTERNRW, INTERNZI)
         drv_gfx_stack_switch_manager.obj (INTERNRW2, INTERNZI2)

; Please Do Not Remove
         m12100.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12160.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12170.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12171.obj (INTERNCONST, INTERNRW, INTERNZI)
    }   

; Because MT6253 Internal RAM is tight, and med_main.obj and MP4DEC2 will not be used at simultaneously,
; on MT6253 platforms, the buffer in med_main.obj will be shared between JPEG and MP4DEC2.
; (Originally MP4DEC2 uses the DCM region shared with audio.)
; The sharing is used to make concurrency for audio and MP4DEC2
    MED_MAIN_REGION 0x4000CC70 OVERLAY 0x9600
    {
         med_main.obj (INTERNRW1, INTERNZI1)
         btmt_mem.obj (INTSRAM_RW, INTSRAM_ZI)
    }
    DYNAMIC_CODE12 0x4000cc70 OVERLAY 0x9600
    {
         * (MP4DEC2_DYNAMIC_ZI, MP4DEC2_DYNAMIC_RO)
    }
    DYNAMIC_CODE16 0x4000cc70 OVERLAY 0x9600
    {
         * (MP4ENC1_DYNAMIC_CODE, MP4ENC1_DYNAMIC_RO, MP4ENC1_DYNAMIC_ZI)
    }
    DYNAMIC_CODE18 0x40016270 OVERLAY 0x0d90
    {
         * (MP4DEC_DYNAMIC_CODE, MP4DEC_DYNAMIC_RO)
    }
    DYNAMIC_CODE19 0x40016270 OVERLAY 0x0d90
    {
         * (MP4ENC_DYNAMIC_CODE, MP4ENC_DYNAMIC_RO)
    }
    DYNAMIC_CODE1 0x40017000 OVERLAY 0x5000
    {
         * (AMR515_DYNAMIC_CODE, AMR515_DYNAMIC_ZI)
    }
    DYNAMIC_CODE11 0x40017000 OVERLAY 0x5000
    {
         * (VRENGINE_DYNAMIC_CODE, VRENGINE_DYNAMIC_ZI)
    }
    DYNAMIC_CODE13 0x40017000 OVERLAY 0x5000
    {
         * (MP4ENC2_DYNAMIC_ZI, MP4ENC2_DYNAMIC_RO)
    }
    DYNAMIC_CODE14 0x40017000 OVERLAY 0x5000
    {
         * (264DEC2_DYNAMIC_ZI, 264DEC2_DYNAMIC_RO)
    }
    DYNAMIC_CODE3 0x40017000 OVERLAY 0x5000
    {
         * (CTM_DYNAMIC_CODE, CTM_DYNAMIC_ZI)
    }
    DYNAMIC_CODE4 0x40017000 OVERLAY 0x5000
    {
         * (G729_DYNAMIC_CODE, G729_DYNAMIC_ZI)
    }
    DYNAMIC_CODE5 0x40017000 OVERLAY 0x5000
    {
         * (SBC_DYNAMIC_CODE, SBC_DYNAMIC_ZI)
    }
    INTSRAM_MULTIMEDIA 0x4001C000  0x4000
    {
         display_intmem.obj  (INTERNRW1, INTERNZI1) 
    }
}



;=========================================================================
; This load region must be behind all the protected load region
;=========================================================================
; 1. DO NOT modify load region naming and pragma naming!
;=========================================================================

__HIDDEN_SECURE_MAC +0x0
{
    __HIDDEN_SECURE_MAC +0x0
    {
         *.obj (SECURE_MAC_SIZE)
    }
    __HIDDEN_SECURE_MAC_CONTENT +0x0
    {
         *.obj (SECURE_MAC_CONTENT)
    }
}

CUSTPACK_ROM 0x08F40000 0x8BB000
{
    SSV_CUSTPACK_ROM +0x00
    { 
        Jrd_ssv_custpack_jmbtl.obj (SSV_JUMP_TBL)
    }
    CUSTPACK_ROM +0x00
    {
        nvram_cust_pack.obj (+RO)
        custom_extdata_cust_pack.obj (+RW, +RO)
        custom_wap_cust_pack.obj (+RO)
        Jrd_ssv_custpack_jmbtl.obj (+RO-Data)
    } 
     CUSTPACK_ROM_JPTBL 0x08F80000 FIXED
    { 
        resource_custpack_jtbl.obj (RESOURCE_JUMP_TBL, +First) 
        resource_custpack_jtbl.obj (CUSTPACK_2ND_JUMP_TBL)
    }
    CUSTPACK_ROM_CONTENT +0x00
    {
        resource_custpack_jtbl.obj (+RW, +RO)
    }
    CUSTPACK_ROM_IMAGE +0x00
    {
        CustImgMap.obj (+RW)
        CustImgMapExt.obj (+RW)
        CustImgRes.obj (+RO)
        CustImgMap.obj (+RO)
        CustImgMapExt.obj (+RO)
        CustImgResExt.obj (+RO)
    }
    CUSTPACK_ROM_MELODY +0x00
    {
        custpack_audio.obj (+RO)
        CustAdoRes.obj (+RO)
        CustAdoResExt.obj (+RO)
    }
    CUSTPACK_ROM_MENU +0x00
    {
        CustMenuRes.obj (+RO)
        CustMenuRes.obj (+RW)
    }
    CUSTPACK_ROM_THEME +0x00
    {
         ThemeRes.obj (RESOURCE_1ST_CONTENT)
         ThemeRes.obj (+RO, +RW)
    }
    CUSTPACK_ROM_JAVA +0x00
    {
        j2me_custom_mids_jtbl.obj (+RW)
        j2me_custom_mids.obj (+RW,+RO)
    }
    CUSTPACK_ROM_MISC +0x00
    {
         custpack_certs.obj (+RO)
         custpack_java_certs.obj (+RO-DATA)
         resource_world_clock_city.obj (+RO-DATA)
         PlmnName.obj(+RO)
         hand_writing_dic.obj (+RO-DATA)
    }
    LANG_PACK_ROM +0x00
    {
         resource_lang_pack_jtbl.obj (+RW,+RO)
    }
    LANG_PACK_STRING +0x00
    {
         CustStrRes.obj (+RO)
         CustStrMap.obj (+RO)    
         CustStrRes.obj (+RW)
         CustStrMap.obj (+RW)
    }
    LANG_PACK_FONT +0x00
    {
         FontRes.obj (+RO)
         FontRes.obj (+RW)
         CustFontMapExt.obj (+RO)
         CustFontResExt.obj (+RO)
    }
    LANG_PACK_IME +0x00
    {
         IMERes.obj (+RW)
         IMERes.obj (+RO)
    }
    LANG_PACK_MISC +0x00
    {   
         mtkmultitap_cust.obj(+RO)
         CharsetTable_jrd.obj(+RO)
         vf_*.obj (+RW,+RO)
         jrd_ssv_resources_generate.obj(SSV_RES)
    }
}

STUDYPARA_ROM 0x097FB000 0x2800 
{ 
    STUDYPARA_ROM +0x00 
    { 
        resource_techpara_jtbl.obj (RESOURCE_JUMP_TBL, +First) 
        resource_techpara_jtbl.obj (+RW)

   }
   STUDYPARA_ROM_CONTENT +0x00
   { 
        custom_techpara_cust_pack.obj (+RW)
        custom_techpara_cust_pack.obj (+RO)
        custom_techpara_acoustic_*.obj (+RO)
        custom_techpara_audcoeff_*.obj (+RO)
        custom_techpara_equalizer_*.obj (+RO)
        custom_techpara_camera.obj (+RO)
        custom_techpara_hw.obj (+RO)
        custom_techpara_bmt_chr.obj (+RO) 
    }
}

JUMP_TABLE 0x097FD800 0x400 
{
    JUMP_TABLE +0x00 0x200 
    {
         custom_jump_tbl.obj (+RO, +RW, +ZI)
    }
    JUMP_TABLE_STR 0x097FDA00 FIXED 
    { 
        custom_jump_tbl_str.obj (+RW) 
    }
    JUMP_TABLE_STR_CONTENT +0x00
    { 
        custom_jump_tbl_str.obj (+RO) 
    }
}

;=========================================================================
; The following load regions must be the end of all the load regions
;=========================================================================
; 1. Only address is configurable.
; 2. Region address must be fixed address.
; 3. Using flash-sector-aligned address in region address for higher security.
; 4. DO NOT modify load region order, load region naming and pragma naming!
;=========================================================================

__HIDDEN_SECURE_RO 0x097FDC00 0x2000
{
    SECURE_RO +0x0
    {
         *.obj (SECURE_RO)
    }
}

__HIDDEN_FLASHTOOL_CFG 0x097FFC00 0x400
{   
    __HIDDEN_FLASHTOOL_CFG +0x0
    {
         *.obj (FLASHTOOL_CFG)
    }
}

__HIDDEN_CUST_PARA 0x09FE0000 0x20000
{
    CUST_PARA +0x0
    {
         *.obj (CUST_PARA_TRACE_ABILITY)
    }
    __HIDDEN_CUST_PARA_RF 0x09FF0000 FIXED
    {
         *.obj (CUST_PARA_RF)
    }
    __HIDDEN_CUST_PARA_TAIL +0x0 
    {
         *.obj (CUST_PARA_TAIL)
    }
}

