;/*****************************************************************************
;*  Copyright Statement:
;*  --------------------
;*  This software is protected by Copyright and the information contained
;*  herein is confidential. The software may not be copied and the information
;*  contained herein may not be used or disclosed except with the written
;*  permission of MediaTek Inc. (C) 2007
;*
;*  BY OPENING THIS FILE, BUYER HEREBY UNEQUIVOCALLY ACKNOWLEDGES AND AGREES
;*  THAT THE SOFTWARE/FIRMWARE AND ITS DOCUMENTATIONS ("MEDIATEK SOFTWARE")
;*  RECEIVED FROM MEDIATEK AND/OR ITS REPRESENTATIVES ARE PROVIDED TO BUYER ON
;*  AN "AS-IS" BASIS ONLY. MEDIATEK EXPRESSLY DISCLAIMS ANY AND ALL WARRANTIES,
;*  EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE IMPLIED WARRANTIES OF
;*  MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE OR NONINFRINGEMENT.
;*  NEITHER DOES MEDIATEK PROVIDE ANY WARRANTY WHATSOEVER WITH RESPECT TO THE
;*  SOFTWARE OF ANY THIRD PARTY WHICH MAY BE USED BY, INCORPORATED IN, OR
;*  SUPPLIED WITH THE MEDIATEK SOFTWARE, AND BUYER AGREES TO LOOK ONLY TO SUCH
;*  THIRD PARTY FOR ANY WARRANTY CLAIM RELATING THERETO. MEDIATEK SHALL ALSO
;*  NOT BE RESPONSIBLE FOR ANY MEDIATEK SOFTWARE RELEASES MADE TO BUYER'S
;*  SPECIFICATION OR TO CONFORM TO A PARTICULAR STANDARD OR OPEN FORUM.
;*
;*  BUYER'S SOLE AND EXCLUSIVE REMEDY AND MEDIATEK'S ENTIRE AND CUMULATIVE
;*  LIABILITY WITH RESPECT TO THE MEDIATEK SOFTWARE RELEASED HEREUNDER WILL BE,
;*  AT MEDIATEK'S OPTION, TO REVISE OR REPLACE THE MEDIATEK SOFTWARE AT ISSUE,
;*  OR REFUND ANY SOFTWARE LICENSE FEES OR SERVICE CHARGE PAID BY BUYER TO
;*  MEDIATEK FOR SUCH MEDIATEK SOFTWARE AT ISSUE.
;*
;*  THE TRANSACTION CONTEMPLATED HEREUNDER SHALL BE CONSTRUED IN ACCORDANCE
;*  WITH THE LAWS OF THE STATE OF CALIFORNIA, USA, EXCLUDING ITS CONFLICT OF
;*  LAWS PRINCIPLES.  ANY DISPUTES, CONTROVERSIES OR CLAIMS ARISING THEREOF AND
;*  RELATED THERETO SHALL BE SETTLED BY ARBITRATION IN SAN FRANCISCO, CA, UNDER
;*  THE RULES OF THE INTERNATIONAL CHAMBER OF COMMERCE (ICC).
;*
;*****************************************************************************/
;
;/*****************************************************************************
; *
; * Filename:
; * ---------
; *   scatJRD35_08A.txt
; *
; * Project:
; * --------
; *   Maui_Software
; *
; * Description:
; * ------------
; *   defines the memory map for the validation board
; *
; * Author:
; * -------
; *   system auto generator v1.55 -> p1.57 -> p1.62 -> p1.67 -> p1.86
; *
; * Auto Generated Date:
; * -------
; *   2009/2/17
; *
; * Revision History:
; * -------
; * removed!
; * removed!
; ****************************************************************************/
;
;--------------------
; SCHEME   : external NAND flash and 64MB LPSDRAM
; PLATFORM : MT6235B
; FEATURES : NFB SECURE 
;--------------------

ROM 0x00
{
    ROM 0x00 
    {
         bootarm.obj                   (C$$code,+First)
         *.obj                         (LEADING_PART)
    }
    ROMHEAD 0x800 FIXED
    {
         *.obj                         (SECINFO)
         *.obj                         (SECOND_PART)
         *.obj                         (MAUI_FOTA_HEAD_INFO)
    }
    ROM0 0xb00 FIXED 0x400 ;1KB
    { 
        maincode_version_string.obj (+RW) 
    }
    ROM1 +0x0 
    {
         Regioninit_ads.obj            (+RO-CODE)
         *.o                           (+RO)
         
         *adaptation.lib               (+RO)
         *bmt.lib                      (+RO)
         *config.lib                   (+RO)
         *drv.lib                      (+RO)
         *drv_display.lib              (+RO)
         *drv_graphics.lib             (+RO)
         *drv_idp.lib                  (+RO)
         *fdm.lib                      (+RO)
         *init.lib                     (+RO)
         *kal.lib                      (+RO)
         *l1_classb.lib                (+RO)
         *stacklib.lib                 (+RO)
         *sst.lib                      (+RO)
         *sss.lib                      (+RO)
         *tst.lib                      (+RO)
         *nucleus.lib                  (+RO)
         *nucleus_int.lib              (+RO)
         *nucleus_debug.lib            (+RO)
         
;nucleus_ctrl_code.lib
         csc.obj                       (+RO)
         tcc.obj                       (+RO)
         tms.obj                       (+RO)
         evc.obj                       (+RO)
         quc.obj                       (+RO)
         pmc.obj                       (+RO)
         smc.obj                       (+RO)
         
; moved from ITCM
         tmt.obj                       (+RO)
         stack_timer.obj               (+RO)
         data_buff_pool.obj            (+RO)
         kal_nucleus_timer.obj         (+RO)
         
; C++ related input sections
         cpp_initialise.o              (+RO)
         cpp_finalise.o                (+RO)
         *                             (C$$pi_ctorvec)
         *                             (C$$pi_dtorvec)
         *                             (C$$ddtorvec)
         *                             (C$$ctor)
         *                             (C$$dtor)
         
; libs must be in primary ROM
         *mmi_framework.lib            (+RO)
         *image_codec.lib              (+RO)
         *image_codec16.lib            (+RO)
         *media.lib                    (+RO)
         *media_sec.lib                (+RO)
         *fs.lib                       (+RO)
         *verno.lib                    (+RO)
         *j2me_hi.lib                  (+RO)
         *dsp_ram.lib                  (+RO)
         
         
         
; specific objects in custom.lib
; directory mcu\custom\system
         custom_emi.obj                (+RO)
         EMI_GEN_custom_EMI_*.pobj     (+RO)
         custom_config.obj             (+RO)
         custom_flash.obj              (+RO)
         custom_scatstruct.obj         (+RO)
         custom_jump_tbl.obj           (+RO)
; directory mcu\custom\drv\common
         gpio_setting.obj              (+RO)
; directory mcu\custom\drv\misc_drv
         adc_channel.obj               (+RO)
         alerter_tone.obj              (+RO)
         alerterdrv.obj                (+RO)
         auxmain.obj                   (+RO)
         chr_parameter.obj             (+RO)
         custom_drv_init.obj           (+RO)
         custom_equipment.obj          (+RO)
         custom_hw_default.obj         (+RO)
         eint_def.obj                  (+RO)
         exif_custom.obj               (+RO)
         gpio_drv.obj                  (+RO)
         irda_custom.obj               (+RO)
         kbdmain_joystick.obj          (+RO)
         keypad_def.obj                (+RO)
         msdc_custom.obj               (+RO)
         pmic_custom.obj               (+RO)
         pwmdrv.obj                    (+RO)
         touch_panel_custom.obj        (+RO)
         touch_panel_spi.obj           (+RO)
         touchpad.obj                  (+RO)
         touchpad_keydef.obj           (+RO)
         tv_custom.obj                 (+RO)
         uart_def.obj                  (+RO)
         uem_gpio.obj                  (+RO)
         lcdbl_custom_SN3226.obj       (+RO)
         usb_custom.obj                (+RO)
         usb_host_ms_custom.obj        (+RO)
         pmu_custom.obj                (+RO)
         
; directory mcu\custom\drv\misc_drv\BB_folder\codegen
         adc_var.obj                   (+RO)
         eint_var.obj                  (+RO)
         gpio_var.obj                  (+RO)
         uem_drv.obj                   (+RO)
; directory mcu\custom\drv\LCD
         lcd.obj                       (+RO)
         lcd_c_*.obj		       (+RO)
         
; specific objects in mmiresource.lib
         custNFBProgressImg.obj        (+RO)
         gui_wrapper.obj               (+RO)
         
; specific objects in media_app.lib
         mdi_tv.obj                    (+RO)
         
; specific objects in bcsi.lib ; C++ const data init
         MiscUtils.obj                 (+RO)
         
; specific objects in che.lib
         md5_engine.obj                (+RO)
         Custom_tracdata_config.obj	(+RO)
         maincode_version_string.obj      (+RO)
    }
    PRIMARY_CACHED_EXTSRAM +0xF0002000 
    {
         *adaptation.lib               (+RW)
         *config.lib                   (+RW)
         *dsp_ram.lib                  (+RW)
         *fs.lib                       (+RW)
         *kal.lib                      (+RW)
         *nucleus.lib                  (+RW)
         *nucleus_int.lib              (+RW)
         *sst.lib                      (+RW)
         *stacklib.lib                 (+RW)
         *.l                           (+RW)
         
         *drv.lib                      (+RW)
         *drv_display.lib              (+RW)
         *drv_graphics.lib             (+RW)
         *drv_idp.lib                  (+RW)
         *fdm.lib                      (+RW)
         *tst.lib                      (+RW)
         
; libs must be in primary ROM
         *mmi_framework.lib            (+RW)
         *media.lib                    (+RW)
         *media_sec.lib                (+RW)
         *verno.lib                    (+RW)
         *j2me_hi.lib                  (+RW)
         
; init
         *init.lib                     (+RW)
         
; hardware driver
         *bmt.lib                      (+RW)
         
; Crypto, Image, and Graphics
         *image_codec.lib              (+RW)
         *image_codec16.lib            (+RW)
         *sw_png_codec.lib             (+RW)
         
; specific objects in custom.lib
; directory mcu\custom\system
         custom_config.obj             (+RW)
         custom_emi.obj                (+RW)
         EMI_GEN_custom_EMI_*.pobj     (+RW)
         custom_flash.obj              (+RW)
         custom_jump_tbl.obj           (+RW)
         custom_scatstruct.obj         (+RW)
; directory mcu\custom\drv\common
         gpio_setting.obj              (+RW)
; directory mcu\custom\drv\misc_drv
         adc_channel.obj               (+RW)
         alerter_tone.obj              (+RW)
         alerterdrv.obj                (+RW)
         auxmain.obj                   (+RW)
         chr_parameter.obj             (+RW)
         custom_drv_init.obj           (+RW)
         custom_equipment.obj          (+RW)
         custom_hw_default.obj         (+RW)
         eint_def.obj                  (+RW)
         exif_custom.obj               (+RW)
         gpio_drv.obj                  (+RW)
         irda_custom.obj               (+RW)
         kbdmain_joystick.obj          (+RW)
         keypad_def.obj                (+RW)
         msdc_custom.obj               (+RW)
         pmic_custom.obj               (+RW)
         pwmdrv.obj                    (+RW)
         touch_panel_custom.obj        (+RW)
         touch_panel_spi.obj           (+RW)
         touchpad.obj                  (+RW)
         touchpad_keydef.obj           (+RW)
         tv_custom.obj                 (+RW)
         uart_def.obj                  (+RW)
         uem_gpio.obj                  (+RW)
         lcdbl_custom_SN3226.obj       (+RW)
         usb_custom.obj                (+RW)
         usb_host_ms_custom.obj        (+RW)
; directory mcu\custom\drv\misc_drv\BB_folder\codegen
         adc_var.obj                   (+RW)
         eint_var.obj                  (+RW)
         gpio_var.obj                  (+RW)
         uem_drv.obj                   (+RW)
; directory mcu\custom\drv\LCD
         lcd.obj                       (+RW)
         lcd_c_*.obj		       (+RW)
; specific objects in mmiresource.lib
         custNFBProgressImg.obj        (+RW)
         gui_wrapper.obj               (+RW)
         
; specific objects in media_app.lib
         mdi_tv.obj                    (+RW)
         
; specific objects in che.lib
         md5_engine.obj                (+RW)
    }
    EMIINIT_CODE 0x50000000 0x800
    {
         custom_emi.obj (INTERNCODE, INTERNRW1, INTERNZI1)
         EMI_GEN_custom_EMI_*.pobj (INTERNCODE, INTERNCONST1, INTERNRW1, INTERNZI1)
         custom_multi_EMI_*.obj (INTERNCODE, INTERNCONST1, INTERNRW1, INTERNZI1)
    }
    INTSRAM_CODE 0x50000800 0x0000B800
    {
; system-realted CODE , ARM9 Family SMALL set
         bootarm.obj (INTERNCODE)
         isrentry.obj (INTERNCODE)
         idle_task.obj (INTERNCODE)
         cache.obj (INTERNCODE)
; Nucleus-related CODE , ARM9 Family SMALL set
         tct.obj (+RO)
; utilities-related CODE , ARM9 Family STANDARD set
         SST_intrCtrl.obj (INTERNCODE, INTERNCONST)
         init.obj (INTERNCODE)
         emi.obj (INTERNCODE)
         ex_item.obj (INTERNCODE)
         custom_scatstruct.obj (INTERNCODE)
; INTSRAM_CODE_OBJ_others_6235
         mpal_gprs_common_func.obj (INTERNCODE)
         m11194.obj (INTERNCODE)
         m11191.obj (INTERNCODE)
         m12167.obj (INTERNCODE)
         m12168.obj (INTERNCODE)
         m12180.obj (INTERNCODE)
         m11303.obj (INTERNCODE)
         m11305.obj (INTERNCODE)
         m12194.obj (INTERNCODE)
         L1Trc.obj (INTERNCODE)
         l1d_data.obj (INTERNCODE)
         l1d_internal_data.obj (INTERNCODE)
         m12100.obj (INTERNCODE)         
         m12110.obj (INTERNCODE)
         m12120.obj (INTERNCODE)
         m12160.obj (INTERNCODE)
         m12170.obj (INTERNCODE)
         divider.obj (INTERNCODE)
         gpt.obj (INTERNCODE)
         lpwr.obj (INTERNCODE)
         l1dsm.obj (INTERNCODE)
         * (SNORCODE_INT)
         * (SNORCONST_INT)
         ofn.obj (INTERNCODE)
    }
    INTSRAM_DATA 0x50100000 0x00008C00
    {
; system-realted data
         bootarm.obj (STACK_POOL_INTSRAM)
         isrentry.obj (INTERNCONST, INTERNRW, INTERNZI)
         ctrl_buff_pool.obj (INTERNCONST, INTERNRW, INTERNZI)
         stack_ltlcom.obj (INTERNCONST, INTERNRW, INTERNZI)
         custom_emi.obj (INTERNCONST, INTERNRW, INTERNZI)
         EMI_GEN_custom_EMI_*.pobj (INTERNCONST, INTERNRW, INTERNZI)
         custom_multi_EMI_*.obj (INTERNCONST, INTERNRW, INTERNZI)
         idle_task.obj (INTERNCONST, INTERNRW, INTERNZI)
; Nucleus-related data ; ARM9 Family STANDARD set
         *nucleus_critical_data.lib (+RW, +ZI)
         *nucleus_ctrl_code.lib (+RW, +ZI)
; utilities-related data , ARM9 Family STANDARD set
         init.obj (INTERNCONST, INTERNRW, INTERNZI)
         emi.obj (INTERNCONST, INTERNRW, INTERNZI)
         ex_item.obj (INTERNCONST, INTERNRW, INTERNZI)
         custom_scatstruct.obj (INTERNCONST, INTERNRW, INTERNZI)
; INTSRAM_DATA_OBJ_others_6235
         mpal_gprs_common_func.obj (INTERNCONST, INTERNRW, INTERNZI)
         mpal_gprs_dl_msg_hdlr.obj (INTERNCONST, INTERNRW, INTERNZI)
         m11194.obj (INTERNCONST, INTERNRW, INTERNZI)
         m11191.obj (INTERNCONST, INTERNRW, INTERNZI)
         l1d_data.obj (INTERNCONST, INTERNRW, INTERNZI)
         l1d_internal_data.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12100.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12110.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12120.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12160.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12167.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12170.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12168.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12180.obj (INTERNCONST, INTERNRW, INTERNZI)                  
         m11303.obj (INTERNCONST, INTERNRW, INTERNZI)
         m11305.obj (INTERNCONST, INTERNRW, INTERNZI)         
         m12194.obj (INTERNCONST, INTERNRW, INTERNZI)                  
         L1Trc.obj (INTERNCONST, INTERNRW, INTERNZI)
         gdi_image.obj (INTERNCONST, INTERNRW, INTERNZI)
         sw_gif_bytestream.obj (INTERNCONST, INTERNRW, INTERNZI)
         gdi.obj (INTERNZI)         
         interpret.obj (INTERNZI)
         file71.o (INTERNCONST, INTERNRW, INTERNZI)
         l1dsm.obj (INTERNCONST, INTERNRW, INTERNZI)
         drv_gfx_stack_switch_manager.obj (INTERNRW, INTERNZI)
         ofn.obj(INTERNZI)
    }   
}

SECONDARY_ROM +0x4000
{
    SECONDARY_ROM +0x0 0x400000
    {
         .ANY (+RO-CODE)
    }
    ROM2 +0x0 0x400000
    {
         .ANY (+RO-CODE)
    }
    ROM3 +0x0 0x400000
    {
         .ANY (+RO-CODE)
    }
    ROM4 +0x0 
    {
         .ANY (+RO-DATA)
    }
    ROM_TAIL +0x0 
    {
         *.obj (SECINFO_TAIL)
    }
    DYNAMIC_CACHEABLE_EXTSRAM_DEFAULT_NONCACHEABLE_ZI +0x2000 
    {
         med_main.obj (LARGEPOOL_ZI)
         * (DYNAMICCACHEABLEZI_NC)
    }
    SECONDARY_EXTSRAM_ZI +0x2000 
    {
         *deniro.lib (+ZI)
         *fs_fig.lib (+ZI)
         *verno.lib  (+ZI)
         memport.obj (+ZI)
; Others that voluntarily NOT cached
         * (NONCACHEDZI)
    }
    SECONDARY_EXTSRAM_RW +0x0 
    {
         *deniro.lib (+RW)
         *fs_fig.lib (+RW)
         memport.obj (+RW)
; Others that voluntarily NOT cached
         * (NONCACHEDRW)
    }
    DYNAMIC_CACHEABLE_EXTSRAM_DEFAULT_NONCACHEABLE_RW +0x2000 
    {
         * (DYNAMICCACHEABLERW_NC)
    }
    PAGE_TABLE +0xF0002000 
    {
         cache.obj (PAGETABLE)
         * (PAGETABLE)
    }
    CACHED_EXTSRAM +0x0
    {
; All ZI are put in CACHED region by default
         * (+RW, +ZI)
    }
    DYNAMIC_CACHEABLE_EXTSRAM_DEFAULT_CACHEABLE +0x2000 
    {
         * (DYNAMICCACHEABLERW_C, DYNAMICCACHEABLEZI_C)
    }
    CACHED_DUMMY_END 0xf3496000 
    {
         bootarm.obj (DUMMY_POOL)
    }
    CODE_PATCH_CODE 0x03fbf000 0x1000 ; 4KB
    {
         * (CODE_PATCH_REGION)
    }
; DSP execution regions cannot be OVERLAY; its size should be specified as 2^N, larger than 4KB, and should align with its start address
    SECONDARY_EXTSRAM_DSP_TX 0x03fc0000 0x20000
    {
         *.obj (EXTRAM_TXDATA)
    }
    SECONDARY_EXTSRAM_DSP_RX 0x03fe0000 0x20000
    {
         *.obj (EXTRAM_RXDATA)
    }
    INTSRAM_BLINUSED 0x40000000 OVERLAY 0x00004000
    {
    ; Execution Region Reserved for Bootloader
    }
    INTSRAM_TMP_PAGE_TABLE 0x40004000 OVERLAY 0x0000C000
    {
         * (TMPPAGETABLE)
    }
    INTSRAM_MULTIMEDIA 0x40000000 OVERLAY 0x00010000
    {
         ae.obj (INTERNRW1, INTERNZI1) 
         isp_comm.obj (INTERNRW1, INTERNZI1) 
         med_main.obj (INTERNRW1, INTERNZI1) 
    }
}

STUDYPARA_ROM 0x03296000  0x4000
{
    STUDYPARA_ROM +0x00 
    { 
	resource_techpara_jtbl.obj (RESOURCE_JUMP_TBL, +First)
	resource_techpara_jtbl.obj (+RW)
    }
    STUDYPARA_ROM_CONTENT +0x00
    { 
    	custom_techpara_cust_pack.obj (+RW) 
	custom_techpara_cust_pack.obj (+RO)
	custom_techpara_acoustic_*.obj (+RO)
	;custom_techpara_acoustic_eu.obj (+RO)
	;custom_techpara_acoustic_us.obj (+RO) 
	;custom_techpara_acoustic_latam.obj (+RO)
	;custom_techpara_acoustic_china.obj (+RO)
	custom_techpara_audcoeff.obj (+RO) 
	custom_techpara_camera.obj (+RO) 
	custom_techpara_equalizer.obj (+RO)
	custom_techpara_hw.obj (+RO) 
	custom_techpara_driver.obj (+RW) 
 	bmt_custom_chr.obj (+RO, +RW)
 	lcd_init_truly_r61513.obj (+RO)
 	lcd_init_truly_ssd2119.obj (+RO)
    } 
}

CUSTPACK_ROM 0x0329a000  0xd20000
{
    CUSTPACK_ROM +0x0
    { 
	resource_custpack_jtbl.obj (RESOURCE_JUMP_TBL, +First) 
	resource_custpack_jtbl.obj (+RW)
    }
    CUSTPACK_ROM_CONTENT +0x00
    { 
       plmnname.obj (+RO)
 	custom_extdata_cust_pack.obj (+RW) 
	j2me_custom_mids.obj (+RW) 
	ThemeRes.obj (+RW)
    	nvram_cust_pack.obj (+RO) 
   	custom_extdata_cust_pack.obj (+RO) 
	custom_wap_cust_pack.obj (+RO) 
	j2me_custom_mids.obj (+RO) 
	ThemeRes.obj (+RO)     
	CustMenuRes.obj (+RO)
	CustImgRes.obj (+RO)
	CustStrRes.obj (+RO)
	CustImgResExt.obj (+RO)
	CustAdoRes.obj (+RO)
	CustAdoResExt.obj (+RO)
	custpack_audio.obj (+RO)
	CustImgMap.obj (+RO)
	CustImgMapExt.obj (+RO) 
        mtkmultitap_cust.obj (+RO)
;language package
	resource_lang_pack_jtbl.obj (+RW)
	CharsetTable_jrd.obj (+RW) 
	FontRes.obj (+RW)
	IMERes.obj (+RW)
	CustImgMap.obj (+RW)
	CustImgMapExt.obj (+RW)
	CharsetTable_jrd.obj (+RO) 
	CustStrMap.obj (+RO)
	FontRes.obj (+RO)
	IMERes.obj (+RO) 
	resource_world_clock_city.obj (+RO)
	*.obj(SSV_RES)
    }
}

THIRD_ROM  +0x0
{
    THIRD_ROM 0x04000004
    {
         * (NFB3RDROM_HEADER_HINT)
    }
}
DEMAND_PAGING_ROM0 0xf4000000 0xD00000
{
    DEMAND_PAGING_ROM0 0xf4000000 0x400000
    {
; FT
         *ft.lib (+RO-CODE)
         *ft.lib (+RO-DATA)
; FMGR
         filemanagersrc.obj (+RO-CODE, +RO-DATA)
         filemgr.obj (+RO-CODE, +RO-DATA)
         filemgrcore.obj (+RO-CODE, +RO-DATA)
         filemgrui.obj (+RO-CODE, +RO-DATA)
; Engineering mode
         engineermodedevicesrc.obj (+RO-CODE, +RO-DATA)
         engineermodedummysrc.obj (+RO-CODE, +RO-DATA)
         engineermodeminigps.obj (+RO-CODE, +RO-DATA)
         engineermodemsghandler.obj (+RO-CODE, +RO-DATA)
         engineermodeprofiling.obj (+RO-CODE, +RO-DATA)
         engineermodesocketapp.obj (+RO-CODE, +RO-DATA)
         engineermodesocketdemoapp.obj (+RO-CODE, +RO-DATA)
         engineermodesrc.obj (+RO-CODE, +RO-DATA)
         engineermodetracer.obj (+RO-CODE, +RO-DATA)
; MMI game
         F1Race.obj (+RO-CODE, +RO-DATA)
         TOH.obj (+RO-CODE, +RO-DATA)
         Riches.obj (+RO-CODE, +RO-DATA)
         ColorBalls.obj (+RO-CODE, +RO-DATA)
         Snake.obj (+RO-CODE, +RO-DATA)
         Smash.obj (+RO-CODE, +RO-DATA)
         Doll.obj (+RO-CODE, +RO-DATA)
         Majung.obj (+RO-CODE, +RO-DATA)
         Puzzle.obj (+RO-CODE, +RO-DATA)
         Ufo.obj (+RO-CODE, +RO-DATA)
         Magicsushi.obj (+RO-CODE, +RO-DATA)
         Vsmj.obj (+RO-CODE, +RO-DATA)
; EXTRA
         bmi.obj (+RO-CODE, +RO-DATA)
         Calculator.obj (+RO-CODE, +RO-DATA)
         Calorie.obj (+RO-CODE, +RO-DATA)
         currencyconvertor.obj (+RO-CODE, +RO-DATA)
         CurrencyConvertorE.obj (+RO-CODE, +RO-DATA)
         Extra.obj (+RO-CODE, +RO-DATA)
         healthmenstural.obj (+RO-CODE, +RO-DATA)
         Shortcuts.obj (+RO-CODE, +RO-DATA)
         StopwatchMultiPurpose.obj (+RO-CODE, +RO-DATA)
         StopwatchTypical.obj (+RO-CODE, +RO-DATA)
         unitconvertor.obj (+RO-CODE, +RO-DATA)
; EBOOK
         EbookFramework.obj (+RO-CODE, +RO-DATA)
         EbookSrc.obj (+RO-CODE, +RO-DATA)
    }
    DEMAND_PAGING_ROM1 +0x00 0x400000
    {
         *obigo03cadp.lib (+RO-CODE)
         *obigo03capp.lib (+RO-CODE)
         *obigo03clib.lib (+RO-CODE)
    }
    DEMAND_PAGING_ROM2 +0x00 
    {
         *obigo03cadp.lib (+RO-DATA)
         *obigo03capp.lib (+RO-DATA)
         *obigo03clib.lib (+RO-DATA)
    }
    DEMAND_PAGING_ROM4 +0x00 
    {
; mmiresource - Audio
         CustAdoMap.obj (+RO-DATA)
         CustAdoMapExt.obj (+RO-DATA)
    }
    DEMAND_PAGING_ROM5 +0x00 0x00400000
    {
; J2ME
         *jal.lib (+RO-CODE)
         *jal.lib (+RO-DATA)
;         *ijet_adp.lib (+RO-CODE) remove it according to MTK guide to fix java reset problem
         *ijet_adp.lib (+RO-DATA)
    }
    DYNAMIC_CODE12 0x50108c00 OVERLAY 0x3c00
    {
         * (MP4DEC2_DYNAMIC_ZI, MP4DEC2_DYNAMIC_RO)
    }
    DYNAMIC_CODE13 0x50108c00 OVERLAY 0x3c00
    {
         * (MP4ENC2_DYNAMIC_ZI, MP4ENC2_DYNAMIC_RO)
    }
    DYNAMIC_CODE14 0x50108c00 OVERLAY 0x3c00
    {
         * (264DEC2_DYNAMIC_ZI, 264DEC2_DYNAMIC_RO)
    }
    DYNAMIC_CODE15 0x5010c800 OVERLAY 0x2800
    {
         * (MP4DEC1_DYNAMIC_ZI, MP4DEC1_DYNAMIC_RO)
    }
    DYNAMIC_CODE16 0x5010c800 OVERLAY 0x2800
    {
         * (MP4ENC1_DYNAMIC_ZI, MP4ENC1_DYNAMIC_RO)
    }
    DYNAMIC_CODE17 0x5010c800 OVERLAY 0x2800
    {
         * (264DEC1_DYNAMIC_ZI, 264DEC1_DYNAMIC_RO)
    }
    DYNAMIC_CODE2 0x5010c800 OVERLAY 0x2800
    {
         * (G3D_DYNAMIC_ZI)
    }
    DYNAMIC_CODE1 0x5010f000 OVERLAY 0x5000
    {
         * (AMR515_DYNAMIC_ZI)
    }
    DYNAMIC_CODE11 0x5010f000 OVERLAY 0x5000
    {
         * (VRENGINE_DYNAMIC_ZI)
    }
    DYNAMIC_CODE3 0x5010f000 OVERLAY 0x5000
    {
         * (CTM_DYNAMIC_ZI)
    }
    DYNAMIC_CODE4 0x5010f000 OVERLAY 0x5000
    {
         * (G729_DYNAMIC_ZI)
    }
    DYNAMIC_CODE5 0x5010f000 OVERLAY 0x5000
    {
         * (SBC_DYNAMIC_ZI)
    }
}
;=========================================================================
; This load region must be behind all the protected load region
;=========================================================================
; 1. Only address is configurable.
; 2. Region address must be fixed address.
; 4. DO NOT modify load region order, load region naming and pragma naming!
;=========================================================================
__HIDDEN_SECURE_MAC 0x03fba000 0x00001000
{
    __HIDDEN_SECURE_MAC +0x0
    {
         *.obj (SECURE_MAC_SIZE)
    }
    __HIDDEN_SECURE_MAC_CONTENT +0x0
    {
         *.obj (SECURE_MAC_CONTENT)
    }
}

__HIDDEN_SECURE_RO 0x03fbb000 0x00001000
{
    SECURE_RO +0x0 
    {
         *.obj (SECURE_RO)
    }
}

__HIDDEN_FLASHTOOL_CFG 0x03fbc000 0x00001000
{
    __HIDDEN_FLASHTOOL_CFG +0x0 
    {
         *.obj (FLASHTOOL_CFG)
    }
}


