;=========================================================================
;                   CHMC. 
;                   NX9200 Script File.
;=========================================================================
;-------------------------------------------------------------------------
;  when       who        what, where, why
;--------    -------    --------------------------------------------------
;08/24/2006   sgho	 Chage pref_mode         {0, 4} 
;06/22/2006   mjkang     Add avr_earjack_enable
;06/04/2005   hgkim      Change QDSP value
;05/27/2005   hgkim      Change Battery Level
;05/18/2005   skgan      Change QDSP Sidetone value
;05/13/2005   hgkim      Change Ear/Beep volume level
;04/02/2006   hgkim      Add Preload Data Item
;03/29/2006   bhlim      Modify mms_uaprof_url value & Delete 1X data item
;03/28/2006   bhlim	 Modify MMS
;02/20/2006   hgkim      Modify    
;02/07/2006   hgkim      Modify Sound Alert Items    
;01/17/2006   jwlee      Add Data Items
;01/15/2006   hgkim      Add UI Items
;12/30/2005   hgkim      Add UI Items
;10/18/2005   bmkim      Created the initial script file.
;--------    -------    --------------------------------------------------
;                  
;

spc "000000"
wait 2
mode offline-d

wait 4



;=========================================================================
; SYSTEM ITEM
;=========================================================================
nv_write rf_config        {2}
nv_write slot_cycle_index {2}

nv_write accolc            {0, 0, 0}
nv_write accolc            {1, 0, 0}
                           
nv_write imsi_mcc          {0, "310"}                                 ; Mobile Country Code. Verizon = 310
nv_write imsi_mcc          {1, "310"}                                 ; Mobile Country Code. Verizon = 310
                           
nv_write imsi_11_12        {0, "00"}                                  ; Mobile network code
nv_write imsi_11_12        {1, "00"}                                  ; Mobile network code
                           
nv_write pref_mode         {0, 4}                                     ; Digital Only
nv_write pref_mode         {1, 4}                                     ; Digital Only
nv_write band_pref         {0, 0xffff}                                ; pref_any
nv_write band_pref         {1, 0xffff}                                ; pref_any
nv_write roam_pref         {0, 0xff}                                  ; pref_any
nv_write roam_pref         {1, 0xff}                                  ; pref_any
nv_write system_pref       {0, 5}                                     ; "Automatic b"
nv_write system_pref       {1, 5}                                     ; "Automatic b"

nv_write home_sid_nid      {0, 0, 2004, 65535}
nv_write home_sid_nid      {0, 1, 0, 0}
nv_write home_sid_nid      {0, 2, 0, 0}
nv_write home_sid_nid      {0, 3, 0, 0}
nv_write home_sid_nid      {0, 4, 0, 0}
nv_write home_sid_nid      {0, 5, 0, 0}
nv_write home_sid_nid      {0, 6, 0, 0}
nv_write home_sid_nid      {0, 7, 0, 0}
nv_write home_sid_nid      {0, 8, 0, 0}
nv_write home_sid_nid      {0, 9, 0, 0}
nv_write home_sid_nid      {0, 10, 0, 0}
nv_write home_sid_nid      {0, 11, 0, 0}
nv_write home_sid_nid      {0, 12, 0, 0}
nv_write home_sid_nid      {0, 13, 0, 0}
nv_write home_sid_nid      {0, 14, 0, 0}
nv_write home_sid_nid      {0, 15, 0, 0}
nv_write home_sid_nid      {0, 16, 0, 0}
nv_write home_sid_nid      {0, 17, 0, 0}
nv_write home_sid_nid      {0, 18, 0, 0}
nv_write home_sid_nid      {0, 19, 0, 0}

nv_write sid_nid_lock      {0, 0, 0,0}
nv_write sid_nid_lock      {0, 1, 0,0}
nv_write sid_nid_lock      {0, 2, 0,0}
nv_write sid_nid_lock      {0, 3, 0,0}
nv_write sid_nid_lock      {0, 4, 0,0}
nv_write sid_nid_lock      {0, 5, 0,0}
nv_write sid_nid_lock      {0, 6, 0,0}
nv_write sid_nid_lock      {0, 7, 0,0}
nv_write sid_nid_lock      {0, 8, 0,0}
nv_write sid_nid_lock      {0, 9, 0,0}

nv_write cdma_sid_lock     {0,  0, 0, 0, 0, 0, 0}
nv_write cdma_sid_lock     {1,  0, 0, 0, 0, 0, 0}

nv_write cdma_sid_acq      {0,  0, 0, 0, 0, 0, 0}
nv_write cdma_sid_acq      {1,  0, 0, 0, 0, 0, 0}

nv_write pcdmach           {0, 283, 384}                               ; A and B primary CDMA channels
nv_write pcdmach           {1, 283, 384}                               ; A and B primary CDMA channels

nv_write scdmach           {0, 691, 777}                               ; set only if secondary channels offered
nv_write scdmach           {1, 691, 777}                               ; set only if secondary channels offered

nv_write mob_term_home     {0, true, true}
nv_write mob_term_home     {1, true, true}

nv_write mob_term_for_sid  {0, true, true}
nv_write mob_term_for_sid  {1, true, true}

nv_write mob_term_for_nid  {0, true, true}
nv_write mob_term_for_nid  {1, true, true}

nv_write count             {0, 0}
nv_write count             {1, 0}

nv_write pref_voice_so     {0, 1, 0x0003, 0x0003, 0x0003}
nv_write pref_voice_so     {1, 1, 0x0003, 0x0003, 0x0003}

nv_write nam_chksum        {0, 0xffff}                                 ; NAM Checksums must all be 0xffff
nv_write nam_chksum        {1, 0xffff}                                 ; NAM Checksums must all be 0xffff




;=========================================================================
; OTA ITEM
;=========================================================================
nv_write otapa_enabled      {0, 1}
nv_write otapa_enabled      {1, 1}
nv_write nam_lock           {0, 1}
nv_write nam_lock           {1, 1}
nv_write spc_change_enabled {1}




;=========================================================================
; FW ITEM
;=========================================================================
nv_write cdma_rssi_val          {111, 104, 98, 88, 0, 0, 0, 0}         ; NV_CDMA_THREHOLD_RSSI_I
nv_write pcs_rssi_val           {110, 102, 95, 85, 0, 0, 0, 0}         ; NV_PCS_THREHOLD_RSSI_I?
nv_write hdr_cdma_rssi_val      {108, 97, 84, 70, 0, 0, 0, 0}          ; NV_HDR_THREHOLD_RSSI_I
nv_write hdr_pcs_rssi_val       {108, 97, 82, 70, 0, 0, 0, 0}          ; NV_HDR_PCS_THREHOLD_RSSI_I

nv_write battbar_tunning_idle   {88, 88, 122, 135, 147, 70, 4}
nv_write battbar_tunning_call   {85, 85, 118, 131, 143, 52, 4}
nv_write battbar_tunning_camera {86, 86, 120, 133, 145, 52, 4}




;=========================================================================
; UI MENU ( Display Settings ) ITEM 
;=========================================================================
nv_write banner                 {""}                                ; NX9200 -> VZW 로 변경
nv_write eri_banner             {0}                                    ; On
nv_write back_light             {7}                                    ; 7초
nv_write keypad_backlight       {7}                                    ; 7초
nv_write wallpaper              {7}                                    ; default Wallpaper
nv_write themes                 {0}                                    ; Default Theme
nv_write dial_fonts             {1}                                    ; Normal
nv_write iws_clock_format       {0, 0}                                 ; Digital, Digital 
nv_write power_saver            {0}                                    ; 2분

nv_write shortcut_key_type      {15}                                   ; Default Shortcut Key : Calender
nv_write language_selection     {0}                                    ; English
nv_write location_set_type      {1}                                    ; E911 
nv_write common_code_type       {0}                                    ; ON
nv_write lock                   {0}                                    ; UnLock
nv_write auto_lock              {off}                                  ; Power On Lock Off
nv_write location_lock          {0}
nv_write RestrictOff            {TRUE}                                 ; (Phone Set) Restrict Calls :: Code Enabled = FALSE, Code Disabled = TRUE
nv_write RestrictOutgoing       {0}                                    ; (Call Set) Restrict Calls :: Allow All = 0, Contacts Only & Data Calls = 1, No Calls
nv_write emergency_num1_type    {"911"} 
nv_write emergency_num2_type    {"*911"} 
nv_write emergency_num3_type    {"#911"}
nv_write curr_nam               {0}                                    ; NAM 1

nv_write auto_answer            {FALSE,0} 
nv_write phone_setup            {0} 
nv_write auto_redial            {0,0} 
nv_write tty                    {3}                                    ; Off
nv_write onetouch_dial          {1}                                    ; Off
nv_write voice_priv             {1}                                    ; On
nv_write ds_default_baudrate    {1}                                    ; 0:19200, 1:115200, 2:230400
nv_write cont_key_dtmf          {0}                                    ; 0: Normal
nv_write ringer_id              {0}                                    ; On
nv_write picture_id             {0}                                    ; On

nv_write avr_enable             {1}                                    ; default Enabled : Enabled(1)/Disable(0) NV_IWS_VR_ACTIVATION_I(6027) 
nv_write avr_earjack_enable     {1}                                    ; default Enabled : Enabled(1)/Disable(0) NV_IWS_AVR_EARJACK_ENABLE_I (6054) 
nv_write avr_choice_list        {0}                                    ; default Automatic : Automatic(0)/Off(2) NV_AVR_CHOICE_LIST_I(6028) 
nv_write avr_prompts_mode       {0}                                    ; default Prompts : Prompts(0)/Readout(1)/Tones Only(2) NV_AVR_PROMPTS_MODE_I (6030) 
nv_write avr_prompts_timeout    {0}                                    ; default 5 Seconds : 5 Seconds(0)/10 Seconds(1) NV_AVR_PROMPTS_TIMEOUT_I(6031) 
nv_write avr_call_alerts        {0}                                    ; default Ring Only : Ring Only(0)/Name+Ring(1)/Name Repeat(2) NV_AVR_CALL_ALERTS_I(6033) 

nv_write qdsp_snd_ctrl          {120, 5700, 27000, 25000, 1000, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}

nv_write audio_adj_phone        {0, 0, 0, 0, 0, 0} 
nv_write audio_adj_earjack      {0, 0, 0, 0, 0, 0} 
nv_write audio_adj_spk          {0, 0, 0, 0, 0, 0} 
nv_write threshold_level        {57} 

;<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<< Description Start
; 0(Off)
; 1(Low)
; 2(Med Low)
; 3(Med)
; 4(High Med)
; 5(High)
; 98(High & Vib)
; 99(Vibrate)
;>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>> Description End
nv_write ringer_lvl             {0x0F}
nv_write beep_lvl               {0x0F}
nv_write ear_lvl                {0x0F}
nv_write speaker_lvl            {0x0B}
nv_write ringer_spkr_lvl        {0x0B}
nv_write beep_spkr_lvl          {0x0B}
nv_write beep_lvl_shadow        {0x0B}
nv_write ear_lvl_shadow         {0x0B}

 
nv_write setting_sound_call      {91, 1, 3}       ;NV_IWS_SETTING_SOUND_CALL_I: RING ID(91),VIB_OFF(1),Reminder(Off) 
nv_write setting_sound_txtmsg    {90, 1, 3}       ;NV_IWS_SETTING_SOUND_TXTMSG_I: NEW MESSAGE, VIB_OFF(1), Reminder(Off)
nv_write setting_sound_pixflix   {90, 1, 3} 	  ; NV_IWS_SETTING_SOUND_PIXFLIX_I: NEW MESSAGE
nv_write setting_sound_voicemail {90, 1, 3} 	  ; NV_IWS_SETTING_SOUND_VOICEMAIL_I: NEW MESSAGE
nv_write setting_sound_alarm     {91, 1, 3} 	  ; NV_IWS_SETTING_SOUND_ALARM_I: VZW Default Tone

nv_write radio_data_context_type {1,1,1,1,1}                           ; eri(off), minute(off), call_connect(off), power_on (off), power_off (off)

nv_write wclock_choice           {47}                                  ; World Time Default City : NewYork




;=========================================================================
; BREW ITEM 
;=========================================================================
nv_write brew_carrier_id     {200}                                     ; NV_BREW_CARRIER_ID_I(1977)
nv_write brew_platform_id    {14006}                                   ; NV_BREW_PLATFORM_ID_I(1978)
nv_write brew_bkey           {00000000000000000000000000000000}        ; NV_BREW_BKEY_I(1979)
nv_write brew_download_flags {4}                                       ; NV_BREW_DOWNLOAD_FLAGS_I(1981)
nv_write brew_auth_policy    {1}                                       ; NV_BREW_AUTH_POLICY_I(1982)
nv_write brew_privacy_policy {3}                                       ; NV_BREW_PRIVACY_POLICY_I(1983)

nv_write mim_clsid      	{0x01013d82}    		       ; NV_BREW_MIM_CLSID_I(5709)
nv_write vod_clsid      	{0x0606060e}    		       ; NV_BREW_VOD_CLSID_I(5708)
                                 
nv_write brew_ads_url1       	{"apps.myvzw.com"}                     ; NV_BREW_ADS_URL1_I(5701)
nv_write brew_ads_url2       	{"apps2.myvzw.com"}                    ; NV_BREW_ADS_URL2_I(5702)

;=========================================================================
; VOD APPLICATION 
;=========================================================================

efs_write "brew/mif/12513.mif"
efs_write "brew/mif/13478.mif"
efs_write "brew/mod/12513/catalog.bar"
efs_write "brew/mod/12513/red_assets240x320.bar"
efs_write "brew/mod/12513/verizonmediaplayer.mod"
efs_write "brew/mod/12513/verizonmediaplayer.sig"
efs_write "brew/mod/12513/vzwresource240x320.bar"
efs_write "brew/mod/13478/mediaasf.mod"
efs_write "brew/mod/13478/mediaasf.sig"

;=========================================================================
; Mobile IM APPLICATION 
;=========================================================================
efs_write "brew/mif/4972.mif"
efs_write "brew/mod/4972/aimmsg.mid"
efs_write "brew/mod/4972/aimol.mid"
efs_write "brew/mod/4972/aimsys.mid"
efs_write "brew/mod/4972/ins_aol"
efs_write "brew/mod/4972/ins_aol_msg"
efs_write "brew/mod/4972/ins_conf"
efs_write "brew/mod/4972/ins_msn"
efs_write "brew/mod/4972/ins_msn_msg"
efs_write "brew/mod/4972/ins_yahoo"
efs_write "brew/mod/4972/ins_yahoo_msg"
efs_write "brew/mod/4972/mobileim.bar"
efs_write "brew/mod/4972/mobileim.mod"
efs_write "brew/mod/4972/mobileim.sig"
efs_write "brew/mod/4972/msnmsg.mid"
efs_write "brew/mod/4972/msnol.mid"
efs_write "brew/mod/4972/yahoomsg.mid"
efs_write "brew/mod/4972/yahoool.mid"


;=========================================================================
; SMS ITEM 
;=========================================================================
nv_write sms_mo_so               {0}                                   ; 0(SO 6), 1(SO 14)
nv_write sms_mo_access           {1}                                   ; 0(Access CH), 1(Traffic CH)
nv_write wms_auto_erase_inbox    {1}                                   ; 0(On), 1(Off)
nv_write wms_auto_save_sent_msg  {0}                                   ; 0(On), 1(Off)
nv_write sms_mo_l3_ack           {0}                                   ; 0(L3 Ack On), 1(L3 Ack Off)




;=========================================================================
; MMS ITEM 
;=========================================================================
nv_write mms_server_name          {0, "mms.vtext.com", 13}             ; NV_MMS_SERVER_NAME_I(5301)
nv_write mms_server_name          {1, "vzpix.com", 9}                  ; NV_MMS_SERVER_NAME_I(5301)
nv_write mms_server_name          {2, "pix.vtext.com", 13}             ; NV_MMS_SERVER_NAME_I(5301)
nv_write mms_pixplace_shortcode   {438749}                             ; NV_MMS_PIXPLACE_SHORTCODE_I(5302)
nv_write mms_enable_callback_num  {0}                                  ; NV_MMS_ENABLE_CALLBACK_NUM_I(5303)
                                                                       ; 0 (ON), 1 (OFF)
nv_write mms_authorization_mode   {0}                                  ; NV_MMS_AUTHORIZATION_MODE_I(5305)
                                                                       ; 0 (Commercial), 1 (LAB)
nv_write mms_enable_auto_receive  {0}                                  ; NV_MMS_ENABLE_AUTO_RECEIVE_I(5310) : 0(ON), 1(OFF)
nv_write mms_retries_num          {3}                                  ; NV_MMS_RETRIES_NUM_I(5306) : 0, 1, 2, 3
nv_write mms_no_resp_timeout_time {0}                                  ; NV_MMS_NO_RESP_TIMEOUT_TIME_I(5308) : 0(60s),1(120s),2(180s),3(240s),4(300s)
nv_write mms_enable_delivery_ack  {0}                                  ; NV_MMS_ENABLE_DELIVERY_ACK_I(5309) : 0(ON), 1(OFF)
nv_write mms_uaprof_url {"http://uaprof.vtext.com/utstar/gz1/gz1v1.xml"}
                                                                       ; NV_MMS_UAPROF_URL_I(5307) -> Verizon will define.




;=========================================================================
; Browser (Hidden Menu) ITEM : 
;=========================================================================
nv_write browser_pxlocal_pxaddr_fqdn {0, "gw.vzwwap.com", 13}          ; Primary Server URL
nv_write browser_pxlocal_pxaddr_fqdn {1, "gw1.vzwwap.com", 14}         ; Secondary Server URL
nv_write browser_pxlocal_portnbr     {"8080", 4}                       ; Gateway Port Number
nv_write browser_pxlocal_pxauth_id   {"0000000000", 10}                ; User Name (현재 값 없음. PRI는 MIN)
nv_write browser_pxlocal_pxauth_pw   {"vzw", 3}                        ; Password
nv_write browser_homepage            {"http://homepage", 15}           ; Homepage
nv_write browser_wappush_sl          {2}                               ; Service Load (Allow=0, Deny=1, Confirm=2)


;=========================================================================
; MMS Preload 데이터(Image & Sound).
;=========================================================================

efs_write "MMS/MEDIA/DRMFUNLOCKED/Image/cool.bmp"
efs_write "MMS/MEDIA/DRMFUNLOCKED/Image/flower.bmp"
efs_write "MMS/MEDIA/DRMFUNLOCKED/Image/sick.bmp"
efs_write "MMS/MEDIA/DRMFUNLOCKED/Image/smiley.bmp"
efs_write "MMS/MEDIA/DRMFUNLOCKED/Image/what.bmp"

efs_write "MMS/MEDIA/DRMFUNLOCKED/Sound/clapping.mid"
efs_write "MMS/MEDIA/DRMFUNLOCKED/Sound/crowd roar.mid"
efs_write "MMS/MEDIA/DRMFUNLOCKED/Sound/happy birthday.mid"
efs_write "MMS/MEDIA/DRMFUNLOCKED/Sound/rainforest.mid"
efs_write "MMS/MEDIA/DRMFUNLOCKED/Sound/train.mid"


;=========================================================================
; MIP Publick KEY
;=========================================================================
efs_write "DMU/10.key"

;=========================================================================
; MIP Publick KEY
;=========================================================================
efs_write "Version.txt"


;=========================================================================
; IOT 인증용 ITEM.
;=========================================================================
;nv_write browser_uaprof             {"http://uaprof.vtext.com/utstar/gz1/gz1v1.xml", 44}     ; NV_BROWSER_UAPROF_I(5515)
;nv_write browser_domain_trust       {"http:.openwave.com", 18}                               ; NV_BROWSER_DOMAIN_TRUST_I(5516)
;nv_write browser_add_favorite_url   {"http://mw2.vzwwap.com/addfavorite", 33}                ; NV_BROWSER_ADD_FAVORITE_URL_I(5542)
;nv_write browser_search_url         {"http://mw2.vzwwap.com/search", 28}                     ; NV_BROWSER_SEARCH_URL_I(5543)
;nv_write browser_go_to_url          {"http://mw2.vzwwap.com/goto", 26}                       ; NV_BROWSER_GO_TO_URL_I(5544)
;nv_write browser_news_and_info_url  {"http://mw2.vzwwap.com/newsandinfo", 33}                ; NV_BROWSER_NEWS_AND_INFO_URL_I(5545)
;nv_write browser_email_url          {"http://mw2.vzwwap.com/email", 27}                      ; NV_BROWSER_EMAIL_URL_I(5546)
;nv_write browser_chat_url           {"http://mw2.vzwwap.com/chat", 26}                       ; NV_BROWSER_CHAT_URL_I(5547)
;nv_write browser_pix_place_url      {"http://mw2.vzwwap.com/pixplace", 30}                   ; NV_BROWSER_PIX_PLACE_URL_I(5548)
;nv_write browser_my_account_url     {"http://myacc.vzwwap.com/selfServe/forms/myacc.jsp" 49} ; NV_BROWSER_MY_ACCOUNT_URL_I(5549)

;nv_write mms_1x_data                {0, "0000000000@vzw3g.com", 20}                          ; NV_MMS_1X_DATA_I(5304)
;nv_write mms_1x_data                {1, "vzw", 3}                                            ; NV_MMS_1X_DATA_I(5304)
;nv_write mms_1x_data                {2, "hlrtest@vzwtest.com", 19}                           ; NV_MMS_1X_DATA_I(5304)
;nv_write mms_1x_data                {3, "vzwtest", 7}                                        ; NV_MMS_1X_DATA_I(5304)

;nv_write imsi_t_mcc                 {0, "310"}
;nv_write imsi_t_mcc                 {1, "310"}
;nv_write imsi_t_11_12               {0, "00"}
;nv_write imsi_t_11_12               {1, "00"}
;nv_write imsi_t_addr_num            {0, 0}
;nv_write imsi_t_addr_num            {1, 0}
;nv_write imsi_t_s1                  {0, "0000000", "0000000"}
;nv_write imsi_t_s1                  {1, "0000000", "0000000"}
;nv_write imsi_t_s2                  {0, "000", "000"}
;nv_write imsi_t_s2                  {1, "000", "000"}
;nv_write imsi_addr_num              {0, 0xff}
;nv_write imsi_addr_num              {1, 0xff}

;nv_write mru2_table {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0}
;nv_write mru2_table {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0}

;nv_write a_key      {0, 0x00000000, 0x00000000 }                           ; Authentication NAM items
;nv_write a_key      {1, 0x00000000, 0x00000000 }                           ; Authentication NAM items
                     
;nv_write ssd_a      {0, 0x00000000, 0x00000000 }                           ; SSD_Asp
;nv_write ssd_a      {1, 0x00000000, 0x00000000 }                           ; SSD_Asp
                     
;nv_write ssd_b      {0, 0x00000000, 0x00000000 }                           ; SSD_Bsp
;nv_write ssd_b      {1, 0x00000000, 0x00000000 }                           ; SSD_Bsp

;nv_write min_chksum {0, 0xffff, 0xffff}
;nv_write min_chksum {1, 0xffff, 0xffff}


;nv_write data_qnc_enabled           { false }                         ; { boolean_string }
;nv_write data_mdr_mode              { 3 }                             ; { byte }
;nv_write ds_qcmip                   { 1 }                             ; { byte }
;nv_write ds_mip_retries             { 2 }                             ; { byte }
;nv_write ds_mip_retry_int           { 3 }                             ; { byte }
;nv_write ds_mip_pre_re_rrq_time     { 0 }                             ; { byte }
;nv_write ds_mip_num_prof            { 1 }                             ; { byte }
;nv_write ds_mip_2002bis_mn_ha_auth  { true }                          ; { boolean_string }
;nv_write ds_mip_qc_drs_opt          { true }                          ; { boolean_string }
;nv_write ds_mip_dmu_pkoid           {0, 10}                           ; {index, byte}
;nv_write ds_mip_rm_nai              {0, 24, "0000000000@dun.vzw3g.com"}  ; {length, nai}

;<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<< Description Start
;Each index Value Range : 0~5
;01st index : index number
;02nd index : nai_length
;03rd index : nai
;04th index : mn_ha_spi_set
;05th index : mn_ha_spi
;06th index : mn_aaa_spi_set
;07th index : mn_aaa_spi
;08th index : rev_tun_pref
;09th index : home_addr
;10th index : primary_ha_addr
;11th index : secondary_ha_addr
;>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>> Description End
;nv_write ds_mip_gen_user_prof        { 0, 20, "0000000000@vzw3g.com", true, 0x12c, true, 0x2, true, 0x00000000, 0xffffffff, 0xffffffff }


;<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<< Description Start
;Each index Value Range : 0~5
;01st index : index number
;02nd index : mn_ha_shared_secret_length
;03rd index : mn_ha_shared_secret
;04th index : mn_aaa_shared_secret_length
;05th index : mn_aaa_shared_secret
;>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>> Description End
;nv_write ds_mip_ss_user_prof         { 0, mn_ha_shared_secret_length, "mn_ha_shared_secret", mn_aaa_shared_secret_length, "mn_aaa_shared_secret" }


;nv_write ds_mip_dmu_mn_auth          {0,0x01,0xb2,0x07}                ; {index,byte,byte,byte}
;nv_write primary_dns                 { 0x00000000 }                    ; { dword }
;nv_write secondary_dns               { 0x00000000 }                    ; { dword }
;nv_write ppp_user_id                 {20, "0000000000@vzw3g.com"}      ; { length, nai }
;nv_write ds_sip_rm_nai               {24, "0000000000@dun.vzw3g.com"}  ; { length, nai }
;nv_write data_pkt_orig_str           { 5, "#777" }                     ; { length, digits }
;nv_write data_scrm_enabled           { true }                          ; { boolean_string }
;nv_write data_trtl_enabled           { true }                          ; { boolean_string }
;nv_write data_auto_packet_detection  { 0 }                             ; { byte }
;nv_write pref_for_rc                 { 3 }                             ; { word }
;nv_write data_so_set                 { 2 }                             ; { byte }
;nv_write hybrid_pref                 { 1 }                             ; { byte }
;nv_write pref_mode                   { 0, 1 }                          ; { nam, mode }
;nv_write hdr_an_auth_user_id_long    { 20, "0000000000@vzw3g.com" }    ; { length, nai }

;nv_write hdr_an_auth_passwd_long     { length, "nai"}                   ; { length, nai }
;nv_write ppp_password                { length, "nai"}                   ; { length, nai }

;================================================================================================
; CAMERA & CAMCODER
;================================================================================================
nv_write Resolution {5}
nv_write Shutter_Sound {0}
nv_write Color_Effects{1}
nv_write PIX_Brightness_Contrast{5}
nv_write PIX_White_Balance {1}
nv_write FLIX_Brightness_Contrast{5}
nv_write FLIX_White_Balance {1}

wait 1

mode reset

