;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;=========================================================================
;  File name: AX260.SCR
;  Made by  : LGE
;  Date     : 06/15/2007
;-------------------------------------------------------------------------
;  when         who        what
;----------    -------    ------------------------------------------------
;06/15/2007      mmkim      Created the initial script file. 




;-------------------------------------------------------------------------
;spc "000000"                                               ; does not need at LGDP DLL
;wait 2
mode offline-d
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model
wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================
nv_write name_nam           {0, "NAM1"}
nv_write name_nam           {1, "NAM2"}
nv_write nam_chksum         {0, 0xffff}
nv_write nam_chksum         {1, 0xffff}
nv_write min_chksum         {0, 0xffff, 0xffff}
nv_write min_chksum         {1, 0xffff, 0xffff}

nv_write imsi_mcc           {0, "311"}
nv_write imsi_mcc           {1, "311"}
nv_write imsi_11_12         {0, "27"}
nv_write imsi_11_12         {1, "27"}
nv_write min1               {0, "000-0000", "000-0000"}
nv_write min1               {1, "000-0000", "000-0000"}
nv_write min2               {0, "000", "000"}
nv_write min2               {1, "000", "000"}
nv_write imsi_addr_num      {0, 255}
nv_write imsi_addr_num      {1, 255} 
nv_write dir_number_pcs     {0, "0000000000"}
nv_write dir_number_pcs     {1, "0000000000"}
nv_write accolc             {0, 0, 0}
nv_write accolc             {1, 0, 0}

nv_write imsi_t_mcc         {0, "311"}               
nv_write imsi_t_mcc         {1, "311"}
nv_write imsi_t_11_12       {0, "27"}
nv_write imsi_t_11_12       {1, "27"}
nv_write imsi_t_s1          {0, "000-0000", "000-0000"}
nv_write imsi_t_s1          {1, "000-0000", "000-0000"}
nv_write imsi_t_s2          {0, "000", "000"}
nv_write imsi_t_s2          {1, "000", "000"}
nv_write imsi_t_addr_num    {0, 255}
nv_write imsi_t_addr_num    {1, 255}

nv_write pref_mode          {0, "automatic"}
nv_write pref_mode          {1, "automatic"}
nv_write band_pref          {0, "pref_any"}
nv_write band_pref          {1, "pref_any"}
nv_write roam_pref          {0, "pref_any"}
nv_write roam_pref          {1, "pref_any"}
nv_write system_pref        {0, "automatic b"}
nv_write system_pref        {1, "automatic b"}

nv_write prl_enabled        {0, 1}
nv_write prl_enabled        {1, 1}

nv_write home_sid_nid       {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write home_sid_nid       {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock       {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock       {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}

nv_write pcdmach            {0, 283, 384}
nv_write pcdmach            {1, 283, 384}
nv_write scdmach            {0, 691, 777}
nv_write scdmach            {1, 691, 777}

nv_write mru2_table         {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru2_table         {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};

nv_write mob_term_home      {0, true, true}
nv_write mob_term_home      {1, true, true}
nv_write mob_term_for_sid   {0, true, true}
nv_write mob_term_for_sid   {1, true, true}
nv_write mob_term_for_nid   {0, true, true}
nv_write mob_term_for_nid   {1, true, true}

nv_write pref_voice_so      {0,  1, 0x0003, 0x0003, 0x0003} ; EVRC Capable, Home Page SO, Home Orig SO, Roam Orig SO
nv_write pref_voice_so      {1,  1, 0x0003, 0x0003, 0x0003}
nv_write cdma_so68_enabled  {1}                        ; 4GV
nv_write pref_for_rc        {3}      

nv_write slot_cycle_index   {2}

nv_write lock_code          {"0000"}
nv_write sec_code           {"000000"}
nv_write fsc                {"000000"}

;=========================================================================
; OTA ITEM
;=========================================================================
nv_write nam_lock           {0, 0}
nv_write nam_lock           {1, 0}
nv_write otapa_enabled      {0, 1}
nv_write otapa_enabled      {1, 1}
nv_write spc_change_enabled {1}

;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key              {0, 0x00000000, 0x00000000 }
nv_write a_key              {1, 0x00000000, 0x00000000 }
nv_write ssd_a              {0, 0x00000000, 0x00000000 }
nv_write ssd_a              {1, 0x00000000, 0x00000000 }
nv_write ssd_b              {0, 0x00000000, 0x00000000 }
nv_write ssd_b              {1, 0x00000000, 0x00000000 }
nv_write count              {0, 0}
nv_write count              {1, 0}

nv_write voice_priv         {0}	  ; 0=Standard  1=Enhanced
;=========================================================================
;UI ITEM
;=========================================================================
;Volume
nv_write ringer_lvl          	{0x4}     ; 0(Silent All), 1(Vibrate All), 2(Level 1), 3(Level 2), 4(Level 3), 5(Level 4), 6(Level 5)
nv_write beep_lvl             {0x4}     ; 0(Off), 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5)
nv_write ear_lvl              {0x4}     ; 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5)
;nv_write speaker_level          {0x4}     ; 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5)
nv_write ringer_spkr_lvl        {0x4}     ; 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5)
nv_write beep_spkr_lvl          {0x4}     ; 0(Off), 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5)
nv_write beep_lvl_shadow        {0x4}     ; 0(Off), 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5)
nv_write ear_lvl_shadow         {0x4}     ; 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5)
nv_write spk_phone_beep_lvl 	{0x4}     ; 0(Off), 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5)
nv_write speaker_shadow 	{0x4}     ; 0(Off), 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5)
nv_write beep_bt_lvl            {0x4}     ; 0(Off), 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5)
nv_write ear_bt_lvl		{0x4}     ; 1(Level 1), 2(Level 2), 3(Level 3), 4(Level 4), 5(Level 5), 6(Level 6), 7(Level 7), 8(Level 8)
;System Setting
nv_write auto_nam               {off}     ; Auto NAM              == disable
nv_write curr_nam               {0}       ; Current NAM           == NAM 1
nv_write pc_port        	{0}       ; PC connection port  0 (USB Modem), 1 (USB Drive), 2 (UART), 3 (BLUETOOTH), 4 (CLOSED)
nv_write location_set 	{0}	  ; 1 -> location on 0-> E911 only

;Call Settings
nv_write auto_answer            {0, 0}    ; Auto answer           == off
nv_write auto_redial            {0, 0}    ; Auto redial           == off;?????????????
nv_write onetouch_dial          {on}      ; One touch dial        == enable!
nv_write auto_volume_enabled    {0}       ; 0-> off , 1-> on
nv_write stand_alone_mode 	{0}       ; 0 default OFF, 1 ON
nv_write tty                    {3}       ; TTY Full(0), TTY+TALK(1),TTY+HEAR(2),TTY off(3)

;Security
nv_write call_rstrc             {0}    ; Restrict(0:off, 1:on) 
nv_write lock                   {off}     ; phone lock            == Unlocked \ now
nv_write auto_lock              {off}     ; phone lock            == Unlocked \ Power_up
nv_write emergency_num1		{"911"}	  ; Up to 48 Digits
nv_write emergency_num2		{"611"}	  ; Up to 48 Digits
nv_write emergency_num3		{"*611"}  ; Up to 48 Digits	

;Display 
nv_write banner         	{"",0}            ; Banner 
nv_write sub_banner     	{"",0}            ; Sub Banner
nv_write back_light             {10}       ; Backlight          change from 7 sec to 10 sec
;nv_write sub_back_light         {7}      ; Sub Backlight         == after 7secs (10 -> 7, by bhjo 02.08.28) AX8600: change from 7 sec to 3 sec
nv_write key_light      	{10}       ;Keylight 		change from 7 sec to 10 sec
nv_write language_selection     {0}       ; Default (English/Spanish/French/Portuguese) == English
nv_write edit_font 	{0,0}
nv_write display_set 	{2,0,0}   ; front clock(0:Normal), main clock(0:Normal), color theme(0:default)
nv_write manner_mode 	{0}       ; 0(false), 1(true)
nv_write number_size	{1,0}	  ; size(0:Normal, 1:Large), style(0:Arial,1:Edge,2:Script,3:HYSerif)
nv_write wallpaper_main 	{0,0,3,""}      ; wallpaper {location_type(0:phone memory 1:phone efs 2:sdcard), location_id(0:sdcard id), item_id(1: index), item_path(NULL: path)}
nv_write wallpaper_sub  	{0,0,0,""}      ; wallpaper {location_type(0:phone memory 1:phone efs 2:sdcard), location_id(0:sdcard id), item_id(1: index), item_path(NULL: path)}

;Sound
nv_write backtop_beep     {true}    ; Back To Top Sound == on       
nv_write call_connect_alert     	{false}   ; Call connect alert    == off
nv_write logo_melody       {1}       ; 1(On), 0(Off)
nv_write sound_ringers 	{9,14,5,0,0xffff,0}  ; Caller ID(Welcome Back), No Caller ID(Happycall), Restricted Calls(Moody Viny), Roam Calls(None)--NOT USED, All Calls(None), Vibrate Alert(Off)
nv_write silence_all 	{0}       ; 0(sound on), 1(sound off)
nv_write sound_alerts 	{0,0,0,0} ; ( Service Change, Minute Beep, Call Connect, ERI alert)
nv_write lowbatt_sound		{1}	  ; 0 (Announce), 1(Tone)

;Add for one-Beep DNguyen
;nv_write  one_beep   		{0}       ; 0(one_beep off), 1(one_beep on)

;MISC  setting
nv_write cont_key_dtmf          {1}       ; key tone length      == 1: Normal, 0: Long  2: Off  (NEW) ; there is no menu in settings
nv_write power_saver            {0}
nv_write eri_text_onoff 	{1}             ; 1 -> On, 0 -> Off
nv_write lg_carrier_id     {1}       ; 0(Alltel), 1(USC), 2(MetroPCS), 3(BP) 
nv_write gps_test_num      {"922"}    ; Up to 48 Digits
nv_write emer_test_num     {"911"}    ; Up to 48 Digits

;AVT Setting
nv_write best_match          	{1}        ; 0: 1best match, 1: 4 best match
nv_write announce_alerts	{0}		; 0: Disable, 1:Announce, 2:Announce + Ring

;Bluetooth Power
nv_write bt_power_onoff      	{0}        ; 0 for bluetooth module off, 1 for bluetooth module on -> default 0 (off)

;camera setting
nv_write dcam_photo_setting_RQS  	{1,1,1,0,0}   ; (photo_set_Resolution,photo_set_Quality,photo_set_ShutterSound,photo_set_Brightness,photo_set_reverse)
nv_write dcam_video_setting_RQ (0) ; (video_set_Resolution)
nv_write media_save_option   	{0,0,0}    ; 0 : Phone memory(Default),  1: SD card memory

;Worlclock Setting
nv_write wclock_choice  	{30,0,46,""}     ; default New York {46,0} 

;Need change DLL(Crystal)
nv_write phone_setup       {0,0,14,0,0,"",""}   ;(pim_id,form_id,shortcut_form_index,isModal,modalType,mymenu_level1_index[12],mymenu_level2_index[12)
nv_write call_answer_options 	{0}
nv_write alarm_vibrate		{0}
nv_write sch_vibrate		{0}

;=========================================================================
; Merge From VX 86000
;=========================================================================

nv_write avr_callalerts          {0}
nv_write avr_prompts_mode         {0}
nv_write avr_choicelist          {0}
nv_write avr_prompts_timeout      {0}
nv_write avr_sensitivity          {1}
nv_write touch_sensitivity       {2}                     ; Super(0), High(1), Medium(2), Low(3)


;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_pkt_orig_str      {5, "#777"}    ; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_mdr_mode          {3}            ; Service Option 33 (1x channel) = 3 Use only low-speed packet data = 2
nv_write data_auto_packet_detection {0}        ; 0-Disable   1-Enable
nv_write data_so_set            {0}            ; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write diag_default_baudrate  {0x000e}       ; 0x000e(38.4kbps), 0x0011(115.2kbps) 
nv_write data_qnc_enabled       {0}            ; 0-QNC Disable  1-QNC Enable (alltel doesn't support QNC anymore.)
nv_write ppp_user_id            {0,""}         ; Max of 127 chars in User ID : ""값이 쓰여지면 폰에서 reset시에 0000000000@alltel.net 로  쓰여진다
nv_write ppp_password           {0,""}       ;  ""값이 쓰여지면 폰에서 reset시에 alltel 로  쓰여진다
nv_write data_scrm_enabled      {1}            ; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled      {1}            ; 0-TRTL Disable 1-TRTL Enable
nv_write ds_default_baudrate    {0x0011}       ; 0x0000 (19.2kbps),0x0011(115.2kbps)
nv_write ds_qcmip               {1}            ; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only
nv_write ds_mip_active_prof     {0}            ; current active profile index
nv_write ds_mip_enable_prof     {1,1,0,0,0,0}  ; diable - 0, enable - 1 {1st Profile, 2nd Profile, 3rd Profile, .... }
nv_write ds_mip_retries         {2}            ; number of retries
nv_write ds_mip_retry_int       {8}            ; retry interval = n*250(ms) + 1000ms (3 sec)
nv_write ds_mip_pre_re_rrq_time {10}            ; pre-registration time - minute
nv_write ds_mip_num_prof        {2}            ; number of profiles (max 6) 
nv_write ds_mip_2002bis_mn_ha_auth  {0}        ; disable - 0, enable -1
nv_write ds_mip_qc_drs_opt      {1}            ; dormant handoff optimization. disable - 0, enable - 1
                                               ; Comment : MIP general profile information {index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
                                               ; Comment : reverse tunneling, home address, primary ha address, secondary ha address}
nv_write ds_mip_gen_user_prof {0,0,"",1,257,1,1000,1,0x00000000,0x00000000,0x00000000}
nv_write ds_mip_gen_user_prof {1,0,"",1,257,1,1000,1,0x00000000,0x00000000,0x00000000}
;DNS IP Settings not supporting any more
;nv_write primary_dns            {0xA666A520}     ;Alltel DNS spec. Server IP = 166.102.165.11 -> 166.102.165.32
;nv_write secondary_dns          {0xCF5B0520}     ;Alltel DNS spec. Server IP = 166.102.165.13 -> 207.91.5.32

;Alltel doesn't use DMU.
;nv_write ds_mip_dmu_pkoid       {0,10}         ; { Index , Public key organization indentifier }
;nv_write ds_mip_dmu_mn_auth     {0,0x01,0xB2,0x07}            ; { Index , DMU MN authenticator - 111111base10 } 

;1X model...
;nv_write hdr_an_auth_user_id_long {0,""}       ; { Length , EVDO AN authetication user id }
nv_write dun_cable_mode         {1}            ; 0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode            {1}            ; 0=disable bt dun,1=enable bt dun

					       ; Comment : MIP&SIP NAI(Network Access Identifier) for DUN 
nv_write ds_mip_rm_nai {0,0,""}	               ;	{index,nai_length,nai}:  ""값이 쓰여지면 폰에서 reset시에 0000000000@alltel.net 로  쓰여진다					       
nv_write ds_sip_rm_nai {0,""}		       ;	{nai_length,nai} : ""값이 쓰여지면 폰에서 reset시에 0000000000@alltel.net 로  쓰여진다

nv_write alltel_fallback_flag          {1}            ; 0 - Auto , 1 - 1X , 2 - QNC  - 1x로 하자. 
;----------------------------------------------------------------------
nv_write ppp_carrier            {2}            ; 0-Verizon 1-USC 7-SCRIPT. Test NV Item.  
;efs write "DMU/10.key"		               ; MIP DMU(Dynamic Mipkeys Update) key file

;CS DLL don't write this item
;remove the ppp password setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
;nv_write ppp_password          {16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}      

;CS DLL don't write this item 
;{0~5(index),16(mn_ha_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,
;16(mn_aaa_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
;remove the ds_mip_ss_user_prof setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;nv_write ds_mip_ss_user_prof {0,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}

;CS DLL don't write this item 
;Comment : remove the hdr_an_auth_passwd_long setting in script file. (Becuase it uses ppp_password value that changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
; 1X model..
;nv_write hdr_an_auth_passwd_long  {0,""}

;=========================================================================
; MSG ITEM
;=========================================================================
nv_write msg_settings_auto_save         {0}     ; MSG_AUTO_SAVE(0), MSG_PROMPT(1), MSG_DO_NOT_SAVE(2)
nv_write msg_settings_auto_delete       {0}     ; 0(Off), 1(On)
nv_write msg_settings_entry_mode        {1}     ; MSG_T9EN(0), MSG_ABC(1), MSG_123(2)
nv_write msg_settings_vibrate_alert   {0} ; On(1), Off(0)
;nv_write msg_settings_speed_messaging	{1}		; On(1), Off(0)

;=========================================================================
; SMS ITEM
;=========================================================================
nv_write sms_priority_sel 		{0}             ; 0(Normal), 1(Urgent)
nv_write sms_mo_so 			{1}             ; 0(8K), 1(13K) -> 1(8K), 0(13K) 
nv_write sms_mo_l3_ack 			{1}             ; 0(Off), 1(On)
nv_write sms_default_cb 	{1}     ; 0(Off), 1(On)
nv_write sms_orig_msg_id  		{1}             ; 0x00 - 0xFFFF  
nv_write sms_mo_max_userdata 		{160}           ; 0x0(=180) - 0xFFFF	; 180 -> 170 (by eklee 02.08.22)
nv_write sms_signature_sel 	{0}     ; 0(None), 1(Custom)
nv_write sms_directview_sel 	{0}     ; 0(Off), 1(On)
nv_write sms_voicemail_alert	{26}     ;0~33(Audio Tones)- Low Beep Once(0), Low Beeps(1),Loud Beep Once(2), Loud Beeps(3), Ring1~10(4~13), No Ring(14)
nv_write sms_textmsg_alert	{25}     ;0~33(Audio Tones)- Low Beep Once(0), Low Beeps(1),Loud Beep Once(2), Loud Beeps(3), Ring1~10(4~13), No Ring(14)
nv_write sms_email_alert       {30}     ; 0~33(Audio Tones) - Low Beep Once(0), Low Beeps(1),Loud Beep Once(2), Loud Beeps(3), Ring1~10(4~13), No Ring(14)
nv_write sms_page_alert        {30}     ; 0~33(Audio Tones)- Low Beep Once(0), Low Beeps(1),Loud Beep Once(2), Loud Beeps(3), Ring1~10(4~13), No Ring(14)
nv_write sms_all_alert        	{0xFFFF}     ; Low Beep Once(0), Low Beeps(1),Loud Beep Once(2), Loud Beeps(3), Ring1~10(4~13), No Ring(14)
nv_write sms_2min_alert_sel           	{3} ; Once(0), Every 2 Minutes(1), Every 15 Minutes(2), Off(3)
nv_write sms_cb			{0, ""}      ; sms_call_back
;=========================================================================
; EMS ITEM
;=========================================================================
nv_write sms_ems_enable               {on}  ; On(1), Off(0)    
nv_write sms_auto_play       {off} ; On(1), Off(0)
;nv_write sms_ems_seg_num        {10}        ; 1~20 
;nv_write sms_info_alert			{1}
;nv_write sms_ems_seg_waiting		{1}
;nv_write sms_ems_obj_enable		{on}

;=========================================================================
; UP ITEM : for magellan 
;=========================================================================
nv_write wap_domain_name1 {"wap1.alltel.net"}                          ; WAP Primary Domain Name default.
nv_write wap_port1 {"80"}                                              ; WAP Primary Port default.
nv_write wap_lvl_port1 {"0443"}                                        ; WAP Primary Secure Port default.
nv_write wap_domain_name2 {"wap2.alltel.net"}                        ; WAP Secondary Domain Name default.
nv_write wap_port2 {"80"}                                            ; Wap Secondary Port default.
nv_write wap_lvl_port2 {"0443"}                                      ; WAP Secondary Secure Port default.
nv_write wap_username {""}                                          ; WAP User Name
nv_write wap_password {""}                                                    ; WAP User Password.
nv_write wap_homepage {"proxy:homepage"}                                      ; WAP Homepage
nv_write wap_uaprof {"http://www.alltel.net/uaprof/lg/ax260/ax260.xml"}     ; WAP UAProf

;=========================================================================
;BREW ITEM
;=========================================================================
nv_write brew_carrier_id {41}
nv_write brew_platform_id {1215}		            ; AX260 Platform ID
nv_write brew_bkey {0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 
nv_write brew_server    {"brewdownload.alltel.net,brewdownload.alltel.net"}  ; 64 byte character
nv_write brew_download_flags {0x0444}                       ; DIF_USE_A_KEY(0x0001) - A Key: 1 or B Key: 0 Option, DIF_TEST_ALLOWED(0x0002) - Test Disable: 0, Test Enable: 2
                                                            ; DIF_MIN_FOR_SID(0x0004) - Use MIN for Subscriber ID: 4,  Not use: 0, DIF_PREPAY(0x0008) - Prepay:8, Postpay:0
nv_write brew_auth_policy {1}                               ; APOLCY_NONE(0), APOLCY_SID(1), APOLCY_TEXT(2), APOLCY_NUM(3) 
nv_write brew_privacy_policy {3}                            ; PPOLICY_BREW(0), PPOLICY_CARRIER(1), PPOLICY_BREW_AND_CARRIER(2), PPOLICY_BREW_OR_CARRIER(3)
nv_write brew_sid_length {16}				    ; SID(Subscriber ID) Length
nv_write brew_disallow_dormancy {0}		            ; FALSE	
nv_write brew_primary_ip        	{166,102,165,11}
nv_write brew_secondary_ip      	{166,102,165,13}
nv_write brew_airtime_charge		{TRUE}
;=========================================================================
; MMS ITEM
;=========================================================================
;New MMS ITEMS
nv_write mms_set_auto_receive        {1}                             ; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_set_read_ack            {1}                             ; 0(ON), 1(OFF)
nv_write mms_set_delivery_ack        {0}                             ; 0(MMS_ON), 1(MMS_OFF)

nv_write mms_set_tone_alert          {27}                             ; 0(Low Beep Once),1(Low Beeps), 2(Laud Beep Once), 3(Loud Beeps), 4~13(Ring1~Ring10)
nv_write mms_set_vibrate_alert       {0}                             ; Not used item now [0(VIBRATE OFF), 1(VIBRATE ON)]
nv_write mms_set_reminder_alert      {3}                             ; Not used item now [0(REMIND ONCE), 1(REMIND EVERY2MIN), 2(REMIND EVERY15MIN), 3(REMIND OFF)]

nv_write mms_mmsc_url                {21, "http://mms.alltel.com"}   ; 48 byte characters
nv_write mms_mmsc_upload_url         {14, "mml.alltel.com" }   	     ; Upload Address
nv_write mms_mmsc_uaprof_url         {43, "http://www.alltel.net/mms/AX260_MMS_V01.xml"} ; 48 byte characters

nv_write mms_set_retry_num           {0}                             ; 0, 1, 2, 3
nv_write mms_send_from_add           {0}                             ; MDN Only (0), 1MDN (1),  +1MDN (2)         

nv_write mms_mmsc_user_agent         {5,"AX260"}                  	 ; User Agent Profile name
nv_write mms_mmsc_server_post_url    {13, "/servlets/mms"}           ; Post URL
nv_write mms_mmsc_server_post_cgi    {12, "?message-id="}            ; CGI URL

nv_write mms_test_authorization      {0}                             ; 0 : Commercial, 1 : Lab  2 : Test Bed
nv_write mms_test_mmsc_url           {36, "http://mms.alltel.com/servlets/mms_t"} 			   ; 48 byte characters
nv_write mms_test_mmsc_upload_url    {14, "mml.alltel.com" }   			 ; Upload Address

nv_write mms_gateway_server_name_ip  {21, "http://mms.alltel.com"} 
nv_write mms_http_method_uri     		 {34, "http://mms.alltel.com/servlets/mms"} 
nv_write mms_mmsc_secondary_name_ip  {0, ""} 

;=========================================================================

;=========================================================================
;F/W ITEM
;=========================================================================
nv_write rf_config           {6}
;nv_write vbatt               {165,239}    ; 
nv_write vbatt               {0,255}     

;=========================================================================
;AUDIO ACOUSTIC, MIDI DATA
;=========================================================================

;qdsp_snd_ctrl {vocRXvol*100, vocTXvol, Codec RX gain, Codec TX gain, ST gain, DTMFgain*100,....}
nv_write qdsp_snd_ctrl       	{5,16384,4617,0,0,0,0,0,0,6,6,0,0,0,0,0}	

;audio_adj_device {DCNCodRXgain,DCNCodTXgain,DCNCodSTvol,  
;		   PCSCodRXgain,PCSCodTXgain,PCSCodSTvol ,
;		   ECmode, NSmode, RX/TX AGC enable} 
;EC mode (0:do not cal, 1:OFF, 2:ESEC, 3:HEADSET, 4:AEC, 5:SPEAKER, 6:DEFAULT)
;NS mode (0:do not cal, 1:OFF, 2:ON, 3:DEFAULT)
;RX AGC enable (1:VOC_AGC_NONE; 2:VOC_AGC_NO_AVC 4:VOC_AGC_ALL)
;TX AGC enable (8:VOC_AGC_NONE; 16:VOC_AGC_ON)
;RX/TX AGC : 9(RX_AGC_NONE&TX_AGC_NONE), 18(RX_AGC_NO_AVC&TX_VOC_AGC_ON), ...
nv_write audio_adj_phone 	{-5000,-2700,15000,   	-5000,-2700,15000,   	2,2,18}
nv_write audio_adj_earjack 	{-7000,18433,0,		-7000,18433,0,		4,2,9}	
nv_write audio_adj_spk		{-7000,4500,0,		-7000,4500,0,		5,2,18}        

nv_write audio_adj_hfk 		{0,0,0,			0,0,0,			0,0,0}
nv_write audio_adj_bt  		{0,0,0,			0,0,0,			2,2,10}        

nv_write qdsp_agc_ctrl 		{8192, 0, 2300, 65321, 7552, 62259, 0, 0, 8192, 0, 1280, 65434, 9600, 62259}
nv_write qdsp_bt_agc_ctrl 	{8192, 0, 1920, 65430, 7552, 62259, 0, 0, 0, 0, 0, 0, 0, 0}
nv_write qdsp_headset_agc_ctrl 	{0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}
nv_write qdsp_spk_agc_ctrl 	{32613, 0, 3200, 65321, 6924, 62259, 0, 0, 8192, 0, 3200, 65321, 6924, 62259}

nv_write rx_pcm_filter_ctrl 		{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6}
nv_write tx_pcm_filter_ctrl 		{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6}
nv_write headset_rx_pcm_filter_ctrl 	{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6}
nv_write headset_tx_pcm_filter_ctrl 	{65523,29,65465,363,64113,3080,12442}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6}
nv_write spk_rx_pcm_filter_ctrl 	{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6}
nv_write spk_tx_pcm_filter_ctrl 	{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6}
nv_write bt_rx_pcm_filter_ctrl 		{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6} 
nv_write bt_tx_pcm_filter_ctrl 		{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6} 

;midi 00 ~ 17 : Airport ~ Move Bell
;midi 
;midi 23 ~ 24 : Power On, Power Off
;midi 25 : headset call connect
;midi 27 : shutter 1, 29 : shutter 2, 30 : shutter 3, 35: shutter 4(cheez)
;midi 31 : moving shot start, 32 : moving shot end
;midi 38 ~ 43 : Ring 1~5, Crescendo
;midi 44 ~ 50 : Message tone 1~7 
;                         (0     ~      4)	(5     ~     9)		(10   ~    14)		(15   ~    19)		(20   ~    24)		(25   ~    29)		(30    ~    34)		(35   ~    39)		(40   ~    44)		(45   ~    49)		50
nv_write midi_data_values {-10, -7, -1, -3, -4,        -9, -6, 2, 3, -2,	0, 0, -3, -8, -5,      -3, 11, 1, 0, 0,  	   0, 12, 0, 0, 0,  	  5, 0, 0, 0, 5,  	  0, 0, 0, 0, 0,  	  5, 0, 0, 0, 1,  	 -5, 4, -2, -4, 6,  	   4, -1, 0, -4, -1,	  0}      
nv_write audio_amp_volume {23, 23, 19, 20, 23, 18, 23, 23, 0, 0, 0, 0, 0, 0 }


;=========================================================================
;ADDED AUDIO NV ITEMS
;=========================================================================
;nv_write headset_rx_pcm_filter_ctrl 	{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6}
;nv_write headset_tx_pcm_filter_ctrl 	{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6}
;nv_write spk_rx_pcm_filter_ctrl 	{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6}
;nv_write spk_tx_pcm_filter_ctrl 	{0,0,0,0,0,0,0}		;{Coeff0, Coeff1, Coeff2, Coeff3, Coeff4, Coeff5, Coeff6}
;nv_write qdsp_headset_agc_ctrl {32613, 0, 3200, 65293, 6924, 62259, 0, 0, 35941, 0, 1920, 65434, 7516, 62259}
;nv_write qdsp_spk_agc_ctrl 	{32613, 0, 3200, 65293, 6924, 62259, 0, 0, 35941, 0, 1920, 65434, 7516, 62259}
;======================================================================================================================


nv_write batt_level_threshold {185,180,175,175,153,202,32,202,32,190,186,182,0,0}  ;2007.01.31
nv_write lcd_re_init_en {1} 				; 2007.02.12 inforpc
nv_write phone_test_mode     {0}			; 2007.08.22 us10
nv_write fw_elt_test     {10,1}				; 2007.09.13 us10

;efs write "testmode/1kHz_0dB_LR_128k.mp3"
;efs write "testmode/1kHz_L_0dB_128.mp3"
;efs write "testmode/1kHz_R_0dB_128.mp3"
;efs write "testmode/MultiSine_20-20kHz-0dBp_128k.mp3"
;efs write "testmode/NoSignal_LR_128k.mp3"

;=========================================================================

;=========================================================================
;GPSONE ITEM
;=========================================================================
nv_write gps1_pde_address {0,0,0,0}
nv_write gps1_pde_port {0}
;=========================================================================

;=========================================================================
;MMS IMAGE ITEM
;=========================================================================
efs write "mms/DecodeErrorAnimation.jpg"
efs write "mms/DecodeErrorImage.jpg"
efs write "mms/NotSupportedImage_UnknownImage.jpg"
efs write "mms/phoneOnConversation.jpg"
efs write "mms/TooBigErrorImage.jpg"
;=========================================================================

;=========================================================================
;ANIMATION IMAGE ITEM
;=========================================================================
;efs write "wallpaper/Wallpaper_6.gif"
;=========================================================================

;=========================================================================
;FOTA ITEM
;=========================================================================
;nv_write dm_sec_nai_enabled {1}                         ;Secondary NAI test, To test in roam area must set to 0, in commercial version must set to 1

efs write "cert/getrootcert.der"

;=========================================================================
;Power On/Off, Wallpaper Item
;=========================================================================


;efs write "dload/image/Ball.bmp"
;efs write "dload/image/Car.bmp"
;efs write "dload/image/Coffee.bmp"
;efs write "dload/image/Flower.bmp"
;efs write "dload/image/Glass.bmp"
;efs write "dload/image/Tomato.bmp"
;efs write "dload/image/Tree.bmp"

;;; power_on/off gifs
;efs write "dload/power_on.gif"         ; myoung - power on/off
;efs write "dload/power_off.gif"	

;=========================================================================



mode reset
