;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;=========================================================================
;  Made by  : LGE
;  Version  : AX585
;  Date     : 4/26/2008
;-------------------------------------------------------------------------
;	File Modification history
; When			Who			Comments
;-------------------------------------------------------------------------
;spc "000000"                         ; does not need at LGDP DLL
;wait 2
mode offline-d
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model
wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================

nv_write lock_code 	{"0000"};                    ; Lock_code
nv_write sec_code       {"000000"}                   ; Security code

nv_write name_nam       {0, "NAM1"}                  ; NAM 1 Name
nv_write name_nam       {1, "NAM2"}                  ; NAM 2 Name

nv_write imsi_mcc       {0, "311"}                   ; Mobile Country Code (310)
nv_write imsi_mcc       {1, "311"}
nv_write imsi_11_12     {0, "27"}                    ; Mobile Network Code
nv_write imsi_11_12     {1, "27"}
nv_write min2           {0, "000", "000"}            ; NAM 0 has one active MIN2,
nv_write min2           {1, "000", "000"}
nv_write min1           {0, "000-0000", "000-0000"}
nv_write min1           {1, "000-0000", "000-0000"}

nv_write imsi_t_mcc     {0, "311"}               
nv_write imsi_t_mcc     {1, "311"}
nv_write imsi_t_11_12   {0, "27"}
nv_write imsi_t_11_12   {1, "27"}
nv_write imsi_t_s2      {0, "000", "000"}
nv_write imsi_t_s2      {1, "000", "000"}
nv_write imsi_t_s1      {0, "000-0000", "000-0000"}
nv_write imsi_t_s1      {1, "000-0000", "000-0000"}

nv_write dir_number_pcs {0, "0000000000"}        ; NAM 0 : NV_DIR_NUMBER_PCS_I  /*123456789012345*/ using 10 digits
nv_write dir_number_pcs {1, "0000000000"}        ; NAM 1 : NV_DIR_NUMBER_PCS_I  

print "Programming Primary CDMA Channel"         ; Primary CDMA Channels for A carrier and B carrier
nv_write pcdmach        {0, 283, 384}            ; A and B primary CDMA channels
nv_write pcdmach        {1, 283, 384}

print "Programming Secondary CDMA Channel"       ; Secondary CDMA Channel
nv_write scdmach        {0, 691, 777}            ; set only if secondary channels offered
nv_write scdmach        {1, 691, 777}

nv_write home_sid_nid {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}; Home SID+NID pair item
nv_write home_sid_nid {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535} ; Home SID+NID pair item
nv_write sid_nid_lock {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535} ; CDMA SID/NID pair to lockout for the given NAM and given index(0-9)
nv_write sid_nid_lock {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535} ; CDMA SID/NID pair to lockout for the given NAM and given index(0-9)

nv_write mob_term_home    {0, true, true}
nv_write mob_term_home    {1, true, true}
nv_write mob_term_for_sid {0, true, true}
nv_write mob_term_for_sid {1, true, true}
nv_write mob_term_for_nid {0, true, true}
nv_write mob_term_for_nid {1, true, true}

nv_write accolc {0, 0, 0}
nv_write accolc {1, 0, 0}

nv_write slot_cycle_index {2}

                      ;{Nam Name(0, 1), EVRC Capability(0:Off, 1:ON), Home_Page_Voice_SO(0: wildcard, Others : SO), Home Orig.SO(13K QCELP,8K EVRC), Roam Orig.SO(13K QCELP,8K EVRC)
nv_write pref_voice_so {0,  1, 0x0003, 0x0003, 0x0003} ; EVRC Capable, Home Page SO, Home Orig.SO, Roam Orig.SO
nv_write pref_voice_so {1,  1, 0x0003, 0x0003, 0x0003} ; EVRC Capable, Home Page SO, Home Orig.SO, Roam Orig.SO

print "Programming Pref Mode"
nv_write pref_mode     {0, "Digital Only"}
nv_write pref_mode     {1, "Digital Only"}
nv_write hybrid_pref   {1}                    ; 1 : hybrid on,  0 : hybrid off

print "Programming Band Preferred"
nv_write band_pref {0, "pref_any"}
nv_write band_pref {1, "pref_any"}

print "Programming Roam Preferred"
nv_write roam_pref {0, "pref_any"}
nv_write roam_pref {1, "pref_any"}

nv_write system_pref {0, "automatic b"}       ; System preference, actually default to band preference
nv_write system_pref {1, "automatic b"}
nv_write pref_for_rc            {3}            ; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)
nv_write stand_alone_mode {0}                 ; 0 default OFF, 1 ON


;------------------------------------------------------------------------
print "Programming MRU table clear"
                                                 ; except nam (first 0), '0' are 48(=4 X 12) times.
nv_write mru3_table {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru3_table {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};


print "Programming NAM Checksums"   ; NAM Checksums must all be 0xffff
nv_write nam_chksum {0, 0xffff}
nv_write nam_chksum {1, 0xffff}
nv_write min_chksum {0, 0xffff, 0xffff}
nv_write min_chksum {1, 0xffff, 0xffff}


;=========================================================================
; OTA ITEM
;=========================================================================
nv_write nam_lock           {0, 0}
nv_write nam_lock           {1, 0}
nv_write otapa_enabled      {0, 1}   ; enable
nv_write otapa_enabled      {1, 1}   ; enable
nv_write spc_change_enabled {1}

;-------------------------------------------------------------------------
; nv_write imsi_t_addr_num    {0, 255}
; nv_write imsi_t_addr_num    {1, 255}


;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key {0, 0x00000000, 0x00000000 } ; Nam 1 64 bits A-Key. Published at factory with Random number.
nv_write a_key {1, 0x00000000, 0x00000000 } ; Nam 2 64 bits A-Key. Published at factory with Random number.
nv_write ssd_a {0, 0x00000000, 0x00000000 }
nv_write ssd_a {1, 0x00000000, 0x00000000 }
nv_write ssd_b {0, 0x00000000, 0x00000000 }
nv_write ssd_b {1, 0x00000000, 0x00000000 }
nv_write count {0, 0}
nv_write count {1, 0}

;=========================================================================


;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_pkt_orig_str      {5, "#777"}    ; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_mdr_mode          {3}            ; Service Option 33 (1x channel) = 3 Use only low-speed packet data = 2
nv_write data_auto_packet_detection {0}        ; 0-Disable   1-Enable
nv_write data_so_set            {0}            ; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write diag_default_baudrate  {0x000e}       ; 0x000e(38.4kbps), 0x0011(115.2kbps) 
nv_write data_qnc_enabled       {0}            ; 0-QNC Disable  1-QNC Enable (alltel doesn't support QNC anymore.)
nv_write ppp_user_id            {0,""}         ; Max of 127 chars in User ID
nv_write ppp_password           {0,""}
nv_write data_scrm_enabled      {1}            ; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled      {1}            ; 0-TRTL Disable 1-TRTL Enable    
nv_write ds_default_baudrate    {0x0011}       ; 0x0000 (19.2kbps),0x0011(115.2kbps)
nv_write ds_qcmip               {1}            ; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only
nv_write ds_mip_active_prof     {0}            ; current active profile index
nv_write ds_mip_enable_prof     {1,1,0,0,0,0}  ; diable - 0, enable - 1 {1st Profile, 2nd Profile, 3rd Profile, .... }
nv_write ds_mip_retries         {2}            ; number of retries
nv_write ds_mip_retry_int       {8}            ; retry interval = n*250(ms) + 1000ms (3 sec)
nv_write ds_mip_pre_re_rrq_time {10}            ; pre-registration time - minute
nv_write ds_mip_num_prof        {2}            ; number of profiles (max 6) 
nv_write ds_mip_2002bis_mn_ha_auth  {0}        ; disable - 0, enable -1
nv_write ds_mip_qc_drs_opt      {1}            ; dormant handoff optimization. disable - 0, enable - 1
                                               ; Comment : MIP general profile information {index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
                                               ; Comment : reverse tunneling, home address, primary ha address, secondary ha address}
nv_write ds_mip_gen_user_prof {0,0,"",1,257,1,1000,1,0x00000000,0x00000000,0x00000000}
nv_write ds_mip_gen_user_prof {1,0,"",1,257,1,1000,1,0x00000000,0x00000000,0x00000000}
;DNS IP Settings not supporting any more
;nv_write primary_dns            {0xA666A520}     ;Alltel DNS spec. Server IP = 166.102.165.11 -> 166.102.165.32
;nv_write secondary_dns          {0xCF5B0520}     ;Alltel DNS spec. Server IP = 166.102.165.13 -> 207.91.5.32

;Alltel doesn't use DMU.
;nv_write ds_mip_dmu_pkoid       {0,10}         ; { Index , Public key organization indentifier }
;nv_write ds_mip_dmu_mn_auth     {0,0x01,0xB2,0x07}            ; { Index , DMU MN authenticator - 111111base10 } 

;1X model...
nv_write hdr_an_auth_user_id_long {0,""}       ; { Length , EVDO AN authetication user id }
nv_write hdr_an_auth_passwd_long  {0,""}        ;{ Length , EVDO AN authentication password }
nv_write dun_cable_mode         {1}            ; 0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode            {1}            ; 0=disable bt dun,1=enable bt dun

					       ; Comment : MIP&SIP NAI(Network Access Identifier) for DUN 
nv_write ds_mip_rm_nai {0,0,""}	               ;	{index,nai_length,nai}					       
nv_write ds_sip_rm_nai {0,""}		       ;	{nai_length,nai}

nv_write fallback_flag          {0}            ; 0 - Auto , 1 - 1X 
;----------------------------------------------------------------------
nv_write ppp_carrier            {2}            ; 0-Verizon, 1-USC, 2-ALLTEL, 7-SCRIPT. Test NV Item.  
;efs write "DMU/10.key"		               ; MIP DMU(Dynamic Mipkeys Update) key file

;CS DLL don't write this item
;remove the ppp password setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
;nv_write ppp_password          {16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}      

;CS DLL don't write this item 
;{0~5(index),16(mn_ha_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,
;16(mn_aaa_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
;remove the ds_mip_ss_user_prof setting in script file. (Becuase ppp_password value is changed after DMU nego.)
nv_write ds_mip_ss_user_prof {0,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}

;CS DLL don't write this item 
;Comment : remove the hdr_an_auth_passwd_long setting in script file. (Becuase it uses ppp_password value that changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
; 1X model..
;nv_write hdr_an_auth_passwd_long  {0,""}

;=========================================================================
;BREW ITEM
;=========================================================================
nv_write brew_primary_ip {166,102,165,11}
nv_write brew_secondary_ip {166,102,165,13}
nv_write brew_carrier_id {41}
nv_write brew_platform_id {1269}
nv_write brew_bkey {0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}
nv_write brew_server    {"brewdownload.alltel.net,brewdownload.alltel.net"}
nv_write brew_download_flags {0x0444}
nv_write brew_auth_policy {1}
nv_write brew_privacy_policy {3}
nv_write brew_sid_length {16}
nv_write brew_disallow_dormancy {1}


;=========================================================================
; MMS ITEM
;=========================================================================
nv_write mms_set_auto_receive                   {1}
nv_write mms_set_read_ack              {1}
nv_write mms_set_delivery_ack          {0} 
nv_write mms_set_tone_alert                     {31}
nv_write mms_set_vibrate_alert                  {0}
nv_write mms_set_reminder_alert                 {3}
nv_write mms_mmsc_url                           {21, "http://mms.alltel.com"}
nv_write mms_mmsc_upload_url                    {14, "mml.alltel.com" }
nv_write mms_mmsc_uaprof_url           {43, "http://www.alltel.net/mms/AX585_MMS_V01.xml"}
nv_write mms_set_retry_num                     {0}   ; 0, 1, 2, 3
nv_write mms_send_from_add                           {0}
nv_write mms_mmsc_user_agent  {5, "AX585"}
nv_write mms_mmsc_server_post_url               {13, "/servlets/mms"}
nv_write mms_mmsc_server_post_cgi               {12, "?message-id="}
nv_write mms_test_authorization                 {0}
nv_write mms_test_mmsc_url                      {36, "http://mms.alltel.com/servlets/mms_t"}
nv_write mms_test_mmsc_upload_url               {14, "mml.alltel.com" }
nv_write mms_gateway_server_name_ip  {21, "http://mms.alltel.com"} 
nv_write mms_http_method_uri     		 {34, "http://mms.alltel.com/servlets/mms"} 
nv_write mms_mmsc_secondary_name_ip  {0, ""} 

;=========================================================================
;MMS IMAGE ITEM
;=========================================================================
efs write "mms/DecodeErrorAnimation.jpg"
efs write "mms/DecodeErrorImage.jpg"
efs write "mms/NotSupportedImage_UnknownImage.jpg"
efs write "mms/phoneOnConversation.jpg"
efs write "mms/TooBigErrorImage.jpg"


;=========================================================================
; WAP ITEM 
;=========================================================================
nv_write wap_primary_domain_name {"wap1.alltel.net"}
nv_write wap_primary_port {"80"}
nv_write wap_primary_lvl_port {"0443"}
nv_write wap_secondary_domain_name {"wap2.alltel.net"}
nv_write wap_secondary_port {"80"}
nv_write wap_secondary_lvl_port {"0443"}
nv_write wap_username {""}
nv_write wap_password {""}
nv_write wap_homepage {"proxy:homepage"}
nv_write wap_uaprof {"http://www.alltel.net/uaprof/lg/ax585/ax585.xml"}


;=========================================================================
; MSG ITEM
;=========================================================================
; messaging -> settings -> All messages
nv_write msg_settings_auto_save         {0}			; MSG_AUTO_SAVE(0), MSG_PROMPT(1), MSG_DO_NOT_SAVE(2)
nv_write msg_settings_auto_delete       {0}			; 0(Off), 1(On)
nv_write msg_settings_entry_mode        {1}			; MSG_T9EN(0), MSG_ABC(1), MSG_123(2)
nv_write sms_settings_signature  {0}				; 0(None), 1(Custom)
nv_write msg_settings_speed_messaging {1}		; On(1), Off(0)

;=========================================================================
; SMS ITEM
;=========================================================================
; messaging -> settings -> Text messages
nv_write sms_settings_direct_view  {0}				; 0(Off), 1(On)
nv_write sms_cb_num    {10, "0000000000"}		 	; sms_call_back
nv_write sms_settings_callback_number   {1}			; 0(Off), 1(On)

; messaging -> New Message -> Edit msg -> options
nv_write sms_priority_sel   {0}						; 0(Normal), 1(Urgent)

;Hidden menu settings
nv_write sms_mo_so    {1}							; 0(8K), 1(13K) -> 1(8K), 0(13K) 
nv_write sms_mo_l3_ack    {1}						; 0(Off), 1(On)


nv_write sms_orig_msg_id    {1}
nv_write sms_mo_max_userdata   {160}

;Menu-9.Settings-sound-Messag Alerts
nv_write sms_settings_textmsg_alert {31}			;Message Tone1
nv_write sms_settings_voicemail_alert {33}			;Message Tone5
nv_write sms_settings_all_alert         {0xFFFF}		;None
nv_write sms_settings_email_alert       {31}			;Message Tone1
nv_write sms_settings_page_alert        {31}			;Message Tone1
nv_write sms_2min_alert_sel            {3}				; Once(0), Every 2 Minutes(1), Every 15 Minutes(2), Off(3)
nv_write msg_settings_vibrate_alert   {0}			; On(1), Off(0)
nv_write sms_wappush_auto_view_type	{0}					;Automatic(0),Prompt(1)
;=========================================================================
; EMS ITEM
;=========================================================================
nv_write sms_ems_enable               {1}				; On(1), Off(0)    
nv_write sms_settings_auto_play       {0}			; On(1), Off(0)

;=========================================================================
;UI ITEM
;=========================================================================
nv_write curr_nam                 {0}
nv_write auto_nam                 {0}
nv_write ear_level                  {0x3}
nv_write speaker_level              {0x3}
nv_write ringer_level               {0x3}
nv_write beep_level                 {0x3}
nv_write cont_key_dtmf            {1}
nv_write banner         	{"",0}     
nv_write auto_answer              {0, 0}
nv_write auto_redial              {0, 0}
nv_write back_light               {10}
nv_write lock                     {0}
nv_write auto_lock                {0}
nv_write call_rstrc               {0}
nv_write message_restriction	  {0}
nv_write restrictions_app	  {0,0,0}
nv_write onetouch_dial            {1}
nv_write beep_lvl_shadow          {0x3}
nv_write ear_lvl_shadow           {0x3}
nv_write send_pin                 {0}
nv_write voice_priv               {0}
nv_write fsc                      {"000000"}
nv_write language_selection       {0}
nv_write ringer_spkr_lvl          {0x3} 
nv_write beep_spkr_lvl            {0x3}
nv_write auto_volume_enabled      {0}
nv_write tty                      {3}
nv_write gps1_lock                {3}	; 0:Location On, 3:E911 Only
nv_write manner_mode              {0}
nv_write alarm_only_mode          {0}
nv_write silence_all              {0}
nv_write spk_phone_beep_lvl       {0x3}
nv_write sub_banner     	{"",0}        
nv_write sub_backlight            {10}
nv_write key_light                {10}
nv_write wallpaper_main           {0,0,0}
nv_write wallpaper_sub            {0,0,0}
nv_write pc_port                  {0}
nv_write emergency_num1           {"911"}
nv_write emergency_num2           {"611"}
nv_write emergency_num3           {"*611"}
nv_write wclock_choice            {30,0,45,""}
nv_write media_save_option        {0,0,0}  ; pix_save_location, flix_save_location, sound_save_location (0 : Phone memory(Default),  1: SD card memory)
nv_write dcam_photo_setting_rqs   {1,1,1,0,1}  ; photo_set_Resolution(640x480),photo_set_Quality(normal),photo_set_ShutterSound(sound1),photo_set_axcessMyPics(enable),photo_set_viewMode(Landscape)
nv_write dcam_video_setting_rq    {1}   ; video_set_Resolution(176X144)
nv_write equalizer_mode           {0}                 ;Equalizer(Natural Sound)
nv_write aod_player_settings      {1, 0, 0, 15}       ;Shuffle(Off), Repeat(Off), BGM(Prompt), AOD Volume(15)
nv_write visualizer_mode          {0}                 ;Visualization(Album View)
nv_write rhythmic_cursor_type     {0}                 ;Music Highlight(Cursor 1)
nv_write bt_power_onoff           {0}
nv_write beep_bt_lvl              {4}
nv_write ear_bt_lvl               {4}
nv_write contrast_lvl             {0,0}
nv_write led_blink                {1}
nv_write power_saver              {0}
nv_write edit_font                {0,0}
nv_write music_only_mode          {0}
nv_write gps_test_num             {"922"}
nv_write emer_test_num            {"911"}
nv_write menu_format              {1}	; 0:icon(grid)	1:arc
nv_write display_set_type         {2,0,0}
nv_write dial_font_type           {1,3}
nv_write sound_ringers_type 	  {1,1,1,0,0xffff,0}
nv_write sound_alerts_type 	  {0,0,0,0}
nv_write call_connect_type        {0}
nv_write back_top_beep_type       {1}
nv_write lowbatt_sound            {1}
nv_write logo_melody_type         {1}
nv_write sound_flip_tone          {0}	; 0:Off, 1:On
nv_write best_match               {1}
nv_write announce_alerts          {0}
nv_write touch_led_color          {0}
nv_write mymedia_image_view_type  {0}
nv_write music_search_type        {1}
nv_write music_play_screen        {1}
nv_write pbooklist_search_style   {1}
nv_write dial_qsearch_on   	  {1}
nv_write wheelboard_on   	  {1}
nv_write touchpad_set   	  {1,2}	; (1-vibe on, 2-off)	(1-low, 2-Med, 3-High)
nv_write fmtrans_info   	  {1,"88.1"}
nv_write ui_call_end_option	  {0}	; 0:slide down, 1:end key only
;=========================================================================
;FOTA ITEM
;=========================================================================
efs write "cert/getrootcert.der"

;=========================================================================
;FW ITEM
;=========================================================================
; GPS
nv_write gps1_pde_address {0,0,0,0}
nv_write gps1_pde_port {0}

nv_write vbatt               {130,210}
nv_write rf_config           {1}
nv_write battery_level_threshold {3,69,69,138,138,155,174,178,188,223, 0, 0, 0, 0};
nv_write qdsp_snd_ctrl       {0,-9068,0,-9068,0,0,0,0,0,6,6,0,-500,0,1,1}
nv_write audio_amp_volume    {0,0,0,0,1,0,0,0,0,0,0,0,0,0}
nv_write audio_adj_phone     {0,0,0,0,0,0,0,0,0}
nv_write audio_adj_earjack   {0,32767,0,0,32767,0,0,0,0}
nv_write audio_adj_hfk       {0,0,0,0,0,0,0,0,0}
nv_write audio_adj_spk       {0,0,0,0,0,0,0,0,0} 
nv_write audio_adj_bt        {0,0,0,0,0,0,0,0,0}
nv_write rx_pcm_filter_ctrl  {0xfff3,0x001d,0xffb9,0x016b,0xfa71,0x0c08,0x309a}           
nv_write tx_pcm_filter_ctrl  {0,150,-1200,1220,-2000,0,20480}
nv_write qdsp_agc_ctrl       {0x2000,0x0000,0x0c80,0xff34,0x1b80,0xf333,0,0,0x7f65,0,0x0780,0xff9a,0x1b0c,0xf333}
nv_write openloop_access_probe_power_up {3, 3, 5, 0 ,0, 120, 115, 105}
;=========================================================================
;VOICE ITEM
;=========================================================================
efs write "mVoice/ment/ment_voc.db"
efs write "mVoice/ment/ment_adpcm.db"


;===========================================================================
; MMS Test
;===========================================================================
efs write "mms/MMSTestMID.mid"
efs write "mms/MMSTestJPG.jpg"
efs write "mms/MMSTestGIF.gif"

mode reset

