[Settings]
Flash Initialization = 16
Image List Size = 10
Driver Auto Restart = 1 
Automatic Mode = 1
[Flasher Property]
Jump Address = **********
Start Address = **********
Flasher Path = 
[Primary Flasher Property]
Jump Address = 0x00000000
Start Address = 0x00000000
Authentication Path = 
Flasher Path = 
[Secondary Flahser Property]
Jump Address = 0x00000000
Start Address = 0x00000000
Authentication Path = 
Flasher Path = 
Enable Secondary Flasher = 0
[Flash Properties]
Configuration File Path = C:\Program Files\DSPC\SWDownloader\LGE_KT850_RawNANDx16.ini
[Tavor Flasher Properties]
Path = C:\Program Files\DSPC\SWDownloader\flasher_tavorCIUSB2.zip
[JTAG TRUSTED]
KEY Path = 
TIM Path = 
[Image List]
10 Image Length = 0
10 Image Type = Custom
10 Image Core ID = TAVOR
10 Image Task ID = PROGRAMMING
10 Image Path = d:\images\20100119\userdata.bin
10 Image Start Address = 0x0ad40000
10 Image Partition Number = 0
10 Image Enable = 1
9 Image Length = 0
9 Image Type = RAW
9 Image Core ID = TAVOR
9 Image Task ID = PROGRAMMING
9 Image Path = d:\images\20100119\opl_v0113_V10l_100119.bin
9 Image Start Address = 0x08d40000
9 Image Partition Number = 0
9 Image Enable = 1
8 Image Length = 0
8 Image Type = Custom
8 Image Core ID = TAVOR
8 Image Task ID = PROGRAMMING
8 Image Path = d:\images\20100119\system.bin
8 Image Start Address = 0x00d40000
8 Image Partition Number = 0
8 Image Enable = 1
7 Image Length = 0
7 Image Type = RAW
7 Image Core ID = TAVOR
7 Image Task ID = PROGRAMMING
7 Image Path = d:\images\20100119\convert_ramdisk-recovery.img
7 Image Start Address = 0x00cb0000
7 Image Partition Number = 0
7 Image Enable = 1
6 Image Length = 0
6 Image Type = RAW
6 Image Core ID = TAVOR
6 Image Task ID = PROGRAMMING
6 Image Path = d:\images\20100119\convert_ramdisk.img
6 Image Start Address = 0x00c40000
6 Image Partition Number = 0
6 Image Enable = 1
5 Image Length = 0
5 Image Type = RAW
5 Image Core ID = TAVOR
5 Image Task ID = PROGRAMMING
5 Image Path = d:\images\20100119\zImage
5 Image Start Address = 0x00a40000
5 Image Partition Number = 0
5 Image Enable = 1
4 Image Length = 0
4 Image Type = RAW
4 Image Core ID = TAVOR
4 Image Task ID = PROGRAMMING
4 Image Path = d:\images\20100119\poweron_reverse_noHdr.bmp
4 Image Start Address = 0x00140000
4 Image Partition Number = 0
4 Image Enable = 1
3 Image Length = 0
3 Image Type = RAW
3 Image Core ID = TAVOR
3 Image Task ID = PROGRAMMING
3 Image Path = d:\images\20100119\blob.256k
3 Image Start Address = 0x00080000
3 Image Partition Number = 0
3 Image Enable = 1
2 Image Length = 0
2 Image Type = RAW
2 Image Core ID = TAVOR
2 Image Task ID = PROGRAMMING
2 Image Path = d:\images\20100119\TAVOR_LINUX_NTOBM.bin
2 Image Start Address = 0x00000000
2 Image Partition Number = 0
2 Image Enable = 1
1 Image Length = 536870912
1 Image Type = RAW
1 Image Core ID = TAVOR
1 Image Task ID = ERASING
1 Image Path = Flash erasing length equal to 536870912 bytes
1 Image Start Address = 0x00000000
1 Image Partition Number = 0
1 Image Enable = 1
