;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;=========================================================================
;  Made by  : LGE
;  Version  : E01
;  Date     : 07/01/2008
;-------------------------------------------------------------------------
;	File Modification history
; When			Who			Comments
;2008/08/26	Weiye Xu	Clear mms_mmsc_secondary_name_ip	
;2008/4/24	Frank		Make V01 Script with new MIP items, default values for production
;2008/4/16      Mai Huynh       Remove U.S Cellular and add and move Crescendo 
;                               to the end of named song list
;2008/4/10	Frank 		Modified all settings for Ntelos
;2008/3/24      Jie Chen	Add HTTP header name and value items 
;2008/3/19      Jie Chen	Set sms_delivery_sel, delivery ACK NV item
;2008/3/19      Jie Chen	Added SMS text callback number NV item
;2008/3/19      Jie Chen	Set SMS voice mail callback number NV ite
;2008/3/19      Ron Fan         add WAP items
;2008/3/2	Chang Lee	Analog clock in a front screen is removed.
;2008/1/21	Jaewoo 		Fliptone value is changed
;2008/1/7	Jaewoo 		Fliptone is added
;2008/1/4	Chisang In	SMS Call back default"on"
;2008/1/4	Jaewoo 		Default Sub Wallpaper Changed
;2008/1/4	Chang Lee	Message Auto-Save Default: "Auto Save", Wallpaper Main
;2007/12/7 	Jaewoo		Default Alert Ringtone Added
;2007/12/7 	Jaewoo		Ringtone EFS added
;2007/12/6      Weiye Xu        rename script items
;2007/12/05     Chang Lee       PRI
;2007/11/30	Jaeky Yu		Data
;2007/11/30     Aaron Shin      BREW
;2007/11/29	Don Nguyen		Create	
;-------------------------------------------------------------------------
;spc "000000"                         ; does not need at LGDP DLL
;wait 2
mode offline-d
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model
wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================
nv_write lock_code      {"0000"}
nv_write sec_code       {"000000"}
nv_write fsc            {"000000"}

nv_write name_nam       {0, "NAM 1"}
nv_write name_nam       {1, "NAM 2"}

nv_write nam_chksum 	{0, 0xffff}
nv_write nam_chksum 	{1, 0xffff}
nv_write min_chksum 	{0, 0xffff, 0xffff}
nv_write min_chksum 	{1, 0xffff, 0xffff}

nv_write imsi_mcc           {0, "310"}			; Jacky 310 <- 311
nv_write imsi_mcc           {1, "310"}			; Jacky 310 <- 311
nv_write imsi_11_12         {0, "00"}			; Jacky 00 <- 27
nv_write imsi_11_12         {1, "00"}	
nv_write min1           {0, "000-0000", "000-0000"}
nv_write min1           {1, "000-0000", "000-0000"}
nv_write min2           {0, "000", "000"}
nv_write min2           {1, "000", "000"}
nv_write dir_number_pcs {0, "0000000000"}
nv_write dir_number_pcs {1, "0000000000"}
nv_write accolc 	{0, 0, 0}
nv_write accolc 	{1, 0, 0}

nv_write imsi_t_mcc         {0, "310"}               	; Jacky 310 <- 311
nv_write imsi_t_mcc         {1, "310"}			; Jacky 310 <- 311
nv_write imsi_t_11_12       {0, "00"}			; Jacky 00 <- 27
nv_write imsi_t_11_12       {1, "00"}	
nv_write imsi_t_s1      {0, "000-0000", "000-0000"}
nv_write imsi_t_s1      {1, "000-0000", "000-0000"}
nv_write imsi_t_s2      {0, "000", "000"}
nv_write imsi_t_s2      {1, "000", "000"}

nv_write pref_mode	{0, "automatic"}
nv_write pref_mode	{1, "automatic"}
nv_write band_pref 	{0, "pref_any"}
nv_write band_pref 	{1, "pref_any"}
nv_write roam_pref 	{0, "pref_any"}
nv_write roam_pref 	{1, "pref_any"}
nv_write system_pref 	{0, "automatic b"}
nv_write system_pref 	{1, "automatic b"}

nv_write prl_enabled   	{0, 1}
nv_write prl_enabled    {1, 1}

nv_write home_sid_nid       {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write home_sid_nid       {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock       {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock       {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}

nv_write pcdmach        {0, 283, 384}
nv_write pcdmach        {1, 283, 384}
nv_write scdmach        {0, 691, 777}
nv_write scdmach        {1, 691, 777}

nv_write mob_term_home    {0, true, true}
nv_write mob_term_home    {1, true, true}
nv_write mob_term_for_sid {0, true, true}
nv_write mob_term_for_sid {1, true, true}
nv_write mob_term_for_nid {0, true, true}
nv_write mob_term_for_nid {1, true, true}

nv_write pref_voice_so {0,  1, 0x0000, 0x0003, 0x0003}	; WildCard, 8K EVRC, 8K EVRC
nv_write pref_voice_so {1,  1, 0x0000, 0x0003, 0x0003}	; WildCard, 8K EVRC, 8K EVRC
nv_write cdma_so68_enabled  {1}                        ; 4GV

nv_write pref_for_rc            {3}            ; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)    
nv_write slot_cycle_index {2}
nv_write mru3_table {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0}
nv_write mru3_table {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0}

nv_write scr_version	   {"T30LGV01_00"}

;=========================================================================
; OTA ITEM  (enabled: 1)
;=========================================================================
nv_write nam_lock           {0, 0}
nv_write nam_lock           {1, 0}
nv_write otapa_enabled      {0, 1}
nv_write otapa_enabled      {1, 1}
nv_write spc_change_enabled {1}


;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key {0, 0x00000000, 0x00000000 }
nv_write a_key {1, 0x00000000, 0x00000000 }
nv_write ssd_a {0, 0x00000000, 0x00000000 }
nv_write ssd_a {1, 0x00000000, 0x00000000 }
nv_write ssd_b {0, 0x00000000, 0x00000000 }
nv_write ssd_b {1, 0x00000000, 0x00000000 }
nv_write count {0, 0}
nv_write count {1, 0}

;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_pkt_orig_str      {5, "#777"}    ; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_mdr_mode          {3}            ; Service Option 33 (1x channel) = 3 Use only low-speed packet data = 2
nv_write data_auto_packet_detection {0}        ; 0-Disable   1-Enable
nv_write data_so_set            {0}            ; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write diag_default_baudrate  {0x000e}       ; 0x000e(38.4kbps), 0x0011(115.2kbps) 
nv_write data_qnc_enabled       {0}            ; Jacky 1 <- 0 0-QNC Disable  1-QNC Enable (alltel doesn't support QNC anymore.)
nv_write ppp_user_id            {24, "0000000000@mycricket.com"} 	; Jacky  Max of 64 chars in User ID
nv_write ppp_password           {7, "cricket"} 			; Jacky  Max of 127 chars in Password
nv_write data_scrm_enabled      {1}            ; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled      {1}            ; 0-TRTL Disable 1-TRTL Enable
nv_write ds_default_baudrate    {0x0011}       ; 0x0000 (19.2kbps),0x0011(115.2kbps)
nv_write ds_qcmip               {0}            ; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only
nv_write ds_mip_active_prof     {0}            ; current active profile index
nv_write ds_mip_enable_prof     {1,1,0,0,0,0}  ; diable - 0, enable - 1 {1st Profile, 2nd Profile, 3rd Profile, .... }
nv_write ds_mip_retries         {2}            ; number of retries
nv_write ds_mip_retry_int       {3}            ; retry interval = n*250(ms) + 1000ms (2 sec)
nv_write ds_mip_pre_re_rrq_time {1}            ; pre-registration time - minute
nv_write ds_mip_num_prof        {1}            ; number of profiles (max 6) 
nv_write ds_mip_2002bis_mn_ha_auth  {1}        ; disable - 0, enable -1
nv_write ds_mip_rrq_if_tfrk     {1}            ; send a registration only in use : disable-0, enable-1
nv_write ds_mip_qc_drs_opt      {1}            ; dormant handoff optimization. disable - 0, enable - 1
                                               ; Comment : MIP general profile information {index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
                                               ; Comment : reverse tunneling, home address, primary ha address, secondary ha address}
nv_write ds_mip_gen_user_prof   {0,26,"0000000000@brightpoint.net",1,598,1,300,1,0x00000000,0x00000000,0x00000000}
nv_write ds_mip_ss_user_prof    {0,0,"",0,""}

nv_write ds_mip_dmu_pkoid       {0,41}         					; { Index , Public key organization indentifier }
nv_write ds_mip_dmu_mn_auth     {0,0xFF,0xFF,0xFF}              		; { Index , DMU MN authenticator - 111111base10 } 

nv_write dun_cable_mode         {1}           					; 0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode            {1}            					; 0=disable bt dun,1=enable bt dun
							       			; Comment : MIP&SIP NAI(Network Access Identifier) for DUN
nv_write ds_mip_rm_nai 		{0,24, "0000000000@mycricket.com"}	        ; {index,nai_length,nai}		       
nv_write ds_sip_rm_nai 		{24, "0000000000@mycricket.com"}	        ; {nai_length,nai}

nv_write ppp_carrier            {0}            ; 0-Verizon 1-USC 7-SCRIPT. Test NV Item. Needs 4 to work with MIP/PPP 
nv_write pap_user_id		{7, "cricket"}	; wluo: sets first 5 bytes of pppUserID to zero to control pppUserId
;efs write "DMU/41.key"		               ; MIP DMU(Dynamic Mipkeys Update) key file. ACG does not use DMU
;=========================================================================
; UP ITEM : for magellan 
;=========================================================================
nv_write wap_domain_name1 	{"wap.mycricket.com"}                                         ; WAP Primary Domain Name default.
nv_write wap_port1 		{"8080"}                                       ; WAP Primary Port default.
nv_write wap_lvl_port1 		{"0443"}                                     ; WAP Primary Secure Port default.
nv_write wap_domain_name2 	{"wap.mycricket.com"}                    		     ; WAP Secondary Domain Name default.
nv_write wap_port2 		{"8080"}                                       ; Wap Secondary Port default.
nv_write wap_lvl_port2 		{"0443"}                                     ; WAP Secondary Secure Port default.
nv_write wap_username 		{"MIN"}                          		     ; WAP User Name
nv_write wap_password 		{"cricket"}                           	             ; WAP User Password.
nv_write wap_homepage 		{"http://homepage"}     				     ; WAP Homepage
nv_write wap_uaprof		{""}    			             ; WAP UAProf
nv_write wap_oma_download 	{1}                                          ; WAP OMA Download flag
;=========================================================================
;BREW ITEM
;=========================================================================
nv_write brew_carrier_id {82}
nv_write brew_platform_id {8074}		            ; 1203:UX380, 1193:AX380, 8086:Lazor(mShop1.1)Platform ID
nv_write brew_bkey {0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 
nv_write brew_server {"Leap-prod-vip.qualcomm.com,Leap-test-vip.qualcomm.com"}            ; 64 byte character
nv_write brew_download_flags {0x0004}                       ; DIF_USE_A_KEY(0x0001) - A Key: 1 or B Key: 0 Option, DIF_TEST_ALLOWED(0x0002) - Test Disable: 0, Test Enable: 2
                                                            ; DIF_MIN_FOR_SID(0x0004) - Use MIN for Subscriber ID: 4,  Not use: 0, DIF_PREPAY(0x0008) - Prepay:8, Postpay:0
nv_write brew_auth_policy {1}                               ; APOLCY_NONE(0), APOLCY_SID(1), APOLCY_TEXT(2), APOLCY_NUM(3) 
nv_write brew_privacy_policy {3}                            ; PPOLICY_BREW(0), PPOLICY_CARRIER(1), PPOLICY_BREW_AND_CARRIER(2), PPOLICY_BREW_OR_CARRIER(3)
nv_write brew_sid_length {16}				    ; SID(Subscriber ID) Length
nv_write brew_disallow_dormancy {0}		            ; FALSE	
nv_write brew_primary_ip        	{0,0,0,0}
nv_write brew_secondary_ip      	{0,0,0,0}
nv_write brew_airtime_charge		{TRUE}

;=========================================================================
; MMS ITEM
;=========================================================================
nv_write mms_set_auto_receive          		{0}
nv_write mms_set_read_ack              		{1}
nv_write mms_set_delivery_ack          		{0} 
nv_write mms_set_tone_alert            		{30}
nv_write mms_set_vibrate_alert         		{0}
nv_write mms_set_reminder_alert        		{3}
nv_write mms_mmsc_url                		{24, "http://mms.mycricket.com"}     ; 48 byte characters
nv_write mms_mmsc_upload_url         		{4, "1111" }                        ; Upload Address
nv_write mms_mmsc_uaprof_url         		{0,""}   ; 48 byte characters
nv_write mms_set_retry_num             		{3}   ; 0, 1, 2, 3
nv_write mms_send_from_add             		{1}
nv_write mms_mmsc_user_agent  	       		{5, "LG300"}
nv_write mms_mmsc_server_post_url   		{13, "/servlets/mms"} 
nv_write mms_mmsc_server_post_cgi  		{0, ""} 
nv_write mms_mmsc_secondary_name_ip		{0, ""}
nv_write mms_test_authorization        		{0}
nv_write mms_callback_number_support   		{1}   ; 0(MMS_ON), 1(MMS_OFF)
nv_write mms_subscribed_provisioned_for_1xrtt 	{0}   ; 0(MMS_ON), 1(MMS_OFF)

nv_write mms_http_hdr_connection		{"Keep-Alive"}
nv_write mms_http_hdr_content_type   		{"application/vnd.wap.mms-message"}
nv_write mms_http_hdr_accept			{"application/vnd.wap.mms-message"}
nv_write mms_http_hdr_accept_language		{"en"}
nv_write mms_http_hdr_accept_charset		{"US-ASCII, ISO-8859-1,  UTF-8"}

; wluo 01232008 LG260: make all HTTP header parameters (name and value) configurable.
nv_write mms_http_hdr_name_content_type		{"Content-Type", 1}		; 0:turn off for both POST and GET, 1:only for POST, 2:only for GET, 3:turn on for both POST and GET
nv_write mms_http_hdr_name_user_agent		{"User-Agent", 3}		; 0:turn off for both POST and GET, 1:only for POST, 2:only for GET, 3:turn on for both POST and GET
nv_write mms_http_hdr_name_uaprofile		{"Profile", 3}			; 0:turn off for both POST and GET, 1:only for POST, 2:only for GET, 3:turn on for both POST and GET
nv_write mms_http_hdr_name_accept		{"Accept", 2}			; 0:turn off for both POST and GET, 1:only for POST, 2:only for GET, 3:turn on for both POST and GET
nv_write mms_http_hdr_name_accept_language	{"", 0}				; 0:turn off for both POST and GET, 1:only for POST, 2:only for GET, 3:turn on for both POST and GET
nv_write mms_http_hdr_name_accept_charset	{"Accept-charset", 2}		; 0:turn off for both POST and GET, 1:only for POST, 2:only for GET, 3:turn on for both POST and GET
nv_write mms_http_hdr_name_accept_encoding	{"", 0}				; 0:turn off for both POST and GET, 1:only for POST, 2:only for GET, 3:turn on for both POST and GET
nv_write mms_http_hdr_name_authentication	{"X-cricket-MDN", 3}		; 0:turn off for both POST and GET, 1:only for POST, 2:only for GET, 3:turn on for both POST and GET
nv_write mms_http_hdr_name_connection		{"Connection", 3}		; 0:turn off for both POST and GET, 1:only for POST, 2:only for GET, 3:turn on for both POST and GET
nv_write mms_http_hdr_name_proxy_authorization	{"Proxy-Authorization", 0}	; 0:turn off for both POST and GET, 1:only for POST, 2:only for GET, 3:turn on for both POST and GET
;=========================================================================
;MMS IMAGE ITEM
;=========================================================================
efs write "mms/DecodeErrorAnimation.jpg"
efs write "mms/DecodeErrorImage.jpg"
efs write "mms/NotSupportedImage_UnknownImage.jpg"
efs write "mms/phoneOnConversation.jpg"
efs write "mms/TooBigErrorImage.jpg"


;=========================================================================
; MSG ITEM
;=========================================================================

;=========================================================================
; SMS ITEM
;=========================================================================
nv_write msg_settings_auto_save         {0}	; 0(Auto Save), 1(Prompt), 2(Do Not Save)
nv_write msg_settings_auto_delete       {0}	; 0(Off), 1(On)
nv_write msg_settings_entry_mode        {1}	; T9Word(0), Abc(1), 123(2)
nv_write msg_settings_vibrate_alert   	{0}
nv_write msg_settings_speed_messaging 	{0}
nv_write sms_voicemail_alert		{29}     ;0~33(Audio Tones)- Low Beep Once(0), Low Beeps(1),Loud Beep Once(2), Loud Beeps(3), Ring1~10(4~13), No Ring(14)
nv_write sms_textmsg_alert		{28}     ;0~33(Audio Tones)- Low Beep Once(0), Low Beeps(1),Loud Beep Once(2), Loud Beeps(3), Ring1~10(4~13), No Ring(14)
nv_write sms_email_alert  		{28}     ; 0~33(Audio Tones) - Low Beep Once(0), Low Beeps(1),Loud Beep Once(2), Loud Beeps(3), Ring1~10(4~13), No Ring(14)
nv_write sms_page_alert  		{28}     ; 0~33(Audio Tones)- Low Beep Once(0), Low Beeps(1),Loud Beep Once(2), Loud Beeps(3), Ring1~10(4~13), No Ring(14)
nv_write sms_all_alert  		{0xFFFF}     ; Low Beep Once(0), Low Beeps(1),Loud Beep Once(2), Loud Beeps(3), Ring1~10(4~13), No Ring(14)

nv_write sms_priority_sel   		{0}	; 0(Normal), 1(High)
nv_write sms_mo_so    			{1}	; 1(8K), 0(13K)
nv_write sms_mo_l3_ack    		{1}	; 1(On), 0(Off)
nv_write sms_default_cb   		{1}	; 1(On), 0(Off)
nv_write sms_orig_msg_id    		{1}
nv_write sms_mo_max_userdata   		{160}
nv_write sms_signature_sel  		{0}
nv_write sms_directview_sel  		{0}
nv_write sms_2min_alert_sel             {1}	; 0(Once), 1(Every 2 Minutes), 2(Every 15 Minutes), 3(Off)
nv_write sms_ems_enable                 {off}  ; On(1), Off(0)
nv_write sms_auto_play       		{0}

nv_write sms_cb				{3, "*86"}      ; sms_voice_mail_call_back
nv_write sms_delivery_sel		{0}     ; 1(sms delivery ACK enhanced), 0(sms delivery ACK normal)
nv_write sms_txt_cb			{10, "0000000000"}   ;1111111111 (MIN), 0000000000(MDN) 
 
;=========================================================================
; EMS ITEM
;=========================================================================
;nv_write sms_ems_enable                {off}  ; On(1), Off(0)    
;nv_write sms_auto_play       		{off}  ; On(1), Off(0)
;=========================================================================
;UI ITEM
;=========================================================================
nv_write curr_nam                 {0}
nv_write auto_nam                 {0}
nv_write ear_lvl                {0x4}
nv_write speaker_lvl            {0x4}
nv_write ringer_lvl             {0x4}
nv_write beep_lvl               {0x4}
nv_write cont_key_dtmf            {1}
nv_write banner         	  {"LG",1}     
nv_write auto_answer              {0, 0}
nv_write auto_redial              {0, 0}
nv_write back_light               {10}
nv_write lock                     {off}     ; phone lock            == Unlocked \ now
nv_write auto_lock                {off}     ; phone lock            == Unlocked \ Power_up
nv_write call_rstrc               {0}
nv_write onetouch_dial            {on}      ; One touch dial        == enable!
nv_write beep_lvl_shadow          {0x4}
nv_write ear_lvl_shadow           {0x4}
nv_write send_pin                 {0}
nv_write voice_priv               {0}	; 0 (Standard)
nv_write language_selection       {0}
nv_write ringer_spkr_lvl          {0x4} 
nv_write beep_spkr_lvl            {0x4}
nv_write auto_volume_enabled      {0}
nv_write tty                      {3}	; 0 (TTY Full), 1 (TTY + Talk), 2 (TTY + Hear), 3 (TTY Off)
nv_write stand_alone_mode 	  {0}
nv_write gps1_lock                {3}	; 0 (Location On), 1 (E911 Only)
nv_write manner_mode              {0}
nv_write alarm_only_mode          {0}
nv_write silence_all              {0}
nv_write spk_phone_beep_lvl       {0x4}
nv_write backtop_beep             {1}
nv_write sub_banner     	  {"LG",1}        
nv_write sub_backlight            {10}
nv_write key_light                {10}
nv_write wallpaper_main 	  {0,0,0}      ; wallpaper {location_type(0:phone memory 1:phone efs 2:sdcard), location_id(0:sdcard id), item_id(1: index), item_path(NULL: path)}
nv_write wallpaper_sub            {0,0,0}
nv_write pc_port                  {0}
nv_write emergency_num1      	  {"911"}
nv_write emergency_num2      	  {"611"}
nv_write emergency_num3      	  {"*611"}
nv_write wclock_choice       	  {30,0,43,""}
nv_write phone_setup              {0,0,14,0,0,"","",2,9,3,1}   ;(pim_id,form_id,shortcut_form_index,isModal,modalType,mymenu_level1_index[12],mymenu_level2_index[12],up_id,down_id,left_id,right_id) ;luke 2008.03.14 - up/down/left/right id added
nv_write media_save_option        {0,0,0}
nv_write dcam_photo_setting_rqs   {1,1,1,0,0,0} 	;Henry's add in due to AX300 ;luke 2008.03.14 - color effect added
nv_write equalizer_mode           {1}
nv_write bt_power_onoff           {0}	; 0 (Off), 1 (On)
nv_write beep_bt_lvl              {4}
nv_write ear_bt_lvl               {6}
nv_write contrast_lvl             {0,0}
nv_write led_blink                {1}
nv_write power_saver              {0}
nv_write edit_font                {0,0}
nv_write music_only_mode          {0}
nv_restrictions_app		  {0,0,0}
nv_write gps_test_num             {"922"}
nv_write emer_test_num            {"911"}
nv_write sound_ringers 	 	  {13,8,5,0,0xffff,0}
nv_write menu_format              {0}
nv_write display_set        	  {1,0,0}
nv_write dial_font         	  {1,0}
nv_write sound_alerts 	 	  {0,0,0,0}
nv_write call_connect_alert       {0}
nv_write lowbatt_sound            {1}	; 0 (Announce), 1 (Tone)
nv_write logo_melody       	  {1}
nv_write best_match               {1}	; 0 (1 Match), 1 (4 Matches)
nv_write announce_alerts          {0}	; 0 (Disable), 1 (Announce), 2 (Announce + Ring)
nv_write sound_fliptone           {0}

;=========================================================================
;FW ITEM
;=========================================================================
; GPS
nv_write gps1_pde_address 	 {0,0,0,0}
nv_write gps1_pde_port 		 {0}
nv_write gps1_capabilities  	 {1}      		; coarse location message  (1) enable, (0) disable
nv_write spare_2 		 {0}
nv_write vbatt		         {150,238}
nv_write rf_config         	 {1}
nv_write batt_level_threshold 	 {3,62,70,135,135,152,170, 158, 173, 200, 0, 0, 0, 0}
nv_write qdsp_snd_ctrl       	 {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0}
nv_write audio_adj_phone    	 {0,0,0,0,0,0,0,0,0}
nv_write audio_adj_earjack  	 {0,0,0,0,0,0,0,0,0}
nv_write audio_adj_hfk      	 {0,0,0,0,0,0,0,0,0}
nv_write audio_adj_spk      	 {0,0,0,0,0,0,0,0,0} 
nv_write audio_adj_bt       	 {0,0,0,0,0,0,0,0,0}

;=========================================================================
;FILE WRITING TO EFS
;=========================================================================
efs write "ringtone/Mystique.mp3"
efs write "ringtone/Deep Blue Calling.mp3"
efs write "ringtone/Shine.mp3"
efs write "ringtone/A Frame of Mind.mp3"
efs write "ringtone/Cigar And Wine.mp3"
efs write "ringtone/Orange Ice.mp3"
efs write "ringtone/Never Stop.mp3"
efs write "ringtone/Cause' U are.mp3"
efs write "ringtone/Metal element.mp3"
efs write "ringtone/Law of Motion.mp3"
efs write "ringtone/Burnning Soul.mp3"
efs write "ringtone/Vinyllist.mp3"
efs write "ringtone/Take Me.mp3"
efs write "ringtone/Crying.mp3"
efs write "ringtone/ColorPage.mp3"
efs write "ringtone/Froggy Night.mp3"
efs write "ringtone/Just Fine.mp3"
efs write "ringtone/Happycall.mp3"
efs write "ringtone/Bellusion.mp3"
efs write "ringtone/Morning.mp3"
efs write "ringtone/Wahwah.mp3"
efs write "ringtone/Cricket Beep.mp3"
efs write "ringtone/Crescendo.mid"

efs write "ringtone/Ring 1.mp3"
efs write "ringtone/Ring 2.mid"
efs write "ringtone/Ring 3.mid"
efs write "ringtone/Ring 4.mid"
efs write "ringtone/Ring 5.mid"

efs write "ringtone/Message Tone 1.mid"
efs write "ringtone/Message Tone 2.mid"
efs write "ringtone/Message Tone 3.mid"
efs write "ringtone/Message Tone 4.mid"
efs write "ringtone/Message Tone 5.mid"
efs write "ringtone/Message Tone 6.mp3"
efs write "ringtone/Message Tone 7.mp3"
efs write "ringtone/Message Tone 8.mp3"

efs write "ringtone/Open.qcp"
efs write "ringtone/Close.qcp"

; luke 2008.02.15
efs write "dload/power_on.gif"
efs write "dload/power_off.gif"
efs write "poweron/animation/flashPowerOn.swf"
efs write "poweroff/animation/flashPowerOff.swf"
efs write "poweron/sound/poweron.mid"
efs write "poweroff/sound/poweroff.mid"
efs write "dload/image/Custom.bmp"
efs write "dload/image/Custom_sub.bmp"
efs write "browser/wap_carrier_logo.bmp"
efs write "browser/wap_carrier_logo_land.bmp"

mode reset
