;=========================================================================
;                   LG Electronics, Ltd.
;                   Mobile Communications Research Lab.
;                   Development Soft Ware Group
;
;=========================================================================
;  File name: LG640F04_00.scr 
;  Made by  : LGE
;  Version  : V04
;  Date     : 2010/07/15
;
;=========================================================================
;
; NV-items are programmed using the nv_write command:
;
;   nv_write itemname { [nam index,] val1, val2, ..., valn }
;
; Only NAM 0 has meaningful values.  Values for NAMs 1-3 are
; zeroed out or set to default values.
;
; Some items require a nam index (0-1). The curly braces
; are required and they surround the values to be written.
; You must supply every value the item expects. Hex values
; you supply need the 0x prefix.
;
; Semi-colons introduce comments. Whole line and
; to-end-of-line comments are possible.
;
; THE FOLLOWING PARAMETERS SHOULD BE SET FOR EACH PHONE:
;-------------------------------------------------------------------------
;
;   1. CDMA preferred serving system (Automatic A or Automatic B)
;   2. Analog preferred serving system (System A or System B)
;   3. Analog Home SID (the SID of the preferred serving system)
;   4. Analog first paging channel (for system A or system B)
;   5. CDMA primary and seconday channels (including PCN, if in use)
;   6. CDMA SID/NID pairs (the SID of the preferred serving system)
;   7. MIN1 and MIN2 parameters.
;   8. Default settings for LG6400
;=========================================================================
;print "Start Service Programming"
; Enter the Service Programming Code (factory defaulted to 000000)
; If you don't have version 116 or later, this command will fail.
; This allows access to the SP items (both reading _and_ writing)

spc "000000"

wait 2

; Put the DMSS in offline mode
mode offline-d

;=========================================================================
; SYSTEM ITEM
;=========================================================================
; Display the ESN and permanent physical station
; configuration parameters
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model
factory reset
wait 2

