;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 2
;=========================================================================
;  File name: MX51IU01_00.SCR (LG-MX510)
;  Made by  : Infobank Parkboo
;  Version  : 01_00
;  Date     : 01/05/2006
;-------------------------------------------------------------------------
;  when         who        what
;----------    -------    ------------------------------------------------
;2005/12/24    JOYS	BREE Item 수정
;			-> "brew_secondary_server" -> "brew.iusacell3g.com"
;		 	-> "brew_platform_id" -> "1111" 임시값.
;2005/12/23    whitekiss  UI item 수정
;2005/12/21    ksm	  Data item 수정
;2005/12/21    ykkim	  MMS,GPS ITEM Initiation for IUSACELL SPEC
;2005/12/21    khr	  SMS ITEM Initiation for IUSACELL.
;2005/12/21    khr	  modify ppp_user_id and ppp_password
;2005/12/21    SELee    Programming  ITEM Initiation by IUSACELL SPEC.
;			-> "sec_code2" item Commented.
;			-> "name_nam" item Commented.
;			-> "banner" item Commented.
;			-> "sub_banner" item Commented.
;			-> "imsi_mcc" item Commented.
;			-> "imsi_t_mcc" item Commented.
;			-> "home_sid_nid" item Commented.
;			-> "hdr_an_auth_user_id_long" item Commented.
;			-> "hdr_an_auth_passwd_long" item Commented.
;2005/12/20    JOYS       BREW ITEM Initiation by IUSACELL SPEC.
;			  -> "brew_secondary_server" item Commented.
;			  -> "brew_platform_id" item Commented.
;2005/12/20    ksm        from MX510(Brazi)
;

;=========================================================================
; INIT (not used lgdp)
;=========================================================================
spc "000000" 
wait 2
mode offline-d

;=========================================================================
; SYSTEM ITEM
;=========================================================================

nv_write slot_cycle_index	{2}
nv_write min1			{0, "000-0000", "000-0000"}
nv_write min1			{1, "000-0000", "000-0000"}
nv_write min2			{0, "000", "000"}	;NAM 0 has one active MIN2,
nv_write min2			{1, "000", "000"}	;NAM 1
nv_write dir_number		{0, "0000000000"}	;NAM 0 : NV_DIR_NUMBER_I
nv_write dir_number		{1, "0000000000"}	;NAM 1 : NV_DIR_NUMBER_I
nv_write imsi_mcc		{0, "000"}			;Mobile Country Code
nv_write imsi_mcc		{1, "000"}			;Mobile Country Code
nv_write imsi_11_12		{0, "00"}			;Mobile Network Code
nv_write imsi_11_12		{1, "00"}			;Mobile Network Code
nv_write imsi_addr_num		{0, 0xff}          ; Class 0 IMSI

; Prefer Mode.
; if hybrid_pref == false, pref_mode set hdr_only or 1x_only
nv_write hybrid_pref 		{1}	;Hybrid pref 1:enable, 0:disable 
nv_write pref_mode		{0, "DIGITAL_ONLY"}	;DIGITAL_ONLY, HDR_ONLY, 1X_ONLY
nv_write pref_mode		{1, "DIGITAL_ONLY"}	;DIGITAL_ONLY, HDR_ONLY, 1X_ONLY

; Band preferred.
;NV_BAND_PREF_BC0_A = 0x0001
;NV_BAND_PREF_BC0_B = 0x0002
;NV_BAND_PREF_BC0   = 0x0003
;NV_BAND_PREF_BC1   = 0x0004
;NV_BAND_PREF_BC3   = 0x0010
;NV_BAND_PREF_BC4   = 0x0020
;NV_BAND_PREF_BC5   = 0x0040
;NV_BAND_PREF_ANY   = 0xFFFF    
nv_write band_pref		{0, "PREF_ANY"};
nv_write band_pref		{1, "PREF_ANY"};

; Roaming preferred.
;NV_ROAM_PREF_HOME  = 0x01  
;NV_ROAM_PREF_AFFIL = 0x03
;NV_ROAM_PREF_ANY   = 0xFF
print "Programming Roam Preferred"
nv_write roam_pref		{0, "PREF_ANY"};
nv_write roam_pref		{1, "PREF_ANY"};
	
nv_write prl_enabled		{0,"true"}
nv_write prl_enabled		{1,"true"}

nv_write home_sid_nid		{0,1525,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write home_sid_nid		{1,1525,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock		{0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0}
nv_write sid_nid_lock		{1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0}

nv_write pcdmach		{0, 283, 384}        ; A and B primary CDMA channels
nv_write pcdmach		{1, 283, 384}
nv_write scdmach		{0, 691, 777}        ; set only if secondary channels offered
nv_write scdmach		{1, 691, 777}

; except nam (first 0), '0' are 48(=4 X 12) times.
nv_write mru3_table {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru3_table {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};

;NAM Checksums must all be 0xffff
print "Programming NAM Checksums"
nv_write nam_chksum		{0, 0xffff}
nv_write nam_chksum		{1, 0xffff}
nv_write accolc			{0, 0, 0}
nv_write accolc			{1, 0, 0}
nv_write mob_term_home		{0, true, true}
nv_write mob_term_home		{1, true, true}
nv_write mob_term_for_sid	{0, true, true}
nv_write mob_term_for_sid	{1, true, true}
nv_write mob_term_for_nid	{0, true, true}
nv_write mob_term_for_nid	{1, true, true}
nv_write min_chksum		{0, 0xffff, 0xffff}
nv_write min_chksum		{1, 0xffff, 0xffff}
nv_write pref_voice_so		{0, 1,0x0003,0x0003,0x0003} ; NAM #No., EVRC Capability Disabled/Enabled, 0=Home Page SO(Wild Card)  3=Home Orig. SO(8K EVRC) 3=Roam Orig. SO(8K EVRC) 	
nv_write pref_voice_so		{1, 1,0x0003,0x0003,0x0003}
nv_write voice_priv		{0}	; 0=Standard(0x00)  1=Enhanced(0x01)  

;=========================================================================

;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key			{0, 0x00000000, 0x00000000 }
nv_write a_key			{1, 0x00000000, 0x00000000 }
nv_write ssd_a			{0, 0x00000000, 0x00000000 }
nv_write ssd_a			{1, 0x00000000, 0x00000000 }
nv_write ssd_b			{0, 0x00000000, 0x00000000 }
nv_write ssd_b			{1, 0x00000000, 0x00000000 }
nv_write count			{0, 0}
nv_write count			{1, 0}

;=========================================================================
; OTA ITEM
;=========================================================================
nv_write otapa_enabled		{0, 1}   ; enable
nv_write otapa_enabled		{1, 1}   ; enable
nv_write nam_lock		{0, 1}
nv_write nam_lock		{1, 1}
nv_write spc_change_enabled	{0};
nv_write imsi_t_mcc		{0, "000"};	   
nv_write imsi_t_mcc		{1, "000"};
nv_write imsi_t_11_12		{0, "00"};
nv_write imsi_t_11_12		{1, "00"};
nv_write imsi_t_addr_num	{0, 0xff};
nv_write imsi_t_addr_num	{1, 0xff};
nv_write imsi_t_s1		{0, "000-0000", "000-0000"};
nv_write imsi_t_s1		{1, "000-0000", "000-0000"};
nv_write imsi_t_s2		{0, "000", "000"};
nv_write imsi_t_s2		{1, "000", "000"};

;=========================================================================
;UI ITEM
;=========================================================================
nv_write lock_code 		{"0000"}		; Lock_code
nv_write sec_code 		{"000000"}	; Security code
nv_write fsc 			{"000000"}	; Field Service code
nv_write otksl 			{"000000"}	; One-time keypad subsidy lock, Hard Coding
nv_write name_nam 		{0, "IUSACELL"}; NAM 1 Name
nv_write name_nam 		{1, "IUSACELL"}; NAM 2 Name
nv_write carrier_sel 		{0x00}	; VIVI:0x00, SP:0x01 ,RJ:02, CO:03, RS:04, NBT:05, GLB:06
nv_write banner      		{"IUSACELL 3G"}; 	;2006.4.8 IUSACELL 3G
nv_write sub_banner  		{"IUSACELL 3G"};sub-banner default initialize ;2006.4.8 IUSACELL 3G
nv_write ringer_lvl 		{0x4}	; 1(Low), 2(Med Low), 3(Med), 4(High Med), 5(High), 1(Vibrate only=manner_mode), 97(alarm only), 1(Sounds Off=silence_all)
nv_write beep_lvl 		{0x1}	; 0(Off), 1(Low), 2(Med Low), 3(Med), 4(High Med), 5(High) ;{2};; 051220 whitekiss ;;
nv_write ear_lvl		{0x4}	; 1(Low), 2(Med Low), 3(Med), 4(High Med), 5(High) ;{2};; 051220 whitekiss ;;
nv_write speaker_lvl 		{0x5}	; 1(Low), 2(Med Low), 3(Med), 4(High Med), 5(High);{2};; 051220 whitekiss ;;
nv_write ringer_spkr_lvl	{0x4}	; 0(Off), 1(Low), 2(Med Low), 3(Med), 4(High Med), 5(High), 98(High & Vib), 99(Vibrate);{2};; 051220 whitekiss ;;
nv_write beep_spkr_lvl		{0x1}	; 0(Off), 1(Low), 2(Med Low), 3(Med), 4(High Med), 5(High)
nv_write beep_lvl_shadow	{0x1}	; 0(Off), 1(Low), 2(Med Low), 3(Med), 4(High Med), 5(High)
nv_write ear_lvl_shadow		{0x4}	; 1(Low), 2(Med Low), 3(Med), 4(High Med), 5(High)
nv_write speaker_shadow		{0x5}	; 1(Low), 2(Med Low), 3(Med), 4(High Med), 5(High)
nv_write auto_lock 		{off}	; phone lock(Power_up시)	Unlock(off)/Lock(off)/On Power Up(on)
nv_write auto_volume_enabled 	{0}	; 0-> off , 1-> on
nv_write lock 		        {off}	; phone lock(Now)	Unlock(off)/Lock(on)/On Power Up(off)
nv_write auto_nam 		{off}	; Auto NAM              == disable
nv_write curr_nam 		{0}	; Current NAM           == NAM 1
nv_write auto_redial 		{0, 0}	; Auto redial           == off
nv_write auto_answer 		{0, 0}	; Auto answer           == off 0,0:off, 1,1:1ring, 1,3:3ring, 1,2:answering machine
nv_write onetouch_dial 		{on}	; One touch dial        == enable!
nv_write cont_key_dtmf 		{0}	; Prssed key tone       == 1:short  0:long
nv_write back_light 		{15}	; Backlight             == after 7secs (10 -> 7, by bhjo 02.08.28) ;2006.4.8 7->15
nv_write sub_backlight 		{7}	; Sub Backlight         == after 7secs (10 -> 7, by bhjo 02.08.28)
nv_write call_connect_alert 	{false}	; Call connect alert    == off
nv_write send_pin 		{off}	; Send pin?             == disable!
nv_write language_selection 	{2}	; Default (English:0x0/Espanol:0x2) == Espanol
nv_write carrier_logo 		{0}	; 0 -> Iusacell, 
nv_write logo_melody 		{1}	; 1 -> On, 0 -> Off
nv_write silence_all 		{0} 	; sound on   {1} sound off
nv_write sound_alerts 		{0,0,0,0}	; ( Service Change, Minute Beep, Call Connect, ERI alert) 4번 item 추가 2003.11.30 sychoi
nv_write key_light 		{5}
nv_write display_set 		{2,2,0,0}  	; sub_clock, main_clock, color theme, menu icon(사용안함)
nv_write display_screen	 	{1,0,0,0}	; main_wall_paper(main), sub_wall_paper, power_on, power_off   
nv_write contrast_lvl 		{50}	; (sub lcd) removed main_lcd
nv_write location_set 		{1}	; 1 -> location on 0-> E911 only
nv_write messaging_set		{1,1}	
nv_write sms_sound 		{8,8,8}
nv_write manner_mode 		{0}	; false , true{1}
nv_write emergency_num1 	{"066"}	; Up to 48 Digits
nv_write emergency_num2 	{"*911"}	; Up to 48 Digits ;2006.3.8 수정
nv_write emergency_num3 	{"*611"}	; Up to 48 Digits ;2006.3.8 수정	
nv_write backtop_beep		{1}
nv_write phone_setup        	{1}	; Answer Call - Open/Any Key : 0, SEND Only : 1 ;2006.3.8 1로 변경
nv_write wclock_choice      	{5}	; default NewYork -> Mexico City
nv_write power_saver		{0}
nv_write photo_setting_RQS	{1,1,2}	; photo_set_ImageSize(1), photo_set_Quality(1), photo_set_ShutterSound(2)
nv_write video_setting_RQ	{0,1}	; video_set_ImageSize(0), video_set_Quality(1) (사용안함)
nv_write tty 			{3}	; TTY Full(0), TTY+TALK(1),TTY+HEAR(2),TTY off(3)
nv_write number_size		{1,0}	; (size, color(사용안함)) 0:normal 1:large ;normal -> large 로 변경 VZW 요구사항 2004.03.03
nv_write ringer_id_onoff 	{1}	; Off   new item 2003.11.30
nv_write picture_id_onoff 	{1}	; Off   new item 2003.11.30
nv_write sound_ringers 		{8,8,0,0xffff,0}	; (caller ID, No Caller ID, Restrict, all calls, vibrate options)  4,5번 item 추가 2003.11.30 -> 임수희 4번값변경 4->0xffff
nv_write status_led 		{0,0,0,0,0,0,0}	;incoming_call, missed_call, new_sms_alert, reminders, in_service_area, roaming, battery_low
nv_write bt_power_onoff		{0}	;bluetooth power on/off

;=========================================================================
;F/W ITEM
;=========================================================================
nv_write rf_config           	{6}
nv_write vbatt               	{165,239}    											; VX8100 2005.03.02 {165, 239} <- {164,238}
nv_write qdsp_snd_ctrl		{0,3072,0,7168,0,0,150,61,0,6,6,0,1200,0,6,0}
nv_write audio_adj_phone	{0,3072,0,0,3072,0,0,0,0}
nv_write audio_adj_earjack	{20476,32767,0,20476,32767,0,0,0,0}
nv_write audio_adj_hfk		{0,0,0,0,4096,0,0,0,0}
;nv_write audio_adj_spk		{0,0,0,0,0,0,0,0,0}	
nv_write audio_adj_spk		{16384,0,0,16384,0,0,0,0,0} ;2006.3.22 최종 조정
nv_write audio_adj_bt		{0,0,0,0,0,0,0,0,0}

;=========================================================================
;BREW ITEM
;=========================================================================
nv_write brew_bkey 		{0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 

;brew_wflags
;DIF_USE_A_KEY		0x0001	;If set, use AKey value
;DIF_TEST_ALLOWED	0x0002	;This phone can be used to test local apps
;DIF_MIN_FOR_SID	0x0004	;Use the MIN for the SID if set
;DIF_PREPAY		0x0008	;Prepay phone

nv_write brew_wflags 		{0x0004}	; (word(2 byte))  Brew Test 4 : Disable, 6 : Enable 		
nv_write brew_user_auth 	{1}			; (1 byte) APOLICY_NONE(0), APOLICY_SID(1), APOLICY_TEXT(2), APOLICY_NUM(3)
nv_write brew_app_policy 	{3}			; (1 byte) PPOLICY_BREW(0), PPOLICY_CARRIER(1), PPOLICY_BREW_AND_CARRIER(2), PPOLICY_BREW_OR_CARRIER(3)
nv_write brew_carrier_id 	{91}			; 8bit  		
nv_write brew_primary_ip 	{207,  83, 200, 200} 
nv_write brew_secondary_ip 	{207,  83, 200, 201}
nv_write brew_primary_server	{"brew.iusacell3g.com"}	; 64 byte character
nv_write brew_secondary_server	{"brew.iusacell3g.com"}	; 64 byte character
nv_write brew_platform_id	{1139}			; (word) ;**************************** SHOULD BE CHANGED LATER **********************

;=========================================================================
;GPSONE ITEM
;=========================================================================
nv_write gps1_lock 		{0}
nv_write gps1_pde_address 	{0xCF53C8EE} 	;0xCF53C8EE=207.083.200.238
nv_write gps1_pde_port 		{0x22b8} 	; 0x22b8=8888
nv_write gps1_pde_transport 	{0} 		; 0:IP, 1:DBM

;=========================================================================
; SMS ITEM
;=========================================================================
nv_write sms_priority_sel 			{0}	; 0(Normal), 1(Urgent)
nv_write sms_mo_max_userdata  			{150}	; 0x0(=180) - 0xFFFF	; 180 -> 170 (by eklee 02.08.22)
nv_write sms_mo_l3_ack				{1}	; 0(False), 1(True) 
nv_write sms_mo_so				{1}	; 0(8K), 1(13K) -> 1(8K:SO6), 0(13K:SO14) 
nv_write sms_settings_signature			{0}	; SMS_SIGNATURE_OFF(0), SMS_SIGNATURE_ON(1), SMS_BUSINESS_CARD(2) 	
nv_write sms_settings_direct_view		{0}	; 0(Off), 1(On)
nv_write sms_settings_voice_mail		{0,8,#9}; ALERT,RINGTONE,NUMBER
nv_write sms_settings_textmsg_alert		{8}	; defalut 
nv_write sms_settings_page_alert		{0}	; SET TO 0
nv_write sms_2min_alert_sel 			{1}	; 2 min alert on -> 1, off -> 0	;2006.3.15 default:off ;2006.4.8 new PRI:on (which is correct, hugh?)
nv_write msg_settings_auto_save 		{0}	; MSG_AUTO_SAVE(0), MSG_PROMPT(1), MSG_DO_NOT_SAVE(2)	
nv_write msg_settings_auto_delete 		{1}	; 0(Off), 1(On) ;2006.3.15 default:off ;2006.4.8 new PRI:on (which is correct, hugh?)
nv_write msg_settings_entry_mode  		{0}	; MSG_T9EN(0), MSG_ABC(1), MSG_123(2)
nv_write sms_settings_voicemail_alert		{8}	;5(Low Beeps)
nv_write sms_voice_record			{0}	;0~255
nv_write page_alert_custom_ring_tone		{8}	;Iusacell Jingle
nv_write sms_alert_custom_ring_tone 		{8}	;Iusacell Jingle
nv_write sms_delivery_sel                       {0}     ; Delivery ACK 1(On), 0(Off)
;=========================================================================
; MMS ITEM
;=========================================================================
;James Dong jae Shin(2004/OCT/16)-------------------------------Start(VIVO Specific)
nv_write mms_settings_auto_download		{1}   	; 1(MMS_ON), 0(MMS_OFF) ;2006.3.8 1로 수정
nv_write mms_settings_photo_alert		{0}	; 0(Low Beep Once), 1(Low Beeps), 2(Laud Beep Once), 3(Loud Beeps), 4~13(Ring1~Ring10)
nv_write mms_ip 				{0,0}	; Argument1 : DNS Q(0), No DNS Q(1) / Argument2: 32byte characters
nv_write mms_mmsc_server_name_ip 		{25, "http://mms.iusacell3g.com"} 		; 48 byte characters
nv_write mms_gateway_server_name_ip		{0, ""}			; 48 byte characters
nv_write mms_http_method_uri 			{25, "http://mms.iusacell3g.com"} ;
nv_write mms_uaprof_url_in_user_agent 		{54, "https://servicios.iusacell.com.mx/lg/MX510/mx510v1.xml"} 	; 54 byte characters
nv_write mms_upload_addr {4, "8888" } ; Upload Address (short code)


;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_qnc_enabled 			{0}		; 0-QNC Disable  1-QNC Enable
nv_write data_so_set      			{2}		; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write data_mdr_mode 				{3}		; DS_MDR_MODE_MDR_ONLY = 0  Use only MDR packet data services
nv_write data_pkt_orig_str 			{4, "#777"}	; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_auto_packet_detection 		{0}		; 0-Disable   1-Enable

; 1x ppp user_id. 이 값이 설정되면 mip profile 보다 우선적으로 사용된다. 없으면 mip profile 0 의 NAI 를 사용.
nv_write ppp_user_id {32,"0000000000@modem.iusasipevdo.com"}	; Max of 127 chars in User ID ;2006.6.12 사업자요구로 변경
; 1x ppp password. 이 값이 설정되면 mip profile 보다 우선적으로 사용된다. 없으면 mip profile 0 의 AAA SS (dec ESN) 를 사용.
nv_write ppp_password          {8,"BJMPW504"}      ; Max of 127 chars in Password

nv_write pref_for_rc 				{3}		; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)    
nv_write data_scrm_enabled 			{1}		; 0-SCRM Disable 1-SCRM Enable
;nv_write data_trtl_enabled 			{1}		; 0-TRTL Disable 1-TRTL Enable ;2006.4.12 삭제.(MSM5XXX 시리즈만 사용)
nv_write ds_default_baudrate 			{0x0011}; 0x0000 (19.2kbps),0x0011(115.2kbps) ,0x00012(230.4kbps)
nv_write diag_default_baudrate			{0x000e}; 0x000e(38.4kbps), 0x0011(115.2kbps)

; hdr ppp user_id. 이 값이 설정되면 mip profile 보다 우선적으로 사용된다. 없으면 mip profile 0 의 NAI 를 사용.
nv_write hdr_an_auth_user_id_long {20,"00000000@iusabam.com"} ; EVDO AN authetication user id
; hdr ppp password. 이 값이 설정되면 mip profile 보다 우선적으로 사용된다. 없으면 mip profile 0 의 AAA SS (dec ESN) 를 사용.
nv_write hdr_an_auth_passwd_long  {10,"0000000000"}                   ; EVDO AN authetication password

nv_write ds_qcmip {2}                         ; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only
nv_write ds_mip_active_prof  {0}              ; current active profile index
nv_write ds_mip_num_prof     {2}              ; number of profiles (max 6) ;parkboo 2006.4.8 2->1 ;2006.6.15 사업자요구로 다시 복구
nv_write ds_mip_enable_prof  {1,1,0,0,0,0}    ; diable - 0, enable - 1 ;2006.6.15 사업자요구로 다시 복구
nv_write ds_mip_retries      {2}              ; number of retries
nv_write ds_mip_retry_int    {3}              ; retry interval = n*250(ms) + 1000ms
nv_write ds_mip_pre_re_rrq_time {60}           ; pre-registration time - minute
nv_write ds_mip_2002bis_mn_ha_auth  {0}       ; disable - 0, enable -1
nv_write ds_mip_rrq_if_tfrk  {1}              ; send a registration only in use : disable-0, enable-1
nv_write ds_mip_qc_drs_opt   {1}              ; dormant handoff optimization

;Comment : MIP general profile information {index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
;Comment : reverse tunneling, home address, primary ha address, secondary ha address}
nv_write ds_mip_gen_user_prof {0,26,"0000000000@iusamipevdo.com",1,257,1,2,1,0x00000000,0xFFFFFFFF,0xCF53C8DE}
nv_write ds_mip_gen_user_prof  {1,32,"0000000000@modem.iusamipevdo.com",1,257,1,2,1,0x00000000,0xFFFFFFFF,0xCF53C8DE} ;2006.6.12 사업자요구로 변경 ;2006.6.15 사업자요구로 다시 복구
;nv_write ds_mip_gen_user_prof {1,22,"0000000000@iusamip.com",1,257,1,2,1,0x00000000,0xC0C8023C,0xC0C8023C} ;2006.4.8 removed

;Comment : MIP shared secret {index,mn-ha ss length,mn-ha ss,mn-aaa ss length,mn-aaa ss,
nv_write ds_mip_ss_user_prof    {0,16,"iusacelliusacell",8,"BJMPW504"} ;add item
nv_write ds_mip_ss_user_prof    {1,16,"iusacelliusacell",8,"BJMPW504"} ;2006.4.8 removed ;2006.6.15 사업자요구로 다시 복구

;=========================================================================
;UP ITEM : for UP 6.2
;=========================================================================
efs_write "OWS/aptable1.fil"
efs_write "OWS/keytable1.fil"
efs_write "OWS/paramtable1.fil"
efs_write "OWS/wdptable1.fil"

;=========================================================================
;ANIMATION IMAGE ITEM
;=========================================================================
efs_write "dload/closing1.bit2"
efs_write "dload/extClosing1.bit2"
efs_write "dload/extOpening1.bit2"
efs_write "dload/opening1.bit2"
efs_write "dload/nigpsAnim.bit2"
efs_write "dload/wapgpsAnim.bit2"

;=========================================================================
;Eri Sound
;=========================================================================

;=========================================================================
;MMS Image
;=========================================================================
efs_write "mms/DecodeErrorAnimation.jpg"
efs_write "mms/DecodeErrorImage.jpg"
efs_write "mms/NotSupportedImage_UnknownIm.jpg"
efs_write "mms/phoneOnConversation.jpg"
efs_write "mms/TooBigErrorImage.jpg"

;=========================================================================
;Charging
;=========================================================================
nv_write spare_1		{1}
