;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;=========================================================================
;  File name: MX85IB00.scr
;  Made by  : LGE
;  Version  : 00_00
;  Date     : 09/15/2006
;-------------------------------------------------------------------------
;  when		who		what
;-----------	-------		------------------------------------------------
; 2006/09/15	hohos		Initial Version
; 2006/09/21	icsly		sms_ems_enable	{1} -> {0}
; 2006/09/21	hohos		ppp_user_id	{32} -> {33}
; 2006/09/27	icsly		wclock_choice	{30,...,47,0} -> {30,...,41,0}
;2006/09/27	JOYS		back_light	{15}   ->   {5}
;				voice_priv	{1}     ->   {0}
;				language_selection {0}     ->   {1}
;				gps1_lock	{3}     ->   {0}
;				call_sounds	{4,9,6,0xFFFF,0}   -> {0,0,0,0,0}
;				eri_text	{1}     ->   {0}
;				display_themes 	주석처리
;				clock_format	{0,0}     ->   {1,0}
;				call_answer	{0}     ->   {1}					
;				charging_alert	{0}     ->   {1}
;				msg_settings_auto_save	 {0}     ->   {1}
;				msg_settings_auto_delete {0}     ->   {1}
;				msg_settings_entry_mode  {1}     ->   {0}
;				sms_voicemail_alert 	 {10}     ->   {0}
;				sms_textmsg_alert   	 {1}     ->   {0}
;				sms_voicemail_cb	 {3,"*86"}  ->  {2,"#9"}
;				mms_set_tone_alert 	 {1}     ->   {0}
; 2006/09/27	hohos		ds_qcmip 기본값을 MIP Only 로 설정	
;				ppp_user_id	{33} -> {32}
;				OWS file 쓰는 부분 임시로 막음.								
; 2006/09/27	icsly		sms_mo_max_userdata	{160} -> {150}
; 2006/09/29	hohos		UAprof  MX 용으로 변경
; 2006/10/11	hohos		ppp_carrier	{3} -> {0}
; 2006/10/12 	hohos		MIP Parameter 초기값 수정
				mip profile 2개 지원하도록 수정
; 2006/10/12 	JHJ		sid_nid_lock    {0,0} -> {0,65535}
;				system_pref 제거	nv_write system_pref {0, "automatic b"}          ; System preference, actually default to band preference
;							nv_write system_pref {1, "automatic b"}
; 2006/10/12	hohos	mms_set_auto_receive {1} -> {0}
;					wallpaper_main	{0,0,1} -> {0,0,0}
;					OWS file write 추가 
; 2006/10/19 	hohos	MIP 관련 Password 쓰는 방식 수정 ( VX 대로 원복 ) 
; 2006/10/21	hohos 	call_answer	{1}     ->   {0} Slide up 이 기본입니다.
;					charging_alert	{1}     ->   {0}
;					OTKSL 추가
; 					nv_write ds_mip_rrq_if_tfrk	{0}	추가
;					mms_test_mmsc_url		{21, "http://203.248.152.20"} 	; 48 byte characters
;					mms_test_mmsc_upload_url	{13, "mml.vzpix.com" }			; Upload Address
; 					msg_settings_auto_save     	{0}		; On
;					mms_set_auto_receive		{1}		; On
; 2006/10/25	hohos	nv_write alarm_sounds		{6,0} -> {0,0}
; 2006/10/29 	hohos	nv_write emer_test_num		{"*911"}
; 2006/10/29	Joys	OTA Items 내의 	nv_write imsi_t_addr_num    	{0, 255} 주석으로 막혀있으므로 제거함.
; 2006/10/29	Joys	OTA Items 내의  nv_write imsi_t_addr_num    	{1, 255} 주석으로 막혀있으므로 제거함.
; 2006/10/29	Joys	UI Items 내의	nv_write backtop_beep		{1}    주석으로 막혀있으므로 제거함.
; 2006/10/29	Joys	UI Items 내의   nv_write display_themes		{0}    주석으로 막혀있으므로 제거함.
; 2006/10/29	Joys	UI Items 내의   nv_write power_onoff_anim	{0}    주석으로 막혀있으므로 제거함.
; 2006/10/29	Joys	DATA Items 내의	nv_write ds_mip_rm_nai 		{0,32,"0000000000@modem.iusamipevdo.com")주석으로 막혀있으므로 제거함.
; 2006/10/29	Joys	DATA Items 내의	nv_write ds_sip_rm_nai 		{32,"0000000000@modem.iusasipevdo.com"}주석으로 막혀있으므로 제거함.
; 2006/10/31	hohos	pref_voice_so {0,  1, 0x0003, 0x0003, 0x0003} , charging_alert	{1}
; 2006/11/01	hohos	msg_settings_auto_save     	{1}		; Off
; 2006/11/07	hohos	clock_format			{1, 0} -> {0, 0}
;					sms_2min_alert_sel       {3,3,3,3} -> {1,1,1,1}
;					mms_set_reminder_alert		{3} -> {2}
;					mms_mmsc_server_post_url	{25, "http://mms.iusacell3g.com"}
;					mms_mmsc_server_post_cgi	{0, ""}
;					mms_test_mmsc_url		{25, "http://mms.iusacell3g.com"} 
;					mms_test_mmsc_upload_url	{4, "8888"}
; 2007/01/17	icsly		home_sid_nid	{1525,65535} -> {25100,65535}
;				msg_settings_auto_delete	{1} -> {0}	; On -> Off
;				msg_settings_auto_save		{1} -> {0}	; MSG_DO_NOT_SAVE(1) -> MSG_AUTO_SAVE(0)
; 2007/01/24	icsly		banner		{"IUSACELL 3G"} -> {"3G EVOLUTION"}
; 2007/02/09	icsly		msg_settings_auto_delete	{0} -> {1}	; Off -> On
;				msg_settings_auto_save		{0} -> {1}	; MSG_AUTO_SAVE(0) -> MSG_DO_NOT_SAVE(1)
; 2007/02/14	icsly		emergency_num2			{"*911"} -> {"*611"}
;				emergency_num3			{"*611"} -> {"*911"}
;-----------	-------		------------------------------------------------


;spc "000000"                         ; does not need at LGDP DLL
;wait 2
mode offline-d
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model
wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================
nv_write name_nam       {0, "IUSACELL"}     ; NAM 1 Name
nv_write name_nam       {1, "IUSACELL"}     ; NAM 2 Name

nv_write imsi_mcc	{0, "000"};	   
nv_write imsi_mcc	{1, "000"};
nv_write imsi_11_12	{0, "00"};
nv_write imsi_11_12	{1, "00"};

nv_write min1           {0, "000-0000", "000-0000"}
nv_write min1           {1, "000-0000", "000-0000"}
nv_write min2           {0, "000", "000"}            ; NAM 0 has one active MIN2,
nv_write min2           {1, "000", "000"}           

nv_write imsi_t_mcc     {0, "000"}               
nv_write imsi_t_mcc     {1, "000"}
nv_write imsi_t_11_12   {0, "00"}
nv_write imsi_t_11_12   {1, "00"}
nv_write imsi_t_s1      {0, "000-0000", "000-0000"}
nv_write imsi_t_s1      {1, "000-0000", "000-0000"}
nv_write imsi_t_s2      {0, "000", "000"}
nv_write imsi_t_s2      {1, "000", "000"}
                                                 ; NV_DIR_NUMBER_PCS_I      /*123456789012345*/ using 10 digits
nv_write dir_number_pcs {0, "0000000000"}        ; NAM 0 : NV_DIR_NUMBER_PCS_I
nv_write dir_number_pcs {1, "0000000000"}        ; NAM 1 : NV_DIR_NUMBER_PCS_I

                                                 ; Primary CDMA Channels for A carrier and B carrier
print "Programming Primary CDMA Channel"
nv_write pcdmach        {0, 283, 384}            ; A and B primary CDMA channels
nv_write pcdmach        {1, 283, 384}

                                                 ; Secondary CDMA Channel
print "Programming Secondary CDMA Channel"
nv_write scdmach        {0, 691, 777}            ; set only if secondary channels offered
nv_write scdmach        {1, 691, 777}

nv_write home_sid_nid	{0,25100,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write home_sid_nid	{1,25100,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock	{0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock	{1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}

nv_write mob_term_home    {0, true, true}
nv_write mob_term_home    {1, true, true}
nv_write mob_term_for_sid {0, true, true}
nv_write mob_term_for_sid {1, true, true}
nv_write mob_term_for_nid {0, true, true}
nv_write mob_term_for_nid {1, true, true}

nv_write accolc {0, 0, 0}
nv_write accolc {1, 0, 0}

nv_write slot_cycle_index {2}

                                                  ;{Nam Name(0, 1), EVRC Capability(0:Off, 1:ON), Home_Page_Voice_SO(0: wildcard, Others : SO), Home_Page_Voice_SO(0 or SO), Home_Page_Voice_SO(0 or SO)}
nv_write pref_voice_so {0,  1, 0x0003, 0x0003, 0x0003} 
nv_write pref_voice_so {1,  1, 0x0003, 0x0003, 0x0003}

print "Programming Pref Mode"
nv_write pref_mode     {0, "Digital Only"}
nv_write pref_mode     {1, "Digital Only"}
nv_write hybrid_pref   {1}                        ; 1 : hybrid on,  0 : hybrid off

print "Programming Band Preferred"
nv_write band_pref {0, "pref_any"}
nv_write band_pref {1, "pref_any"}

print "Programming Roam Preferred"
nv_write roam_pref {0, "pref_any"}
nv_write roam_pref {1, "pref_any"}

nv_write stand_alone_mode {0}               ; 0 default OFF, 1 ON


;------------------------------------------------------------------------
print "Programming MRU table clear"
                                            ; except nam (first 0), '0' are 48(=4 X 12) times.
nv_write mru3_table {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru3_table {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};

                                             ; NAM Checksums must all be 0xffff
print "Programming NAM Checksums"
nv_write nam_chksum {0, 0xffff}
nv_write nam_chksum {1, 0xffff}
nv_write min_chksum {0, 0xffff, 0xffff}
nv_write min_chksum {1, 0xffff, 0xffff}

;=========================================================================

;=========================================================================
; OTA ITEM
;=========================================================================
nv_write nam_lock           		{0, 1}
nv_write nam_lock           		{1, 1}
nv_write otapa_enabled      		{0, 1}   ; enable
nv_write otapa_enabled      		{1, 1}   ; enable
nv_write spc_change_enabled 	{1}

;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key 	{0, 0x00000000, 0x00000000 } ; Nam 1 64 bits A-Key. Published at factory with Random number.
nv_write a_key 	{1, 0x00000000, 0x00000000 } ; Nam 2 64 bits A-Key. Published at factory with Random number.
nv_write ssd_a 	{0, 0x00000000, 0x00000000 }
nv_write ssd_a 	{1, 0x00000000, 0x00000000 }
nv_write ssd_b 	{0, 0x00000000, 0x00000000 }
nv_write ssd_b 	{1, 0x00000000, 0x00000000 }
nv_write count 	{0, 0}
nv_write count 	{1, 0}

;=========================================================================
;UI ITEM
;=========================================================================
nv_write sec_code       	{"000000"}      	; Security code
nv_write lock_code      	{"0000"}        	; Lock_code
nv_write otksl			{"000000"}		; One-time keypad subsidy lock
nv_write fsc			{"000000"}		; Field Service code

nv_write curr_nam				{0}                     ; Current NAM == NAM1
nv_write auto_nam				{0}                     ; Auto NAM == disable
nv_write ear_lvl				{6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write speaker_lvl			{6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write ringer_lvl				{4}                     ; 1~5 (Low, Med Low, Med, Med High, High), 1 (Vibrate only), 97 (Alarm Only), 1 (All Sounds Off)"
nv_write beep_lvl				{4}                     ; 0 (Off), 1~5 (Low, Med Low, Med, Med High, High)
nv_write cont_key_dtmf			{0}                     ; Normal (1), Long (0),  Off (2)
nv_write banner				{"3G EVOLUTION"}; 	;2007.01.24
nv_write auto_answer			{0, 0}                  ; On (1, 1), Off (0, 0)
nv_write auto_redial			{0, 0}                  ; Off (0, 0), Every 10 Seconds (1, 1), Every 30 Seconds (1, 3), Every 60 Seconds (1, 6)
nv_write back_light			{5}                    ; Default 5 Sec
nv_write lock				{0}                     ; Lock (1), Unlock (0)
nv_write auto_lock			{0}                     ; Power_up (1)
nv_write call_rstrc			{0}                     ; Off (0), On (1)
nv_write onetouch_dial			{1}                     ; Off (0), On (1)
nv_write beep_lvl_shadow		{4}                     ; 0 (Off), 1~5 (Low, Med Low, Med, Med High, High)
nv_write ear_lvl_shadow			{6}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write send_pin			{0}                     ; Off (0)
nv_write voice_priv			{0}                     ; Standard (0), Enhanced (1)
nv_write ringer_spkr_lvl		{6}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8), 98 (High & Vib), 99 (Vibrate)
nv_write beep_spkr_lvl			{6}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write language_selection		{1}                     ; English (0), Spanish (1)
nv_write auto_volume_enabled		{0}                     ; Off (0), On (1)
nv_write tty				{3}                     ; TTY Full (0), TTY+TALK (1),TTY+HEAR (2),TTY off (3)
nv_write gps1_lock			{0}                     ; Location ON/OFF (Location ON (0), MI (1), MT (2), E911 Only (3) )
nv_write manner_mode			{0}                     ; False (0), True (1)
nv_write alarm_only_mode		{0}                     ; False (0), True (1)
nv_write silence_all			{0}                     ; Sound On (0), Sound Off (others)
nv_write speaker_shadow_lvl		{6}                     ; Earpiece Volume on Speaker Phone Mode: 1~8 (Volume1 ~ Volume8)
nv_write spk_phone_beep_lvl		{6}                     ; Keypad Volume on Speaker Phone Mode: 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write call_sounds			{0,0,0,0,0}	        ; {Caller ID (0:Iusacell Jingle), No Caller ID(0:Iusacell Jingle), Restrict Calls(0:Iusacell Jingle), All Calls(0:Iusacell Jingle), Vibrate (0: Off, 1: On)}"
nv_write sms_sound			{1,0,0}
nv_write service_alerts			{0,0,0,0}               ; {Service Change (Not use), Minute Beep, Call Connect, ERI}, On (1), Off (0)
nv_write power_onoff_sounds		{1,1}                   ; {Power On, Power Off}, On (1), Off (0)
nv_write alarm_sounds			{0,0}                   ; {tone(6: Ringtone 2), vibrate (0: Off)}
nv_write eri_text			{0}                     ; On (1), Off (0)
nv_write key_light			{5}                     ; Default 5 Sec
nv_write wallpaper_main			{0,0,0}                 ; {location_type (0:phone memory, 1:phone efs, 2:sdcard), location_id (0:sdcard id), item_id (0: index)}
nv_write number_size			{1}                     ;  Normal (0), Large (1)
nv_write clock_format			{0, 0}                  ; {main (0: Normal, 1: Digital, 2: Analog, 3: Dual, 4: Off), front (0: Digital, 1: Minimize, 2: Off)}
nv_write shortcut				{0,0,0,0}               ; {Left, Up, Right, Down}
nv_write call_answer			{0}                     ; Slide Up (0), Send Only (1)
nv_write pc_port				{0}                     ; PC connection port  0 (USB), 1 (UART), 2 (BLUETOOTH), 3 (CLOSED)
nv_write ringer_id				{1}                     ; On (1), Off (0)
nv_write picture_id				{1}                     ; On (1), Off (0)
nv_write emergency_num1		{"066"}                 ; Up to 48 Digits
nv_write emergency_num2		{"*611"}                 ; Up to 48 Digits
nv_write emergency_num3		{"*911"}                ; Up to 48 Digits
nv_write wclock_choice			{30,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,41,0}
				                          ; {cur_Itm (30), set_DST, choice_city ( Mexico City: 41), line longtitude}
nv_write media_save_option		{0,0,0}                 ; {PIX, FLIX, SOUND} Phone memory (0), SD card (1)
nv_write dcam_video_elapsed_time  {15}                    ; elapsed time options (15, Available Memory)
nv_write dcam_photo_set_rqs	{1,2,0}                 ; {resolution(1: 640*480), quality(2: Fine), shutter sound(0: Shutter1)}
nv_write dcam_photo_menu_set	{0,0,0,9,0,1,0,0}       ; Initialize camera menu
nv_write dcam_video_set_rq		{0,1}                   ; {resolution (0), quality (1)}
nv_write dcam_video_menu_set	{0,0,0,9,0,0,0,0}       ; Initialize video menu
nv_write camera_flash_test		{81}                    ; Camera Flash On (85(0x55)), Off (others)
nv_write flix_set_as			{1,0,0,0,0,0,0,0,0,0}
nv_write equalizer_mode		{0}
nv_write visualizer_mode		{0}                     ; OFF (0), ON (1)
nv_write avr_call_alerts			{0}
nv_write avr_prompts_mode		{0}
nv_write avr_choice_list			{0}
nv_write avr_prompts_timeout	{0}
nv_write avr_sensitivity			{1}                     ; 0: High 1: Medium 2: Low
nv_write avr_prompts_sound		{0}                     ; 0: Speaker 1: Earpiece
nv_write bt_power_onoff			{0}                     ; OFF (0), ON (1)
nv_write beep_bt_lvl			{6}                     ; Off (0), 1~8 (Volume1 ~ Volume8)
nv_write ear_bt_lvl				{6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write use_my_mp3			{0}                     ; MOD Center Key Define: MOD Player (0), MP3 Player (1)
nv_write carrier_logo			{0}                     ; IUSACELL(0)
nv_write contrast_lvl			{0,0}
nv_write led_blink				{1}                     ; ON(1) OFF(0)
nv_write power_saver			{0}
nv_write edit_font				{0,0}
nv_write gps_test_num			{"922"}                 ; Up to 48 Digits
nv_write emer_test_num			{"*911"}                 ; Up to 48 Digits
nv_write flash_music_theme		{0}			  ; Music Theme 1 (0), Music Theme 2 (1)
nv_write charging_alert			{1}     		  ; OFF (0), ON (1)
nv_write status_softkey_color	{5}     		  ; (0~5) Color 1 ~ Color 6
nv_write touch_sensitivity		{0x41}     		  ; 0x41 : medium
nv_write location_set_lock		{0}     		  ; Security Location Lock Mode 0: unlock, 1:Lock
nv_write end_call_option		{0}     		  ; 0: slide down, 1:end key only
nv_write sidekey_guide			{1}     		  ; ON(1) OFF(0)
nv_write touchkey_activate_option {1}			  ; VoiceKey Once{0}, Press Once{1}, Press Twice{2}

;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_pkt_orig_str      			{5, "#777"}    ; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_mdr_mode          			{3}            ; Service Option 33 (1x channel) = 3 Use only low-speed packet data = 2
nv_write data_auto_packet_detection 		{0}        ; 0-Disable   1-Enable
nv_write data_so_set            			{2}            ; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write diag_default_baudrate  			{0x000e}       ; 0x000e(38.4kbps), 0x0011(115.2kbps) 
nv_write data_qnc_enabled       			{0}            ; 0-QNC Disable  1-QNC Enable
nv_write ppp_user_id            			{32,"0000000000@modem.iusasipevdo.com"}	; Max of 127 chars in User ID
nv_write ppp_password   	       			{8,"BJMPW504"}      ; Max of 127 chars in Password
nv_write data_scrm_enabled      			{1}            	; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled      			{1}            	; 0-TRTL Disable 1-TRTL Enable
nv_write pref_for_rc            				{3}            	; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)    
nv_write ds_default_baudrate    			{0x0011}		; 0x0000 (19.2kbps),0x0011(115.2kbps) ,0x00012(230.4kbps)
nv_write ds_qcmip               			{2}            	; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only
nv_write ds_mip_active_prof     			{0}            	; current active profile index
nv_write ds_mip_enable_prof     			{1,1,0,0,0,0}  ; diable - 0, enable - 1 {1st Profile, 2nd Profile, 3rd Profile, .... }
nv_write ds_mip_num_prof        			{2}            	; number of profiles (max 6) 
nv_write ds_mip_retries         			{2}            	; number of retries
nv_write ds_mip_retry_int       			{3}            	; retry interval = n*250(ms) + 1000ms
nv_write ds_mip_pre_re_rrq_time 			{60}            	; pre-registration time - minute
nv_write ds_mip_rrq_if_tfrk				{0}			; disable - 0, enable -1
nv_write ds_mip_2002bis_mn_ha_auth  	{0}        		; disable - 0, enable -1
nv_write ds_mip_qc_drs_opt      			{1}            	; dormant handoff optimization. disable - 0, enable - 1
                                               ;Comment : MIP general profile information {index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
                                               ;Comment : reverse tunneling, home address, primary ha address, secondary ha address}
nv_write ds_mip_gen_user_prof   			{0,26,"0000000000@iusamipevdo.com",1,257,1,2,1,0x00000000,0xFFFFFFFF,0xCF53C8DE} 
nv_write ds_mip_gen_user_prof  			{1,32,"0000000000@modem.iusamipevdo.com",1,257,1,2,1,0x00000000,0xFFFFFFFF,0xCF53C8DE}
nv_write ds_mip_dmu_pkoid       			{0,10}         ; { Index , Public key organization indentifier }
nv_write ds_mip_dmu_mn_auth     		{0,0x01,0xB2,0x07}            ; { Index , DMU MN authenticator - 111111base10 } 
nv_write hdr_an_auth_user_id_long 		{20,"00000000@iusabam.com"} ; { Length , EVDO AN authetication user id }
nv_write hdr_an_auth_passwd_long  		{10,"0000000000"}                   ; EVDO AN authetication password
nv_write dun_cable_mode         			{1}            ;0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode            			{1}            ;0=disable bt dun,1=enable bt dun
					       ;Comment : MIP&SIP NAI(Network Access Identifier) for DUN 

nv_write ppp_carrier            				{0}            ; 0-IUSACELL 1-Verizon 2-USC 3-SKT  4-Script. Test NV Item.  

nv_write ds_mip_ss_user_prof    			{0,16,"iusacelliusacell",8,"BJMPW504"}
nv_write ds_mip_ss_user_prof    			{1,16,"iusacelliusacell",8,"BJMPW504"}

;=========================================================================
; MSG ITEM
;=========================================================================
nv_write msg_settings_auto_save     	{1}    		; MSG_AUTO_SAVE(0), MSG_DO_NOT_SAVE(1), MSG_PROMPT(2) 
nv_write msg_settings_auto_delete   	{1}     		; 0(Off), 1(On)
nv_write msg_settings_entry_mode    	{0}     		; MSG_T9EN(0), MSG_ABC(1), MSG_123(2)
nv_write msg_settings_vibrate_alert   	{0,0,0,0}		; On(1), Off(0)

;=========================================================================
; SMS ITEM
;=========================================================================
nv_write sms_orig_msg_id              	{1}   		; 0X0001 - 0XFFFF
nv_write sms_mo_max_userdata         {150} 		; Up to 220 Byte (160 character(= 140 Byte))
nv_write sms_mo_l3_ack                	{1}   		; On(1), Off(0)
nv_write sms_mo_so                    	{1}   		; 8K(1), 13K(0)
nv_write sms_txt_cb_enable            	{1}   		; On(1), Off(0)
nv_write sms_voicemail_record     	{0,0} 		;
nv_write sms_settings_signature       	{0}   		; None(0), Custom(1)
nv_write sms_settings_auto_view     	{0}   		; On(1), Off(0)
nv_write sms_mo_causecode 		{0} 
nv_write sms_ems_concat_reference	{0}
nv_write sms_voicemail_alert 		{0}  		; 0(Iusacell Jingle), 1(Low Beeps),
nv_write sms_textmsg_alert   		{0}  	 	; 0(Iusacell Jingle)
nv_write sms_info_alert				{1}   		; 0(silent) 1(icon only) 2(vibrate icon)
nv_write sms_mo_errorclass			{0}
nv_write sms_settings_font_size		{1}   		; small(0) large(1)
nv_write sms_voicemail_cb			{2,"#9"} 	; 32Byte(ASCII)
nv_write sms_urgent_voice_record  	{0}   		; 
nv_write sms_mo_access                	{1}   		;
nv_write sms_2min_alert_sel           	{1,1,1,1} 	; Once(0), Every 2 Minutes(1), Every 15 Minutes(2), Off(3)
nv_write sms_message_cb          	{10, 0}		;
nv_write sms_settings_name_card    	{0} 		; Off(0)  On(1)

;=========================================================================
; EMS ITEM
;=========================================================================
nv_write sms_settings_auto_play       	{0} 		; On(1), Off(0)
nv_write sms_ems_enable               	{0}  		; On(1), Off(0) 

;=========================================================================
; UP ITEM : for magellan 
;=========================================================================
efs write "OWS/paramtable1.fil"
efs write "OWS/wdptable1.fil"

;=========================================================================
;BREW ITEM
;=========================================================================
nv_write brew_carrier_id 				{91}
nv_write brew_platform_id 			{1136}				            ;VX8500 platform id
nv_write brew_bkey 				{0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 
nv_write brew_server    				{"brew.iusacell3g.com,brew.iusacell3g.com"}  ; 64 byte character
nv_write brew_download_flags 		{0x0004}                   	; DIF_USE_A_KEY(0x0001) - A Key: 1 or B Key: 0 Option, DIF_TEST_ALLOWED(0x0002) - Test Disable: 0, Test Enable: 2
                                                        	; DIF_MIN_FOR_SID(0x0004) - Use MIN for Subscriber ID: 4,  Not use: 0, DIF_PREPAY(0x0008) - Prepay:8, Postpay:0
nv_write brew_auth_policy 			{1}                             	; APOLCY_NONE(0), APOLCY_SID(1), APOLCY_TEXT(2), APOLCY_NUM(3) 
nv_write brew_privacy_policy 		{3}                            	; PPOLICY_BREW(0), PPOLICY_CARRIER(1), PPOLICY_BREW_AND_CARRIER(2), PPOLICY_BREW_OR_CARRIER(3)
nv_write brew_sid_length 			{32}	
nv_write brew_disallow_dormancy		{1}				; TRUE	
;=========================================================================
; MMS ITEM
;=========================================================================
nv_write mms_set_auto_receive		{1}   ; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_set_read_ack			{1}   ; 0(ON), 1(OFF)
nv_write mms_set_delivery_ack		{0}   ; 0(MMS_ON), 1(MMS_OFF)

nv_write mms_set_tone_alert			{0}   ; 0(Iusacell Jingle), 1(Low Beeps), 2(Laud Beep Once), 3(Loud Beeps),4(VZW Default Tone),5~14(Ring1~Ring10), 15(No Ring)
nv_write mms_set_vibrate_alert		{0}   ; 0(VIBRATE OFF), 1(VIBRATE ON)
nv_write mms_set_reminder_alert		{2}   ; 0(REMIND ONCE), 1(REMIND EVERY2MIN), 2(REMIND EVERY15MIN), 3(REMIND OFF)

nv_write mms_mmsc_url				{25, "http://mms.iusacell3g.com"} ; 48 byte characters
nv_write mms_mmsc_upload_url		{4, "8888"}   ; Upload Address
nv_write mms_mmsc_uaprof_url		{56, "https://servicios.iusacell.com.mx/lg/MX8500/mx8500v1.xml"} ; Max 64 byte characters

nv_write mms_set_retry_num			{3}   ; 0, 1, 2, 3

nv_write mms_send_from_add 		{2}   ; MDN Only (0), 1MDN (1),  +1MDN (2)         

nv_write mms_mmsc_server_post_url	{25, "http://mms.iusacell3g.com"}	; Post URL
nv_write mms_mmsc_server_post_cgi	{0, ""}							; CGI URL
nv_write mms_mmsc_user_agent		{14,"LGE-MX8500/1.0"}			; User Agent Profile name

nv_write mms_test_authorization		{0}								; 0 : Commercial, 1 : Lab
nv_write mms_test_mmsc_url			{25, "http://mms.iusacell3g.com"} 	; 48 byte characters
nv_write mms_test_mmsc_upload_url	{4, "8888"}						; Upload Address

;=========================================================================
;F/W ITEM
;=========================================================================
nv_write rf_config					{6}

nv_write vbatt						{87,226}                                    ; VX8500 2006.03.16 for REV.D {87, 226} <- {165,239}
nv_write qdsp_snd_ctrl				{0,0,0,0,0,0,0,0,0,7,6,0,0,0,0,-800}        ;
nv_write audio_adj_phone			{0,0,0,0,0,0,0,0,0}                         ;
nv_write audio_adj_earjack			{0,0,0,0,0,0,0,0,0}                         ;
nv_write audio_adj_hfk				{0,0,0,0,0,0,0,0,0}                         ;
nv_write audio_adj_spk				{0,0,0,0,0,0,0,0,0}                         ;
nv_write audio_adj_bt				{0,0,0,0,0,0,0,0,0}                         ;
;=========================================================================

;=========================================================================
;GPSONE ITEM
;=========================================================================
nv_write gps1_pde_address 			{207,083,200,238}
nv_write gps1_pde_port 			{8888}
;=========================================================================

;=========================================================================
;MMS IMAGE ITEM
;=========================================================================
efs write "mms/DecodeErrorAnimation.jpg"
efs write "mms/DecodeErrorImage.jpg"
efs write "mms/NotSupportedImage_UnknownImage.jpg"
efs write "mms/phoneOnConversation.jpg"
efs write "mms/TooBigErrorImage.jpg"
;=========================================================================

;=========================================================================
;ANIMATION IMAGE ITEM
;=========================================================================
efs write "dload/closing1.bit2"
efs write "dload/opening1.bit2"
;=========================================================================

;=========================================================================


mode reset
