;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;=========================================================================
;  File name: CX855T02.SCR
;  Made by  : LGE
;  Version  : T02
;  Date     : 01/10/2007
;-------------------------------------------------------------------------
;  when         who        what
;----------    -------    ------------------------------------------------
;12/12/2007    June      임시 설정
;01/03/2008    Joys      아래 값들 변경함
;			ds_qcmip {0} -> {2}                                              																																																																																																																											
;			ppp_carrier {3} -> {0}                                           																																																																																																																											
;			brew_server {"brew.iusacell3g.com,brew.iusacell3g.com"} 으로 변경																																																																																																																											
;			brew_carrier_id		{91} 로 변경                             																																																																																																																											
;			brew_platform_id	{1198}	VX8550 PID 로 변경               																																																																																																																											
;		        아래의 주석으로 막힌 아이템들 제거                                            																																																																
;			FLASH UI ITEM / ANIMATION IMAGE ITEM / JAVA & CALL ITEM                     																																																																
;01/09/2008    Joys     world clock city change to Mexico City.
;			nv_write wclock_choice 49->44
;01/16/2008    Joys     ppp_password {8,0x42, 0x4A, ...} -> {16,0x42, 0x4A, ...} 
;			ds_mip_ss_user_prof {0,8,0x69,0x75,...,8,0x42, ...} -> {0,16,0x69,0x75,...,16,0x42, ...}
;			ds_mip_ss_user_prof {1,8,0x69,0x75,...,8,0x42, ...} -> {1,16,0x69,0x75,...,16,0x42, ...}
;			hdr_an_auth_passwd_long {10,0x30,0x30,... } -> {16,0x30,0x30,... }
;			msg_priority_sel 사용지 않는 것으로 확인되어 제거
;			msg_delivery_sel 사용지 않는 것으로 확인되어 제거
;			mms_mmsc_uaprof_url 모델명 8550으로 변경.{56, "https://servicios.iusacell.com.mx/lg/MX8550/mx8550v1.xml"}
;			mms_mmsc_user_agent{47,"LGE-MX8700/1.0.UP.Browser/6.2.3.2.(GUI).MMP/2.0"}-> {14,"LGE-MX8550/1.0"}
;01/21/2008	hayley	emer_test_num 911 -> *911 로 변경.
;01/23/2008	hayley	ppp_password	{8,"BJMPW504"}
;			ds_mip_ss_user_prof {0,16,"iusacelliusacell",8,"BJMPW504"}
;			ds_mip_ss_user_prof {1,16,"iusacelliusacell",8,"BJMPW504"}
;			hdr_an_auth_passwd_long {10,"0000000000"}
;01/24/2008	June	MMS 관련 Item 추가
;			mms_mmsc_server_post_url, mms_mmsc_server_post_cgi, mms_test_authorization
;01/28/2008	June	MMS UA String 변경
;02/01/2008     CBCHO   cont_key_dtmf  Normal (1)-> Long (0) 으로 변경 IUS 사업자 요구
;02/03/2008	flower80	answer_option (3) -> (2) 로 변경. 현지 법인 요구사항
				end_call_option (3) -> (2) 로 변경. 현지 법인 요구사항.
;03/02/2008	hayley	world clock city change to Mexico City.
;			nv_write wclock_choice 49->44
;02/04/2008	flower80 name_nam IUSACELL -> 3G EVOLUTION 으로 변경
;02/05/2008	flower80	answer_option (2) -> (3) 로 다시 변경. 현지 법인 요구사항
;				end_call_option (2) -> (3) 로 변경. 현지 법인 요구사항.
;02/06/2008	hayley	wclcok_choice 갯수 수정. 60-> 53
;02/16/2008	hyk	OWS 값 추가.

;02/22/2008	Joys	nv_write vbatt (20, 190) -> (30, 180) 변경.
;02/22/2008	Joys	nv_write system_pref 막여있던 부분 적용함.
;02/26/2008	flower80	wclock_choice 국가 번호를 맨뒤로 옮김.. 왜 이런지 알 수 없음..
;
;02/26/2008	ariesgon	Primary DNS IP/Secondary DNS IP 207.83.200.200/207.83.200.201 추가적용
;02/27/2008	PARKJINSOO	auto_redial off로 수정
;03/12/2008	HYK		New UA Prof apply
;03/25/2008	Joys	nv_write pref_voice_so	주석내용을 13K 에서 EVRC로 변경함(QM2차 사항)
:			{0,  1, 0x0003, 0x0003, 0x0003} ; True, EVRC, EVRC, EVRC
;			{1,  1, 0x0003, 0x0003, 0x0003} ; True, EVRC, EVRC, EVRC
;03/25/2008	Joys	nv_write nam_lock  주석내용 enable 로 추가 작성.(QM2차 사항)
;			nv_write nam_lock           {0, 1}	;enable
;03/25/2008	Joys	nv_write end_call_option , nv_write answer_option 주석 변경.(QM2차 사항)
;			nv_write end_call_option     	  {3}     		  ; 1: Slide down, 2:Any Key, 3: Slide down + Any Key
;			nv_write answer_option            {3}                     ; 1: Slide Open, 2:Any Key, 3: Slide up + Any Key 4:Auto
;
;
;----------	------	------------------------------------------------


mode offline-d
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model
wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================
nv_write sec_code			{"000000"}			; Security code
nv_write lock_code			{"0000"}			; Lock_code
nv_write otksl				{"000000"} 			; OTKSL code

nv_write min1           {0, "000-0000", "000-0000"}  ; Min0 number
nv_write min1           {1, "000-0000", "000-0000"}  ; Min1 number
nv_write min2           {0, "000", "000"}            ; NAM 0 has one active MIN2,
nv_write min2           {1, "000", "000"}            ; NAM 1

nv_write name_nam			{0, "3G EVOLUTION"}			; NAM 1 Name	IUSACELL -> 3G EVOLUTION
nv_write name_nam			{1, "3G EVOLUTION"}			; NAM 2 Name

nv_write imsi_mcc			{0, "000"}			; Mobile Country Code (000)
nv_write imsi_mcc			{1, "000"}
nv_write imsi_11_12			{0, "00"}			; Mobile Network Code
nv_write imsi_11_12			{1, "00"}

nv_write imsi_t_mcc			{0, "000"}
nv_write imsi_t_mcc			{1, "000"}
nv_write imsi_t_11_12			{0, "00"}
nv_write imsi_t_11_12			{1, "00"}
nv_write imsi_t_s1      {0, "000-0000", "000-0000"}
nv_write imsi_t_s1      {1, "000-0000", "000-0000"}
nv_write imsi_t_s2      {0, "000", "000"}
nv_write imsi_t_s2      {1, "000", "000"}
                                                 ; NV_DIR_NUMBER_PCS_I      /*123456789012345*/ using 10 digits
nv_write dir_number_pcs {0, "0000000000"}        ; NAM 0 : NV_DIR_NUMBER_PCS_I
nv_write dir_number_pcs {1, "0000000000"}        ; NAM 1 : NV_DIR_NUMBER_PCS_I

                                                 ; Primary CDMA Channels for A carrier and B carrier
print "Programming Primary CDMA Channel"
nv_write pcdmach        {0, 283, 384}            ; A and B primary CDMA channels
nv_write pcdmach        {1, 283, 384}

                                                 ; Secondary CDMA Channel
print "Programming Secondary CDMA Channel"
nv_write scdmach        {0, 691, 777}            ; set only if secondary channels offered
nv_write scdmach        {1, 691, 777}

nv_write home_sid_nid			{0,1525,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write home_sid_nid			{1,1525,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock   {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock   {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}

nv_write mob_term_home    {0, true, true}
nv_write mob_term_home    {1, true, true}
nv_write mob_term_for_sid {0, true, true}
nv_write mob_term_for_sid {1, true, true}
nv_write mob_term_for_nid {0, true, true}
nv_write mob_term_for_nid {1, true, true}

nv_write accolc           {0, 0, 0}
nv_write accolc           {1, 0, 0}

nv_write slot_cycle_index {2}

nv_write pref_voice_so		{0,  1, 0x0003, 0x0003, 0x0003} ; 8K EVR, 8K EVR, 8K EVR
nv_write pref_voice_so		{1,  1, 0x0003, 0x0003, 0x0003} ; 8K EVR, 8K EVR, 8K EVR

print "Programming Pref Mode"
nv_write pref_mode     {0, "Digital Only"}
nv_write pref_mode     {1, "Digital Only"}
nv_write voice_priv    {1}                     ; Standard (0), Enhanced (1)

print "Programming Band Preferred"
nv_write band_pref     {0, "pref_any"}
nv_write band_pref     {1, "pref_any"}

print "Programming Roam Preferred"
nv_write roam_pref     {0, "pref_any"}
nv_write roam_pref     {1, "pref_any"}

nv_write hybrid_pref   {1}                             ; 1 : hybrid on,  0 : hybrid off

nv_write system_pref   {0, "automatic b"}              ; System preference, actually default to band preference
nv_write system_pref   {1, "automatic b"}

print "Programming MRU table clear"
                                            ; except nam (first 0), '0' are 48(=4 X 12) times.
nv_write mru3_table {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru3_table {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};

print "Programming NAM Checksums"
nv_write nam_chksum {0, 0xffff}
nv_write nam_chksum {1, 0xffff}
nv_write min_chksum {0, 0xffff, 0xffff}
nv_write min_chksum {1, 0xffff, 0xffff}

nv_write stand_alone_mode {0}                          ; 0 default OFF, 1 ON
;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key {0, 0x00000000, 0x00000000 } ; Nam 1 64 bits A-Key. Published at factory with Random number.
nv_write a_key {1, 0x00000000, 0x00000000 } ; Nam 2 64 bits A-Key. Published at factory with Random number.
nv_write ssd_a {0, 0x00000000, 0x00000000 }
nv_write ssd_a {1, 0x00000000, 0x00000000 }
nv_write ssd_b {0, 0x00000000, 0x00000000 }
nv_write ssd_b {1, 0x00000000, 0x00000000 }
nv_write count {0, 0}
nv_write count {1, 0}
;=========================================================================

;=========================================================================
; OTA ITEM
;=========================================================================
nv_write otapa_enabled      {0, 1}   ; enable
nv_write otapa_enabled      {1, 1}   ; enable
nv_write spc_change_enabled		{1}
nv_write nam_lock           {0, 1}	;enable
nv_write nam_lock           {1, 1}	;enable

;=========================================================================
;UI ITEM
;=========================================================================
nv_write call_sounds			{0,0,0,0,0}			; {Caller ID (0:Iusacell Jingle), No Caller ID(0:Iusacell Jingle), Restrict Calls(0:Iusacell Jingle), All Calls(0:Iusacell Jingle), Vibrate (0: Off, 1: On)}"
nv_write ringer_lvl               {4}                     ; 1~5 (Low, Med Low, Med, Med High, High), 1 (Vibrate only), 97 (Alarm Only), 1 (All Sounds Off)"
nv_write ringer_spkr_lvl          {4}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8), 98 (High & Vib), 99 (Vibrate)
nv_write beep_lvl                 {4}                     ; 0 (Off), 1~5 (Low, Med Low, Med, Med High, High)
nv_write beep_lvl_shadow          {4}                     ; 0 (Off), 1~5 (Low, Med Low, Med, Med High, High)
nv_write beep_spkr_lvl            {4}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write spk_phone_beep_lvl       {4}                     ; Keypad Volume on Speaker Phone Mode: 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write ear_lvl                  {6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write ear_lvl_shadow           {6}                     ; 1(Low)~8(High)
nv_write speaker_lvl              {6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write speaker_shadow_lvl       {6}                     ; Earpiece Volume on Speaker Phone Mode: 1~8 (Volume1 ~ Volume8) -> Activate this item after DLL 0.0.4.0
nv_write call_restrict            {0,0,0,0,0}             ; 0(off), 1(on) inCall-outCall-MT-MO-DUN
nv_write charging_alert_onoff		{1}				; Charging Alert On(1), Off(0) 
nv_write sound_alerts			{0,0,0,0}			; {Service Change (Not use), Minute Beep, Call Connect, ERI}, On (1), Off(0)
nv_write power_onoff_sounds		{1,1}				; {Power On, Power Off}, On (1), Off (0)
nv_write banner				{"3G EVOLUTION"}
;nv_write sub_banner			{"3G EVOLUTION"}		; 불필요
nv_write eri_text_onoff			{0}				; 1 -> On, 0 -> Off
nv_write back_light               {7}                     ; Default 7 Sec
;nv_write sub_backlight			{7}		; 불필요
nv_write key_light                {7}                     ; 
nv_write wallpaper_main			{0,0,0}				; {location_type (0:phone memory, 1:phone efs, 2:sdcard), location_id (0:sdcard id), item_id (0: index)}
nv_write display_set              {0,0,1}                 ; sub Clock (not used), clock format(0.normal 1.analog 2.digital 3.dual 4.off), display themes(0.rhythm & blues 1.rock & roll)
nv_write number_size              {0,0}                   ;  Normal (0), Large (1)
nv_write auto_nam                 {0}                     ; Auto NAM == disable
nv_write curr_nam                 {0}                     ; Current NAM == NAM1
nv_write location_set_lock     	  {0}     		  ; 0: unlock, 1:Lock
nv_write auto_lock                {0}                     ; Power_up (1)
nv_write lock                     {0}                     ; Lock (1), Unlock (0)
nv_write emergency_num1			{"066"}				; Up to 48 Digits
nv_write emergency_num2			{"*911"}			; Up to 48 Digits
nv_write emergency_num3			{"911"}				; Up to 48 Digits
nv_write language_selection		{1}				; English (0), Spanish (1)
nv_write shortcut_main			{0,1,10,4}			; {Left->SHORTCUT_MY_MEDIA, Up->SHORTCUT_3G_REVOLUTION, Right->SHORTCUT_MESSAGE, Down->SHORTCUT_MOBILE_WEB}
;nv_write shortcut_main            {1,10,8,0}              ; {Left->SHORTCUT_WIRELESS_WEB, Up->SHORTCUT_MESSAGES, Right->SHORTCUT_MY_MUSIC, Down->SHORTCUT_ALLCALLS}
;nv_write shortcut_main            {2,4,0,17}              ; {Left, Up, Right, Down}
nv_write bt_power_onoff			{0}				; 1 -> On, 0 -> Off
;nv_write beep_bt_lvl              {4}                     ; Off (0), 1~5 (Volume1 ~ Volume5) ;CX는 사용하지 않았음
;nv_write ear_bt_lvl               {6}                     ; 1~8 (Volume1 ~ Volume8);CX는 사용하지 않았음

nv_write avr_call_alerts		{0}
nv_write avr_prompts_mode		{0}
nv_write avr_choice_list		{0}
nv_write avr_prompts_timeout		{0}
nv_write avr_sensitivity		{1}; 0: High 1: Medium 2: Low

nv_write silence_all			{0}				; sound on   {1} sound off
nv_write edit_font			{0,0}

nv_write manner_mode			{0}				; false {0}, true {1}
nv_write power_saver			{0}
nv_write alarm_only_mode		{0}				; 0 -> Disable, 1 -> Enable
nv_write pc_port			{0}				; PC connection port  0 (USB), 2 (BLUETOOTH), 3 (CLOSED)
nv_write dual_nam_set_enable		{1}				; dual_nam_set_enable(nam set menu) ( 0 : disable , 1 : enable)
nv_write wclock_choice            {30,	0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,42}
nv_write media_save_option        {0,0,0}                 ; {PIX, FLIX, SOUND} Phone memory (0), SD card (1)
nv_write camera_flash_test        {81}                    ; Camera Flash On (85(0x55)), Off (others)
nv_write equalizer_mode           {0}
nv_write visualizer_mode          {0}                     ; OFF (0), ON (1)
nv_write avr_digit_dial_readout   {0}                     ; 0: Off, 1: On
nv_write avr_audio_playback       {0}                     ; 0: Speakerphone, 1: Earpiece
nv_write bt_audio_auto_pair       {0}                     ; auto pairing mode ON(1) OFF(0)
nv_write use_mymp3                {0}                     ; MOD Center Key Define: MOD Player (0), MP3 Player (1)
nv_write carrier_logo             {0}                     ; Verizon(0)
nv_write contrast_lvl             {0,0}
nv_write led_blink                {1}                     ; ON(1) OFF(0)
nv_write gps_test_num             {"922"}                 ; Up to 48 Digits
nv_write emer_test_num            {"*911"}                 ; Up to 48 Digits
nv_write end_call_option     	  {3}     		  ; 1: Slide down, 2:Any Key, 3: Slide down + Any Key
nv_write answer_option            {3}                     ; 1: Slide Open, 2:Any Key, 3: Slide up + Any Key 4:Auto
nv_write wheel_light              {0,0,0}                 ; trace motion (0:On 1:Off) , PowerOnOff(0:On 1:Off),call(0: sound_theme 1,1: sound_theme 2,2: sound_theme 3, 3: Off)
nv_write vx8550_color_variation   {0}                     ; VX8550 color varitation {0: Black , 1: Dark Blue , 2: Dark Red }
nv_write wheel_sensitivity        {1}                     ; wheel speed ( 0: High 1: Medium 2: Low)
nv_write usb_auto_detection       {1}                     ; usb_auto_detection ( 0: Sync Music 1: Sync Data 2: Ask On Plug)
nv_write touch_vibration          {0}                     ; touch_vibration ( 0: On, 1: Off)
nv_write touch_sound   		  {1}                     ; touch sound set ( 0 : Off , 1 : On)
nv_write slide_sound    	  {1}                     ; slide sound set ( 0 : Off , 1 : On)
nv_write wheel_sound    	  {1}                     ; wheel sound set ( 0 : Off , 1 : On)
nv_write auto_key_lock            {0}                     ; 0(On), 1(Off)
nv_write flash_clip_board     	  {0}     		  ; set flash clip board ( 0 : off , 1 : Classic ,2 : Diary, 3 : Modern)
nv_write auto_prepend		  {0}			  ; NV_AUTO_PREPEND_I
nv_write do_not_disturb_enabled		{0}			;  ( 0 : Off , 1 : On ) 
nv_write cont_key_dtmf            {0}                     ; Normal (1), Long (0),  Off (2)
;nv_write auto_answer             {0, 0}                  ; On (1, 1), Off (0, 0)
nv_write auto_redial              {0, 0}                  ; 0ff(0x00), Every 10 Seconds(0x01), Every 30 Seconds(0x03), Every 60 Seconds(0x06)
nv_write call_rstrc               {0}                     ; Off (0), On (1)
nv_write onetouch_dial            {1}                     ; Off (0), On (1)
nv_write send_pin                 {0}                     ; Off (0)
nv_write fsc                      {"000000"}              ; Field Service code
nv_write auto_volume_enabled      {0}                     ; Off (0), On (1)
nv_write tty                      {3}                     ; TTY Full (0), TTY+TALK (1),TTY+HEAR (2),TTY off (3)
nv_write call_connect_alert	  {false}		; Call connect alert	== off
nv_write alarm_sounds             {6,0}                   ; {tone(6: Ringtone 2), vibrate (0: Off)}
;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_pkt_orig_str		{5, "#777"}			; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_mdr_mode			{3}				; DS_MDR_MODE_MDR_ONLY=0, DS_MDR_MODE_IF_AVAIL=1, DS_MDR_MODE_NO_MDR=2, DS_MDR_MODE_SO33_PREF=3; Service Option 33 (1x channel) = 3 Use only low-speed packet data = 2
nv_write data_auto_packet_detection	{0}				; 0-Disable   1-Enable
nv_write data_so_set			{2}				; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write diag_default_baudrate		{0x000e}			; 0x000e(38.4kbps), 0x0011(115.2kbps)
nv_write data_qnc_enabled		{0}				; 0-QNC Disable  1-QNC Enable

nv_write ppp_user_id			{32,"0000000000@modem.iusasipevdo.com"}	; Max of 64 chars in User ID
nv_write ppp_password			{8,"BJMPW504"}			; Max of 127 chars in Password

nv_write data_scrm_enabled		{1}				; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled		{1}				; 0-TRTL Disable 1-TRTL Enable
nv_write pref_for_rc			{3}				; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)    
nv_write ds_default_baudrate		{0x0011}			; 0x0000 (19.2kbps),0x0011(115kbps) ,0x00012(230.4kbps)

nv_write ds_qcmip			{2}				; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only
nv_write ds_mip_active_prof		{0}				; current active profile index
nv_write ds_mip_enable_prof		{1,1,0,0,0,0}			; diable - 0, enable - 1{1st Profile, 2nd Profile, 3rd Profile, .... }
nv_write ds_mip_retries			{2}				; number of retries
nv_write ds_mip_retry_int		{3}				; retry interval = n*250(ms) + 1000ms
nv_write ds_mip_pre_re_rrq_time		{60}				; pre-registration time - minute
nv_write ds_mip_num_prof		{2}				; number of profiles (max 6) 
nv_write ds_mip_2002bis_mn_ha_auth	{0}				; disable - 0, enable -1

nv_write ds_mip_qc_drs_opt		{1}				; dormant handoff optimization. disable - 0, enable - 1
									;Comment : MIP general profile information {index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
									;Comment : reverse tunneling, home address, primary ha address, secondary ha address}

; MIP general profile information 		{index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
;		reverse tunneling, home address, primary ha address, secondary ha address}
nv_write ds_mip_gen_user_prof		{0,26,"0000000000@iusamipevdo.com",1,257,1,2,1,0x00000000,0xFFFFFFFF,0xCF53C8DE}
nv_write ds_mip_gen_user_prof		{1,32,"0000000000@modem.iusamipevdo.com",1,257,1,2,1,0x00000000,0xFFFFFFFF,0xCF53C8DE}

nv_write ds_mip_dmu_pkoid		{0,10}				; public key organization indentifier
nv_write ds_mip_dmu_mn_auth		{0,0x01,0xB2,0x07}		; { Index , DMU MN authenticator - 111111base10 }
nv_write hdr_an_auth_user_id_long	{22,"0000000000@iusabam.com"}	; { Length , EVDO AN authetication user id }

nv_write dun_cable_mode			{1}				; 0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode			{1}				; 0=disable bt dun,1=enable bt dun

nv_write ds_mip_ss_user_prof		{0,16,"iusacelliusacell",8,"BJMPW504"}
nv_write ds_mip_ss_user_prof		{1,16,"iusacelliusacell",8,"BJMPW504"}

nv_write ppp_carrier			{0}				; 0-IUSACELL 1-Verizon 2-USC 3-SKT  4-Script. Test NV Item.  
;CS DLL don't write this item 
;Comment : remove the hdr_an_auth_passwd_long setting in script file. (Becuase it uses ppp_password value that changed after DMU nego.)
nv_write hdr_an_auth_passwd_long	{10,"0000000000"}		; EVDO AN authetication password
;=========================================================================
; MSG ITEM
;=========================================================================
nv_write msg_settings_auto_save		{1}				; ON(0) Off(1) Prompt(2)
nv_write msg_settings_auto_delete	{1}				; On(1), Off(0)
nv_write msg_settings_entry_mode	{0}				; Word(0), Abc(1), ABC(2), 123(3)
nv_write msg_settings_vibrate_alert	{0,0,0,0}			; On(1), Off(0)
nv_write msg_settings_signature		{0}				; None(0), Custom(1)	

;=========================================================================

;=========================================================================
; SMS ITEM
;=========================================================================
nv_write sms_txt_cb_enable		{1}				; On(1), Off(0)
nv_write sms_orig_msg_id		{1}				; 0X0001 - 0XFFFF
nv_write sms_mo_max_userdata		{150}		             ; 160 character
nv_write sms_mo_l3_ack			{1}				; On(1), Off(0)
nv_write sms_mo_so			{1}				; 6K(1), 14K(0)
nv_write sms_voicemail_record		{0,0}				; {Count,Time}
nv_write sms_settings_signature		{0}				; None(0), Custom(1)
nv_write sms_settings_direct_view	{0}				; Off(0), On(1)

nv_write sms_voicemail_alert		{0}				; 0 (Iusacell Jingle) , 1 (Low Beep Once), 2 (Low Beeps), 3 (Loud Beep Once), 4 (Loud Beeps), 5~16 (Ringtone 1~12), 17 (No Ring)
nv_write sms_textmsg_alert		{0}				; 0 (Iusacell Jingle) , 1 (Low Beep Once), 2 (Low Beeps), 3 (Loud Beep Once), 4 (Loud Beeps), 5~16 (Ringtone 1~12), 17 (No Ring)
nv_write sms_voicemail_cb		{2,"#9"}			; 20Byte(ASCII)
nv_write sms_urgent_voice_record	{0}				; None(0), Exist(1)
nv_write sms_2min_alert_sel		{1,1,1,1}			; Once(0), Every 2 Minutes(1), Every 15 Minutes(2), Off(3)
nv_write sms_message_cb			{10,"0000000000"}		;
;=========================================================================

; SMS ITEM
;=========================================================================
nv_write sms_settings_auto_play		{0}				; On(1), Off(0)
nv_write sms_ems_enable			{0}				; On(1), Off(0)
;=========================================================================

;=========================================================================
;BREW ITEM
;=========================================================================
nv_write brew_server			{"brew.iusacell3g.com,brew.iusacell3g.com"}	; 64 byte character
nv_write brew_carrier_id		{91}				; 
nv_write brew_bkey 			{0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 
nv_write brew_download_flags 		{0x0004}                   	; DIF_USE_A_KEY(0x0001) - A Key: 1 or B Key: 0 Option, DIF_TEST_ALLOWED(0x0002) - Test Disable: 0, Test Enable: 2
                                                        	; DIF_MIN_FOR_SID(0x0004) - Use MIN for Subscriber ID: 4,  Not use: 0, DIF_PREPAY(0x0008) - Prepay:8, Postpay:0
nv_write brew_auth_policy 		{1}                             	; APOLCY_NONE(0), APOLCY_SID(1), APOLCY_TEXT(2), APOLCY_NUM(3) 
nv_write brew_privacy_policy 		{3}                            	; PPOLICY_BREW(0), PPOLICY_CARRIER(1), PPOLICY_BREW_AND_CARRIER(2), PPOLICY_BREW_OR_CARRIER(3)
nv_write brew_platform_id		{1252}				; VX8550 platform id = 1198, MX8700 = 1174, OEMDEMO = 600
nv_write brew_disallow_dormancy 	{1}				; TRUE	
nv_write brew_sid_length		{16}
nv_write brew_primary_ip		{207,83,200,200}
nv_write brew_secondary_ip		{207,83,200,201}
;=========================================================================

;=========================================================================
; MMS ITEM
;=========================================================================
nv_write mms_set_auto_receive		{1}				; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_set_read_ack		{1}				; 0(ON), 1(OFF)
nv_write mms_set_delivery_ack		{0}				; 0(MMS_ON), 1(MMS_OFF)

nv_write mms_set_tone_alert		{0}				; 0 (Iusacell Jingle) , 1 (Low Beep Once), 2 (Low Beeps), 3 (Loud Beep Once), 4 (Loud Beeps), 5~16 (Ringtone 1~12), 17 (No Ring)
nv_write mms_set_vibrate_alert		{0}				; 0(VIBRATE OFF), 1(VIBRATE ON)
nv_write mms_set_reminder_alert		{1}				; 0(REMIND ONCE), 1(REMIND EVERY2MIN), 2(REMIND EVERY15MIN), 3(REMIND OFF)
nv_write mms_settings_signature		{0}				; None(0), Custom(1)

nv_write mms_mmsc_url			{25, "http://mms.iusacell3g.com"}	; 48 byte characters
nv_write mms_mmsc_upload_url		{4, "8888"}			; Upload Address
nv_write mms_mmsc_uaprof_url		{60, "http://uaprof.iusacell3g.com:8080/xml/lg/mx8550/mx8550v1.xml"}	; Max 64 byte characters

nv_write mms_set_retry_num		{3}				; 0, 1, 2, 3
nv_write mms_send_from_add		{2}				; MDN Only (0), 1MDN (1),  +1MDN (2)         

nv_write mms_mmsc_user_agent		{47,"LGE-MX8550/1.0.UP.Browser/6.2.3.9.(GUI).MMP/2.0"}	; User Agent Profile name
nv_write mms_mmsc_server_post_url	{25, "http://mms.iusacell3g.com"}		; Post URL
nv_write mms_mmsc_server_post_cgi	{0, ""}				; CGI URL
nv_write mms_test_authorization		{0}				; 0 : Commercial, 1 : Lab, 2 : Domestic
;=========================================================================

;=========================================================================
;F/W ITEM
;=========================================================================
nv_write rf_config			{6}

nv_write vbatt				{30, 180}			; VX8550

nv_write audio_codec_gain            { 0, 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write audio_voc_gain              { 0, 0, 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write audio_agc                   { 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write audio_rx_fir_pcm_filter     { 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write audio_tx_fir_pcm_filter     { 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write audio_qdsp                  { 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write touch_sensitivity_setting   {2,2,0xA0,0xA1,0xA0,0xA1,0x9B,0x9C,0x9B,0x9C,0x96,0x97,0x96,0x97,0x91,0x92,0x91,0x92}     ; set Mode(0:Unrestricted, 1:Strongest, 2: First), Level(0:Super, 1:High, 2:Med, 3:Low), Value(0xS0,0xS1,0xS5,0xS7,0xH0,0xH1,0xH5,0xH7,0xM0,0xM1,0xM5,0xM7,0xL0,0xL1,0xL5,0xL7)
;=========================================================================

;=========================================================================
;GPSONE ITEM
;=========================================================================
nv_write gps1_lock			{0}; Location On(0), E911 Only(3)
nv_write gps1_pde_address		{207,083,200,238}
nv_write gps1_pde_port			{8888}
;=========================================================================
; DATA EFS
;=========================================================================
;efs write				"DMU/10.key"			; MIP DMU(Dynamic Mipkeys Update) key file

;=========================================================================
; UP EFS : for magellan 
;=========================================================================
efs write				"OWS/paramtable1.fil"
efs write				"OWS/wdptable1.fil"

;=========================================================================
;JAVA & CALL ITEM 
;=========================================================================
;=========================================================================
;ERI SOUND ITEM
;=========================================================================
efs write "eri_sound/extendednetwork.qcp"                                                     ;size = 2326;
efs write "eri_sound/lossofservice.qcp"                                                       ;size = 2118;
efs write "eri_sound/roaming.qcp"                                                             ;size = 1120;
efs write "eri_sound/verizonwireless.qcp"                                                     ;size = 2410;
;=========================================================================


;=========================================================================
; DCAMERA EFS
;=========================================================================
efs write                            "dload/default_img/DecodeErrorAnimation.jpg"             ;size = 6035;
efs write                            "dload/default_img/DecodeErrorImage.jpg"                 ;size = 4803;
efs write                            "dload/default_img/NotSupportedImage_UnknownImage.jpg"   ;size = 5069;
efs write                            "dload/default_img/phoneOnConversation.jpg"              ;size = 4823;         
efs write                            "dload/default_img/TooBigErrorImage.jpg"                 ;size = 4903;
efs write                            "dload/default_img/video_FirstFrame_PMD.bmp"             ;size = 32454;
efs write                            "dload/default_img/video_FirstFrame_SVG.bmp"             ;size = 32456;
efs write                            "dload/default_img/VideoImageSymbol.jpg"                 ;size = 19689;
;=========================================================================

;=========================================================================
;ANIMATION IMAGE ITEM
;=========================================================================                                                            ;size = 2526006;	not use...
;=========================================================================
;=========================================================================
; CAMERA ITEM 
;=========================================================================
nv_write camera_lock			{0}   ;NV_CAMERA_LOCK_I 
nv_write time_format			{0}   ; NV_TIME_FORMAT_I

;=========================================================================
;FLASH UI ITEM
;=========================================================================
;=========================================================================
mode reset
