|======================================= Component Information ============================================

|      DLL     	    Version                     Path														

| Port Manager 	:: 0, 0, 9, 0   C:\LG Electronics\LGNPST\components 1.0\LGNPST_PortManager.dll 

| Log          	:: 0, 0, 11, 0  C:\LG Electronics\LGNPST\components 1.0\LGNPST_Log.dll 

| NV Storage		:: 0, 1, 28, 0  C:\LG Electronics\LGNPST\components 1.0\LGNPST_NVStorage.dll 

| Flash		:: 0, 0, 16, 0  C:\LG Electronics\LGNPST\components 1.0\LGNPST_FlashManager.dll 



|======================================= Environment Information =======================================

| Model DLL    	:: 1, 0, 0, 3   D:\software\flash lg cdma\movilnet\LG_MX8550_Movilnet_ver_MVN04_00\LG MX8550 Movilnet ver MVN04 00\MX8550MVN.dll  

| Log File Path	::              D:\software\flash lg cdma\movilnet\LG_MX8550_Movilnet_ver_MVN04_00\LG MX8550 Movilnet ver MVN04 00\LOG\MX8550DLL_Log_COM2.txt 

| Working Path 	::              D:\software\flash lg cdma\movilnet\LG_MX8550_Movilnet_ver_MVN04_00\LG MX8550 Movilnet ver MVN04 00 

| Current Path 	::              D:\software\flash lg cdma\movilnet\LG_MX8550_Movilnet_ver_MVN04_00\LG MX8550 Movilnet ver MVN04 00 

| Frame   Path 	::              D:\leonel pull@tel\lg todo\LG TOOLS\LG TOOLS.EXE   

======================================= NV Backup Environment =========================================

	 RANGE =      H/W + User NV Items ,      USEAREA =    World C/S mode     Simple/Professional = Professional version
	 Life Count = Backup              ,      Life Timer = Backup    
|=======================================================================================================

| Binary File 	:: D:\software\flash lg cdma\movilnet\LG_MX8550_Movilnet_ver_MVN04_00\LG MX8550 Movilnet ver MVN04 00\MX855M04_00.bin 

CComPort::GetError, Port is not opened.
Port is not opened.
CBasicComControl::ChangeBaudrate, Handle is not available. No Port Found.
CBasicComControl::Open, Constructed Port Successfully for COM 2, HANDLE : 0x33c
COM2 port open

PROGRESS STATUS = Initialize ...

PROGRESS STATUS = Erasing ...

PROGRESS STATUS = Burning ...

PROGRESS STATUS = Finalize

	TX. 0    : 24 5E 97 7E                                                                                      $^..

	RX. 0    : 02                                                                                               .

Finish the Image Flashing

PROGRESS STATUS = Reset

	TX. 1    : 0A 00 49 38 00 D5 61 7E                                                                          ..I8..a.

	RX. 1    : 02                                                                                               .

CComPort::ClosePort, Closed Port Successfully for COM 2
PROGRESS STATUS = Rebooting...

Sleep 20000 sec for Reboot

-------------------Start Tracing Warning Level Log message -----------------------------
CComPort::GetError, Port is not opened.
Port is not opened.
CBasicComControl::ChangeBaudrate, Handle is not available. No Port Found.

-------------------End of Tracing Warning Level Log message 3 items-----------------------------
CComPort::GetError, Port is not opened.
Port is not opened.
CBasicComControl::ChangeBaudrate, Handle is not available. No Port Found.
Clear ALL NV Instance of NV Storage  Current Storage size=467912  

	Successfully Clear NV Storage

