;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;=========================================================================
;  File name: MX87MN04.SCR
;  Made by  : LGE
;  Version  : V04
;  Date     : 2007/06/24
;-------------------------------------------------------------------------
;+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
;2007/06/08     JHJ		qdsp_snd_ctrl의 VOC_DATA_QDSP_VOC_RX_GAIN 값 0->-128 변경
;2007/06/04	ischo		brew_sid_length 32->16으로 변경 
;2007/06/03	ischo		brew_primary_ip,brew_secondary_ip 추가 
;2007/05/30	crow		msg_settings_auto_save ON으로 변경  (MVNissue 8 )
;2007/05/10	crow		phone_setup에서 Send Only로 수정 (MVN요구 )
;2007/05/08	ischo		brew secondary ads 변경(brewprepago.movilnet.com.ve)
;2007/04/04	crow		Movilnet 초기작업
;2007/04/04	ischo		BREW server,BREW cid 값 변경 및 BREW bar file 수정
;2007/04/11	dkkang		shortcut_main값 변경(베네주엘라향 메뉴트리 적용)
;2007/04/11	ischo		brew appln 바파일 변경
;+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++


mode offline-d
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model
wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================
nv_write sec_code			{"000000"}			; Security code
nv_write lock_code			{"1234"}			; Lock_code
nv_write fsc 				{"000000"}                   	; Field Service code 		// NV_FSC_I = 184
nv_write otksl 				{"000000"} 			; OTKSL code 			// NV_OTKSL_I = 219

nv_write min1				{0, "000-0000", "000-0000"}	; Min0 number
nv_write min1				{1, "000-0000", "000-0000"}	; Min1 number
nv_write min2				{0, "158", "158"}		; NAM 0 has one active MIN2,
nv_write min2				{1, "199", "199"}		; NAM 1

nv_write name_nam			{0, "MOVILNET"}			; NAM 1 Name
nv_write name_nam			{1, "MOVILNET"}			; NAM 2 Name

nv_write imsi_mcc			{0, "000"}			; Mobile Country Code (000)
nv_write imsi_mcc			{1, "000"}
nv_write imsi_11_12			{0, "00"}			; Mobile Network Code
nv_write imsi_11_12			{1, "00"}
;nv_write imsi_addr_num			{0, 0}
;nv_write imsi_addr_num			{1, 0}

nv_write imsi_t_mcc			{0, "000"}
nv_write imsi_t_mcc			{1, "000"}
nv_write imsi_t_11_12			{0, "00"}
nv_write imsi_t_11_12			{1, "00"}
nv_write imsi_t_s1			{0, "000-0000", "000-0000"}
nv_write imsi_t_s1			{1, "000-0000", "000-0000"}
nv_write imsi_t_s2			{0, "000", "000"}
nv_write imsi_t_s2			{1, "000", "000"}

nv_write dir_number_pcs			{0, "1580000000"}		; NAM 0 : NV_DIR_NUMBER_PCS_I
nv_write dir_number_pcs			{1, "1990000000"}		; NAM 1 : NV_DIR_NUMBER_PCS_I

print "Programming Primary CDMA Channel"
nv_write pcdmach			{0, 283, 384}			; A and B primary CDMA channels
nv_write pcdmach			{1, 283, 384}

print "Programming Secondary CDMA Channel"
nv_write scdmach			{0, 691, 777}			; set only if secondary channels offered
nv_write scdmach			{1, 691, 777}

nv_write home_sid_nid 			{0,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535}
nv_write home_sid_nid 			{1,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535,31488,65535}

nv_write sid_nid_lock 			{0,31553,65535,31499,65535,31509,65535,31531,65535,31541,65535,31491,65535,31501,65535,31513,65535,31533,65535,31543,65535}
nv_write sid_nid_lock 			{1,31553,65535,31499,65535,31509,65535,31531,65535,31541,65535,31491,65535,31501,65535,31513,65535,31533,65535,31543,65535}


nv_write mob_term_home			{0, true, true}
nv_write mob_term_home			{1, true, true}
nv_write mob_term_for_sid		{0, true, true}
nv_write mob_term_for_sid		{1, true, true}
nv_write mob_term_for_nid		{0, true, true}
nv_write mob_term_for_nid		{1, true, true}

nv_write accolc				{0, 0, 0}
nv_write accolc				{1, 0, 0}

nv_write slot_cycle_index		{2}

nv_write pref_voice_so			{0,  1, 0x0003, 0x0003, 0x0003}	; True, wildcard, EVRC, EVRC
nv_write pref_voice_so			{1,  1, 0x0003, 0x0003, 0x0003}	; True, wildcard, EVRC, EVRC


print "Programming Pref Mode"
nv_write pref_mode			{0, "Digital Only"}
nv_write pref_mode			{1, "Digital Only"}

nv_write voice_priv			{0}				; 0=Standard  1=Enhanced

print "Programming Band Preferred"
nv_write band_pref			{0, "pref_any"}
nv_write band_pref			{1, "pref_any"}

print "Programming Roam Preferred"
nv_write roam_pref			{0, "pref_any"}
nv_write roam_pref			{1, "pref_any"}

nv_write hybrid_pref			{1}				; 1 : hybrid on,  0 : hybrid off


print "Programming MRU table clear"
					; except nam (first 0), '0' are 48(=4 X 12) times.
nv_write mru3_table			{0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru3_table			{1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};

print "Programming NAM Checksums"
nv_write nam_chksum			{0, 0xffff}
nv_write nam_chksum			{1, 0xffff}
nv_write min_chksum			{0, 0xffff, 0xffff}
nv_write min_chksum			{1, 0xffff, 0xffff}

nv_write stand_alone_mode		{0}				; 0 default OFF, 1 ON
;=========================================================================

;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key				{0, 0x00000000, 0x00000000 }
nv_write a_key				{1, 0x00000000, 0x00000000 }
nv_write ssd_a				{0, 0x00000000, 0x00000000 }
nv_write ssd_a				{1, 0x00000000, 0x00000000 }
nv_write ssd_b				{0, 0x00000000, 0x00000000 }
nv_write ssd_b				{1, 0x00000000, 0x00000000 }
nv_write count				{0, 0}
nv_write count				{1, 0}
;=========================================================================

;=========================================================================
; OTA ITEM
;=========================================================================
nv_write otapa_enabled			{0, 1}				; enable
nv_write otapa_enabled			{1, 1}				; enable
nv_write spc_change_enabled		{1}
nv_write nam_lock			{0, 1}
nv_write nam_lock			{1, 1}
;=========================================================================

;=========================================================================
;UI ITEM
;=========================================================================
nv_write call_sounds			{4,4,4,4,0}			; {Caller ID (4:Ringer 1), No Caller ID(4:Ringer 1e), Restrict Calls(4:Ringer 1), All Calls(4:Ringer 1), Vibrate (0: Off, 1: On)}"
nv_write ringer_lvl			{0x4}				; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 1(Vibrate only=manner_mode), 97(alarm only), 1(Sounds Off=silence_all)
nv_write ringer_spkr_lvl		{0x4}				; 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 98(High & Vib), 99(Vibrate)
nv_write beep_lvl			{0x4}				; 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write beep_lvl_shadow		{0x4}				; 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write beep_spkr_lvl			{0x4}				; 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write spk_phone_beep_lvl		{0x4}				; 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) - Keypad Volume on Speaker Phone Mode
nv_write ear_lvl			{0x6}				; 1(Low)~8(High)
nv_write ear_lvl_shadow			{0x6}				; 1(Low)~8(High)
nv_write speaker_lvl			{0x6}				; 1(Low)~8(High)
nv_write speaker_shadow			{0x6}				; 1(Low)~8(High) - Earpiece Volume on Speaker Phone Mode

nv_write vp_spkr_lvl			{0x6}				; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 6(High), 7(High)
nv_write vp_lvl_shadow			{0x6}				; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 6(High), 7(High)
nv_write vp_bt_lvl			{0x6}				; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 6(High), 7(High)
nv_write vp_spkr_shadow_lvl		{0x6}				; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) , 6(High), 7(High)
nv_write vp_lvl				{0x6}				; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) , 6(High), 7(High)
nv_write vibrate_factory_test		{false}				; vibrate_factory_test enable(TRUE), disable(FALSE)
nv_write call_restrict			{0,0,0,0,0}											 ; 0(off), 1(on) inCall-outCall-MT-MO-DUN
nv_write restriction_lock_code		{"1234"}												 ; 4 Digit Number
nv_write first_time_security_access	{true}
nv_write charging_alert_onoff		{1}				; Charging Alert On(1), Off(0) 

nv_write sound_alerts			{0,0,0,0}			; {Service Change (Not use), Minute Beep, Call Connect, ERI}, On (1), Off(0)
nv_write backtop_beep			{true}				; Back To Top Sound == on       
nv_write power_onoff_sounds		{1,1}				; {Power On, Power Off}, On (1), Off (0)
nv_write banner				{"Movilnet"}
nv_write sub_banner			{"Movilnet"}
nv_write eri_text_onoff			{0}				; 1 -> On, 0 -> Off
nv_write back_light			{7}
nv_write sub_backlight			{7}
nv_write key_light			{7}
nv_write wallpaper_main			{0,0,0}				; {location_type (0:phone memory, 1:phone efs, 2:sdcard), location_id (0:sdcard id), item_id (0: index)}
nv_write display_set			{0,0,0}				; sub_clock, main_clock, color theme
nv_write number_size			{1,0}				; (size, color(don't use)) 0:normal 1:large
nv_write auto_nam			{off}				; Auto NAM              == disable
nv_write curr_nam			{0}				; Current NAM           == NAM1
nv_write location_set			{0}				; 1 -> location on 0-> E911 only
nv_write auto_lock			{off}				; phone lock            == Unlocked \ Power_up
nv_write lock				{off}				; phone lock            == Unlocked \ now
nv_write emergency_num1			{"*1"}				; Up to 48 Digits
nv_write emergency_num2			{"911"}			; Up to 48 Digits
nv_write emergency_num3			{"*171"}			; Up to 48 Digits
nv_write language_selection		{1}				; English (0), Spanish (1)
nv_write phone_setup			{0,0,0,0,0,0,0,0,0,0,0,0,2,0,0}	; (pim_id, form_id, shortcut_form_index[10], call_answer, isModal, modalType)
									; pim_id, form_id : 0 -> Schedule, call_answer : 0 -> Flip open
nv_write shortcut_main			{1,0,4,10}			; {Left->Neo Aplicaciones, Up->Multimeida, Right->Neo Navegacion, Down->MESSAGE}
nv_write bt_power_onoff			{0}				; 1 -> On, 0 -> Off
nv_write beep_bt_lvl			{0x4}				; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write ear_bt_lvl			{0x6}				; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)

nv_write avr_call_alerts		{0}
nv_write avr_prompts_mode		{0}
nv_write avr_choice_list		{0}
nv_write avr_prompts_timeout		{0}
nv_write avr_sensitivity		{1}

nv_write silence_all			{0}				; sound on   {1} sound off
nv_write edit_font			{0,0}
nv_write display_screen			{0}				; power_onoff animation
nv_write front_lcd_alignment		{0}				; Left Alignment{0}, Right Alignment{1}

nv_write manner_mode			{0}				; false {0}, true {1}
nv_write power_saver			{0}
nv_write alarm_only_mode		{0}				; 0 -> Disable, 1 -> Enable

nv_write pc_port			{0}				; PC connection port  0 (USB), 1 (UART), 2 (BLUETOOTH), 3 (CLOSED)
nv_write screen_saver			{0,0}				;  ( sub ( 0 : no screen  1: digital) main ( 0 : no screen 1 : digital + calenda ,2 : digital)
nv_write lg_wdc				{0,0,0,0,0}
nv_write location_set_lock		{0}				; location_set_lock ( 0 : unlock , 1 : lock)
nv_write dual_nam_set_enable		{1}				; dual_nam_set_enable(nam set menu) ( 0 : disable , 1 : enable)
nv_write service_num			{"611"}				; Up to 48 Digits
;=========================================================================

;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_pkt_orig_str		{5, "#777"}			; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_mdr_mode			{3}				; DS_MDR_MODE_MDR_ONLY = 0  Use only MDR packet data services
nv_write data_auto_packet_detection	{0}				; 0-Disable   1-Enable
nv_write data_so_set			{2}				; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write diag_default_baudrate		{0x000e}			; 0x000e(38.4kbps), 0x0011(115kbps)
nv_write data_qnc_enabled		{0}				; 0-QNC Disable  1-QNC Enable

nv_write data_scrm_enabled		{1}				; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled		{1}				; 0-TRTL Disable 1-TRTL Enable
nv_write pref_for_rc			{3}				; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)    
nv_write ds_default_baudrate		{0x0011}			; 0x0000 (19.2kbps),0x0011(115kbps) ,0x00012(230.4kbps)

nv_write ds_qcmip			{0}				; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only
nv_write hdr_an_auth_user_id_long	{15,"1580000000@evdo"}	; { Length , EVDO AN authetication user id }

nv_write dun_cable_mode			{1}				; 0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode			{1}				; 0=disable bt dun,1=enable bt dun

nv_write ppp_carrier			{0}				; 0-Movilnet 1-Verizon 2-USC 3-SKT  4-Script. Test NV Item.  
;nv_write hdr_an_auth_passwd_long	{10,"0000000000"}		; EVDO AN authetication password
;=========================================================================

;=========================================================================
; MSG ITEM
;=========================================================================
nv_write msg_settings_auto_save		{0}				; ON(0) Off(1) Prompt(2)
nv_write msg_settings_auto_delete	{0}				; On(1), Off(0)
nv_write msg_settings_entry_mode	{0}				; Word(0), Abc(1), ABC(2), 123
nv_write msg_settings_vibrate_alert	{0,0,0,0}			; On(1), Off(0)
nv_write msg_settings_signature		{0}				; None(0), Custom(1)	
;=========================================================================

;=========================================================================
; SMS ITEM
;=========================================================================
nv_write sms_txt_cb_enable		{1}				; On(1), Off(0)
nv_write sms_orig_msg_id		{1}				; 0X0001 - 0XFFFF
nv_write sms_mo_max_userdata		{160}				; Up to 220 Byte
nv_write sms_mo_l3_ack			{1}				; On(1), Off(0)
nv_write sms_mo_so			{1}				; 6K(1), 14K(0)
nv_write sms_voicemail_record		{0,0}				; {Count,Time}
nv_write sms_settings_signature		{0}				; None(0), Custom(1)
nv_write sms_settings_direct_view	{0}				; Off(0), On(1)

nv_write sms_voicemail_alert		{9}				; 0 (Low Beep Once), 1 (Low Beeps), 2 (Loud Beep Once), 3 (Loud Beeps), 4~15 (Ringtone 1~12), 16 (No Ring)
nv_write sms_textmsg_alert		{1}				; 0 (Low Beep Once), 1 (Low Beeps), 2 (Loud Beep Once), 3 (Loud Beeps), 4~15 (Ringtone 1~12), 16 (No Ring)

nv_write sms_voicemail_cb		{2,"*9"}			; 20Byte(ASCII)
nv_write sms_urgent_voice_record	{0}				; None(0), Exist(1)
nv_write sms_2min_alert_sel		{1,1,1,1}			; Once(0), Every 2 Minutes(1), Every 15 Minutes(2), Off(3)
nv_write sms_message_cb			{10,"0000000000"}		;
;=========================================================================

;=========================================================================
; SMS/EMS ITEM
;=========================================================================
nv_write sms_settings_auto_play		{0}				; On(1), Off(0)
nv_write sms_ems_enable			{0}				; On(1), Off(0)
;=========================================================================

;=========================================================================
;BREW ITEM modified by Kim sungkung
;=========================================================================
nv_write brew_server			{"brewpostpago.movilnet.com.ve,brewprepago.movilnet.com.ve"}		; 64 byte character
nv_write brew_carrier_id		{62}				; 91->62
nv_write brew_bkey			{0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 
nv_write brew_download_flags		{0x0004}			; DIF_USE_A_KEY(0x0001) - A Key: 1 or B Key: 0 Option, DIF_TEST_ALLOWED(0x0002) - Test Disable: 0, Test Enable: 2
									; DIF_MIN_FOR_SID(0x0004) - Use MIN for Subscriber ID: 4,  Not use: 0, DIF_PREPAY(0x0008) - Prepay:8, Postpay:0
nv_write brew_auth_policy		{1}				; APOLCY_NONE(0), APOLCY_SID(1), APOLCY_TEXT(2), APOLCY_NUM(3) 
nv_write brew_privacy_policy		{3}				; PPOLICY_BREW(0), PPOLICY_CARRIER(1), PPOLICY_BREW_AND_CARRIER(2), PPOLICY_BREW_OR_CARRIER(3)
nv_write brew_platform_id		{1174}				; VX8700 platform id
nv_write brew_disallow_dormancy		{1}				; TRUE
nv_write brew_sid_length		{16}
nv_write brew_primary_ip		{200,44,32,12}
nv_write brew_secondary_ip		{200,44,32,13}
;=========================================================================

;=========================================================================
; MMS ITEM
;=========================================================================
nv_write mms_set_auto_receive		{0}				; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_set_read_ack		{1}				; 0(ON), 1(OFF)
nv_write mms_set_delivery_ack		{0}				; 0(MMS_ON), 1(MMS_OFF)

nv_write mms_set_tone_alert		{1}				; 0 (Low Beep Once), 1 (Low Beeps), 2 (Loud Beep Once), 3 (Loud Beeps), 4~15 (Ringtone 1~12), 16 (No Ring)
nv_write mms_set_vibrate_alert		{0}				; 0(VIBRATE OFF), 1(VIBRATE ON)
nv_write mms_set_reminder_alert		{2}				; 0(REMIND ONCE), 1(REMIND EVERY2MIN), 2(REMIND EVERY15MIN), 3(REMIND OFF)
nv_write mms_settings_signature		{0}				; None(0), Custom(1)

nv_write mms_mmsc_url			{26, "http://mms.movilnet.com.ve"}			; 64 byte characters
nv_write mms_mmsc_upload_url		{30, "4160000000@mml.movilnet.com.ve"}			; Upload Address
nv_write mms_mmsc_uaprof_url		{43, "http://mms.movilnet.com.ve/lgemx8700vez.rdf"}	; Max 64 byte characters

nv_write mms_set_retry_num		{3}				; 0, 1, 2, 3
nv_write mms_send_from_add		{2}				; MDN Only (0), 1MDN (1),  +1MDN (2)         

nv_write mms_mmsc_user_agent		{18,"LGE-MX8700_VEZ/1.0"}	; User Agent Profile name {14,"LGE-MX8700/1.0"}
nv_write mms_mmsc_server_post_url	{5, "/mms/"}		; Post URL
nv_write mms_mmsc_server_post_cgi	{12, "?message-id="}				; CGI URL

nv_write mms_test_authorization		{0}				; 0 : Commercial, 1 : Lab
nv_write mms_test_mmsc_url		{26, "http://mms.movilnet.com.ve"}	; 48 byte characters
nv_write mms_test_mmsc_upload_url	{30, "0000000000@mml.movilnet.com.ve"}			; Upload Address

nv_write mms_set_hidden_menu_enable	{0}				; 0: Disable, 1: Enable
;=========================================================================

;=========================================================================
;F/W ITEM
;=========================================================================
nv_write rf_config			{6}
nv_write gps_rf_config			{3}
nv_write vbatt				{20, 190}			; VX8700
nv_write elapsed_time			{50}				; ympark 59=>50

nv_write qdsp_snd_ctrl			{-128, 0, 0, 0, 1024, -500, 160, 11, 23, 6, 6, 0, 0, 0, 0, -2500}	;2007.1.4 sidetone(2500->1024) 2007.1.2 tango FALSE 2006.12.28 folderOpen be changed
nv_write audio_adj_phone		{-10713, 0, 0, -10713, 0, 0, 0, 0, 0}	;2007.1.11 tamedwolph hw req 0 -> -10713
nv_write audio_adj_earjack		{0, 0, 0, 0, 0, 0, 0, 0, 0}
nv_write audio_adj_hfk			{0, 0, 0, 0, 0, 0, 0, 0, 0}
nv_write audio_adj_spk			{9581, 0, 0, 9581, 0, 0, 0, 0, 0}	;2006.12.28 tamedwolph hw req
nv_write audio_adj_bt			{0, 0, 0, 0, 0, 0, 0, 0, 0}

nv_write charging_bypass_boot		{0}				; 0=FALSE/1=TRUE
;=========================================================================

;=========================================================================
; UP EFS : for magellan 
;=========================================================================
efs write				"OWS/paramtable1.fil"
efs write				"OWS/wdptable1.fil"
;=========================================================================

;=========================================================================
;VOICE EFS
;=========================================================================
efs write				"mVoice/ment/ment_adpcm.db"
efs write				"mVoice/ment/ment_adpcm_spn.db"
efs write				"mVoice/ment/ment_voc.db"
efs write				"mVoice/ment/ment_voc_spn.db"
;=========================================================================

;=========================================================================
; DCAMERA EFS
;=========================================================================
efs write				"dload/default_img/DecodeErrorAnimation.jpg"
efs write				"dload/default_img/DecodeErrorImage.jpg"
efs write				"dload/default_img/NotSupportedImage_UnknownImage.jpg"
efs write				"dload/default_img/phoneOnConversation.jpg"
efs write				"dload/default_img/TooBigErrorImage.jpg"
efs write				"dload/default_img/video_FirstFrame_PMD.bmp"
efs write				"dload/default_img/video_FirstFrame_SVG.bmp"
efs write				"dload/default_img/VideoImageSymbol.jpg"
;=========================================================================

;=========================================================================
;FLASH CONTENT EFS
;=========================================================================
efs write				"flash/ui/wallpaper/wallpaperType1.swf"
efs write				"flash/ui/wallpaper/wallpaperType2.swf"
;=========================================================================

mode reset
