;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;=========================================================================
;-------------------------------------------------------------------------
;  when         version    Name      what
;-----------  ----------  ------------------------------------------------
;04/15/2008    RD10K01D   jaeshick   VX10K -> RD10KF
;12/10/2007    VX10KV05   sjbae      add set_envHotKey,set_touch_shortcut
;12/10/2007    VX10KV05   withjam    MOD 02.00.021 (SDCARD 8G)
;11/23/2007    VX10KV04   cesmile    VOD 4.0
;11/20/2007    VX10KV04   jeyunpark  Change skin file (VerizonStandardWQVGA.ows)
;11/09/2007    VX10KV04   cesmile    MIM 2.1.1.35 Added
;11/07/2007    VX10KV04   jeyunpark  Change skin file (VerizonStandardWQVGA.ows)
;10/25/2007    VX10KV04   kblee      Browser setting(VerizonStandardWQVGA.ows)
;10/17/2007    VX10KV03   bsryoo     Changed to VX10KV03_01.SCR(mflo app changed)
;10/15/2007    VX10KV03   parkwh     Changed to VX10KV03_00.SCR
;10/07/2007    VX10KV02   cesmeil    version.txt (ver 09 ) changed
;10/05/2007    VX10KV02   cesmile    version.txt(ver.08) - csch_eula.xml file is changed.
;10/05/2007    VX10KV02   jaeykim    update Mflow csch_eula.xml file
;10/04/2007    VX10KV02   sjbae	     sub_backlight{10} ==> sub_backlight{7}
;10/02/2007    VX10KV02   cesmile    version.txt
;10/02/2007    VX10KV01   cesmile&   jaeyKim version.txt and Mflo string update
;09/16/2007    VX10KV01   cesmile    version.txt
;09/15/2007    VX10KV01   ester      default image change (DecodeErrorAnimation.jpg, DecodeErrorImage.jpg, 
;                                    NotSupportedImage_UnknownImage.jpg, phoneOnConversation.jpg, TooBigErrorImage.jpg)
;09/15/2007    VX10KV01   thunder    VX10KV01_05 -> VX10KV01_06
;09/14/2007    VX10KV01   cesmile    preloaded app, version.txt, preload.txt
;09/13/2007    VX10KV01   thunder    VX10KV01_04 -> VX10KV01_05
;09/13/2007    VX10KV01   S.Y.HONG   FlashContents Update(EzTip)
;09/13/2007    VX10KV01   huni       Change Internal Wallpaper 6 ->3
;09/12/2007    VX10KV01   thunder    Added factory_mode
;09/11/2007    VX10KV01   S.Y.HONG   Update Flash Contents(World Clock)
;09/11/2007    VX10KV01   thunder    VX10KV01_03 -> VX10KV01_04
;09/09/2007    VX10KV01   thunder    VX10KV01_02 -> VX10KV01_03
;09/09/2009    VX10KV01   jeyunpark  Change skin file (VerizonStandardWQVGA.ows) change inbox cursor thickness
;09/08/2007    VX10KV01   cesmile    preloaded VZNavi, Email.
;09/08/2007    VX10KV01   S.Y.HONG   Delete Flash Contents(Top Menu, Wiget)
;09/07/2007    VX10KV01   jeyunpark  adding certification key write
;09/07/2007    VX10KV01   parkwh     Delete AUDIO_ASE
;09/06/2007    VX10KV01   huni       delete Tool Palette, change wallpaper value(m 0->6,s 0->7)
;09/03/2007    VX10KV01   hwseo      VZNavi gain restore (600->900)
;09/03/2007    VX10KV01   hwseo      VZNavi gain adjust (900->600)
;09/03/2007    VX10KV01   thunder    VX10KE22 -> VX10KV01
;09/03/2007    VX10KE22   jskim      mms_mmsc_uaprof_url, mms_mmsc_user_agent
;09/03/2007    VX10KE22   hwseo      EC Modified
;09/03/2007    VX10KE22   thunder    VX10KE21 -> VX10KE22
;09/01/2007    VX10KE21   khk        MIM Added
;08/31/2007    VX10KE21   S.Y.HONG   Flash Contents Update(wallpaper, widget)
;08/31/2007    VX10KE21   hwseo      VZNavi Nv Setting(QCP 6dB up, MIDI 9dB up)
;08/30/2007    VX10KE21   S.Y.HONG   Flash Contents Update(widget)
;08/28/2007    VX10KE21   thunder    version up, VX10KE20 -> VX10KE21
;08/27/2007    VX10KE20   lej        bt_audio_auto_pair default value 1(ON) 
;08/27/2007    VX10KE20   S.Y.HONG   Flash Contents Update(ezTip, widget) 
;08/27/2007    VX10KE20   jeyunpark  Change skin file (VerizonStandardWQVGA.ows) add javascript setting and change zoom level
;08/27/2007    VX10KE20   thunder    version up, VX10KE19 -> VX10KE20, pre-IUT 4th
;08/26/2007    VX10KE19   thunder    version up, VX10KE18 -> VX10KE19, pre-IUT 4th
;08/26/2007    VX10KE18   cesmile    Brew App Erase
;08/26/2007    VX10KE18   thunder    version up, VX10KE17 -> VX10KE18, QM3rd resummit, IUT
;08/25/2007    VX10KE17   jeyunpark  Change skin file (VerizonStandardWQVGA.ows)
;08/24/2007    VX10KE17   S.Y.HONG   Flash Contents Update(add topMenuType1Color2Sub.swf) 
;08/23/2007    VX10KE17   thunder    version up, VX10KE16 -> VX10KE17, QM3rd, Pre-FIT
;08/23/2007    VX10KE16   cesmile    MediaAsf file added
;08/23/2007    VX10KE16   S.Y.HONG   Flash Contents Update(del widget_timeList.xml, bg.jpg)
;08/22/2007    VX10KE16   hwseo      restore AUDIO_QDSP Folder Open Gain (3dB -> 0dB)
;08/22/2007    VX10KE16   khk BREW   App Update
;08/18/2007    VX10KE16   S.Y.HONG   Update Flash(widget, bg.jpg, delete xml file)
;08/18/2007    VX10KE16   hwseo      AUDIO_QDSP modified ( Folder open midi 0dB -> 3.0dB)
;08/18/2007    VX10KE16   thunder    version up, VX10KE15 -> VX10KE16
;08/17/2007    VX10KE15   J.Y.PARK   Change browser skin(external lcd zoom menu)
;08/17/2007    VX10KE15   S.Y.HONG   Update Flash Menu(worldClockType1Main.swf, worldClockType1Sub.swf)
;08/16/2007    VX10KE15   S.Y.HONG   Update Flash Menu(topMenuType1ColorSub.swf, subMenuType1ColorSub.swf)
;08/15/2007    VX10KE15              Update TTS DB Files
;08/15/2007    VX10KE15   kangjuil   Call end_option(flip close -> End Key Only)
;08/15/2007    VX10KE15   BT_PSH     change default value of bt_audio_auto_pair TRUE to FALSE
;08/13/2007    VX10KE15              Version up to VX10KE15
;                                    Delete Flash UI of sub menu list
;08/09/2007    VX10KE14              block touch_cal_data
;08/05/2007    VX10KE13              Version up, VX10KE12 -> VX10KE13
;08/07/2007    VX10KE13              Browser setting(VerizonStandardWQVGA.ows), 
;                                    flash contents (topMenuType1ColorSub.swf, subMenuType1ColorSub.swf,
;                                    ezTipType1Sub.swf, wallpaperType7Main.swf)
;                                    added touch_cal_data write to {0,0,0,0}
;08/01/2007    VX10KE12              Version up, VX10KE11 -> VX10KE12
;07/24/2007    VX10KE11              Enable warranty date item(nv_write lg_wdc)
;07/21/2007    VX10KE11              Version up to VX10KE11
;07/21/2007    VX10KE10              Change brew version.txt in brew_scr 
;07/20/2007    VX10KE10              add Flash UI(world clock, Idle widget)
;07/20/2007    VX10KE10              remove OWS folder in efs_scr
;07/16/2007    VX10KE09              update nv items number and UI setting values(attatched more flash wallpapers)
;07/09/2007    VX10KE07              Delete Image Files(Wallpaper, Animation)
;07/06/2007    VX10KE07              ASE added
;07/06/2007    VX10KE07              SMS msg_settings added
;07/05/2007    VX10KE07              Flash top/sub menu added
;06/29/2007    VX10KE06              Flash UI/Browser EFS data update
;06/15/2007    VX10KE05              SFN release User Agent Profile name
;04/13/2007    VX10KE01              first release
;----------    -------    ------------------------------------------------

mode offline-d
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model

wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================
nv_write sec_code                    {"000000"}                      ; Security code
nv_write lock_code                   {"0000"}                        ; Lock_code

nv_write min1                        {0, "000-0000", "000-0000"}     ; Min0 number
nv_write min1                        {1, "000-0000", "000-0000"}     ; Min1 number
nv_write min2                        {0, "000", "000"}               ; NAM 0 has one active MIN2,
nv_write min2                        {1, "000", "000"}               ; NAM 1

nv_write name_nam                    {0, "Reliance"}                     ; NAM 1 Name
nv_write name_nam                    {1, "Reliance"}                     ; NAM 2 Name

nv_write imsi_mcc                    {0, "405"}                      ; Mobile Country Code (000)
nv_write imsi_mcc                    {1, "405"}
nv_write imsi_11_12                  {0, "00"}                       ; Mobile Network Code
nv_write imsi_11_12                  {1, "00"}
;nv_write imsi_addr_num              {0, 0}
;nv_write imsi_addr_num              {1, 0}

nv_write imsi_t_mcc                  {0, "405"}
nv_write imsi_t_mcc                  {1, "405"}
nv_write imsi_t_11_12                {0, "00"}
nv_write imsi_t_11_12                {1, "00"}
nv_write imsi_t_s1                   {0, "000-0000", "000-0000"}
nv_write imsi_t_s1                   {1, "000-0000", "000-0000"}
nv_write imsi_t_s2                   {0, "000", "000"}
nv_write imsi_t_s2                   {1, "000", "000"}

nv_write dir_number_pcs              {0, "0000000000"}               ; NAM 0 : NV_DIR_NUMBER_PCS_I
nv_write dir_number_pcs              {1, "0000000000"}               ; NAM 1 : NV_DIR_NUMBER_PCS_I

print "Programming Primary CDMA Channel"
nv_write pcdmach                     {0, 239, 553}                   ; A and B primary CDMA channels
nv_write pcdmach                     {1, 239, 553}

print "Programming Secondary CDMA Channel"
nv_write scdmach                     {0, 280, 594}                   ; set only if secondary channels offered
nv_write scdmach                     {1, 280, 594}

nv_write home_sid_nid 		     {0,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535}
nv_write home_sid_nid 		     {1,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535}
nv_write sid_nid_lock                {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535} ; CDMA SID/NID pair to lockout for the given NAM and given index(0-9)
nv_write sid_nid_lock                {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535} ; CDMA SID/NID pair to lockout for the given NAM and given index(0-9)

nv_write mob_term_home               {0, true, true}
nv_write mob_term_home               {1, true, true}
nv_write mob_term_for_sid            {0, true, true}
nv_write mob_term_for_sid            {1, true, true}
nv_write mob_term_for_nid            {0, true, true}
nv_write mob_term_for_nid            {1, true, true}

nv_write accolc                      {0, 0, 0}
nv_write accolc                      {1, 0, 0}

nv_write slot_cycle_index            {2}

nv_write pref_voice_so               {0,  1, 0x0003, 0x0003, 0x0003} ; True, EVRC, EVRC, EVRC
nv_write pref_voice_so               {1,  1, 0x0003, 0x0003, 0x0003} ; True, EVRC, EVRC, EVRC

print "Programming Pref Mode"
nv_write pref_mode                   {0, 9}                          ;"1x Only"
nv_write pref_mode                   {1, 9}                          ;"1x Only"

nv_write voice_priv                  {0}                             ; 179 - 0=Standard  1=Enhanced  (1->0 [20080528]jaeshick: reliance pri )

print "Programming Band Preferred"
nv_write band_pref                   {0, "pref_any"}
nv_write band_pref                   {1, "pref_any"}

print "Programming Roam Preferred"
nv_write roam_pref                   {0, "pref_any"}
nv_write roam_pref                   {1, "pref_any"}

nv_write hybrid_pref                 {0}                             ; 1 : hybrid on,  0 : hybrid off

nv_write system_pref                 {0, "standard"}              ; System preference, actually default to band preference
nv_write system_pref                 {1, "standard"}

print "Programming MRU table clear"
                                                                     ; except nam (first 0), '0' are 48(=4 X 12) times.
nv_write mru3_table                  {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru3_table                  {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};

print "Programming NAM Checksums"
nv_write nam_chksum                  {0, 0xffff}
nv_write nam_chksum                  {1, 0xffff}
nv_write min_chksum                  {0, 0xffff, 0xffff}
nv_write min_chksum                  {1, 0xffff, 0xffff}

nv_write stand_alone_mode            {0}                             ; 0 default OFF, 1 ON

nv_write pref_for_rc                 {3}                             ; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)  
;=========================================================================

;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key                       {0, 0x00000000, 0x00000000 }
nv_write a_key                       {1, 0x00000000, 0x00000000 }
nv_write ssd_a                       {0, 0x00000000, 0x00000000 }
nv_write ssd_a                       {1, 0x00000000, 0x00000000 }
nv_write ssd_b                       {0, 0x00000000, 0x00000000 }
nv_write ssd_b                       {1, 0x00000000, 0x00000000 }
nv_write count                       {0, 0}
nv_write count                       {1, 0}
;=========================================================================

;=========================================================================
; OTA ITEM
;=========================================================================
nv_write otapa_enabled               {0, 1}                          ; enable
nv_write otapa_enabled               {1, 1}                          ; enable
nv_write spc_change_enabled          {1}
nv_write nam_lock                    {0, 1}
nv_write nam_lock                    {1, 1}
;=========================================================================

;=========================================================================
; MSG ITEM
;=========================================================================
nv_write msg_settings_auto_save     {1}                              ; MSG_AUTO_SAVE(0), MSG_DO_NOT_SAVE(1), MSG_PROMPT(2)
nv_write msg_settings_auto_delete   {0}                              ; 0(Off), 1(On)
nv_write msg_settings_entry_mode    {0}                              ; MSG_T9EN(0), MSG_ABC(1), MSG_123(2)
nv_write msg_settings_vibrate_alert {0,0}                            ; 0(Off), 1(On)
nv_write msg_settings_signature     {0}     ; None(0), Custom(1)
;=========================================================================

;=========================================================================
; SMS/EMS ITEM
;=========================================================================
nv_write sms_txt_cb_enable      	{0}     		    ; On(1), Off(0) 
nv_write sms_orig_msg_id        	{1}     		    ; 0X0001 - 0XFFFF  
nv_write sms_mo_max_userdata		{160}			    ; support up to 220 bytes
nv_write sms_mo_l3_ack			{1}			    ; SMS_OFF(0), SMS_ON(1)
nv_write sms_mo_so			{1}			    ; SMS_SO14(0), SMS_SO6(1)
nv_write sms_voicemail_record   	{0,0}   		    ; {Count,Time}
nv_write sms_settings_direct_view    	{0}	            	    ; Off(0), On(1)
nv_write sms_voicemail_alert         	{1}    	        	    ; 5(VZW Default Tone), 6~16(Ringtone 1~10), 17(No Ring), 0xffff(Get New Ringtones) 
nv_write sms_textmsg_alert           	{1}             	    ; 0(Low Beep Once),1(Low Beeps),2(Laud Beep Once),3(Loud Beeps)  
nv_write sms_voicemail_cb		{4,"*600"} 		    ; 32Byte(ASCII)
nv_write sms_urgent_voice_record     	{0}                         ; None(0), Exist(1) 
nv_write sms_2min_alert_sel          	{3,3}              	    ; Once(0), Every 2 Minutes(1), Every 15 Minutes(2), Off(3) 
nv_write sms_message_cb              	{10,"0000000000"}           ; 
;=========================================================================

;=========================================================================
; SMS/EMS ITEM
;=========================================================================
nv_write sms_settings_auto_play      	{0}                         ; On(1), Off(0)  
nv_write sms_ems_enable              	{0}                         ; On(1), Off(0)
;=========================================================================

;=========================================================================
; MMS ITEM 
;=========================================================================
nv_write mms_set_auto_receive        {1}                             ; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_set_read_ack            {1}                             ; 0(ON), 1(OFF)
nv_write mms_set_delivery_ack        {0}                             ; 0(MMS_ON), 1(MMS_OFF)

nv_write mms_set_tone_alert          {1}                             ; 0(Low Beep Once), 1(Low Beeps), 2(Loud Beep Once), 3(Loud Beeps), 4(Door Bell), 5(VZW Default Tone), 6~25(Ringtone 1~20), 26(No Ring)
nv_write mms_set_vibrate_alert       {0}                             ; 0(VIBRATE OFF), 1(VIBRATE ON)
nv_write mms_set_reminder_alert      {3}                             ; 0(REMIND ONCE), 1(REMIND EVERY2MIN), 2(REMIND EVERY15MIN), 3(REMIND OFF)

nv_write mms_mmsc_url                {20, "http://mms.vtext.com"}    ; 48 byte characters
nv_write mms_mmsc_upload_url         {6, "438749"}                   ; Upload Address
nv_write mms_mmsc_uaprof_url         {44, "http://uaprof.vtext.com/lg/vx10k/vx10kv1.xml"} ; 48 byte characters

nv_write mms_set_retry_num           {0}                             ; 0, 1, 2, 3
nv_write mms_send_from_add           {2}                             ; MDN Only (0), 1MDN (1),  +1MDN (2)         

nv_write mms_mmsc_user_agent         {7,"vx10kv1"}                  ; User Agent Profile name
nv_write mms_mmsc_server_post_url    {13, "/servlets/mms"}           ; Post URL
nv_write mms_mmsc_server_post_cgi    {12, "?message-id="}            ; CGI URL

nv_write mms_test_authorization      {0}                             ; 0 : Commercial, 1 : Lab
nv_write mms_test_mmsc_url           {20, "http://66.174.75.171"}    ; 48 byte characters
nv_write mms_test_mmsc_upload_url    {6, "666612" }                  ; Upload Address
;=========================================================================

;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_pkt_orig_str      {5, "#777"}    ; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_mdr_mode          {3}            ; Service Option 33 (1x channel) = 3 Use only low-speed packet data = 2
nv_write data_auto_packet_detection {0}        ; 0-Disable   1-Enable
nv_write data_so_set            {2}            ; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write diag_default_baudrate  {0x000e}       ; 0x000e(38.4kbps), 0x0011(115.2kbps) 
nv_write data_qnc_enabled       {0}            ; 0-QNC Disable  1-QNC Enable (alltel doesn't support QNC anymore.)
nv_write ppp_user_id            {0,""}         ; Max of 127 chars in User ID. reset 시에 모델에 따라 맞는 패스워드로 쓰여진다...ex. 모델명@relianceinfo.com
nv_write ppp_password           {0,""}       ;  ""값이 쓰여지면 폰에서 reset시에 모델에 따라 맞는 패스워드로 쓰여진다...
nv_write data_scrm_enabled      {1}            ; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled      {1}            ; 0-TRTL Disable 1-TRTL Enable
nv_write pref_for_rc            {3}            ; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)    
nv_write ds_default_baudrate    {0x0011}       ; 0x0000 (19.2kbps),0x0011(115.2kbps)
nv_write ds_qcmip               {0}            ; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only

nv_write dun_cable_mode         {1}            ; 0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode            {1}            ; 0=disable bt dun,1=enable bt dun

nv_write ppp_carrier            {8}            ; 0-Verizon 1-USC 7-SCRIPT. Test NV Item.     
;=========================================================================

;=========================================================================
; BROWSER ITEM 
;=========================================================================
efs write "brew/mod/obigo/usr_data/skins/VerizonStandardWQVGA.ows"
efs write "brew/mod/obigo/ids/storage/S_0"
efs write "brew/mod/obigo/ids/storage/S_1"
efs write "brew/mod/obigo/ids/storage/S_2"
efs write "brew/mod/obigo/ids/storage/S_3"
efs write "brew/mod/obigo/ids/storage/S_4"
efs write "browser/setting/fileDB"
efs write "browser/setting/fileDBList"
efs write "browser/fileDBComplete"
;=========================================================================

;=========================================================================
; PIM ITEM
;=========================================================================
;efs write "pim/call_hist_nv.dat"                                    ;delete
;=========================================================================

;=========================================================================
;UI ITEM
;=========================================================================
nv_write bt_audio_auto_pair          {1}                             ; 5002 - 1(ON), 0(OFF)
nv_write call_sounds                 {5,5,5,5,0}                     ; 5004 - {Caller ID (5: ADAG Tuen), No Caller ID (5: ADAG Tuen), Restrict Calls (5: ADAG Tuen), All Calls (5: ADAG Tuen), Vibrate (0: Off, 1: On)}
nv_write ringer_lvl                  {0x4}                           ; 64 - 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 99(Vibrate only=manner_mode), 97(alarm only), 100(Sounds Off=silence_all)
nv_write ringer_spkr_lvl             {0x4}                           ; 229 - 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 98(High & Vib), 99(Vibrate)
nv_write beep_lvl                    {0x4}                           ; 65 - 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) handset(earjack) vol
nv_write beep_lvl_shadow             {0x4}                           ; 164 - 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) headset(earpiece) vol
nv_write beep_spkr_lvl               {0x4}                           ; 230 - 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) - carkit vol
nv_write spk_phone_beep_lvl          {0x4}                           ; 5049 - 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) - Keypad Volume on Speaker Phone Mode
nv_write ear_lvl                     {0x6}                           ; 62 - Low(Volume 1)~ High(Volume 8)
nv_write ear_lvl_shadow              {0x6}                           ; 165 - Low(Volume 1)~ High(Volume 8)
nv_write speaker_lvl                 {0x6}                           ; 63 - Low(Volume 1)~ High(Volume 8) - carkit vol
nv_write backtop_beep                {true}                          ; 5029 - Back To Top Sound == on       
nv_write power_onoff_sounds          {1,1}                           ; 5003 - {Power On, Power Off}, On (1), Off (0)
nv_write banner                      {"Reliance"}                    ; 71 - Banner - default blank, because confuse Banner with ERI text
nv_write sub_banner                  {"Reliance"}                    ; 5047 - Sub Banner - default blank, because VX9400 doesn't have sub LCD.
nv_write eri_text_onoff              {1}                             ; 5050 - 1 -> On, 0 -> Off
nv_write back_light                  {7}                             ; 77 - Backlight
nv_write sub_backlight               {7}                             ; 5022 - Sub Backlight
nv_write key_light                   {7}                             ; 5007
nv_write wallpaper_main              {0,0,4}                         ; 5061 - {location_type (0 : PHONE_MEM), itemType (0 : ONE_CUT), item_id}
nv_write wallpaper_sub               {1,6,50}                        ; {location_type (1 : PHONE_EFS), itemType (6 : Default Flash), item_id}
nv_write number_size                 {0,0}                           ; 5025 - (size, color(don't use)) 0:normal 1:large //lej 2006.10.25 Large -> Normal
nv_write curr_nam                    {0}                             ; Current NAM           == NAM1
nv_write auto_nam                    {off}                           ; Auto NAM              == disable
nv_write location_set_lock           {0}                             ; 1 -> location on 0-> E911 only
nv_write auto_lock                   {off}                           ; phone lock            == Unlocked \ Power_up
nv_write lock                        {off}                           ; phone lock            == Unlocked \ now
;nv_write emergency_num1              {"911"}                         ; 5026 - Up to 48 Digits
;nv_write emergency_num2              {"*911"}                        ; 5027 - Up to 48 Digits
;nv_write emergency_num3              {"#911"}                        ; 5028 - Up to 48 Digits
nv_write language_selection          {0}                             ; 227 - Default (English/Spanish) == English
nv_write answer_option               {1}                             ; 5015 - Answer option	[20080528]jaeshick: reliance pri 3 -> 1
nv_write auto_answer                 {0, 0}                          ; Auto answer           == off
nv_write end_option            	     {1}                             ; 5017 - End call_option
nv_write auto_redial                 {0, 0}                          ; Auto redial           == off
nv_write tty                         {3}                             ; 409 - TTY Full(0), TTY+TALK(1),TTY+HEAR(2),TTY off(3)
nv_write onetouch_dial               {on}                            ; One touch dial        == disable!
nv_write shortcut_main               {0,9,18,7}                      ; 5077 - {Left, Up, Right, Down}	[20080528]jaeshick: reliance pri
nv_write call_rstrc                  {0x00}                          ; Restrict(0:off, 1:on) 
nv_write bt_power_onoff              {0}                             ; 5059 - 1 -> On, 0 -> Off
nv_write beep_bt_lvl                 {0x4}                           ; 5064 - 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write ear_bt_lvl                  {12}                           ; 5065 - 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 6(High), 7(High)
nv_write media_save_option           {1,1,1}                         ; 5063 - 	media_save_option{pix_save_location(0 : phone memory 1: sdcard) ,flix_save_location(0 : phone memory 1: sdcard) ,sound_save_location(0 : phone memory 1: sdcard) }
nv_write alarm_sounds                {5,0}                           ; {tone(5: ADAG Tuen), vibrate (0: Off)}

nv_write fsc                         {"000000"}                      ; Field Service code
nv_write auto_volume_enabled         {0}                             ; 0-> off , 1-> on
nv_write cont_key_dtmf               {1}                             ; Prssed key tone       == 1: Normal, 0: Long  2: Off  (NEW)
nv_write send_pin                    {off}                           ; Send pin?             == disable!
;nv_write carrier_logo                {0}                             ; 0 -> Verizon, 
nv_write avr_call_alerts             {0}                             ; 5072
nv_write avr_prompts_mode            {0}                             ; 5073
nv_write avr_choice_list             {0}                             ; 5074
nv_write avr_prompts_timeout         {0}                             ; 5075
nv_write avr_sensitivity             {1}                             ; 5076
nv_write avr_digit_dial_readout      {0}                             ; 0 : Off, 1: On
nv_write avr_audio_playback          {0}                             ; 0 : Speakerphone, 1: Earpiece

;nv_write sound_ringers               {4,9,6,0xFFFF,0}                ; (caller ID, No Caller ID, Restrict, all calls, vibrate options) added item 4th & 5th 2003.11.30 ;KHW 2004.06.16 MODIFY in NJ

nv_write silence_all                 {0}                             ; 5004 - sound on   {1} sound off
nv_write edit_font                   {0,0} 
nv_write manner_mode                 {0}                             ; 5024 - false {0}, true {1}

; nv_write backtop_beep               {1}

nv_write wclock_choice               {11,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,20,0}
;                                    5016 - {cur_Itm (11), Set_DST, choice_city ( NewDelhi: 20), line longtitude}
;nv_write stack_idx                   {0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff} ; call history clear

nv_write power_saver                 {0}
nv_write alarm_only_mode             {0}                             ; 5048 - 0 -> Disable, 1 -> Enable
nv_write camera_flash_test           {0}                             ; 0 : Normal, 0x55 : For Manufacture

;nv_write bd_addr                    {0x9a,0xbc,0x56,0x78,0x12,0x34} ; Bluetooth Address

nv_write pc_port                     {0}                             ; 5067 - PC connection port  0 (USB), 1 (UART), 2 (BLUETOOTH), 3 (CLOSED)
;nv_write key_guard_set               {30}                            ; key_guard   0(Always off)  7( 7 Seconeds)  30( 30 Seconeds)  120( 2 Min)
;nv_write keyguard_release_options    {0}                             ; keyguard options   0(Press Once)  1(Press Twice) //lej 2006.09.20
nv_write equalizer_mode              {1}                             ; 0(flat) , 1(3D Surround) ,2 (Concert Hall) , 3 (Rock) , 4 (Jazz)  , 5 (POP) , 6 (Classical) 
nv_write visualizer_mode             {0}                             ; 0 enable   ,  1 disable
;nv_write use_mymp3                   {1}                             ; 0 : MUSIC_NONE,   1 : MUSIC_MP3_ONLY,   2 : MUSIC_MOD_ONLY,     3 : MUSIC_MP3_MOD
;nv_write lg_sys_cdg_enable           {0}                             ; 0 DISABLE , 1 ENABLE
nv_write lg_wdc                      {0,0,0,0,0}
nv_write  mf_mru_chan                {4980}

nv_write vp_spkr_lvl                 {0x6}                          ; Low(Volume1)~ High(Volume8)
nv_write vp_lvl_shadow	             {0x6}	            	          ; Low(Volume1)~ High(Volume8)
nv_write vp_bt_lvl                   {0x6}	             	          ; Low(Volume1)~ High(Volume8)
nv_write vp_spkr_shadow_lvl          {0x6}	             	          ; Low(Volume1)~ High(Volume8)
nv_write vp_lvl	                     {0x6}	             	          ; Low(Volume1)~ High(Volume8)
nv_write dual_nam_set_enable         {1}                            ; Enable(1)/Disable(0)
nv_write vibrate_factory_test        {0}	             	            ; TRUE(1), FALSE(0)

nv_write music_only_mode             {0}                            ; 0 default OFF, 1 ON
nv_write display_set                 {0,0,1}                        ; 5009 (Sub Clock, Main Clock, Theme)

;nv_write service_num                 {"611"}                        ; Up to 48 Digits
nv_write set_touch                   {1,0,0,1,0}                    ; 5097 - (Auto Lock, Sensitivity, Vib Type, Vib Level, Sound)
nv_write set_menu_fonts              {0}                            ; 5099
nv_write set_usb_auto_detection      {1}                            ; 5100
nv_write sound_alerts                {0,0,1,0}                      ; 5006 
nv_write charging_alert_onoff        {0}                            ; 5092 
nv_write screen_saver                {1,0}                          ; 5081   swkim 080602 Reliance requirement : Desk Clock is default


nv_write set_envHotKey                {0,0,1,2,3,4,5,6,7,8,9}       ; 5096 
nv_write set_touch_shortcut           {0,0,1,2,3,4,5,6,7,8,9,10,11} ; 5325 
nv_write service_menu_enter	      {1}                            ;1 - can access ([20080418]jaeshick: Reliance model hidden menu access process)

;=========================================================================

;=========================================================================
;F/W ITEM
;=========================================================================
;nv_write ftm_mode {1}                                               ; ystk 2003.10.06 - for Initial Booting Mode to DMSS mode!
;nv_write fm_rssi {0x2c, 0x7f}                                       ; modify {0x4a, 0x77} -> {0x2c, 0x7f};hkshin 200.10.28 - for hw request
nv_write rf_config {6}
;nv_write lcd {39}                                                   ; don't use for VX8100
;hkshin 200.10.28 - for hw request
;nv_write vbatt {166, 244}                                           ; VX9800

;nv_write cdma_rx_comp_vs_freq { -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12 }
;nv_write pcs_rx_comp_vs_freq  { -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10 }
;nv_write elapsed_time {59}

; modified by Heo Si Hang
;nv_write qdsp_snd_ctrl {0,0,0,49149,1280,0,190,22,31,6,6,0,0,19,6,0};
;nv_write audio_adj_phone             {0, 0, 0, 0, 0, 0, 0, 0, 0}
;nv_write audio_adj_earjack {0, 0, 0, 0, 0, 0, 0, 0, 0}
;nv_write audio_adj_spk {0,0,0,0,0,0,0,0,0}
;nv_write rx_pcm_filter_ctrl {0x7, 0x2, 0xFFF9, 0x213, 0x742, 0x1020, 0x3120}
;nv_write tx_pcm_filter_ctrl {0xb, 0xFFF4, 0xFFA6, 0xFF2B, 0xFD31, 0xF883, 0x48C3}
;nv_write qdsp_agc_ctrl{ 0x2000,0x0,0x780,0xFF52,0x1D00,0xF333,0,0,0x2000,0x0,0x780,0xFF52,0x2580,0xF333}
;nv_write charging_bypass_boot {0}

nv_write AUDIO_CODEC_GAIN {0,0,0,0,0,0,0,0,0}; 
nv_write AUDIO_VOC_GAIN {0,0,0,0,0,0,0,0,0,0}; 
nv_write AUDIO_AGC {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write AUDIO_RX_FIR_PCM_FILTER {0,0,0,0,0,0,0,0};
nv_write AUDIO_TX_FIR_PCM_FILTER {0,0,0,0,0,0,0,0};
nv_write AUDIO_QDSP {0,0,0,0,0,0,20,0,7,7,0,0,0,0,0,0,0,900,600,0};
;nv_write AUDIO_ASE {0}  	;Adaptive Speech Enhancement
;nv_write touch_cal_data	{0,0,0,0}; set to all 0 for User Calibration start
nv_write factory_mode {0}

;=========================================================================

;=========================================================================
;BREW ITEM modified by Kim sungkung
;=========================================================================
nv_write brew_bkey {0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 
nv_write brew_download_flags {0x0004}                           ; 
nv_write brew_auth_policy {1}                             ; 
nv_write brew_privacy_policy {3}                            ;
nv_write brew_carrier_id {75}                          ;   //reliance carrier_id
nv_write brew_server    {"adsprepay.wdsap.ricinfo.com"}      ; 64 byte character //reliance RD10K
nv_write brew_platform_id {1208}			;VX10K PID //for RD10K same as VX10K
;nv_write brew_disallow_dormancy {1}			; TRUE
nv_write brew_sid_length {32}		
;nv_write mflo_enable {1}                                             ; 0:OFF, 1:ON //lej 2006.10.26

;=========================================================================


;lej 2006.09.07 default img efs로
;=========================================================================
;WALLPAPER DEFAULT IMAGE ITEM
;=========================================================================
;efs write "dload/default_img/wallpaper_3_320x204.bmp"
;efs write "dload/default_img/wallpaper_4_320x204.bmp"
;efs write "dload/default_img/wallpaper_5_320x204.bmp"
;efs write "dload/default_img/wallpaper_6_320x204.bmp"
;efs write "dload/default_img/wallpaper_7_320x204.bmp"
;efs write "dload/default_img/wallpaper_8_320x204.bmp"
;efs write "dload/default_img/wallpaper_3_240x284.bmp"
;efs write "dload/default_img/wallpaper_4_240x284.bmp"
;efs write "dload/default_img/wallpaper_5_240x284.bmp"
;efs write "dload/default_img/wallpaper_6_240x284.bmp"
;efs write "dload/default_img/wallpaper_7_240x284.bmp"
;efs write "dload/default_img/wallpaper_8_240x284.bmp"

;lkg 031002 added eri sound.
;=========================================================================
;ERI SOUND ITEM
;=========================================================================
efs write "eri_sound/extendednetwork.qcp"
efs write "eri_sound/lossofservice.qcp"
efs write "eri_sound/roaming.qcp"
efs write "eri_sound/verizonwireless.qcp"

;HKSHIN 2003.12.19
;=========================================================================
;MMS IMAGE ITEM
;=========================================================================

;HKSHIN 2003.12.19
;=========================================================================
;MMS SOUND ITEM
;=========================================================================


;=========================================================================
; DCAMERA ITEM
;=========================================================================
efs write "dload/dcammenu.dat"
efs write "dload/default_img/DecodeErrorAnimation.jpg"
efs write "dload/default_img/DecodeErrorImage.jpg"
efs write "dload/default_img/NotSupportedImage_UnknownImage.jpg"
efs write "dload/default_img/phoneOnConversation.jpg"
efs write "dload/default_img/TooBigErrorImage.jpg"

efs write "dload/default_img/video_FirstFrame_PMD.bmp"
efs write "dload/default_img/video_FirstFrame_SVG.bmp"
efs write "dload/default_img/VideoImageSymbol.jpg"



;=========================================================================

;=========================================================================
; SHUTTER SOUND 
;=========================================================================
efs write "dload/shutter1.wav"
efs write "dload/saycheese.wav"
efs write "dload/ready123.wav"
;=========================================================================

;=========================================================================
; VIDEO SOUND 
;=========================================================================
;efs write "dload/videostart.wav"
;efs write "dload/videoend.wav"

;=========================================================================
; 2005.06.02 thunder - TTS 
;=========================================================================
; TTS ITEM
;=========================================================================
efs write "mTalk/sms-etts.cnt"
efs write "mTalk/sms-etts.dat"
efs write "mTalk/sms-etts.etc"
efs write "mTalk/sms-etts.hdx"
efs write "mTalk/sms-etts.idx"
efs write "mTalk/sms-etts.key"
;=========================================================================


;=========================================================================
;GPSONE ITEM added in 2005-03-04
;=========================================================================
nv_write gps1_lock {3}

nv_write gps1_pde_address {0,0,0,0}
nv_write gps1_pde_port {0}
;=========================================================================


;=========================================================================
; Flash UI ITEM
;=========================================================================
efs write "flash/ui/wallpaper/wallpaperType1Main.swf"
efs write "flash/ui/wallpaper/wallpaperType1Sub.swf"
efs write "flash/ui/wallpaper/wallpaperType2Main.swf"
efs write "flash/ui/wallpaper/wallpaperType2Sub.swf"
efs write "flash/ui/wallpaper/wallpaperType3Main.swf"
efs write "flash/ui/wallpaper/wallpaperType3Sub.swf"
efs write "flash/ui/wallpaper/wallpaperType4Main.swf"
efs write "flash/ui/wallpaper/wallpaperType4Sub.swf"
efs write "flash/ui/wallpaper/wallpaperType5Main.swf"
efs write "flash/ui/wallpaper/wallpaperType5Sub.swf"
efs write "flash/ui/wallpaper/wallpaperType6Main.swf"
efs write "flash/ui/wallpaper/wallpaperType6Sub.swf"
efs write "flash/ui/tools/ezTipType1Main.swf"
efs write "flash/ui/tools/ezTipType1Sub.swf"
efs write "flash/ui/tools/worldClockType1Main.swf"
efs write "flash/ui/tools/worldClockType1Sub.swf"

mode reset
