;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;  when         who        what
;----------------    ------------     ------------------------------------------------
;20/07/2006   kwangsoo     modify wallpaper_main and wallpaper_sub to {0,0,1,""}
;10/07/2006   kwangsoo     modify wallpaper_main and wallpaper_sub to {0,0,2,""}
;10/07/2006   kwangsoo     modify phone_setup to {0,0,26,27,28,29,0,0,0,0,0,0,0,0,0}
;07/07/2006	cy	   Change the diag_default_baudrate to 0x0011{115kbps)
;07/05/2006   AriesGon	   Change the msg_settings_auto_save to MSG_DO_NOT_SAVE(2)
;07/05/2006   AriesGon	   Change the msg_settings_entry_mode to MSG_T9EN(0)
;07/01/2006      cy	   Change the data_so_set to IS707(2)
;06/19/2006    fuxing      Remove the brew_disallow_dormancy
;06/19/2006    fuxing      Remove the brew_sid_length
;06/07/2006	cy	   Change  the QNC Enable to Disable.
;06/04/2006     JHJ        Change  the NAM Name to "Reliance"
;05/22/2006	cy	   Change  the emergency_num1 to "100"
;05/22/2006	cy	   Change  the emergency_num2 to "101"
;05/22/2006	cy	   Change  the emergency_num3 to "102"
;05/22/2006	cy	   Remove  the mms_mmsc_server_post_cgi
;05/22/2006	cy	   Remove  the mms_upload_addr
;05/22/2006	cy	   Remove  the mms_settings_authorization
;05/15/2006	cy	   Remove  the hdr_an_auth_passwd_long
;05/15/2006	cy	   Remove  the ds_mip_ss_user_prof
;05/15/2006	cy	   Remove  the "DMU/10.key"
;05/15/2006	cy	   Remove  the ds_sip_rm_nai
;05/15/2006	cy	   Remove  the ds_mip_rm_nai
;05/15/2006	cy	   Remove  the ppp_password
;05/15/2006	cy	   Remove  the ppp_user_id
;05/15/2006	cy	   Remove  the ppp_carrier
;05/15/2006	cy	   Remove  the hdr_an_auth_user_id_long
;05/15/2006	cy	   Remove  the ds_mip_dmu_mn_auth
;05/15/2006	cy	   Remove  the ds_mip_dmu_pkoid
;05/15/2006	cy	   Remove  the ds_mip_qc_drs_opt
;05/15/2006	cy	   Remove  the ds_mip_gen_user_prof
;05/15/2006	cy	   Remove  the ds_mip_rrq_if_tfrk
;05/15/2006	cy	   Remove  the ds_mip_2002bis_mn_ha_auth
;05/15/2006	cy	   Remove  the ds_mip_num_prof
;05/15/2006	cy	   Remove  the ds_mip_pre_re_rrq_time
;05/15/2006	cy	   Remove  the ds_mip_retry_int
;05/15/2006	cy	   Remove  the ds_mip_retries
;05/15/2006	cy	   Remove  the ds_mip_enable_prof
;05/15/2006	cy	   Remove  the ds_mip_active_prof
;05/15/2006	cy	   Remove  the ds_qcmip
;05/10/2006     JHJ        Bloking to ERI_SOUND Items
;05/10/2006     JHJ        change the "eri_text_onoff : 1" to "0"
;05/10/2006     JHJ        change the "system_pref : automatic A" to "standard"
;02/05/2006    kwangsoo    modify phone_setup   to  {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0}
;04/21/2006	JHJ	   change the "imsi_t_mcc : 310" to "404"
;04/21/2006	JHJ	   change the "voice_priv : 1" to "0"
;04/21/2006	JHJ	   change the "pref_voice_so : True, wildcard, EVRC, EVRC" to "True,EVRC, EVRC, EVRC"
;04/21/2006     JHJ        change the "hybrid on" to hybrid off
;04/21/2006     JHJ        change the "pcdmach :283,384" to "239, 553"
;04/21/2006     JHJ        change the "scdmach :691,777" to "280, 594"
;04/21/2006	JHJ	   Change the "home_sid_nid : 2004,65535" to "14655,65535"
;04/21/2006	JHJ	   Change the "imsi_mcc: 310" to "404"
;01/06/2006    Jaehyek     modify phone_setup   to  {0,0,20,18,130,146,140,0,0,0,0,0,0,0,0}
;01/06/2006    Jaehyek     change the "use_mymp3" to 2 
;01/06/2006    Jaehyek     change the "brew_platform_id " to 1111
;12/16/2005    Jaehyek     change the "brew_platform_id " to 1072
;12/17/2005    Jaehyek     change the "slot_cycle_index" to 2
;12/16/2005    Jaehyek     change the "brew_platform_id " to 1111
;12/02/2005    Jaehyek     change the brew ver 07 to 08 within version.txt for mass-product.
;11/16/2005    Jaehyek     modify data_pkt_orig_str to {5, "#777"} 
;11/02/2005    Jaehyek     modify phone_setup   to  {0,0,20,18,130,146,190,0,0,0,0,0,0,0,0}
;10/13/2005    Jaehyek     update the item value "use_mymp3" to 1
;09/23/2005    Jaehyek     change the brew ver 06 to 07 within version.txt
;09/22/2005    Jaehyek     update the BREW App Signature file for the Email, MIM
;09/12/2005    Jaehyek     update the item "use_mymp3" and set to 2 for only MOD version
;08/31/2005    Jaehyek     update the wall paper ( that is , island image )
;08/31/2005    Jaehyek     update the VOD app ( that is , sig file )
;08/26/2005    Jaehyek     make the data items   initialized to 0  "ppp_password, ds_mip_ss_user_prof, hdr_an_auth_passwd_long "
;08/14/2005    Jaehyek     delete the stack_idx  no more needed.
;08/11/2005    Jaehyek     modify the item value"ds_mip_dmu_mn_auth"
;08/05/2005    Jaehyek     add nv item "sms_tts_readout "
;08/03/2005    Jaehyek     modify elapsed_time to 59
;08/02/2005    Jaehyek     modify a item "audio_adj_phone"
;08/01/2005    Jaehyek     modify sms_2min_alert_sel          {3,3,3,3}
;08/01/2005    Jaehyek     modify audio_adj_phone {0, 0, 0, -800, 0, 0, 0, 0, 0}
;08/01/2005    Jaehyek     modify phone_setup    {0,0,20,18,130,146,140,0,0,0,0,0,0,0,0}
;07/28/2005    Jaehyek     modify the data item for DUN to multi NAI
;07/28/2005    Jaehyek     add the sub LCD image for error
;07/28/2005    Jaehyek     change the audio gain parameter.
;07/28/2005    Jaehyek     add nvitem "MP3" provied from sjbae
;07/27/2005    Jaehyek     remove the  mTalk DB
;07/27/2005    Jaehyek     remove the mVoice DB
;07/19/2005    Jaehyek     remove the wallpaper_05.bmp and  ext_wallpaper_05.bmp
;07/18/2005    Jaehyek     add the item "elapsed_time"
;07/15/2005    Jaehyek     remove the power on/off animation
;07/06/2005    Jaehyek     remove the camera item "contrast_lvl", and add "camera_flash_test"
;07/04/2005    Jaehyek     update the wave file "shutter2.wav"
;06/27/2005    Jaehyek     restore the dsp value "1000" to "1400"
;06/16/2005    Jaehyek     modify the qdsp value "1400" to "1000"
;06/14/2005    Jaehyek     Update the mTalk DB
;06/13/2005    Jaehyek     Just rename the script file
;06/10/2005    Jaehyek     modify the item "phone_setup"
;06/09/2005    Jaehyek     modify the handfree kit gain "audio_adj_hfk"
;06/07/2005    Jaehyek     add the item "wallpaper_05.bmp" and "ext_wallpaper_05.bmp"
;06/07/2005    Jaehyek     add the item "key_guard_set"
;06/02/2005    Jaehyek     add the TTS DB files
;05/25/2005    Jaehyek     add the "video_FirstFrame_PMD.bmp"
;05/23/2005    Jaehyek     update the BREW file "version.txt"
;05/19/2005    Jaehyek     add the default images when decording fails by reguest from Seo Hoyung Woo.
;05/18/2005    Jaehyek     remove the item "imsi_addr_num" from request of bae chan se
;05/18/2005    Jaehyek     modify the audio nv, and added a nv item "audio_adj_bt"
;05/18/2005    Jaehyek     modify the value of imsi_mcc, imsi_mcc to 310
;05/15/2005    Jaehyek     added nv_item "pc_port"
;05/15/2005    Jaehyek     modify the imsi_t_mcc.
;05/12/2005    Jaehyek     delete the imsi_t_addr_num. by system part
;05/09/2005    Jaehyek     change the value of mms_settings_auto_download to 1
;05/08/2005    Jaehyek     Delete the Wallpaper image "wallpaper_02.bmp", "ext_wallpaper_02.bmp"
;05/08/2005    Jaehyek     Update the mVoice directory
;04/25/2005    Jaehyek     Mask the AVT line "etts_name.dat", "etts_name.idx", and update the lib
;04/21/2005    Jaehyek     Unmask the "efs write "DMU/10.key""
;04/20/2005    Jaehyek     change the AVT script.
;04/07/2005    Jaehyek     Stand-Alone modified by Lhu Bong Suk : v108990@lge.com
;04/07/2005    Jaehyek     added by Kim Hyunwoo for Bluetooth
;04/07/2005    Jaehyek     Add the sound item video start/end wave.
;04/07/2005    Jaehyek     remove the data item "used_packet_amount"
;04/07/2005    Jaehyek     add the data item "dun_cable_mode" and "dun_bt_mode"
;04/06/2005    Jaehyek     update the Brew script whole body.
;03/29/2005    Jaehyek     add the AVT engine lib by Lee eun Ju
;03/25/2005    Jaehyek	   move the midi, bmp to Brew dir  marked by sjbae
;03/18/2005    Jaehyek     unblock some item of GPSONE ITEM 
;03/10/2005    Jaehyek     change the BREW 3.1 Script
;03/04/2005    Jaehyek     Added GPS1 nv item 	
;11/19/2004    Jaehyek     Created the initial script file. (T98VZT01.SCR)
;----------    -------    ------------------------------------------------


;spc "000000"                         ; does not need at LGDP DLL
;wait 2
mode offline-d
;=========================================================================
; SYSTEM ITEM
;=========================================================================
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model

wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================

nv_write slot_cycle_index {2}

nv_write mob_model {0xD3}	; VX9800 mob_model

nv_write imsi_mcc {0, "404"}          ; Mobile Country Code (000)
nv_write imsi_mcc {1, "404"}
nv_write imsi_11_12 {0, "00"}         ; Mobile Network Code
nv_write imsi_11_12 {1, "00"}
nv_write min1 {0, "000-0000", "000-0000"}
nv_write min1 {1, "000-0000", "000-0000"}
nv_write min2 {0, "000", "000"}       ; NAM 0 has one active MIN2,
nv_write min2 {1, "000", "000"}       ; NAM 1
;nv_write imsi_addr_num {0, 0}
;nv_write imsi_addr_num {1, 0}

; NV_DIR_NUMBER_PCS_I      /*123456789012345*/ using 10 digits
nv_write dir_number_pcs {0, "0000000000"} ; NAM 0 : NV_DIR_NUMBER_PCS_I
nv_write dir_number_pcs {1, "0000000000"} ; NAM 1 : NV_DIR_NUMBER_PCS_I

; Prefer Mode.
print "Programming Pref Mode"
nv_write pref_mode {0, "Digital Only"}
nv_write pref_mode {1, "Digital Only"}

; Band preferred.
print "Programming Band Preferred"
nv_write band_pref {0, "pref_any"}
nv_write band_pref {1, "pref_any"}

; Roaming preferred.
print "Programming Roam Preferred"
nv_write roam_pref {0, "pref_any"}
nv_write roam_pref {1, "pref_any"}

; System preference, actually default to band preference
nv_write system_pref {0, "standard"}
nv_write system_pref {1, "standard"}

nv_write hybrid_pref  {0}    ; 1 : hybrid on,  0 : hybrid off

; SID 2004 ->14655 JHJ 2006.04.21 
nv_write home_sid_nid {0,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535}
nv_write home_sid_nid {1,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535,14655,65535}
nv_write sid_nid_lock {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}

; Primary CDMA Channels for A carrier and B carrier
print "Programming Primary CDMA Channel"
nv_write pcdmach {0, 239, 553}        ; A and B primary CDMA channels 283,384 ->239,553
nv_write pcdmach {1, 239, 553}

; Secondary CDMA Channel
print "Programming Secondary CDMA Channel"
nv_write scdmach {0, 280, 594}        ; set only if secondary channels offered 691,777 ->280,594
nv_write scdmach {1, 280, 594}

print "Programming MRU table clear"
; except nam (first 0), '0' are 48(=4 X 12) times.
nv_write mru3_table {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru3_table {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};


; NAM Checksums must all be 0xffff
print "Programming NAM Checksums"
nv_write nam_chksum {0, 0xffff}
nv_write nam_chksum {1, 0xffff}

nv_write accolc {0, 0, 0}
nv_write accolc {1, 0, 0}
nv_write mob_term_home {0, true, true}
nv_write mob_term_home {1, true, true}
nv_write mob_term_for_sid {0, true, true}
nv_write mob_term_for_sid {1, true, true}
nv_write mob_term_for_nid {0, true, true}
nv_write mob_term_for_nid {1, true, true}
nv_write min_chksum {0, 0xffff, 0xffff}
nv_write min_chksum {1, 0xffff, 0xffff}

nv_write pref_voice_so {0,  1, 0x0003, 0x0003, 0x0003} ; True, wildcard, EVRC, EVRC ->EVRC, EVRC, EVRC
nv_write pref_voice_so {1,  1, 0x0003, 0x0003, 0x0003} ; True, wildcard, EVRC, EVRC ->EVRC, EVRC, EVRC

nv_write voice_priv {0}               ; 0=Standard  1=Enhanced  (1->0->1, by bhjo 02.08.28/09.06)->0

nv_write pref_for_rc {3}              ; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)  

;err_clr 0xff                         ; never forget clr err log
;=========================================================================


;=========================================================================
;Stand-Alone modified by Lhu Bong Suk : v108990@lge.com
;=========================================================================
nv_write stand_alone_mode {0}         ; 0 default OFF, 1 ON

;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key {0, 0x00000000, 0x00000000 }
nv_write a_key {1, 0x00000000, 0x00000000 }
nv_write ssd_a {0, 0x00000000, 0x00000000 }
nv_write ssd_a {1, 0x00000000, 0x00000000 }
nv_write ssd_b {0, 0x00000000, 0x00000000 }
nv_write ssd_b {1, 0x00000000, 0x00000000 }
nv_write count {0, 0}
nv_write count {1, 0}

;=========================================================================
; OTA ITEM
;=========================================================================
nv_write otapa_enabled {0, 1}   ; enable
nv_write otapa_enabled {1, 1}   ; enable
nv_write nam_lock {0, 1}
nv_write nam_lock {1, 1}
nv_write spc_change_enabled {1}
nv_write imsi_t_mcc {0, "404"}               
nv_write imsi_t_mcc {1, "404"}
nv_write imsi_t_11_12 {0, "00"}
nv_write imsi_t_11_12 {1, "00"}
nv_write imsi_t_s1 {0, "000-0000", "000-0000"}
nv_write imsi_t_s1 {1, "000-0000", "000-0000"}
nv_write imsi_t_s2 {0, "000", "000"}
nv_write imsi_t_s2 {1, "000", "000"}
;=========================================================================

;=========================================================================
; MSG ITEM
;=========================================================================
nv_write msg_settings_auto_save     {2}     ; MSG_AUTO_SAVE(0), MSG_PROMPT(1), MSG_DO_NOT_SAVE(2)
nv_write msg_settings_auto_delete   {0}     ; 0(Off), 1(On)
nv_write msg_settings_entry_mode    {0}     ; MSG_T9EN(0), MSG_ABC(1), MSG_123(2)
;nv_write msg_settings_vibrate_alert {0}     ; 0(Off), 1(On)
;=========================================================================

;=========================================================================
; SMS/EMS ITEM
;=========================================================================
;2006.06.15 AriesGon - N/A
;nv_write sms_deferred_sel       {0}         ; 0(Immediate), 5(30M), 11(1H), 47(2H), 143(12H), 167(1D), 168(2D)
;nv_write sms_validity_sel       {0}         ; 0(Default), 5(30M), 11(1H), 47(2H), 143(12H), 167(1D), 168(2D)

nv_write sms_priority_sel       {0}         ; 0(Normal), 1(Urgent)
nv_write sms_delivery_sel       {0}         ;!!WARNING!! (off:0, on:1, enhanced:2) 
nv_write sms_mo_max_userdata    {160}       ; 0x0(=180) - 0xFFFF ; 180 -> 170 (by eklee 02.08.22)
nv_write sms_orig_msg_id        {1}         ; 0x00 - 0xFFFF   ; 0 -> 1 (by eklee 02.08.22)
nv_write sms_settings_callback_number   {0} ;!!WARNING!! (0:Off, 1:On)
;nv_write sms_auto_delete_menu  {0}         ; 0(Off), 1(On)
;nv_write sms_auto_save_sel     {0}         ; SMS_AUTO_SAVE(0), SMS_PROMPT(1), SMS_DO_NOT_SAVE(2) 
;nv_write sms_mo_edit_mode      {1}         ; SMS_T9EN(0), SMS_ABC(1), SMS_123(2) (0->1 ; 02.10.17, SMS_SYMBOLS(3) Delete)
nv_write sms_mo_l3_ack          {1}         ; 0(Off), 1(On)
nv_write sms_mo_so              {1}         ; 0(8K), 1(13K) -> 1(8K), 0(13K) 
nv_write smsVoiceRecord         {0}         ;(02.09.02)
nv_write sms_settings_signature         {0} ; SMS_SIGNATURE_OFF(0), SMS_SIGNATURE_ON(1), SMS_BUSINESS_CARD(2)
nv_write sms_settings_direct_view       {0} ; 0(Off), 1(On)
nv_write sms_settings_read_ack          {0} ; 0(Off), 1(On)
nv_write sms_cb_num             {4, "*600"}  ; sms_call_back (02.09.18 / {"*86"} -> {4, "*600"} )
nv_write sms_cbs_enable         {0}         ; 0(Off), 1(On) / Hidden menu BroadCast On/Off (02.08.26)
nv_write sms_settings_voicemail_alert   {10}; 0(Low Beep Once), 1(Low Beeps), ; KHW 2004.06.23 MODIFY in NJ (Ringtone6)
nv_write sms_settings_textmsg_alert     {1} ; 2(Laud Beep Once), 3(Loud Beeps),
nv_write sms_settings_email_alert       {1} ; 4(VZW Default Tone), 5~14(Ringtone 1~10),
nv_write sms_settings_page_alert        {1} ; 15(No Ring), 0xffff(Get New), On/Off (Alert Vibrate)
nv_write sms_settings_info_alert        {1} ; SMS_INFO_ALERT_SILENT(0), SMS_INFO_ALERT_ICON_ONLY(1), SMS_INFO_ALERT_VIBRATE_ICON(2)

;2006.06.08 AriesGon - ems N/A
;nv_write sms_ems_seg_waiting    {1}         ; 1 minute
;nv_write sms_ems_seg_num        {10}        ; 1~20 
;nv_write sms_ems_obj_enable     {off}       ; 
;nv_write sms_ems_enable         {on}        ; 0(Off), 1(On)    

nv_write sms_settings_auto_play {off}       ;
nv_write smsUrgentVoiceRecord   {false}     ; (02.10.17)

; modified by Koo Jahyoung
nv_write sms_2min_alert_sel          {3,3,3,3}   ; {txt, voice, e-mail, page} 0:Once, 1:Every 2 Min, 2:Every 15 Min, 3: OFF
nv_write msg_settings_vibrate_alert  {0,0,0,0}   ; {txt, voice, e-mail, page} 0:OFF, 1:ON

; 2005.08.02 jhkoo - sms auto readout option inserted
nv_write sms_tts_readout          {0}   ; 0:MANUAL, 1:AUTO

;=========================================================================

;=========================================================================
; MMS ITEM modified by Kim Jong Suk  // 2005-04-15
;=========================================================================
nv_write mms_settings_auto_download             {1}             ; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_settings_photo_alert         	{1}         	; 0(Low Beep Once),1(Low Beeps), 2(Laud Beep Once), 3(Loud Beeps), 4~13(Ring1~Ring10)
nv_write mms_mmsc_server_name_ip {33, "http://mms.wdsap.ricinfo.com:6081"}   ; 48 byte characters;nullnet Change
nv_write mms_number_of_retried_to_send_retrieve {3}         	; 0, 1, 2, 3
nv_write mms_uaprof_url_in_user_agent {46, "http://mms.wdsap.ricinfo.com/uaprof/rd9800.xml"} ; 48 byte characters;nullnet. now 6230! soon change to 9800
nv_write mms_settings_delivery_ack        	{0}		; 0(MMS_ON),1(MMS_OFF)
nv_write mms_from_add 				{0}             ; MDN Only (0), 1MDN (1),  +1MDN (2);nullnet mdn but used min
nv_write mms_settings_pix_vibrate_alert 	{0}             ; 0(MSG_OFF), 1(MSG_ON)
nv_write mms_settings_pix_2min_alert_sel 	{3}             ; Once (0), 2Min (1), 15Min (2), Off(3)
nv_write mms_mmsc_server_post_url {4, "/mms"}         ; Post URL;nullnet 
;nv_write mms_mmsc_server_post_cgi {12, "?message-id="}          ; CGI URL;;nullnet not used
;nv_write mms_upload_addr {13, "pix.vtext.com" }        		; Upload Address;;nullnet not used
;nv_write mms_settings_authorization 		{0}             ; Comercial(0), Lab (1), Domestic(2);nullnet not used

;=========================================================================

;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_qnc_enabled       {0}           ; 0-QNC Disable  1-QNC Enable
nv_write data_so_set            {2}           ; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write data_mdr_mode          {3}           ; DS_MDR_MODE_MDR_ONLY = 0  Use only MDR packet data services
nv_write data_pkt_orig_str {5, "#777"}        ; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_auto_packet_detection {0}       ; 0-Disable   1-Enable
;nv_write ppp_carrier           {0}            ; 0-Verizon 1-USC;nullnet 2006.05.15 no more used
;nv_write ppp_user_id {20,"0000000000@vzw3g.com"}; Max of 127 chars in User ID;nullnet 2006.05.15 no more used
;remove the ppp password setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;nv_write ppp_password          {3,"vzw"}      ; Max of 127 chars in Password
nv_write pref_for_rc           {3}            ; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)    
nv_write data_scrm_enabled     {1}            ; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled     {1}            ; 0-TRTL Disable 1-TRTL Enable
nv_write ds_default_baudrate   {0x0011}       ; 0x0000 (19.2kbps),0x0011(115kbps) ,0x00012(230.4kbps)
nv_write diag_default_baudrate {0x0011}       ; 0x000e(38.4kbps), 0x0011(115kbps)
;Comment : VX9800 use EFS FILE instead of NV ITEM for packet amount
;nv_write used_packet_amount    {0,0,0,0,0,0}  ; {TX used, TX remain, RX used, RX remain, used, remain}

;nv_write ds_qcmip {1}                         ; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only ;nullnet 2006.05.15 no more used
;nv_write ds_mip_active_prof  {0}              ; current active profile index;nullnet 2006.05.15 no more used
;nv_write ds_mip_enable_prof  {1,0,0,0,0,0}    ; diable - 0, enable - 1;nullnet 2006.05.15 no more used
;nv_write ds_mip_retries      {2}              ; number of retries;nullnet 2006.05.15 no more used
;nv_write ds_mip_retry_int    {3}              ; retry interval = n*250(ms) + 1000ms;nullnet 2006.05.15 no more used
;nv_write ds_mip_pre_re_rrq_time {0}           ; pre-registration time - minute;nullnet 2006.05.15 no more used
;nv_write ds_mip_num_prof     {1}              ; number of profiles (max 6) ;nullnet 2006.05.15 no more used
;nv_write ds_mip_2002bis_mn_ha_auth  {1}       ; disable - 0, enable -1;nullnet 2006.05.15 no more used
;nv_write ds_mip_rrq_if_tfrk  {0}              ; send a registration only in use : disable-0, enable-1;nullnet 2006.05.15 no more used
;nv_write ds_mip_qc_drs_opt   {1}              ; dormant handoff optimization;nullnet 2006.05.15 no more used
;Comment : MIP general profile information {index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
;Comment : reverse tunneling, home address, primary ha address, secondary ha address}
;nv_write ds_mip_gen_user_prof {0,20,"0000000000@vzw3g.com",1,300,1,2,1,0x00000000,0xffffffff,0xffffffff};nullnet 2006.05.15 no more used
;Comment : MIP shared secret {index,mn-ha ss length,mn-ha ss,mn-aaa ss length,mn-aaa ss,
;remove the ds_mip_ss_user_prof setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;nv_write ds_mip_ss_user_prof {0,16,"testtesttesttes$",3,"vzw"}
;nv_write ds_mip_dmu_pkoid    {0,10}                 ; public key organization indentifier;nullnet 2006.05.15 no more used
;nv_write ds_mip_dmu_mn_auth  {0,0x01,0xB2,0x07}            ; { Index , DMU MN authenticator - 111111base10 };nullnet 2006.05.15 no more used
;nv_write hdr_an_auth_user_id_long {20,"0000000000@vzw3g.com"} ; EVDO AN authetication user id;nullnet 2006.05.15 no more used
;Comment : remove the hdr_an_auth_passwd_long setting in script file. (Becuase it uses ppp_password value that changed after DMU nego.)
;nv_write hdr_an_auth_passwd_long  {3,"vzw"}                  ; EVDO AN authetication password

nv_write dun_cable_mode      {1}              ;0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode         {1}              ;0=disable bt dun,1=enable bt dun

;efs write "DMU/10.key"				      ; MIP DMU(Dynamic Mipkeys Update) key file;nullnet 2006.05.15 no more used

;Comment : MIP&SIP NAI(Network Access Identifier) for DUN 
;nv_write ds_mip_rm_nai {0,24,"0000000000@dun.vzw3g.com"} ; {index,nai_length,nai};nullnet 2006.05.15 no more used            
;nv_write ds_sip_rm_nai {24,"0000000000@dun.vzw3g.com"}  ; {nai_length,nai};nullnet 2006.05.15 no more used

;CS DLL don't write this item
;remove the ppp password setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,
;    0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
;nv_write ppp_password          {16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}      ;nullnet 2006.05.15 no more used

;CS DLL don't write this item 
;{0~5(index),16(mn_ha_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,
;0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,16(mn_aaa_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
;remove the ds_mip_ss_user_prof setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;nv_write ds_mip_ss_user_prof {0,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00};nullnet 2006.05.15 no more used

;CS DLL don't write this item 
;Comment : remove the hdr_an_auth_passwd_long setting in script file. (Becuase it uses ppp_password value that changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
;nv_write hdr_an_auth_passwd_long  {16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}   ;nullnet 2006.05.15 no more used

;=========================================================================

; dwjang 2003.12.09 by 장현석
; 2004.11.29 thunder - VX8200 은 OWS 디렉토리 없음, 임시 막음
;=========================================================================
; UP ITEM : for magellan 
;=========================================================================
efs write "OWS/aptable1.fil"
efs write "OWS/keytable1.fil"
efs write "OWS/paramtable1.fil"
efs write "OWS/wdptable1.fil"
;=========================================================================

;=========================================================================
; PIM ITEM
;=========================================================================
;efs write "pim/call_hist_nv.dat"         ;delete
;=========================================================================

;=========================================================================
;UI ITEM
;=========================================================================
nv_write lock_code      {"0000"}        ; Lock_code
nv_write sec_code       {"000000"}      ; Security code
nv_write fsc            {"000000"}      ; Field Service code
nv_write name_nam       {0, "Reliance"}     ; NAM 1 Name    NAM1 -> Reliance
nv_write name_nam       {1, "Reliance"}     ; NAM 2 Name    NAM2 -> Reliance
nv_write banner         {"Reliance"}            ; Banner - default blank, because confuse Banner with ERI text
nv_write sub_banner     {"Reliance"}            ; Sub Banner - default blank, because confuse Sub Banner with ERI text
nv_write ringer_lvl     {0x4}           ; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 1(Vibrate only=manner_mode), 97(alarm only), 1(Sounds Off=silence_all)
nv_write beep_lvl       {0x4}           ; 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write ear_lvl        {0x4}           ; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write speaker_lvl    {0x4}           ; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write ringer_spkr_lvl {0x4}          ; 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 98(High & Vib), 99(Vibrate)
nv_write beep_spkr_lvl  {0x4}           ; 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write beep_lvl_shadow {0x4}          ; 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write ear_lvl_shadow {0x4}           ; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write spk_phone_beep_lvl {0x4}       ; 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) - Keypad Volume on Speaker Phone Mode
nv_write speaker_shadow	    {0x4}       ; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) - Earpiece Volume on Speaker Phone Mode
nv_write auto_volume_enabled {0}        ; 0-> off , 1-> on
;nv_write call_rstrc     {0x00}          ; Restrict(0:off, 1:on) ;knjung delete
nv_write auto_lock      {off}           ; phone lock            == Unlocked \ Power_up
nv_write lock           {off}           ; phone lock            == Unlocked \ now
nv_write auto_nam       {off}           ; Auto NAM              == disable
nv_write curr_nam       {0}             ; Current NAM           == NAM1
nv_write auto_redial    {0, 0}          ; Auto redial           == off
nv_write auto_answer    {0, 0}          ; Auto answer           == off
nv_write onetouch_dial  {on}            ; One touch dial        == enable!
nv_write cont_key_dtmf  {1}             ; Prssed key tone       == 1: Normal, 0: Long  2: Off  (NEW)
nv_write back_light     {7}             ; Backlight             == after 7secs (10 -> 7, by bhjo 02.08.28)
nv_write sub_backlight  {7}             ; Sub Backlight         == after 7secs (10 -> 7, by bhjo 02.08.28)
nv_write backtop_beep   {true}          ; Back To Top Sound == on       
nv_write call_connect_alert {TRUE}     ; Call connect alert    == off kwkang 060705 pri false -> true
nv_write send_pin       {off}           ; Send pin?             == disable!
nv_write language_selection {0}         ; Default (English/Spanish/French/Portuguese) == English
nv_write carrier_logo   {0}             ; 0 -> Verizon, 
nv_write logo_melody    {1}             ; 1 -> On, 0 -> Off
nv_write ringer_id_onoff {1}            ; 1 -> On, 0 -> Off   new item 2003.11.30
nv_write picture_id_onoff {1}           ; 1 -> On, 0 -> Off   new item 2003.11.30
nv_write sound_ringers  {4,4,4,4,0}; (caller ID, No Caller ID, Restrict, all calls, vibrate options) added item 4th & 5th 2003.11.30 ;KHW 2004.06.16 MODIFY in NJ kwkang 060705 pri {4,9,6,0xFFFF,0}->{4,4,4,4,0}
nv_write silence_all    {0}             ; sound on   {1} sound off
nv_write sound_alerts   {0,0,0,0}       ; (Service Change, Minute Beep, don't care, ERI alert) added item 4th 2003.11.30
nv_write key_light      {7}
nv_write edit_font      {0,0}
nv_write display_set    {0,0,0}         ; sub_clock, main_clock, color theme
;sjbae : wallpaper change
;nv_write display_screen {1,1,0}         ; main_wallpaper(main), sub_wallpaper, power_onoff(on/off) by baeg changhyun
nv_write display_screen {0}             ; power_onoff animation
nv_write wallpaper_main {0,0,1,""}       ; wallpaper {location_type(0:phone memory 1:phone efs 2:sdcard), location_id(0:sdcard id), item_id(1: index), item_path(NULL: path)}
nv_write wallpaper_sub  {0,0,1,""}       ; wallpaper {location_type(0:phone memory 1:phone efs 2:sdcard), location_id(0:sdcard id), item_id(1: index), item_path(NULL: path)}
nv_write media_save_option {0,0,0,0}     ; media_save_option{pix_save_location(0 : phone memory 1: sdcard) ,flix_save_location(0 : phone memory 1: sdcard) ,sound_save_location(0 : phone memory 1: sdcard) }

nv_write location_set   {0}             ; 1 -> location on 0-> E911 only
nv_write messaging_set  {1,1}
nv_write sms_sound      {1,0,0}
nv_write manner_mode    {0}             ; false {0}, true {1}
nv_write number_size    {1,0}           ; (size, color(don't use)) 0:normal 1:large
nv_write emergency_num1 {"100"}         ; Up to 48 Digits;nullnet change EMER.2006.05.25
nv_write emergency_num2 {"101"}         ; Up to 48 Digits;nullnet change EMER.2006.05.25
nv_write emergency_num3 {"102"}        ; Up to 48 Digits;nullnet change EMER.2006.05.25
; nv_write backtop_beep   {1}
nv_write phone_setup     {0,0,26,27,28,29,0,0,0,0,0,0,0,0,0}   ; (pim_id, form_id, shortcut_form_index[10], call_answer, isModal, modalType)
                                        ; pim_id, form_id : 0 -> Schedule, call_answer : 0 -> Flip open
;nv_write wclock_choice  {46,0}          ; default NewYork (45->46, Add Tel Avive)
;nv_write stack_idx      {0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff} ; call history clear
nv_write power_saver    {0}
nv_write status_led     {0,0,0,0,0,0,0} ; incoming_call, missed_call, new_sms_alert, reminders, in_service_area, roaming, battery_low
nv_write tty            {3}             ; TTY Full(0), TTY+TALK(1),TTY+HEAR(2),TTY off(3)
nv_write alarm_only_mode {0}            ; 0 -> Disable, 1 -> Enable
nv_write photo_setting_RQS   {1,1,0}    ; photo_set_Resolution(1 : 640*480), photo_set_Quality(1 : Normal), photo_set_ShutterSound(0 : Shutter1)
nv_write video_setting_RQ    {0,1}      ; video_set_Resolution(0), video_set_Quality(1)
;nv_write elapsed_time_video  {15}       ; elapsed time(15), elapsed time(20), elapsed time(25)
;nv_write elapsed_time_video  {3600}       ; elapsed time(15), elapsed time(20), elapsed time(25), elapsed time(3600)
nv_write dcam_video_brand    {3}        ; dcam_video_brand(3) -> VIDEO_FMT_BRAND_3G2
nv_write dcam_stream_video   {0}        ; dcam_stream_video(0) -> VIDEO_FMT_STREAM_VIDEO_MPEG4
nv_write dcam_stream_audio   {1}        ; dcam_stream_audio(1) -> VIDEO_FMT_STREAM_AUDIO_QCELP13K_FULL
nv_write dcam_short_header   {0}        ; dcam_short_header(0) -> FALSE
nv_write eri_text_onoff      {0}        ; 1 -> On, 0 -> Off ;1 ->0   JHJ 2006.05.10 
nv_write gps_test_num        {"922"}    ; Up to 48 Digits
nv_write emer_test_num       {"911"}    ; Up to 48 Digits

;use for Camera flash testing in Factory
;nv_write contrast_lvl   {81, 0x12}      ; (Flash on/off, don't care) Camera Flash On -> 85(0x55), Off -> others
nv_write camera_flash_test {0x01}       ; (Flash on/off) Camera Flash On -> 85(0x55), Off -> others

; added by lej
nv_write avt_best_match {1}             ; 0 -> 1 Match, 1 -> 4 Match for AVT
nv_write avt_start_command {1}          ; 0 -> Flip open, 1 -> Side key only for AVT
nv_write avt_announce_alerts {0}        ; 0 -> Disable, 1 -> Announce, 2-> Announce + Ring
nv_write AVT_speed_mode {0}             ; 0 -> Normal, 1 -> Speed
nv_write AVT_mode_key {0}               ; 0 -> Send key, 1 -> Voice Service

; added by Kim Hyunwoo for Bluetooth
;nv_write bd_addr	{0x9a,0xbc,0x56,0x78,0x12,0x34}	; Bluetooth Address
nv_write bt_power_onoff	{0}		; 1 -> On, 0 -> Off
nv_write beep_bt_lvl	{0x4}		; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
nv_write ear_bt_lvl	{0x4}		; 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
; added by Kim heesoo for BZ card reader 
efs write "dload/bzcard/CamOCR_eng.bin" 
; added by sjbae
nv_write pc_port        {0}             ; PC connection port  0 (USB), 1 (UART), 2 (BLUETOOTH), 3 (CLOSED)
; added by sjbae
nv_write key_guard_set {30}             ; key_guard   0(Always off)  7( 7 Seconeds)  30( 30 Seconeds)  120( 2 Min)

; added by sjbae
nv_write nvitem_equalizer_mode    {1}      ; 0(flat) , 1(3D Surround) ,2 (Concert Hall) , 3 (Rock) , 4 (Jazz)  , 5 (POP) , 6 (Classical) 
nv_write visualizer_mode      {0}               ;  0 enable   ,  1 disable
nv_write  use_mymp3     {2}                    ;  0 : MUSIC_NONE,   1 : MUSIC_MP3_ONLY,   2 : MUSIC_MOD_ONLY,     3 : MUSIC_MP3_MOD


;=========================================================================

;=========================================================================
;F/W ITEM
;=========================================================================
;nv_write ftm_mode {1}                   ; ystk 2003.10.06 - for Initial Booting Mode to DMSS mode!
;nv_write fm_rssi {0x2c, 0x7f}           ; modify {0x4a, 0x77} -> {0x2c, 0x7f};hkshin 200.10.28 - for hw request
nv_write rf_config {6}
;nv_write lcd {39}                       ; don't use for VX8100
;hkshin 200.10.28 - for hw request
nv_write vbatt {166, 244}                ; VX9800

;nv_write cdma_rx_comp_vs_freq { -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12 }
;nv_write pcs_rx_comp_vs_freq  { -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10 }
nv_write elapsed_time {59}

; modified by Heo Si Hang
nv_write qdsp_snd_ctrl {0, 0, 0, 0, 0, -500, 150, 25, 30, 6, 6, 0,1300,20,6, 0}
nv_write audio_adj_phone {0, 0, 0, -300, 0, 0, 0, 0, 0}
nv_write audio_adj_earjack {4096, 0, 0, 0, 0, 0, 0, 0, 0}
nv_write audio_adj_hfk {200, 10638, 0, -1024, 10638, 0, 0, 0, 0}
nv_write audio_adj_spk {4096, 0, 0, 4096, 0, 0, 0, 0, 0}
nv_write audio_adj_bt {0, 0, 0, 0, 0, 0, 0, 0, 0}

;=========================================================================

;=========================================================================
;BREW ITEM modified by Kim sungkung
;fuxing.2006.04.21 - for Reliance
;=========================================================================
nv_write brew_bkey {0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 
nv_write brew_download_flags {0x0004}    ;MIN_FOR_SID+PREPAID
nv_write brew_auth_policy {1}                             ; 
nv_write brew_privacy_policy {3}                            ;
nv_write brew_carrier_id {75}                          ; 
nv_write brew_server    {"adsprepay.wdsap.ricinfo.com"}      ; 64 byte character
nv_write brew_platform_id {1156}			;

;=========================================================================


;sjbae 2005.02.28 ITEM 추가 
;=========================================================================
;WALLPAPER DEFAULT IMAGE ITEM
;=========================================================================
;efs write "dload/default_img/wallpaper_02.bmp"
efs write "dload/default_img/wallpaper_03.bmp"
efs write "dload/default_img/wallpaper_04.bmp"
;efs write "dload/default_img/ext_wallpaper_2.bmp"
efs write "dload/default_img/ext_wallpaper_3.bmp"
efs write "dload/default_img/ext_wallpaper_4.bmp"
;sjbae 2005.06.07 ITEM 추가
;efs write "dload/default_img/wallpaper_05.bmp"
;efs write "dload/default_img/ext_wallpaper_5.bmp"

;JHJ bloking to ERI Sounds 2006.05.10
;lkg 031002 added eri sound.
;=========================================================================
;ERI SOUND ITEM
;=========================================================================
;efs write "eri_sound/extendednetwork.qcp"
;efs write "eri_sound/lossofservice.qcp"
;efs write "eri_sound/roaming.qcp"
;efs write "eri_sound/verizonwireless.qcp"

;HKSHIN 2003.12.19
;=========================================================================
;MMS IMAGE ITEM
;=========================================================================
;efs write "brew/16452/mp/Bear_heart.bmp"
;efs write "brew/16452/mp/Elvis_birthday_sm.jpg"
;efs write "brew/16452/mp/Hi_pig_sm.jpg"
;efs write "brew/16452/mp/Love_you_cat_sm.jpg"
;efs write "brew/16452/mp/Martini.bmp"
;efs write "brew/16452/mp/Party_time_sm.jpg"
;efs write "brew/16452/mp/Roses.bmp"
;efs write "brew/16452/mp/Sorry_monster_sm.jpg"
;efs write "brew/16452/mp/Sun.bmp"
;efs write "brew/16452/mp/Surfing.bmp"

;HKSHIN 2003.12.19
;=========================================================================
;MMS SOUND ITEM
;=========================================================================
;efs write "brew/16452/ms/Beethovens_fifth.mid"
;efs write "brew/16452/ms/Dreamsequence.mid"
;efs write "brew/16452/ms/Ode_to_joy.mid"
;efs write "brew/16452/ms/Rainforest.mid"
;efs write "brew/16452/ms/Train.mid"

;Kim HyunWoo 2005.02.12
;=========================================================================
;ANIMATION IMAGE ITEM
;=========================================================================
;efs write "dload/opening_01.jpg"
;efs write "dload/opening_02.jpg"
;efs write "dload/opening2_01.jpg"
;efs write "dload/opening2_02.jpg"
;efs write "dload/closing_01.jpg"
;efs write "dload/closing_02.jpg"
;efs write "dload/closing2_01.jpg"
;efs write "dload/closing2_02.jpg"






;LYSLION 2004.04.19
;=========================================================================
;VOICE ITEM
;=========================================================================
efs write "VoiceDB/All/Memos/uivrState.dat"

;lej 2005.04.20 Voice Command Data
;efs write "mVoice/ment/ment_adpcm.db"
;efs write "mVoice/ment/ment_adpcm_spn.db"
;efs write "mVoice/ment/ment_voc.db"
;efs write "mVoice/ment/ment_voc_spn.db"

;efs write "mVoice/name/eng-cid.dat"
;efs write "mVoice/name/eng-cid.idx"
;efs write "mVoice/name/spn-cid.dat"
;efs write "mVoice/name/spn-cid.idx"
;efs write "mVoice/name/etts_name.dat" ;CMX 적용시 삭제.
;efs write "mVoice/name/etts_name.idx" ;CMX 적용시 삭제.

;efs write "mVoice/recog/en_digit_recog_mfcc.bin"
;efs write "mVoice/recog/en_lex_data.bin"
;efs write "mVoice/recog/en_name_recog.bin"
;efs write "mVoice/recog/sp_digit_recog_mfcc.bin"
;efs write "mVoice/recog/sp_lex_data.bin"
;efs write "mVoice/recog/sp_name_recog.bin"
;=========================================================================
; DCAMERA ITEM
;=========================================================================
efs write "dload/dcammenu.dat"
efs write "dload/default_img/DecodeErrorAnimation.jpg"
efs write "dload/default_img/DecodeErrorImage.jpg"
efs write "dload/default_img/NotSupportedImage_UnknownImage.jpg"
efs write "dload/default_img/phoneOnConversation.jpg"
efs write "dload/default_img/TooBigErrorImage.jpg"

efs write "dload/default_img/video_FirstFrame_PMD.bmp"

efs write "dload/default_img/sub_DecodeErrorAnimation.jpg"
efs write "dload/default_img/sub_DecodeErrorImage.jpg"
efs write "dload/default_img/sub_NotSupportedImage_UnknownImage.jpg"
efs write "dload/default_img/sub_phoneOnConversation.jpg"
efs write "dload/default_img/sub_TooBigErrorImage.jpg"



;=========================================================================

;=========================================================================
; SHUTTER SOUND 
;=========================================================================
efs write "dload/shutter1.wav"
efs write "dload/shutter2.wav"
;=========================================================================

;=========================================================================
; MIDI TEST SOUND // for test mode 6.4 // capbong 2006.06.19
;=========================================================================
;efs write "dload/630Hz_0db_LR.mid"
;efs write "dload/1KHz_0db_LR.mid"
;efs write "dload/16KHz_0dB_LR.mid"

;=========================================================================
; VIDEO SOUND 
;=========================================================================
efs write "dload/videostart.wav"
efs write "dload/videoend.wav"

;=========================================================================
; 2005.06.02 thunder - TTS 
;=========================================================================
; TTS ITEM
;=========================================================================
;efs write "mTalk/sms-etts.cnt"
;efs write "mTalk/sms-etts.dat"
;efs write "mTalk/sms-etts.etc"
;efs write "mTalk/sms-etts.hdx"
;efs write "mTalk/sms-etts.idx"
;efs write "mTalk/sms-etts.key"
;=========================================================================


;=========================================================================
;GPSONE ITEM added in 2005-03-04
;=========================================================================
nv_write gps1_lock {3}

nv_write gps1_pde_address {0,0,0,0}
nv_write gps1_pde_port {0}
;=========================================================================


mode reset
