;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;=========================================================================
;  File name: T85VZG07.SCR
;  Made by  : LGE
;  Version  : G07_01
;  Date     : 11/06/2007
;-------------------------------------------------------------------------
;  when         who        what
;----------    -------    ------------------------------------------------
;11/06/2007    ChoiYS      Rename
;01/30/2007    ChoiYS      Change version name to 06_01
;10/17/2006    ChoiYS      Changed VOD/MOD/MIM Applications. 
;              ChoiYS      Changed brew\mod\brewappmgr\en\appmgrls.bar, brew\mod\brewappmgr\es\appmgrls.bar
;                                  Green Color Variation, Color of lower bar is changed.
;                          Changed version.txt 
;08/17/2006    ChoiYS      Insert NV Item touchkey_activate_option {1}
;                          back_light is from 5 sec to 15 sec
;07/27/2006    ChoiYS      Version Renamed. Delete BIN Version and Date in BREW version.txt
;07/13/2006    ChoiYS      Version Renamed
;06/10/2006    ChoiYS      Modified version.txt. modified appmgrls.bar
;06/10/2006    ChoiYS      Modified version.txt. remove prefs.dat size calculation. 
;06/08/2006    ChoiYS      Modified version.txt
;05/31/2006    ChoiYS      Brew Pre-Loaded VOD 03.03.006
;05/24/2006    ChoiYS      Delete Flash Write command and Flash contents. Merged into source code.
;05/18/2006    ChoiYS      BREW Pre-loaded MOD 01.02.002  MIM Ver. 1.3.1.19
;05/17/2006    ChoiYS      Changed Version.txt, 16452/mp/*.jpg, mms_mmsc_upload_url
;05/17/2006    ChoiYS      Change Flash Content, Added NV Item touch_sensitivity, location_set_lock, end_call_option 
;05/06/2006    ChoiYS      Change nv_write sms_message_cb {0, 0}  -> {10, 0}
;04/28/2006    ChoiYS      Inserted nv_write status_softkey_color
;04/20/2006    ChoiYS      Changed wclock_choice
;04/16/2006    ChoiYS      Changed nv_write qdsp_snd_ctrl {0,0,0,0,0,0,0,0,0,7,6,0,0,0,0,-800}
;                          Updated Flash Contents
;03/31/2006    ChoiYS      Changed BREW folder
;03/25/2006    ChoiYS      Changed nv_write mms_set_retry_num {0} -> {3}
;03/24/2006    ChoiYS      Delete efs write "mVoice/ment/ment_voc.db"
;                          Changed Flash UI
;                          Changed Volume Level
;03/16/2006    ChoiYS      Changed vbatt MIN, MAX
;03/14/2006    ChoiYS 	   Changed nv_write flash_music_theme   {0}     ; OFF (0), ON (1) 
;                          Delete mms_send_retry_num
;                          Insert nv_write mms_set_retry_num {0}   ; 0, 1, 2, 3
;                          Insert nv_write mms_mmsc_user_agent {8,"VX8500v1"}
;03/07/2006    ChoiYS      Changed brew\mod\brewappmgr
;                          Changed EFS/Flash/UI, Flash UI Items
;02/27/2006    ChoiYS      Changed brew/sys/es, en
;                          Changed EFS/Flash/UI, Flash UI Items
;02/20/2006    ChoiYS      Changed MMS Items
;02/17/2006    ChoiYS      Changed EFS/Flash/UI, Flash UI Item
;02/13/2006    ChoiYS      Changed dcam_video_set_rq recommended by BY Lee
;                          Changed closing1.bit2, opening1.bit2 recommended by HW Kim
;                          Changed qdsp_snd_ctrl, audio_adj_phone, audio_adj_earjack
;                                  audio_adj_hfk, audio_adj_spk, audio_adj_bt by Bryan
;                          Changed OWS/2 files by LEEJH
;02/08/2006    ChoiYS      Initial Release
;----------    -------    ------------------------------------------------

;spc "000000"                         ; does not need at LGDP DLL
;wait 2
mode offline-d
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model
wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================

nv_write sec_code       {"000000"}      ; Security code
nv_write lock_code      {"0000"}        ; Lock_code

nv_write name_nam       {0, "NAM1"}     ; NAM 1 Name
nv_write name_nam       {1, "NAM2"}     ; NAM 2 Name

nv_write imsi_mcc       {0, "310"}                   ; Mobile Country Code (310)
nv_write imsi_mcc       {1, "310"}
nv_write imsi_11_12     {0, "00"}                    ; Mobile Network Code
nv_write imsi_11_12     {1, "00"}
nv_write min1           {0, "000-0000", "000-0000"}
nv_write min1           {1, "000-0000", "000-0000"}
nv_write min2           {0, "000", "000"}            ; NAM 0 has one active MIN2,
nv_write min2           {1, "000", "000"}           

nv_write imsi_t_mcc     {0, "310"}               
nv_write imsi_t_mcc     {1, "310"}
nv_write imsi_t_11_12   {0, "00"}
nv_write imsi_t_11_12   {1, "00"}
nv_write imsi_t_s1      {0, "000-0000", "000-0000"}
nv_write imsi_t_s1      {1, "000-0000", "000-0000"}
nv_write imsi_t_s2      {0, "000", "000"}
nv_write imsi_t_s2      {1, "000", "000"}
                                                 ; NV_DIR_NUMBER_PCS_I      /*123456789012345*/ using 10 digits
nv_write dir_number_pcs {0, "0000000000"}        ; NAM 0 : NV_DIR_NUMBER_PCS_I
nv_write dir_number_pcs {1, "0000000000"}        ; NAM 1 : NV_DIR_NUMBER_PCS_I

                                                 ; Primary CDMA Channels for A carrier and B carrier
print "Programming Primary CDMA Channel"
nv_write pcdmach        {0, 283, 384}            ; A and B primary CDMA channels
nv_write pcdmach        {1, 283, 384}

                                                 ; Secondary CDMA Channel
print "Programming Secondary CDMA Channel"
nv_write scdmach        {0, 691, 777}            ; set only if secondary channels offered
nv_write scdmach        {1, 691, 777}

nv_write home_sid_nid {0,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535}
nv_write home_sid_nid {1,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535}
nv_write sid_nid_lock {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}

nv_write mob_term_home    {0, true, true}
nv_write mob_term_home    {1, true, true}
nv_write mob_term_for_sid {0, true, true}
nv_write mob_term_for_sid {1, true, true}
nv_write mob_term_for_nid {0, true, true}
nv_write mob_term_for_nid {1, true, true}

nv_write accolc {0, 0, 0}
nv_write accolc {1, 0, 0}

nv_write slot_cycle_index {2}

                                                  ;{Nam Name(0, 1), EVRC Capability(0:Off, 1:ON), Home_Page_Voice_SO(0: wildcard, Others : SO), Home_Page_Voice_SO(0 or SO), Home_Page_Voice_SO(0 or SO)}
nv_write pref_voice_so {0,  1, 0x0000, 0x0003, 0x0003} 
nv_write pref_voice_so {1,  1, 0x0000, 0x0003, 0x0003}

print "Programming Pref Mode"
nv_write pref_mode     {0, "Digital Only"}
nv_write pref_mode     {1, "Digital Only"}
nv_write hybrid_pref   {1}                        ; 1 : hybrid on,  0 : hybrid off

print "Programming Band Preferred"
nv_write band_pref {0, "pref_any"}
nv_write band_pref {1, "pref_any"}

print "Programming Roam Preferred"
nv_write roam_pref {0, "pref_any"}
nv_write roam_pref {1, "pref_any"}

nv_write system_pref {0, "automatic b"}          ; System preference, actually default to band preference
nv_write system_pref {1, "automatic b"}

nv_write stand_alone_mode {0}               ; 0 default OFF, 1 ON

;------------------------------------------------------------------------
print "Programming MRU table clear"
                                            ; except nam (first 0), '0' are 48(=4 X 12) times.
nv_write mru3_table {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru3_table {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};

                                             ; NAM Checksums must all be 0xffff
print "Programming NAM Checksums"
nv_write nam_chksum {0, 0xffff}
nv_write nam_chksum {1, 0xffff}
nv_write min_chksum {0, 0xffff, 0xffff}
nv_write min_chksum {1, 0xffff, 0xffff}

;=========================================================================
; OTA ITEM
;=========================================================================
nv_write nam_lock           {0, 1}
nv_write nam_lock           {1, 1}
nv_write otapa_enabled      {0, 1}   ; enable
nv_write otapa_enabled      {1, 1}   ; enable
nv_write spc_change_enabled {1}

;-------------------------------------------------------------------------
; nv_write imsi_t_addr_num    {0, 255}
; nv_write imsi_t_addr_num    {1, 255}

;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key {0, 0x00000000, 0x00000000 } ; Nam 1 64 bits A-Key. Published at factory with Random number.
nv_write a_key {1, 0x00000000, 0x00000000 } ; Nam 2 64 bits A-Key. Published at factory with Random number.

;-------------------------------------------------------------------------
nv_write ssd_a {0, 0x00000000, 0x00000000 }
nv_write ssd_a {1, 0x00000000, 0x00000000 }
nv_write ssd_b {0, 0x00000000, 0x00000000 }
nv_write ssd_b {1, 0x00000000, 0x00000000 }
nv_write count {0, 0}
nv_write count {1, 0}
;=========================================================================

;=========================================================================
;UI ITEM
;=========================================================================
nv_write curr_nam                 {0}                     ; Current NAM == NAM1
nv_write auto_nam                 {0}                     ; Auto NAM == disable
nv_write ear_lvl                  {6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write speaker_lvl              {6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write ringer_lvl               {4}                     ; 1~5 (Low, Med Low, Med, Med High, High), 1 (Vibrate only), 97 (Alarm Only), 1 (All Sounds Off)"
nv_write beep_lvl                 {4}                     ; 0 (Off), 1~5 (Low, Med Low, Med, Med High, High)
nv_write cont_key_dtmf            {1}                     ; Normal (1), Long (0),  Off (2)
nv_write banner                   {"VCAST"}
nv_write auto_answer              {0, 0}                  ; On (1, 1), Off (0, 0)
nv_write auto_redial              {0, 0}                  ; Off (0, 0), Every 10 Seconds (1, 1), Every 30 Seconds (1, 3), Every 60 Seconds (1, 6)
nv_write back_light               {15}                    ; Default 5 Sec
nv_write lock                     {0}                     ; Lock (1), Unlock (0)
nv_write auto_lock                {0}                     ; Power_up (1)
nv_write call_rstrc               {0}                     ; Off (0), On (1)
nv_write onetouch_dial            {1}                     ; Off (0), On (1)
nv_write beep_lvl_shadow          {4}                     ; 0 (Off), 1~5 (Low, Med Low, Med, Med High, High)
nv_write ear_lvl_shadow           {6}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write send_pin                 {0}                     ; Off (0)
nv_write voice_priv               {1}                     ; Standard (0), Enhanced (1)
nv_write fsc                      {"000000"}              ; Field Service code
nv_write ringer_spkr_lvl          {6}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8), 98 (High & Vib), 99 (Vibrate)
nv_write beep_spkr_lvl            {6}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write language_selection       {0}                     ; English (0), Spanish (1)
nv_write auto_volume_enabled      {0}                     ; Off (0), On (1)
nv_write tty                      {3}                     ; TTY Full (0), TTY+TALK (1),TTY+HEAR (2),TTY off (3)
nv_write gps1_lock                {3}                     ; Location ON (0), MI (1), MT (2), E911 Only (3)
nv_write manner_mode              {0}                     ; False (0), True (1)
nv_write alarm_only_mode          {0}                     ; False (0), True (1)
nv_write silence_all              {0}                     ; Sound On (0), Sound Off (others)
nv_write speaker_shadow_lvl       {6}                     ; Earpiece Volume on Speaker Phone Mode: 1~8 (Volume1 ~ Volume8)
nv_write spk_phone_beep_lvl       {6}                     ; Keypad Volume on Speaker Phone Mode: 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write call_sounds              {4,9,6,0xFFFF,0}        ; {Caller ID (4: VZW Default Tone), No Caller ID (9: Ringtone 5), Restrict Calls (6: Ringtone 2), All Calls (0xFFFF: Get New Ringtones), Vibrate (0: Off, 1: On)}"
nv_write sms_sound                {1,0,0}
nv_write service_alerts           {0,0,0,0}               ; {Service Change (Not use), Minute Beep, Call Connect, ERI}, On (1), Off (0)
nv_write power_onoff_sounds       {1,1}                   ; {Power On, Power Off}, On (1), Off (0)
nv_write alarm_sounds             {6,0}                   ; {tone(6: Ringtone 2), vibrate (0: Off)}
;nv_write backtop_beep            {1}                     ; On (1), Off (0)
;nv_write sub_banner              {""}
nv_write eri_text                 {1}                     ; On (1), Off (0)
;nv_write sub_backlight           {5}                     ; Default 5 Sec
nv_write key_light                {5}                     ; Default 5 Sec
nv_write wallpaper_main           {0,0,1}                 ; {location_type (0:phone memory, 1:phone efs, 2:sdcard), location_id (0:sdcard id), item_id (1: index)}
;nv_write wallpaper_sub           {0,0,1}                 ; {location_type (0:phone memory, 1:phone efs, 2:sdcard), location_id (0:sdcard id), item_id (1: index)}
nv_write display_themes           {1}                     ; Default (0), Rock & Roll-flash1 (1), Jazz - flash2 (2), Business(3), Tropical(4), Blue (5)
nv_write number_size              {1}                     ;  Normal (0), Large (1)
;nv_write power_onoff_anim        {0}                     ; Animation 3 (0)
nv_write clock_format             {0, 0}                  ; {main (0: Normal, 1: Digital, 2: Analog, 3: Dual, 4: Off), front (0: Digital, 1: Minimize, 2: Off)}
nv_write shortcut                 {0,0,0,0}               ; {Left, Up, Right, Down}
nv_write call_answer              {0}                     ; Flip Open (0), Any Key (1), Send Only (2), Auto Answer (3)
nv_write pc_port                  {0}                     ; PC connection port  0 (USB), 1 (UART), 2 (BLUETOOTH), 3 (CLOSED)
nv_write ringer_id                {1}                     ; On (1), Off (0)
nv_write picture_id               {1}                     ; On (1), Off (0)
nv_write emergency_num1           {"911"}                 ; Up to 48 Digits
nv_write emergency_num2           {"611"}                 ; Up to 48 Digits
nv_write emergency_num3           {"*611"}                ; Up to 48 Digits
nv_write wclock_choice            {30,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,47,0}             
				                          ; {cur_Itm (30), set_DST, choice_city ( NewYork: 47), line longtitude}
nv_write media_save_option        {0,0,0}                 ; {PIX, FLIX, SOUND} Phone memory (0), SD card (1)
nv_write dcam_video_elapsed_time  {15}                    ; elapsed time options (15, 20, 25)
nv_write dcam_photo_set_rqs       {1,2,0}                 ; {resolution(1: 640*480), quality(2: Fine), shutter sound(0: Shutter1)}
nv_write dcam_photo_menu_set      {0,0,0,9,0,1,0,0}       ; Initialize camera menu
nv_write dcam_video_set_rq        {0,1}                   ; {resolution (0), quality (1)}
nv_write dcam_video_menu_set      {0,0,0,9,0,0,0,0}       ; Initialize video menu
nv_write camera_flash_test        {81}                    ; Camera Flash On (85(0x55)), Off (others)
nv_write flix_set_as              {1,0,0,0,0,0,0,0,0,0}
nv_write equalizer_mode           {0}
nv_write visualizer_mode          {0}                     ; OFF (0), ON (1)
nv_write avr_call_alerts          {0}
nv_write avr_prompts_mode         {0}
nv_write avr_choice_list          {0}
nv_write avr_prompts_timeout      {0}
nv_write avr_sensitivity          {1}                     ; 0: High 1: Medium 2: Low
nv_write avr_prompts_sound        {0}                     ; 0: Speaker 1: Earpiece
nv_write bt_power_onoff           {0}                     ; OFF (0), ON (1)
nv_write beep_bt_lvl              {6}                     ; Off (0), 1~8 (Volume1 ~ Volume8)
nv_write ear_bt_lvl               {6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write use_my_mp3               {0}                     ; MOD Center Key Define: MOD Player (0), MP3 Player (1)
nv_write carrier_logo             {0}                     ; Verizon(0)
nv_write contrast_lvl             {0,0}
nv_write led_blink                {1}                     ; ON(1) OFF(0)
nv_write power_saver              {0}
nv_write edit_font                {0,0}
nv_write gps_test_num             {"922"}                 ; Up to 48 Digits
nv_write emer_test_num            {"911"}                 ; Up to 48 Digits
nv_write flash_music_theme	  {0}			  ; Music Theme 1 (0), Music Theme 2 (1)
nv_write charging_alert           {0}     		  ; OFF (0), ON (1)
nv_write status_softkey_color     {5}     		  ; (0~5) Color 1 ~ Color 6
nv_write touch_sensitivity     	  {0x41}     		  ; 0x41 : medium
nv_write location_set_lock     	  {0}     		  ; 0: unlock, 1:Lock
nv_write end_call_option     	  {0}     		  ; 0: slide down, 1:end key only
nv_write sidekey_guide     	  {1}     		  ; ON(1) OFF(0)
nv_write touchkey_activate_option {1}			  ; VoiceKey Once{0}, Press Once{1}, Press Twice{2}

;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_pkt_orig_str      {5, "#777"}    ; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_mdr_mode          {3}            ; Service Option 33 (1x channel) = 3 Use only low-speed packet data = 2
nv_write data_auto_packet_detection {0}        ; 0-Disable   1-Enable
nv_write data_so_set            {2}            ; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write diag_default_baudrate  {0x000e}       ; 0x000e(38.4kbps), 0x0011(115.2kbps) 
nv_write data_qnc_enabled       {0}            ; 0-QNC Disable  1-QNC Enable
nv_write ppp_user_id            {20,"0000000000@vzw3g.com"}; Max of 127 chars in User ID
nv_write data_scrm_enabled      {1}            ; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled      {1}            ; 0-TRTL Disable 1-TRTL Enable
nv_write pref_for_rc            {3}            ; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)    
nv_write ds_default_baudrate    {0x0011}       ; 0x0000 (19.2kbps),0x0011(115.2kbps) ,0x00012(230.4kbps)
nv_write ds_qcmip               {1}            ; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only
nv_write ds_mip_active_prof     {0}            ; current active profile index
nv_write ds_mip_enable_prof     {1,0,0,0,0,0}  ; diable - 0, enable - 1 {1st Profile, 2nd Profile, 3rd Profile, .... }
nv_write ds_mip_retries         {2}            ; number of retries
nv_write ds_mip_retry_int       {3}            ; retry interval = n*250(ms) + 1000ms
nv_write ds_mip_pre_re_rrq_time {0}            ; pre-registration time - minute
nv_write ds_mip_num_prof        {1}            ; number of profiles (max 6) 
nv_write ds_mip_2002bis_mn_ha_auth  {1}        ; disable - 0, enable -1
nv_write ds_mip_qc_drs_opt      {1}            ; dormant handoff optimization. disable - 0, enable - 1
                                               ;Comment : MIP general profile information {index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
                                               ;Comment : reverse tunneling, home address, primary ha address, secondary ha address}
nv_write ds_mip_gen_user_prof   {0,20,"0000000000@vzw3g.com",1,300,1,2,1,0x00000000,0xffffffff,0xffffffff}
nv_write ds_mip_dmu_pkoid       {0,10}         ; { Index , Public key organization indentifier }
nv_write ds_mip_dmu_mn_auth     {0,0x01,0xB2,0x07}            ; { Index , DMU MN authenticator - 111111base10 } 
nv_write hdr_an_auth_user_id_long {20,"0000000000@vzw3g.com"} ; { Length , EVDO AN authetication user id }
nv_write dun_cable_mode         {1}            ;0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode            {1}            ;0=disable bt dun,1=enable bt dun

					       ;Comment : MIP&SIP NAI(Network Access Identifier) for DUN 
nv_write ds_mip_rm_nai {0,24,"0000000000@dun.vzw3g.com"}	;	{index,nai_length,nai}					       
nv_write ds_sip_rm_nai {24,"0000000000@dun.vzw3g.com"}		;	{nai_length,nai}

;----------------------------------------------------------------------
nv_write ppp_carrier            {0}            ; 0-Verizon 1-USC 7-SCRIPT. Test NV Item.  
efs write "DMU/10.key"		                   ; MIP DMU(Dynamic Mipkeys Update) key file

;CS DLL don't write this item
;remove the ppp password setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
nv_write ppp_password          {16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}      

;CS DLL don't write this item 
;{0~5(index),16(mn_ha_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,
;16(mn_aaa_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
;remove the ds_mip_ss_user_prof setting in script file. (Becuase ppp_password value is changed after DMU nego.)
nv_write ds_mip_ss_user_prof {0,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}

;CS DLL don't write this item 
;Comment : remove the hdr_an_auth_passwd_long setting in script file. (Becuase it uses ppp_password value that changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
nv_write hdr_an_auth_passwd_long  {16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}    

;=========================================================================
; MSG ITEM
;=========================================================================
nv_write msg_settings_auto_save     	{0}    		; MSG_AUTO_SAVE(0), MSG_PROMPT(1), MSG_DO_NOT_SAVE(2)
nv_write msg_settings_auto_delete   	{0}     	; 0(Off), 1(On)
nv_write msg_settings_entry_mode    	{1}     	; MSG_T9EN(0), MSG_ABC(1), MSG_123(2)
nv_write msg_settings_vibrate_alert   	{0,0,0,0}	; On(1), Off(0)

;=========================================================================
; SMS ITEM
;=========================================================================
nv_write sms_orig_msg_id              	{1}   		; 0X0001 - 0XFFFF
nv_write sms_mo_max_userdata          	{160} 		; Up to 220 Byte (160 character(= 140 Byte))
nv_write sms_mo_l3_ack                	{1}   		; On(1), Off(0)
nv_write sms_mo_so                    	{1}   		; 8K(1), 13K(0)
nv_write sms_txt_cb_enable            	{1}   		; On(1), Off(0)
nv_write sms_voicemail_record     	{0,0} 		;
nv_write sms_settings_signature       	{0}   		; None(0), Custom(1)
nv_write sms_settings_auto_view     	{0}   		; On(1), Off(0)
nv_write sms_mo_causecode               {0} 
nv_write sms_ems_concat_reference       {0}
nv_write sms_voicemail_alert 		{10}  		; 0(Low Beep Once), 1(Low Beeps),
nv_write sms_textmsg_alert   		{1}  	 	; 2(Laud Beep Once), 3(Loud Beeps),
nv_write sms_info_alert             	{1}   		; 0(silent) 1(icon only) 2(vibrate icon)
nv_write sms_mo_errorclass      	{0}
nv_write sms_settings_font_size  	{1}   		; small(0) large(1)
nv_write sms_voicemail_cb               {3,"*86"} 	; 32Byte(ASCII)
nv_write sms_urgent_voice_record  	{0}   		; 
nv_write sms_mo_access                	{1}   		;
nv_write sms_2min_alert_sel           	{3,3,3,3} 	; Once(0), Every 2 Minutes(1), Every 15 Minutes(2), Off(3)
nv_write sms_message_cb          	{10, 0}		;
nv_write sms_settings_name_card    	{0} 		; Off(0)  On(1)

;=========================================================================
; EMS ITEM
;=========================================================================
nv_write sms_settings_auto_play       	{0} 		; On(1), Off(0)
nv_write sms_ems_enable               	{1}  		; On(1), Off(0) 

;=========================================================================
; UP ITEM : for magellan 
;=========================================================================
efs write "OWS/paramtable1.fil"
efs write "OWS/wdptable1.fil"

;=========================================================================
;BREW ITEM
;=========================================================================
nv_write brew_carrier_id {200}
nv_write brew_platform_id {1136}				            ;VX8500 platform id
nv_write brew_bkey {0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 
nv_write brew_server    {"apps.myvzw.com,apps2.myvzw.com"}  ; 64 byte character
nv_write brew_download_flags {0x0004}                   	; DIF_USE_A_KEY(0x0001) - A Key: 1 or B Key: 0 Option, DIF_TEST_ALLOWED(0x0002) - Test Disable: 0, Test Enable: 2
                                                        	; DIF_MIN_FOR_SID(0x0004) - Use MIN for Subscriber ID: 4,  Not use: 0, DIF_PREPAY(0x0008) - Prepay:8, Postpay:0
nv_write brew_auth_policy {1}                             	; APOLCY_NONE(0), APOLCY_SID(1), APOLCY_TEXT(2), APOLCY_NUM(3) 
nv_write brew_privacy_policy {3}                            	; PPOLICY_BREW(0), PPOLICY_CARRIER(1), PPOLICY_BREW_AND_CARRIER(2), PPOLICY_BREW_OR_CARRIER(3)
nv_write brew_sid_length {32}	
nv_write brew_disallow_dormancy {1}				; TRUE	
;=========================================================================
; MMS ITEM
;=========================================================================
nv_write mms_set_auto_receive                   {1}   ; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_set_read_ack                       {1}   ; 0(ON), 1(OFF)
nv_write mms_set_delivery_ack                   {0}   ; 0(MMS_ON), 1(MMS_OFF)

nv_write mms_set_tone_alert                     {1}   ; 0(Low Beep Once), 1(Low Beeps), 2(Laud Beep Once), 3(Loud Beeps),4(VZW Default Tone),5~14(Ring1~Ring10), 15(No Ring)
nv_write mms_set_vibrate_alert                  {0}   ; 0(VIBRATE OFF), 1(VIBRATE ON)
nv_write mms_set_reminder_alert                 {3}   ; 0(REMIND ONCE), 1(REMIND EVERY2MIN), 2(REMIND EVERY15MIN), 3(REMIND OFF)

nv_write mms_mmsc_url                           {20, "http://mms.vtext.com"} ; 48 byte characters
;nv_write mms_mmsc_upload_url                    {13, "pix.vtext.com" }   ; Upload Address
nv_write mms_mmsc_upload_url                    {6, "438749"}   ; Upload Address
nv_write mms_mmsc_uaprof_url           		{44, "http://uaprof.vtext.com/lg/vx85k/vx85kv1.xml"} ; 48 byte characters

;nv_write mms_send_retry_num                    {0}   ; 0, 1, 2, 3
nv_write mms_set_retry_num                      {3}   ; 0, 1, 2, 3

nv_write mms_send_from_add                      {2}   ; MDN Only (0), 1MDN (1),  +1MDN (2)         

nv_write mms_mmsc_server_post_url               {13, "/servlets/mms"}        ; Post URL
nv_write mms_mmsc_server_post_cgi               {12, "?message-id="}         ; CGI URL
nv_write mms_mmsc_user_agent                    {8,"VX8500v1"}               ; User Agent Profile name

nv_write mms_test_authorization                 {0}                          ; 0 : Commercial, 1 : Lab
nv_write mms_test_mmsc_url                      {20, "http://66.174.75.171"} ; 48 byte characters
nv_write mms_test_mmsc_upload_url               {6, "666612" }               ; Upload Address

;=========================================================================
;F/W ITEM
;=========================================================================
nv_write rf_config           {6}

nv_write vbatt               {87,226}                                    ; VX8500 2006.03.16 for REV.D {87, 226} <- {165,239}
nv_write qdsp_snd_ctrl       {0,0,0,0,0,0,0,0,0,7,6,0,0,0,0,-800}        ;
nv_write audio_adj_phone     {0,0,0,0,0,0,0,0,0}                         ;
nv_write audio_adj_earjack   {0,0,0,0,0,0,0,0,0}                         ;
nv_write audio_adj_hfk       {0,0,0,0,0,0,0,0,0}                         ;
nv_write audio_adj_spk       {0,0,0,0,0,0,0,0,0}                         ;
nv_write audio_adj_bt        {0,0,0,0,0,0,0,0,0}                         ;


;=========================================================================

;=========================================================================
;GPSONE ITEM
;=========================================================================
nv_write gps1_pde_address {0,0,0,0}
nv_write gps1_pde_port {0}
;=========================================================================


;=========================================================================
;ERI SOUND ITEM
;=========================================================================
efs write "eri_sound/extendednetwork.qcp"
efs write "eri_sound/lossofservice.qcp"
efs write "eri_sound/roaming.qcp"
efs write "eri_sound/verizonwireless.qcp"
;=========================================================================

;=========================================================================
;MMS IMAGE ITEM
;=========================================================================
efs write "mms/DecodeErrorAnimation.jpg"
efs write "mms/DecodeErrorImage.jpg"
efs write "mms/NotSupportedImage_UnknownImage.jpg"
efs write "mms/phoneOnConversation.jpg"
efs write "mms/TooBigErrorImage.jpg"
;=========================================================================

;=========================================================================
;ANIMATION IMAGE ITEM
;=========================================================================
efs write "dload/closing1.bit2"
efs write "dload/opening1.bit2"
;=========================================================================

;=========================================================================
;VOICE ITEM
;=========================================================================
;efs write "mVoice/ment/ment_voc.db"
;=========================================================================


;=========================================================================
;FLASH UI ITEM
;=========================================================================
;efs write "flash/ui/wallpaper/wallpaperType1.swf"
;efs write "flash/ui/wallpaper/wallpaperType2.swf"
;efs write "flash/ui/menu/menuType1.swf"
;efs write "flash/ui/menu/menuType2.swf"
;efs write "flash/ui/music/musicPlayerType1.swf"
;efs write "flash/ui/music/musicPlayerType2.swf"
;efs write "flash/ui/music/musicType1.swf"
;efs write "flash/ui/music/musicType2.swf"
;=========================================================================
mode reset
