;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;=========================================================================
;  File name: VX855V04.SCR
;  Made by  : LGE
;  Version  : V04_03
;  Date     : 06/27/2008
;-------------------------------------------------------------------------
;  when         who        what
;----------    -------    ------------------------------------------------
;06/27/2008    ChoiYS      Change to nv_write bt_audio_auto_pair       {1}
;06/25/2008    ChoiYS      Insert mvoice lib into script
;06/17/2008    ChoiYS      MOD 2.07.013  for LG VX8550 (PID 1198)
;                          nv_write nam_lock {0, 1} -> {0, 0}
;11/01/2007    ChoiYS      Rename
;10/24/2007    ChoiYS      Rename
;05/22/2007    ChoiYS      VZNavi Pre-Loaded App. modifed for 1 day expire
;05/16/2007    ChoiYS      MIM / VZNavi Pre-Loaded App. modifed
;05/11/2007    ChoiYS      Song ID / VZNavi Pre-Loaded - Official Version
;05/10/2007    ChoiYS      MOD/VOD/MIM/VZTones Pre-Loaded - Official Version
;05/08/2007    KoEM        Insert preload.txt
;04/30/2007    JangYG      Register MMS VX8550 UA Profile  
;04/26/2007    ParkSH      Add bt_audio_auto_pair
;04/25/2007    ChoiYS      Delete ear_bt_lvl
;04/22/2007    BaeSJ	   ADD usb_auto_detection  {1} ,touch_vibration  {0}
;			   Delete nmp_option               {7,0,0,0,0,0,0,0,0,0}
;			   changed key_light{5} ==> {7}
;04/16/2007    BaeSJ	   changed display_set {0,0,1} ==> display_set {0,0,2} Delete banner{"VCAST"} ==> banner{""}
;04/03/2007    BaeSJ       ADD wheel_sensitivity        {2}
;04/02/2007    misunp79    Deleted touch_sensitivity: 5030, Added touch_sensitivity_setting: 5149
;04/02/2007    BaeSJ       changed back_light{5} ==} {7}          
;03/31/2007    misunp79    changed touch_sensitivity type (byte -> struct: total 18 byte)
;03/30/2007    CHKim       Changed flash_clipboard_theme ==>  vx8550_color_variation
;03/30/2007    CHKim       Changed mms_mmsc_user_agent from {8,"VX8700v1"} to {8,"VX8700v2"}               
;03/26/2007    BaeSJ	   ADD touch_sound ,slide_sound,wheel_sound,Changed answer_option{7}==>{3}
;03/22/2007    BaeSJ	   Changed wheel_light {0}==>{0,0,0} , Add flash_clipboard_theme{0}
;03/21/2007    BaeSJ	   Changed answer_option{0}==>{7},end_call_option {0}==> {3} ,spk_phone_beep_lvl{6}==>{4}
;03/16/2007    ChoiYS      Changed display_set {0,0,1}, flash_clip_board {0}  
;03/15/2007    ChoiYS      Changed nv_write vbatt {30,180}
;                          Changed nv_write mms_set_read_ack {0}, mms_set_delivery_ack {1}
;03/14/2007    Sungmui     nv_write call_sounds {5,5,5,5,5} -> {5,5,5,5,0}  
;03/12/2007    ChoiYS      BREW PID Changed 1198
;03/08/2007    BaeSJ       Added flash_clip_board
;03/07/2007    LimSH       Added avr_digit_dial_readout, avr_audio_playback
;03/05/2007    LeeKB       Modified paramtable1.fil for OWS
;02/26/2007    ChoiYS      Activate speaker_shadow_lvl after DLL 0.4.0.0
;02/21/2007    ChoiYS      Deleted Brew Folder and rearrange EFS directory Map.
;                          Deleted Brew NV Item brew_sid_length 
;                          Changed MMS EFS directory 
;02/20/2007    ChoiYS      Modified SMS/EMS, Setting, AVR related items. 
;02/16/2007    ChoiYS      Initial Release
;----------    -------    ------------------------------------------------

;spc "000000"                         ; does not need at LGDP DLL
;wait 2
mode offline-d
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model
wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================

nv_write sec_code       {"000000"}      ; Security code
nv_write lock_code      {"0000"}        ; Lock_code

nv_write name_nam       {0, "NAM1"}     ; NAM 1 Name
nv_write name_nam       {1, "NAM2"}     ; NAM 2 Name

nv_write imsi_mcc       {0, "310"}                   ; Mobile Country Code (310)
nv_write imsi_mcc       {1, "310"}
nv_write imsi_11_12     {0, "00"}                    ; Mobile Network Code
nv_write imsi_11_12     {1, "00"}
nv_write min1           {0, "000-0000", "000-0000"}
nv_write min1           {1, "000-0000", "000-0000"}
nv_write min2           {0, "000", "000"}            ; NAM 0 has one active MIN2,
nv_write min2           {1, "000", "000"}           

nv_write imsi_t_mcc     {0, "310"}               
nv_write imsi_t_mcc     {1, "310"}
nv_write imsi_t_11_12   {0, "00"}
nv_write imsi_t_11_12   {1, "00"}
nv_write imsi_t_s1      {0, "000-0000", "000-0000"}
nv_write imsi_t_s1      {1, "000-0000", "000-0000"}
nv_write imsi_t_s2      {0, "000", "000"}
nv_write imsi_t_s2      {1, "000", "000"}
                                                 ; NV_DIR_NUMBER_PCS_I      /*123456789012345*/ using 10 digits
nv_write dir_number_pcs {0, "0000000000"}        ; NAM 0 : NV_DIR_NUMBER_PCS_I
nv_write dir_number_pcs {1, "0000000000"}        ; NAM 1 : NV_DIR_NUMBER_PCS_I

                                                 ; Primary CDMA Channels for A carrier and B carrier
print "Programming Primary CDMA Channel"
nv_write pcdmach        {0, 283, 384}            ; A and B primary CDMA channels
nv_write pcdmach        {1, 283, 384}

                                                 ; Secondary CDMA Channel
print "Programming Secondary CDMA Channel"
nv_write scdmach        {0, 691, 777}            ; set only if secondary channels offered
nv_write scdmach        {1, 691, 777}

nv_write home_sid_nid   {0,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535}
nv_write home_sid_nid   {1,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535}
nv_write sid_nid_lock   {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock   {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}

nv_write mob_term_home    {0, true, true}
nv_write mob_term_home    {1, true, true}
nv_write mob_term_for_sid {0, true, true}
nv_write mob_term_for_sid {1, true, true}
nv_write mob_term_for_nid {0, true, true}
nv_write mob_term_for_nid {1, true, true}

nv_write accolc           {0, 0, 0}
nv_write accolc           {1, 0, 0}

nv_write slot_cycle_index {2}

                                                  
nv_write pref_voice_so {0,  1, 0x0000, 0x0003, 0x0003} ;{Nam Name(0, 1), EVRC Capability(0:Off, 1:ON), Home_Page_Voice_SO(0: wildcard, Others : SO), Home_Page_Voice_SO(0 or SO), Home_Page_Voice_SO(0 or SO)}
nv_write pref_voice_so {1,  1, 0x0000, 0x0003, 0x0003} ;{Nam Name(0, 1), EVRC Capability(0:Off, 1:ON), Home_Page_Voice_SO(0: wildcard, Others : SO), Home_Page_Voice_SO(0 or SO), Home_Page_Voice_SO(0 or SO)}

print "Programming Pref Mode"
nv_write pref_mode     {0, "Digital Only"}
nv_write pref_mode     {1, "Digital Only"}
nv_write hybrid_pref   {1}                             ; 1 : hybrid on,  0 : hybrid off

print "Programming Band Preferred"
nv_write band_pref     {0, "pref_any"}
nv_write band_pref     {1, "pref_any"}

print "Programming Roam Preferred"
nv_write roam_pref     {0, "pref_any"}
nv_write roam_pref     {1, "pref_any"}

nv_write system_pref   {0, "automatic b"}              ; System preference, actually default to band preference
nv_write system_pref   {1, "automatic b"}

nv_write stand_alone_mode {0}                          ; 0 default OFF, 1 ON

;------------------------------------------------------------------------
print "Programming MRU table clear"
                                            ; except nam (first 0), '0' are 48(=4 X 12) times.
nv_write mru3_table {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru3_table {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};

                                             ; NAM Checksums must all be 0xffff
print "Programming NAM Checksums"
nv_write nam_chksum {0, 0xffff}
nv_write nam_chksum {1, 0xffff}
nv_write min_chksum {0, 0xffff, 0xffff}
nv_write min_chksum {1, 0xffff, 0xffff}

;=========================================================================
; OTA ITEM
;=========================================================================
nv_write nam_lock           {0, 0}
nv_write nam_lock           {1, 0}
nv_write otapa_enabled      {0, 1}   ; enable
nv_write otapa_enabled      {1, 1}   ; enable
nv_write spc_change_enabled {1}

;-------------------------------------------------------------------------
; nv_write imsi_t_addr_num    {0, 255}
; nv_write imsi_t_addr_num    {1, 255}

;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key {0, 0x00000000, 0x00000000 } ; Nam 1 64 bits A-Key. Published at factory with Random number.
nv_write a_key {1, 0x00000000, 0x00000000 } ; Nam 2 64 bits A-Key. Published at factory with Random number.

;-------------------------------------------------------------------------
nv_write ssd_a {0, 0x00000000, 0x00000000 }
nv_write ssd_a {1, 0x00000000, 0x00000000 }
nv_write ssd_b {0, 0x00000000, 0x00000000 }
nv_write ssd_b {1, 0x00000000, 0x00000000 }
nv_write count {0, 0}
nv_write count {1, 0}
;=========================================================================

;=========================================================================
;UI ITEM
;=========================================================================
nv_write curr_nam                 {0}                     ; Current NAM == NAM1
nv_write auto_nam                 {0}                     ; Auto NAM == disable
nv_write ear_lvl                  {6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write speaker_lvl              {6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write ringer_lvl               {4}                     ; 1~5 (Low, Med Low, Med, Med High, High), 1 (Vibrate only), 97 (Alarm Only), 1 (All Sounds Off)"
nv_write beep_lvl                 {4}                     ; 0 (Off), 1~5 (Low, Med Low, Med, Med High, High)
nv_write cont_key_dtmf            {1}                     ; Normal (1), Long (0),  Off (2)

nv_write auto_answer              {0, 0}                  ; On (1, 1), Off (0, 0)
nv_write auto_redial              {0, 0}                  ; Off (0, 0), Every 10 Seconds (1, 1), Every 30 Seconds (1, 3), Every 60 Seconds (1, 6)
nv_write back_light               {7}                     ; Default 7 Sec
nv_write lock                     {0}                     ; Lock (1), Unlock (0)
nv_write auto_lock                {0}                     ; Power_up (1)
nv_write call_rstrc               {0}                     ; Off (0), On (1)
nv_write onetouch_dial            {1}                     ; Off (0), On (1)
nv_write beep_lvl_shadow          {4}                     ; 0 (Off), 1~5 (Low, Med Low, Med, Med High, High)
nv_write ear_lvl_shadow           {6}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write send_pin                 {0}                     ; Off (0)
nv_write voice_priv               {1}                     ; Standard (0), Enhanced (1)
nv_write fsc                      {"000000"}              ; Field Service code
nv_write ringer_spkr_lvl          {4}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8), 98 (High & Vib), 99 (Vibrate)
nv_write beep_spkr_lvl            {4}                     ; 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write language_selection       {0}                      ; English (0), Spanish (1)
nv_write auto_volume_enabled      {0}                     ; Off (0), On (1)
nv_write tty                      {3}                     ; TTY Full (0), TTY+TALK (1),TTY+HEAR (2),TTY off (3)
nv_write gps1_lock                {3}                     ; Location ON (0), MI (1), MT (2), E911 Only (3)
nv_write manner_mode              {0}                     ; False (0), True (1)
nv_write alarm_only_mode          {0}                     ; False (0), True (1)
nv_write silence_all              {0}                     ; Sound On (0), Sound Off (others)

nv_write speaker_shadow_lvl       {6}                     ; Earpiece Volume on Speaker Phone Mode: 1~8 (Volume1 ~ Volume8) -> Activate this item after DLL 0.0.4.0
nv_write spk_phone_beep_lvl       {4}                     ; Keypad Volume on Speaker Phone Mode: 0 (Off), 1~8 (Volume1 ~ Volume8)
nv_write call_sounds              {5,5,5,5,0}             ; {Caller ID (4: VZW Default Tone), No Caller ID (9: Ringtone 5), Restrict Calls (6: Ringtone 2), All Calls (0xFFFF: Get New Ringtones), Vibrate (0: Off, 1: On)}"
nv_write sound_alerts             {0,0,0,0}               ; {Service Change (Not use), Minute Beep, Call Connect, ERI}, On (1), Off (0)
nv_write power_onoff_sounds       {1,1}                   ; {Power On, Power Off}, On (1), Off (0)
nv_write alarm_sounds             {6,0}                   ; {tone(6: Ringtone 2), vibrate (0: Off)}
nv_write eri_text_onoff           {1}                     ; 1 -> On, 0 -> Off
nv_write key_light                {7}                     ; Default 5 Sec
nv_write wallpaper_main           {0,0,50}                 ; {location_type (0:phone memory, 1:phone efs, 2:sdcard), location_id (0:sdcard id), item_id (1: index)}
nv_write display_set              {0,0,2}                 ; sub_clock, main_clock, color theme
nv_write number_size              {0,0}                   ;  Normal (0), Large (1)
nv_write pc_port                  {0}                     ; PC connection port  0 (USB), 1 (UART), 2 (BLUETOOTH), 3 (CLOSED)
nv_write emergency_num1           {"911"}                 ; Up to 48 Digits
nv_write emergency_num2           {"*911"}                ; Up to 48 Digits
nv_write emergency_num3           {"#911"}                ; Up to 48 Digits
nv_write service_num              {"611"}                 ; Up to 48 Digits        
nv_write wclock_choice            {30,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,0x0,47,0}             
				                          ; {cur_Itm (30), set_DST, choice_city ( NewYork: 47), line longtitude}
nv_write media_save_option        {0,0,0}                 ; {PIX, FLIX, SOUND} Phone memory (0), SD card (1)
nv_write camera_flash_test        {81}                    ; Camera Flash On (85(0x55)), Off (others)
nv_write equalizer_mode           {0}
nv_write visualizer_mode          {0}                     ; OFF (0), ON (1)
nv_write avr_call_alerts          {0}
nv_write avr_prompts_mode         {0}
nv_write avr_choice_list          {0}
nv_write avr_prompts_timeout      {0}
nv_write avr_sensitivity          {1}                     ; 0: High 1: Medium 2: Low
nv_write avr_digit_dial_readout   {0}                     ; 0: Off, 1: On
nv_write avr_audio_playback       {0}                     ; 0: Speakerphone, 1: Earpiece
nv_write bt_power_onoff           {0}                     ; OFF (0), ON (1)
nv_write beep_bt_lvl              {4}                     ; Off (0), 1~5 (Volume1 ~ Volume5)
nv_write bt_audio_auto_pair       {1}                     ; auto pairing mode ON(1) OFF(0)
;nv_write ear_bt_lvl               {6}                     ; 1~8 (Volume1 ~ Volume8)
nv_write use_mymp3                {0}                     ; MOD Center Key Define: MOD Player (0), MP3 Player (1)
nv_write carrier_logo             {0}                     ; Verizon(0)
nv_write contrast_lvl             {0,0}
nv_write led_blink                {1}                     ; ON(1) OFF(0)
nv_write power_saver              {0}
nv_write edit_font                {0,0}
nv_write gps_test_num             {"922"}                 ; Up to 48 Digits
nv_write emer_test_num            {"911"}                 ; Up to 48 Digits
nv_write location_set_lock     	  {0}     		  ; 0: unlock, 1:Lock
nv_write end_call_option     	  {3}     		  ; 0: slide down, 1:end key only
nv_write dual_nam_set_enable	  {1}                     ; dual_nam_set_enable(nam set menu) ( 0 : disable , 1 : enable)
nv_write charging_alert_onoff     {0}                     ; Charging Alert On(1), Off(0)
nv_write call_restrict            {0,0,0,0,0}             ; 0(off), 1(on) inCall-outCall-MT-MO-DUN
nv_write answer_option            {3}                     ;
nv_write wheel_light              {0,0,0}                 ; trace motion (0:On 1:Off) , PowerOnOff(0:On 1:Off),call(0: sound_theme 1,1: sound_theme 2,2: sound_theme 3, 3: Off)
nv_write vx8550_color_variation   {0}                     ; VX8550 color varitation {0: Black , 1: Dark Blue , 2: Dark Red }
nv_write wheel_sensitivity        {2}                     ; wheel speed ( 0: High 1: Medium 2: Low)
nv_write usb_auto_detection       {1}                     ; usb_auto_detection ( 0: Sync Music 1: Sync Data 2: Ask On Plug)
nv_write touch_vibration          {0}                     ; touch_vibration ( 0: On, 1: Off)
nv_write touch_sound   		  {1}                     ; touch sound set ( 0 : Off , 1 : On)
nv_write slide_sound    	  {1}                     ; slide sound set ( 0 : Off , 1 : On)
nv_write wheel_sound    	  {1}                     ; wheel sound set ( 0 : Off , 1 : On)
nv_write auto_key_lock            {0}                     ; 0(On), 1(Off)
nv_write shortcut_main            {2,4,0,17}              ; {Left, Up, Right, Down}
nv_write flash_clip_board     	  {0}     		  ; set flash clip board ( 0 : off , 1 : Classic ,2 : Diary, 3 : Modern)


;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_pkt_orig_str      {5, "#777"}    ; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_mdr_mode          {3}            ; Service Option 33 (1x channel) = 3 Use only low-speed packet data = 2
nv_write data_auto_packet_detection {0}        ; 0-Disable   1-Enable
nv_write data_so_set            {2}            ; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write diag_default_baudrate  {0x000e}       ; 0x000e(38.4kbps), 0x0011(115.2kbps) 
nv_write data_qnc_enabled       {0}            ; 0-QNC Disable  1-QNC Enable

nv_write ppp_user_id            {20,"0000000000@vzw3g.com"}; Max of 127 chars in User ID

nv_write data_scrm_enabled      {1}            ; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled      {1}            ; 0-TRTL Disable 1-TRTL Enable
nv_write pref_for_rc            {3}            ; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)    
nv_write ds_default_baudrate    {0x0011}       ; 0x0000 (19.2kbps),0x0011(115.2kbps) ,0x00012(230.4kbps)
nv_write ds_qcmip               {1}            ; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only
nv_write ds_mip_active_prof     {0}            ; current active profile index
nv_write ds_mip_enable_prof     {1,0,0,0,0,0}  ; diable - 0, enable - 1 {1st Profile, 2nd Profile, 3rd Profile, .... }
nv_write ds_mip_retries         {2}            ; number of retries
nv_write ds_mip_retry_int       {3}            ; retry interval = n*250(ms) + 1000ms
nv_write ds_mip_pre_re_rrq_time {0}            ; pre-registration time - minute
nv_write ds_mip_num_prof        {1}            ; number of profiles (max 6) 
nv_write ds_mip_2002bis_mn_ha_auth  {1}        ; disable - 0, enable -1
nv_write ds_mip_qc_drs_opt      {1}            ; dormant handoff optimization. disable - 0, enable - 1
                                               ;Comment : MIP general profile information {index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
                                               ;Comment : reverse tunneling, home address, primary ha address, secondary ha address}

nv_write ds_mip_gen_user_prof   {0,20,"0000000000@vzw3g.com",1,300,1,2,1,0x00000000,0xffffffff,0xffffffff}

nv_write ds_mip_dmu_pkoid       {0,10}         ; { Index , Public key organization indentifier }

nv_write ds_mip_dmu_mn_auth     {0,0x01,0xB2,0x07}            ; { Index , DMU MN authenticator - 111111base10 } 

nv_write hdr_an_auth_user_id_long {20,"0000000000@vzw3g.com"} ; { Length , EVDO AN authetication user id }

nv_write dun_cable_mode         {1}            ;0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode            {1}            ;0=disable bt dun,1=enable bt dun

					       ;Comment : MIP&SIP NAI(Network Access Identifier) for DUN 
nv_write ds_mip_rm_nai {0,24,"0000000000@dun.vzw3g.com"}	;	{index,nai_length,nai}					       
nv_write ds_sip_rm_nai {24,"0000000000@dun.vzw3g.com"}		;	{nai_length,nai}

;----------------------------------------------------------------------
nv_write ppp_carrier            {0}            ; 0-Verizon 1-USC 7-SCRIPT. Test NV Item.  
efs write "DMU/10.key"		               ; MIP DMU(Dynamic Mipkeys Update) key file                     ;size = 260;

;CS DLL don't write this item
;remove the ppp password setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
nv_write ppp_password          {16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}      

;CS DLL don't write this item 
;{0~5(index),16(mn_ha_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,
;16(mn_aaa_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
;remove the ds_mip_ss_user_prof setting in script file. (Becuase ppp_password value is changed after DMU nego.)
nv_write ds_mip_ss_user_prof {0,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}

;CS DLL don't write this item 
;Comment : remove the hdr_an_auth_passwd_long setting in script file. (Becuase it uses ppp_password value that changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
nv_write hdr_an_auth_passwd_long  {16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}    

;=========================================================================
; MSG ITEM
;=========================================================================
nv_write msg_settings_auto_save     	{0}    		; MSG_AUTO_SAVE(0), MSG_PROMPT(1), MSG_DO_NOT_SAVE(2)
nv_write msg_settings_auto_delete   	{0}     	; 0(Off), 1(On)
nv_write msg_settings_entry_mode    	{1}     	; MSG_T9EN(0), MSG_ABC(1), MSG_123(2)
nv_write msg_settings_vibrate_alert   	{0,0,0,0}	; On(1), Off(0)
;=========================================================================

;=========================================================================
; SMS/EMS ITEM
;=========================================================================
nv_write sms_txt_cb_enable           {1}                             ; On(1), Off(0)
nv_write sms_orig_msg_id             {1}                             ; 0X0001 - 0XFFFF
nv_write sms_mo_max_userdata         {160}                           ; Up to 220 Byte (160 character(= 140 Byte))
nv_write sms_mo_l3_ack               {1}                             ; On(1), Off(0)
nv_write sms_mo_so                   {1}                             ; 8K(1), 13K(0)
nv_write sms_voicemail_record        {0,0}                           ; {Count,Time}
nv_write sms_settings_signature      {0}                             ; None(0), Custom(1)
nv_write sms_settings_direct_view    {0}                             ; Off(0), On(1)
nv_write sms_voicemail_alert         {11}                            ; 5(VZW Default Tone), 6~17(Ringtone 1~11), 18(No Ring), 0xffff(Get New Ringtones)
nv_write sms_textmsg_alert           {1}                             ; 0(Low Beep Once),1(Low Beeps),2(Laud Beep Once),3(Loud Beeps)
nv_write sms_voicemail_cb            {3,"*86"}                       ; 20Byte(ASCII)
nv_write sms_urgent_voice_record     {0}                             ; None(0), Exist(1)
nv_write sms_2min_alert_sel          {3,3,3,3}                       ; Once(0), Every 2 Minutes(1), Every 15 Minutes(2), Off(3)
nv_write sms_message_cb              {10,"0000000000"}                          ;
;nv_write sms_settings_name_card      {0}                            ; Off(0)  On(1)
;nv_write sms_tts_readout             {0}                            ; Manual(0), Auto(1)

nv_write sms_settings_auto_play      {0}                             ; On(1), Off(0)
nv_write sms_ems_enable              {1}                             ; On(1), Off(0)
;=========================================================================

;=========================================================================
; WAP ITEM
;=========================================================================
efs write "OWS/paramtable1.fil"                                      ;size = 2375; 
efs write "OWS/wdptable1.fil"                                        ;size = 261;
;=========================================================================

;=========================================================================
;BREW ITEM
;=========================================================================
nv_write brew_carrier_id {200}
nv_write brew_platform_id {1198}				            ;VX8550 platform id
nv_write brew_bkey {0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 

nv_write brew_server    {"apps.myvzw.com,apps2.myvzw.com"}  ; 64 byte character

nv_write brew_download_flags {0x0004}                   	; DIF_USE_A_KEY(0x0001) - A Key: 1 or B Key: 0 Option, DIF_TEST_ALLOWED(0x0002) - Test Disable: 0, Test Enable: 2
                                                        	; DIF_MIN_FOR_SID(0x0004) - Use MIN for Subscriber ID: 4,  Not use: 0, DIF_PREPAY(0x0008) - Prepay:8, Postpay:0

nv_write brew_auth_policy {1}                             	; APOLCY_NONE(0), APOLCY_SID(1), APOLCY_TEXT(2), APOLCY_NUM(3) 
nv_write brew_privacy_policy {3}                            	; PPOLICY_BREW(0), PPOLICY_CARRIER(1), PPOLICY_BREW_AND_CARRIER(2), PPOLICY_BREW_OR_CARRIER(3)
nv_write brew_disallow_dormancy {1}				; TRUE	
;=========================================================================

;=========================================================================
; MMS ITEM
;=========================================================================
nv_write mms_set_auto_receive                   {1}   ; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_set_read_ack                       {0}   ; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_set_delivery_ack                   {1}   ; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_set_tone_alert                     {1}   ; 0(Low Beep Once), 1(Low Beeps), 2(Loud Beep Once), 3(Loud Beeps), 4(Door Bell), 5(VZW Default Tone), 6~19(Ringtone 1~14), 20(No Ring)
nv_write mms_set_vibrate_alert                  {0}   ; 0(VIBRATE OFF), 1(VIBRATE ON)
nv_write mms_set_reminder_alert                 {3}   ; 0(REMIND ONCE), 1(REMIND EVERY2MIN), 2(REMIND EVERY15MIN), 3(REMIND OFF)
nv_write mms_mmsc_url                           {20, "http://mms.vtext.com"} ; 48 byte characters

;nv_write mms_mmsc_upload_url                    {13, "pix.vtext.com" }   ; Upload Address
nv_write mms_mmsc_upload_url                    {6, "438749"}   ; Upload Address
nv_write mms_mmsc_uaprof_url           		{46, "http://uaprof.vtext.com/lg/vx8550/vx8550v1.xml"} ; 48 byte characters

;nv_write mms_send_retry_num                    {0}   ; 0, 1, 2, 3
nv_write mms_set_retry_num                      {3}   ; 0, 1, 2, 3
nv_write mms_send_from_add                      {2}   ; MDN Only (0), 1MDN (1),  +1MDN (2)   
nv_write mms_mmsc_server_post_url               {13, "/servlets/mms"}        ; Post URL
nv_write mms_mmsc_server_post_cgi               {12, "?message-id="}         ; CGI URL
nv_write mms_mmsc_user_agent                    {8,"VX8550v1"}               ; User Agent Profile name
nv_write mms_test_authorization                 {0}                          ; 0 : Commercial, 1 : Lab, 2 : Domestic
nv_write mms_test_mmsc_url                      {20, "http://66.174.75.171"} ; 48 byte characters
nv_write mms_test_mmsc_upload_url               {6, "666612" }               ; Upload Address
nv_write msg_settings_signature                 {0}                          ; SIGNATURE_OFF : 0, SIGNATURE_ON : 1
;=========================================================================

;=========================================================================
;F/W ITEM
;=========================================================================
nv_write rf_config                   {6}
nv_write vbatt                       {30,180}                                    ; VX8550 2007.02.27 for REV.B {30, 180} <- {87, 226} 
nv_write audio_codec_gain            { 0, 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write audio_voc_gain              { 0, 0, 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write audio_agc                   { 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write audio_rx_fir_pcm_filter     { 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write audio_tx_fir_pcm_filter     { 0, 0, 0, 0, 0, 0, 0, 0 }
nv_write audio_qdsp                  { 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0 }
;nv_write touch_sensitivity_setting   {2,2,0xBB,0xB8,0xB8,0xB4,0xAC,0xAA,0xAA,0xA8,0x9D,0x9C,0x9C,0x9C,0x8E,0x8E,0x8E,0x90}     ; set Mode(0:Unrestricted, 1:Strongest, 2: First), Level(0:Super, 1:High, 2:Med, 3:Low), Value(0xS0,0xS1,0xS5,0xS7,0xH0,0xH1,0xH5,0xH7,0xM0,0xM1,0xM5,0xM7,0xL0,0xL1,0xL5,0xL7)
;=========================================================================

;=========================================================================
;GPSONE ITEM
;=========================================================================
nv_write gps1_pde_address           {0,0,0,0}
nv_write gps1_pde_port              {0}
;=========================================================================


;=========================================================================
;ERI SOUND ITEM
;=========================================================================
efs write "eri_sound/extendednetwork.qcp"                                                     ;size = 2326;
efs write "eri_sound/lossofservice.qcp"                                                       ;size = 2118;
efs write "eri_sound/roaming.qcp"                                                             ;size = 1120;
efs write "eri_sound/verizonwireless.qcp"                                                     ;size = 2410;
;=========================================================================


;=========================================================================
; DCAMERA EFS
;=========================================================================
efs write                            "dload/default_img/DecodeErrorAnimation.jpg"             ;size = 6035;
efs write                            "dload/default_img/DecodeErrorImage.jpg"                 ;size = 4803;
efs write                            "dload/default_img/NotSupportedImage_UnknownImage.jpg"   ;size = 5069;
efs write                            "dload/default_img/phoneOnConversation.jpg"              ;size = 4823;         
efs write                            "dload/default_img/TooBigErrorImage.jpg"                 ;size = 4903;
efs write                            "dload/default_img/video_FirstFrame_PMD.bmp"             ;size = 32454;
efs write                            "dload/default_img/video_FirstFrame_SVG.bmp"             ;size = 32456;
efs write                            "dload/default_img/VideoImageSymbol.jpg"                 ;size = 19689;
;=========================================================================

;=========================================================================
; AVR EFS (for Play)
;=========================================================================
efs write                            "mVoice/dict/dict_en.dat"
efs write                            "mVoice/dict/dictinfo_en.dat"

;=========================================================================
;ANIMATION IMAGE ITEM
;=========================================================================
;efs write "dload/closing1.bit2"                                                               ;size = 1300898;	not use...
;efs write "dload/opening1.bit2"                                                               ;size = 2526006;	not use...
;=========================================================================

;=========================================================================
;FLASH UI ITEM
;=========================================================================
;efs write "flash/ui/wallpaper/wallpaperType1.swf"
;efs write "flash/ui/wallpaper/wallpaperType2.swf"
;efs write "flash/ui/menu/menuType1.swf"
;efs write "flash/ui/menu/menuType2.swf"
;efs write "flash/ui/music/musicPlayerType1.swf"
;efs write "flash/ui/music/musicPlayerType2.swf"
;efs write "flash/ui/music/musicType1.swf"
;efs write "flash/ui/music/musicType2.swf"
;=========================================================================
mode reset
