CCommandCom::SetLogCom, The Log has now been set.
CCommandCom::SetLogCom, The Log has now been set.
CCommandCom::SetLogCom, The Log has now been set.
NVS Event = 1
OVERRIDE NV Structure of NV_ESN_I 
OVERRIDE NV Structure of NV_VERNO_MAJ_I 
OVERRIDE NV Structure of NV_VERNO_MIN_I 
OVERRIDE NV Structure of NV_SCM_I 
OVERRIDE NV Structure of NV_SLOT_CYCLE_INDEX_I 
OVERRIDE NV Structure of NV_MOB_CAI_REV_I 
OVERRIDE NV Structure of NV_MOB_FIRM_REV_I 
OVERRIDE NV Structure of NV_MOB_MODEL_I 
OVERRIDE NV Structure of NV_PREF_MODE_I 
OVERRIDE NV Structure of NV_A_KEY_I 
OVERRIDE NV Structure of NV_MIN1_I 
OVERRIDE NV Structure of NV_MIN2_I 
OVERRIDE NV Structure of NV_LOCK_CODE_I 
OVERRIDE NV Structure of NV_SEC_CODE_I 
OVERRIDE NV Structure of NV_IMSI_MCC_I 
OVERRIDE NV Structure of NV_IMSI_11_12_I 
OVERRIDE NV Structure of NV_DIR_NUMBER_PCS_I 
OVERRIDE NV Structure of NV_SYSTEM_PREF_I 
OVERRIDE NV Structure of NV_IMSI_T_S1_I 
OVERRIDE NV Structure of NV_IMSI_T_S2_I 
OVERRIDE NV Structure of NV_IMSI_T_MCC_I 
OVERRIDE NV Structure of NV_IMSI_T_11_12_I 
OVERRIDE NV Structure of NV_BAND_PREF_I 
OVERRIDE NV Structure of NV_ROAM_PREF_I 
OVERRIDE NV Structure of NV_DS_MIP_GEN_USER_PROF_I 
OVERRIDE NV Structure of NV_DS_MIP_SS_USER_PROF_I 
OVERRIDE NV Structure of NV_PPP_PASSWORD_I 
OVERRIDE NV Structure of NV_MRU3_TABLE_I 

[//COMPONENT_INFO/LGNPST_COMPONENTS/ERS] xml node is not defined at setting.xml
CBasicComControl::Open, the port(COM 43) is constructed successfully => HANDLE : 0x4a60
PortOpen Success.
CBasicComControl::ChangeDataToDM  = 575.8 sys-time

|======================================= Device Information ============================================
| BIN Version         :: VX857V03     
| Compiled Date       :: Sep 07 2009 14:38:38 
| H/W Version         :: 1.0          
|=======================================================================================================
GenerateRestrictionKeyValue, SeedKeyValue: 14
CCommandCom::SetLogCom, The Log has now been set.
CCommandCom::SetLogCom, The Log has now been set.

|======================================= Component Information ============================================
|      DLL     	         Version                     Path														
| CommandProcessor    :: 3, 0, 2, 0   C:\LG Electronics\LGNPST\Components 3.0\CommandProcessor3.dll 
| BaseModel           :: 3, 0, 2, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_BaseModel3.dll 
| BasicComControl     :: 3, 0, 3, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_BasicComControl3.dll 
| Command             :: 3, 0, 2, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_Command3.dll 
| DLManager           :: 3, 0, 5, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_DLManager3.dll 
| EFS                 :: 3, 0, 5, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_EFS3.dll 
| Flash               :: 3, 0, 6, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_FLASH3.dll 
| Log                 :: 3, 0, 7, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_Log3.dll 
| MemoryTransfer      :: 3, 0, 4, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_MemoryTransfer3.dll 
| NVStorage           :: 3, 2, 4, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_NVStorage3.dll 
| OneBinary           :: 3, 0, 8, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_OneBinary3.dll 
| PortManager         :: 3, 0, 5, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_PortManager3.dll 
| Script              :: 3, 0, 1, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_Script3.dll 
| UI                  :: 3, 0, 1, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_UI3.dll 
| Utility             :: 3, 0, 1, 0   C:\LG Electronics\LGNPST\Components 3.0\LGNPST_Utility3.dll 
|=======================================================================================================
| Model DLL           :: 0, 1, 2, 0   C:\LG Electronics\LGNPST\model\vx8575\LGNPST_VX8575.dll 
| Log File Path                       C:\LG Electronics\LGNPST\model\vx8575\LOG\VX8575Log_COM43.log 
|=======================================================================================================

|======================================= USB Driver Information ============================================
| FriendlyName        :: LGE CDMA USB Serial Port (COM43) 
| DriverVersion       :: 4.9.4.0      
| DriverDate          :: 11-11-2008   
|=======================================================================================================


======================================= Environment Setting =========================================
=======================================================================================================
Error! D:\Work\TDR\2006\LGNPST_RC\Basic_Unit\LGNPST_Utility\FileUtilCom.cpp [310]
	Failed to get the attributes of the file [C:\LG Electronics\LGNPST\model\vx8575\Backup\COM43_00000000].


กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ   Progress Count Info กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ

ขบ SubProcess NAME : [Writing NV          ], ขบ Expected ProgressCount   679: 
ขบ SubProcess NAME : [Rebooting           ], ขบ Expected ProgressCount   150: 

กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ


 ============================  START PROCESS  =========================== 

 ขบ Expected Process TotalCount 829: 

 ======================================================================== 
Clear ALL NV Instance of NV Storage  Current Storage size=601736  
Successfully Clear NV Storage
=================================== Start NV Restore  ===================================
FAIL Writing  0     NV_ESN_I                                           Cause > Parameter is write-protected and thus read only
	Retry -> FAIL Writing  0     NV_ESN_I                                           Cause > Parameter is write-protected and thus read only
FAIL Writing  2     NV_VERNO_MAJ_I                                     Cause > Parameter is write-protected and thus read only
	Retry -> FAIL Writing  2     NV_VERNO_MAJ_I                                     Cause > Parameter is write-protected and thus read only
FAIL Writing  3     NV_VERNO_MIN_I                                     Cause > Parameter is write-protected and thus read only
	Retry -> FAIL Writing  3     NV_VERNO_MIN_I                                     Cause > Parameter is write-protected and thus read only
FAIL Writing  1943  NV_MEID_I                                          Cause > Parameter is write-protected and thus read only
	Retry -> FAIL Writing  1943  NV_MEID_I                                          Cause > Parameter is write-protected and thus read only
=================================== End of NV Restore  ===================================
[Writing NV] SUBPROCESS Completed!CBasicComControl::Close, the port(COM43) is closed successfully
[Rebooting] SUBPROCESS Completed!

กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ   Progress Count Info กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ

ขบ SubProcess NAME : [Writing NV          ], ขบ Expected SubProcess ProgressCount   679: ขบ Actual Executed StepItCount   679:
ขบ SubProcess NAME : [Rebooting           ], ขบ Expected SubProcess ProgressCount   150: ขบ Actual Executed StepItCount   150:

กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ กแ


-------------------Start Tracing Warning Level Log message -----------------------------

[//COMPONENT_INFO/LGNPST_COMPONENTS/ERS] xml node is not defined at setting.xml
PortOpen Success.
CBasicComControl::ChangeDataToDM  = 575.8 sys-time
Error! D:\Work\TDR\2006\LGNPST_RC\Basic_Unit\LGNPST_Utility\FileUtilCom.cpp [310]
	Failed to get the attributes of the file [C:\LG Electronics\LGNPST\model\vx8575\Backup\COM43_00000000].
FAIL Writing  0     NV_ESN_I                                           Cause > Parameter is write-protected and thus read only
	Retry -> FAIL Writing  0     NV_ESN_I                                           Cause > Parameter is write-protected and thus read only
FAIL Writing  2     NV_VERNO_MAJ_I                                     Cause > Parameter is write-protected and thus read only
	Retry -> FAIL Writing  2     NV_VERNO_MAJ_I                                     Cause > Parameter is write-protected and thus read only
FAIL Writing  3     NV_VERNO_MIN_I                                     Cause > Parameter is write-protected and thus read only
	Retry -> FAIL Writing  3     NV_VERNO_MIN_I                                     Cause > Parameter is write-protected and thus read only
FAIL Writing  1943  NV_MEID_I                                          Cause > Parameter is write-protected and thus read only
	Retry -> FAIL Writing  1943  NV_MEID_I                                          Cause > Parameter is write-protected and thus read only

-------------------End of Tracing Warning Level Log message 19 items-----------------------------
Error! D:\Work\TDR\2006\LGNPST_RC\Basic_Unit\LGNPST_Utility\FileUtilCom.cpp [310]
	Failed to get the attributes of the file [C:\LG Electronics\LGNPST\model\vx8575\Backup\COM43_00000000].
CComPort::ClosePort, the port is not open
CBasicComControl::Close, can not close the port
CPortHandler::Close, fail to close the port
Clear ALL NV Instance of NV Storage  Current Storage size=601736  
Successfully Clear NV Storage
