;=========================================================================
;                   LG Electronics Inc.
;                   CDMA Handsets Laboratory.
;                   Development Dept. 3
;=========================================================================
;-------------------------------------------------------------------------
;  when         version    Name     what
;-----------  ----------  ------------------------------------------------
;05/07/2008    VX970E46   jeyunpark Change browser file DB
;05/03/2008    VX970E46   jeyunpark Change and add skin file (VerizonStandardWQVGA.ows, VerizonStandardBlackWQVGA.ows)
;05/02/2008    VX970E46   jeyunpark Change and add skin file (VerizonStandardWQVGA.ows, VerizonStandardBlackWQVGA.ows)
;04/26/2008    VX970E44   jeyunpark Change browser file DB
;04/22/2008    VX970E44   jeyunpark Change and add skin file (VerizonStandardWQVGA.ows, VerizonStandardBlackWQVGA.ows)
;04/19/2008    VX970E44   jeyunpark Change and add skin file (VerizonStandardWQVGA.ows, VerizonStandardBlackWQVGA.ows)
;04/15/2008    VX970E41   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;04/03/2008    VX970E28   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;03/31/2008    VX970E28   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;03/28/2008    VX970E27   jeyunpark Change browser file DB
;03/27/2008    VX970E27   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;03/19/2008    VX970E26   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;03/18/2008    VX970E26   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;03/13/2008    VX970E24   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;03/12/2008    VX970E24   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;03/11/2008    VX970E24   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;03/05/2008    VX970E05   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;03/02/2008    VX970E05   jeyunpark Change browser file DB
;02/27/2008    VX970E05   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;02/26/2008    VX970E05   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;02/18/2008    VX970E05   jeyunpark Change browser file DB
;01/30/2008    VX970T02   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;11/20/2007    VX970T02   jeyunpark write browser file DB
;11/20/2007    VX970T02   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;11/16/2007    VX970T02   jeyunpark Change skin file (VerizonStandardWQVGA.ows)
;10/30/2007    VX970T02             first release
;01/28/2008    VX970T02             Add 3D contents
;----------    -------    ------------------------------------------------

mode offline-d
nv_read esn
nv_read verno_maj
nv_read verno_min
nv_read scm
nv_read slot_cycle_index
nv_read mob_firm_rev
nv_read mob_model

wait 2

;=========================================================================
; SYSTEM ITEM
;=========================================================================
nv_write sec_code                    {"000000"}                      ; Security code
nv_write lock_code                   {"0000"}                        ; Lock_code

nv_write min1                        {0, "000-0000", "000-0000"}     ; Min0 number
nv_write min1                        {1, "000-0000", "000-0000"}     ; Min1 number
nv_write min2                        {0, "000", "000"}               ; NAM 0 has one active MIN2,
nv_write min2                        {1, "000", "000"}               ; NAM 1

nv_write name_nam                    {0, "NAM1"}                     ; NAM 1 Name
nv_write name_nam                    {1, "NAM2"}                     ; NAM 2 Name

nv_write imsi_mcc                    {0, "310"}                      ; Mobile Country Code (000)
nv_write imsi_mcc                    {1, "310"}
nv_write imsi_11_12                  {0, "00"}                       ; Mobile Network Code
nv_write imsi_11_12                  {1, "00"}
;nv_write imsi_addr_num              {0, 0}
;nv_write imsi_addr_num              {1, 0}

nv_write imsi_t_mcc                  {0, "310"}
nv_write imsi_t_mcc                  {1, "310"}
nv_write imsi_t_11_12                {0, "00"}
nv_write imsi_t_11_12                {1, "00"}
nv_write imsi_t_s1                   {0, "000-0000", "000-0000"}
nv_write imsi_t_s1                   {1, "000-0000", "000-0000"}
nv_write imsi_t_s2                   {0, "000", "000"}
nv_write imsi_t_s2                   {1, "000", "000"}

nv_write dir_number_pcs              {0, "0000000000"}               ; NAM 0 : NV_DIR_NUMBER_PCS_I
nv_write dir_number_pcs              {1, "0000000000"}               ; NAM 1 : NV_DIR_NUMBER_PCS_I

print "Programming Primary CDMA Channel"
nv_write pcdmach                     {0, 283, 384}                   ; A and B primary CDMA channels
nv_write pcdmach                     {1, 283, 384}

print "Programming Secondary CDMA Channel"
nv_write scdmach                     {0, 691, 777}                   ; set only if secondary channels offered
nv_write scdmach                     {1, 691, 777}

nv_write home_sid_nid                {0,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535}
nv_write home_sid_nid                {1,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535,2004,65535}
nv_write sid_nid_lock                {0,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}
nv_write sid_nid_lock                {1,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535,0,65535}

nv_write mob_term_home               {0, true, true}
nv_write mob_term_home               {1, true, true}
nv_write mob_term_for_sid            {0, true, true}
nv_write mob_term_for_sid            {1, true, true}
nv_write mob_term_for_nid            {0, true, true}
nv_write mob_term_for_nid            {1, true, true}

nv_write accolc                      {0, 0, 0}
nv_write accolc                      {1, 0, 0}

nv_write slot_cycle_index            {2}

nv_write pref_voice_so               {0,  1, 0x0000, 0x0003, 0x0003} ; True, wildcard, EVRC, EVRC
nv_write pref_voice_so               {1,  1, 0x0000, 0x0003, 0x0003} ; True, wildcard, EVRC, EVRC

print "Programming Pref Mode"
nv_write pref_mode                   {0, "Digital Only"}
nv_write pref_mode                   {1, "Digital Only"}

nv_write voice_priv                  {1}                             ; 179 - 0=Standard  1=Enhanced  (1->0->1, by bhjo 02.08.28/09.06)

print "Programming Band Preferred"
nv_write band_pref                   {0, "pref_any"}
nv_write band_pref                   {1, "pref_any"}

print "Programming Roam Preferred"
nv_write roam_pref                   {0, "pref_any"}
nv_write roam_pref                   {1, "pref_any"}

nv_write hybrid_pref                 {1}                             ; 1 : hybrid on,  0 : hybrid off

nv_write system_pref                 {0, "automatic b"}              ; System preference, actually default to band preference
nv_write system_pref                 {1, "automatic b"}

print "Programming MRU table clear"
                                                                     ; except nam (first 0), '0' are 48(=4 X 12) times.
nv_write mru3_table                  {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write mru3_table                  {1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};

print "Programming NAM Checksums"
nv_write nam_chksum                  {0, 0xffff}
nv_write nam_chksum                  {1, 0xffff}
nv_write min_chksum                  {0, 0xffff, 0xffff}
nv_write min_chksum                  {1, 0xffff, 0xffff}

nv_write stand_alone_mode            {0}                             ; 0 default OFF, 1 ON
nv_write cdma_so68_enabled           {1}                             ;4GV
nv_write pref_for_rc                 {3}                             ; 1(RC1),2(RC2),3(RC3),4(RC4),5(RC5)  
;=========================================================================

;=========================================================================
; AUTH ITEM
;=========================================================================
nv_write a_key                       {0, 0x00000000, 0x00000000 }
nv_write a_key                       {1, 0x00000000, 0x00000000 }
nv_write ssd_a                       {0, 0x00000000, 0x00000000 }
nv_write ssd_a                       {1, 0x00000000, 0x00000000 }
nv_write ssd_b                       {0, 0x00000000, 0x00000000 }
nv_write ssd_b                       {1, 0x00000000, 0x00000000 }
nv_write count                       {0, 0}
nv_write count                       {1, 0}
;=========================================================================

;=========================================================================
; OTA ITEM
;=========================================================================
nv_write otapa_enabled               {0, 1}                          ; enable
nv_write otapa_enabled               {1, 1}                          ; enable
nv_write spc_change_enabled          {1}
nv_write nam_lock                    {0, 0}
nv_write nam_lock                    {1, 0}
;=========================================================================

;=========================================================================
; MSG ITEM
;=========================================================================
nv_write msg_settings_auto_save     	{0}                      ; MSG_AUTO_SAVE(0), MSG_DO_NOT_SAVE(1), MSG_PROMPT(2)
nv_write msg_settings_auto_delete   	{0}                      ; On(1), Off(0)
nv_write msg_settings_entry_mode    	{1}                      ; Word(0), Abc(1), ABC(2), 123(3)
nv_write msg_settings_vibrate_alert 	{0,0,0,0}                ; On(1), Off(0)
nv_write msg_settings_signature     	{0}                	 ; None(0), Custom(1)

;=========================================================================

;=========================================================================
; SMS/EMS ITEM
;=========================================================================
nv_write sms_txt_cb_enable      	{1}     		    ; On(1), Off(0) 
nv_write sms_orig_msg_id        	{1}     		    ; 0X0001 - 0XFFFF  
nv_write sms_mo_max_userdata		{160}			    ; support up to 220 bytes
nv_write sms_mo_l3_ack			{1}			    ; SMS_OFF(0), SMS_ON(1)
nv_write sms_mo_so			{1}			    ; SMS_SO14(0), SMS_SO6(1)
nv_write sms_voicemail_record   	{0,0}   		    ; {Count,Time}
nv_write sms_settings_direct_view    	{0}             	    ; Off(0), On(1)
nv_write sms_voicemail_alert         	{11}            	    ; 4(Door Bell), 5(VZW Default Tone), 6~17(Ringtone 1~12), 18(No Ring), 0xffff(Get New Ringtones)
nv_write sms_textmsg_alert           	{1}             	    ; 0(Low Beep Once),1(Low Beeps),2(Laud Beep Once),3(Loud Beeps)  
nv_write sms_voicemail_cb		{3,"*86"} 		    ; 20Byte(ASCII)
nv_write sms_urgent_voice_record     	{0}                         ; None(0), Exist(1) 
nv_write sms_2min_alert_sel          	{3,3,3,3}             	    ; Once(0), Every 2 Minutes(1), Every 15 Minutes(2), Off(3) 
nv_write sms_message_cb              	{10,"0000000000"}           ; 
;=========================================================================

;=========================================================================
; SMS/EMS ITEM
;=========================================================================
nv_write sms_settings_auto_play      	{0}                         ; On(1), Off(0)  
nv_write sms_ems_enable              	{1}                         ; On(1), Off(0)
;=========================================================================

;=========================================================================
; MMS ITEM 
;=========================================================================
nv_write mms_set_auto_receive        {1}                             ; 0(MMS_OFF), 1(MMS_ON)
nv_write mms_set_read_ack            {1}                             ; 0(ON), 1(OFF)
nv_write mms_set_delivery_ack        {0}                             ; 0(MMS_ON), 1(MMS_OFF)

nv_write mms_set_tone_alert          {1}                             ; 0(Low Beep Once), 1(Low Beeps), 2(Loud Beep Once), 3(Loud Beeps), 4(Door Bell), 5(VZW Default Tone), 6~25(Ringtone 1~20), 26(No Ring)
nv_write mms_set_vibrate_alert       {0}                             ; 0(VIBRATE OFF), 1(VIBRATE ON)
nv_write mms_set_reminder_alert      {3}                             ; 0(REMIND ONCE), 1(REMIND EVERY2MIN), 2(REMIND EVERY15MIN), 3(REMIND OFF)

nv_write mms_mmsc_url                {20, "http://mms.vtext.com"}    ; 48 byte characters
nv_write mms_mmsc_upload_url         {6, "438749"}                   ; Upload Address
;nv_write mms_mmsc_uaprof_url         {44, "http://uaprof.vtext.com/lg/vx10k/vx10kv1.xml"} ; 48 byte characters for 10k
nv_write mms_mmsc_uaprof_url         {44, "http://uaprof.vtext.com/lg/vx97k/vx97kv1.xml"} ; 48 byte characters

nv_write mms_set_retry_num           {0}                             ; 0, 1, 2, 3
nv_write mms_send_from_add           {2}                             ; MDN Only (0), 1MDN (1),  +1MDN (2)         

;nv_write mms_mmsc_user_agent         {7,"vx10kv1"}                  ; User Agent Profile name for 10k
nv_write mms_mmsc_user_agent         {8,"vx9700v1"}                  ; User Agent Profile name
nv_write mms_mmsc_server_post_url    {13, "/servlets/mms"}           ; Post URL
nv_write mms_mmsc_server_post_cgi    {12, "?message-id="}            ; CGI URL

nv_write mms_test_authorization      {0}                             ; 0 : Commercial, 1 : Lab
nv_write mms_test_mmsc_url           {20, "http://66.174.75.171"}    ; 48 byte characters
nv_write mms_test_mmsc_upload_url    {6, "666612" }                  ; Upload Address
;=========================================================================

;=========================================================================
; DATA ITEM
;=========================================================================
nv_write data_qnc_enabled       {0}                                  ; 0-QNC Disable  1-QNC Enable
nv_write data_so_set            {2}                                  ; DS_SO_SET_PRE707 =  0     IS-707.0 (pre-707) service option numbers
nv_write data_mdr_mode          {3}                                  ; DS_MDR_MODE_MDR_ONLY = 0  Use only MDR packet data services
nv_write data_pkt_orig_str {5, "#777"}                               ; {length,"dialstring"}  valu range 1-16   default value #777
nv_write data_auto_packet_detection {0}                              ; 0-Disable   1-Enable
nv_write ppp_carrier           {0}                                   ; 0-Verizon 1-USC
nv_write ppp_user_id {20,"0000000000@vzw3g.com"}                     ; Max of 127 chars in User ID
;remove the ppp password setting in script file. (Becuase ppp_password value is changed after DMU nego.)

nv_write data_scrm_enabled     {1}                                   ; 0-SCRM Disable 1-SCRM Enable
nv_write data_trtl_enabled     {1}                                   ; 0-TRTL Disable 1-TRTL Enable
nv_write ds_default_baudrate   {0x0011}                              ; 0x0000 (19.2kbps),0x0011(115kbps) ,0x00012(230.4kbps)
nv_write diag_default_baudrate {0x000e}                              ; 0x000e(38.4kbps), 0x0011(115kbps)
;Comment : VX9800 use EFS FILE instead of NV ITEM for packet amount
;nv_write used_packet_amount    {0,0,0,0,0,0}                        ; {TX used, TX remain, RX used, RX remain, used, remain}
nv_write ds_qcmip {1}                                                ; 0-SIP(MobileIP disable), 1-MIP preferred(Default Value), 2-MIP only
nv_write ds_mip_active_prof  {0}                                     ; current active profile index
nv_write ds_mip_enable_prof  {1,0,0,0,0,0}                           ; diable - 0, enable - 1
nv_write ds_mip_retries      {2}                                     ; number of retries
nv_write ds_mip_dereg_retries      {2}                               ; number of MIP Deregistration retries
nv_write ds_mip_retry_int    {3}                                     ; retry interval = n*250(ms) + 1000ms
nv_write ds_mip_pre_re_rrq_time {0}                                  ; pre-registration time - minute
nv_write ds_mip_num_prof     {1}                                     ; number of profiles (max 6) 
nv_write ds_mip_2002bis_mn_ha_auth  {1}                              ; disable - 0, enable -1
nv_write ds_mip_qc_drs_opt   {1}                                     ; dormant handoff optimization
;Comment : MIP general profile information {index, nai_length, nai, mn-ha spi-set, mn-ha spi, mn-aaa spi-set, mn-aaa spi,
;Comment : reverse tunneling, home address, primary ha address, secondary ha address}
nv_write ds_mip_gen_user_prof {0,20,"0000000000@vzw3g.com",1,300,1,2,1,0x00000000,0xffffffff,0xffffffff}
;Comment : MIP shared secret {index,mn-ha ss length,mn-ha ss,mn-aaa ss length,mn-aaa ss,
;remove the ds_mip_ss_user_prof setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;nv_write ds_mip_ss_user_prof {0,16,"testtesttesttes$",3,"vzw"}
nv_write ds_mip_dmu_pkoid    {0,10}                                  ; public key organization indentifier
nv_write ds_mip_dmu_mn_auth  {0,0x01,0xB2,0x07}                      ; { Index , DMU MN authenticator - 111111base10 }
nv_write hdr_an_auth_user_id_long {20,"0000000000@vzw3g.com"}        ; EVDO AN authetication user id
;Comment : remove the hdr_an_auth_passwd_long setting in script file. (Becuase it uses ppp_password value that changed after DMU nego.)
;nv_write hdr_an_auth_passwd_long  {3,"vzw"}                         ; EVDO AN authetication password

nv_write dun_cable_mode      {1}                                     ;0=disable cable dun,1=enable cable dun
nv_write dun_bt_mode         {1}                                     ;0=disable bt dun,1=enable bt dun

efs write "DMU/10.key"					             ; MIP DMU(Dynamic Mipkeys Update) key file

;Comment : MIP&SIP NAI(Network Access Identifier) for DUN 
nv_write ds_mip_rm_nai {0,24,"0000000000@dun.vzw3g.com"}             ; {index,nai_length,nai}            
nv_write ds_sip_rm_nai {24,"0000000000@dun.vzw3g.com"}               ; {nai_length,nai}

;CS DLL don't write this item
;remove the ppp password setting in script file. (Becuase ppp_password value is changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
nv_write ppp_password          {16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}      

;CS DLL don't write this item 
;{0~5(index),16(mn_ha_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,
;16(mn_aaa_ss_length),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
;remove the ds_mip_ss_user_prof setting in script file. (Becuase ppp_password value is changed after DMU nego.)
nv_write ds_mip_ss_user_prof {0,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}

;CS DLL don't write this item 
;Comment : remove the hdr_an_auth_passwd_long setting in script file. (Becuase it uses ppp_password value that changed after DMU nego.)
;{16(password_len),0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF,0x~0xFF}
nv_write hdr_an_auth_passwd_long  {16,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00}    
;=========================================================================

;=========================================================================
; BROWSER ITEM 
;=========================================================================
efs write "brew/mod/obigo/usr_data/skins/VerizonStandardWQVGA.ows"
efs write "brew/mod/obigo/usr_data/skins/VerizonStandardBlackWQVGA.ows"
efs write "brew/mod/obigo/ids/storage/S_0"
efs write "brew/mod/obigo/ids/storage/S_1"
efs write "brew/mod/obigo/ids/storage/S_2"
efs write "brew/mod/obigo/ids/storage/S_3"
efs write "brew/mod/obigo/ids/storage/S_4"
efs write "browser/setting/fileDB"
efs write "browser/setting/fileDBList"
efs write "browser/fileDBComplete"
;=========================================================================

;=========================================================================
; PIM ITEM
;=========================================================================
;efs write "pim/call_hist_nv.dat"                                    ;delete
;=========================================================================

;=========================================================================
;UI ITEM
;=========================================================================
;nv_write bt_audio_auto_pair          {1}                             ; 5002 - 1(ON), 0(OFF)
nv_write call_sounds                 {5,5,5,5,0}                     ; 5004 - {Caller ID (5: VZW Default Tone), No Caller ID (9: Ringtone 5), Restrict Calls (6: Ringtone 2), All Calls (5: VZW Default Tone), Vibrate (0: Off, 1: On)}
nv_write ringer_lvl                  {0x4}                           ; 64 - 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 99(Vibrate only=manner_mode), 97(alarm only), 100(Sounds Off=silence_all)
nv_write ringer_spkr_lvl             {0x4}                           ; 229 - 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 98(High & Vib), 99(Vibrate)
nv_write beep_lvl                    {0x4}                           ; 65 - 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) handset(earjack) vol
nv_write beep_lvl_shadow             {0x4}                           ; 164 - 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) headset(earpiece) vol
nv_write beep_spkr_lvl               {0x4}                           ; 230 - 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) - carkit vol
nv_write spk_phone_beep_lvl          {0x4}                           ; 5049 - 0(Off), 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High) - Keypad Volume on Speaker Phone Mode
nv_write ear_lvl                     {0x6}                           ; 62 - Low(Volume 1)~ High(Volume 8)
nv_write ear_lvl_shadow              {0x6}                           ; 165 - Low(Volume 1)~ High(Volume 8)
nv_write speaker_lvl                 {0x6}                           ; 63 - Low(Volume 1)~ High(Volume 8) - carkit vol
nv_write backtop_beep                {true}                          ; 5029 - Back To Top Sound == on       
nv_write power_onoff_sounds          {1,1}                           ; 5003 - {Power On, Power Off}, On (1), Off (0)
nv_write banner                      {""}                            ; 71 - Banner - default blank, because confuse Banner with ERI text
nv_write sub_banner                  {""}                            ; 5047 - Sub Banner - default blank, because VX9400 doesn't have sub LCD.
nv_write eri_text_onoff              {1}                             ; 5050 - 1 -> On, 0 -> Off
nv_write back_light                  {30}                             ; 77 - Backlight
nv_write sub_backlight               {30}                             ; 5022 - Sub Backlight
nv_write key_light                   {30}                             ; 5007
nv_write wallpaper_main              {0,0,3}                         ; 5061 - {location_type, location_id, item_id}
nv_write wallpaper_sub               {1,6,53}                         ; {location_type , location_id, item_id}
nv_write number_size                 {0,0}                           ; 5025 - (size, color(don't use)) 0:normal 1:large //lej 2006.10.25 Large -> Normal
nv_write curr_nam                    {0}                             ; Current NAM           == NAM1
nv_write auto_nam                    {off}                           ; Auto NAM              == disable
nv_write location_set_lock           {0}                             ; 1 -> location on 0-> E911 only
nv_write auto_lock                   {off}                           ; phone lock            == Unlocked \ Power_up
nv_write lock                        {off}                           ; phone lock            == Unlocked \ now
nv_write emergency_num1              {"911"}                         ; 5026 - Up to 48 Digits
nv_write emergency_num2              {"*911"}                        ; 5027 - Up to 48 Digits
nv_write emergency_num3              {"#911"}                        ; 5028 - Up to 48 Digits
nv_write gps_test_num			    {"000"}				; GPS Test Num
nv_write language_selection          {0}                             ; 227 - Default (English/Spanish) == English
nv_write answer_option               {2}                             ; 5015 - Answer option
nv_write auto_answer                 {0, 0}                          ; Auto answer           == off
nv_write end_option            	     {1}                             ; 5017 - End call_option
nv_write auto_redial                 {0, 0}                          ; Auto redial           == off
nv_write tty                         {3}                             ; 409 - TTY Full(0), TTY+TALK(1),TTY+HEAR(2),TTY off(3)
nv_write onetouch_dial               {on}                            ; One touch dial        == disable!
nv_write shortcut_main               {2,4,0,15}                      ; 5077 - {Left, Up, Right, Down}
nv_write call_rstrc                  {0x00}                          ; Restrict(0:off, 1:on) 
;nv_write bt_power_onoff              {0}                             ; 5059 - 1 -> On, 0 -> Off
;nv_write beep_bt_lvl                 {0x4}                           ; 5064 - 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High)
;nv_write ear_bt_lvl                  {12}                           ; 5065 - 1(Low), 2(Medium Low), 3(Medium), 4(medium High), 5(High), 6(High), 7(High)
nv_write media_save_option           {0,0,0}                         ; 5063 - 	media_save_option{pix_save_location(0 : phone memory 1: sdcard) ,flix_save_location(0 : phone memory 1: sdcard) ,sound_save_location(0 : phone memory 1: sdcard) }
nv_write alarm_sounds                {6,0}                           ; {tone(6: Ringtone 2), vibrate (0: Off)}

nv_write fsc                         {"000000"}                      ; Field Service code
nv_write auto_volume_enabled         {0}                             ; 0-> off , 1-> on
nv_write cont_key_dtmf               {1}                             ; Prssed key tone       == 1: Normal, 0: Long  2: Off  (NEW)
nv_write send_pin                    {off}                           ; Send pin?             == disable!
;nv_write carrier_logo                {0}                             ; 0 -> Verizon, 
nv_write avr_call_alerts             {0}                             ; 5072
nv_write avr_prompts_mode            {0}                             ; 5073
nv_write avr_choice_list             {0}                             ; 5074
nv_write avr_prompts_timeout         {0}                             ; 5075
nv_write avr_sensitivity             {1}                             ; 5076
nv_write avr_digit_dial_readout      {0}                             ; 0 : Off, 1: On
nv_write avr_audio_playback          {0}                             ; 0 : Speakerphone, 1: Earpiece

;nv_write sound_ringers               {4,9,6,0xFFFF,0}                ; (caller ID, No Caller ID, Restrict, all calls, vibrate options) added item 4th & 5th 2003.11.30 ;KHW 2004.06.16 MODIFY in NJ

nv_write silence_all                 {0}                             ; 5004 - sound on   {1} sound off
nv_write edit_font                   {0,0} 
nv_write manner_mode                 {0}                             ; 5024 - false {0}, true {1}

; nv_write backtop_beep               {1}

nv_write wclock_choice               {30,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,47,0}
;                                    5016 - {cur_Itm (30), Set_DST, choice_city ( NewYork: 47), line longtitude}
;nv_write stack_idx                   {0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff} ; call history clear

nv_write power_saver                 {0}
nv_write alarm_only_mode             {0}                             ; 5048 - 0 -> Disable, 1 -> Enable
nv_write camera_flash_test           {0}                             ; 0 : Normal, 0x55 : For Manufacture

;nv_write bd_addr                    {0x9a,0xbc,0x56,0x78,0x12,0x34} ; Bluetooth Address

nv_write pc_port                     {0}                             ; 5067 - PC connection port  0 (USB), 1 (UART), 2 (BLUETOOTH), 3 (CLOSED)
;nv_write key_guard_set               {30}                            ; key_guard   0(Always off)  7( 7 Seconeds)  30( 30 Seconeds)  120( 2 Min)
;nv_write keyguard_release_options    {0}                             ; keyguard options   0(Press Once)  1(Press Twice) //lej 2006.09.20
nv_write equalizer_mode              {1}                             ; 0(flat) , 1(3D Surround) ,2 (Concert Hall) , 3 (Rock) , 4 (Jazz)  , 5 (POP) , 6 (Classical) 
nv_write visualizer_mode             {0}                             ; 0 enable   ,  1 disable
;nv_write use_mymp3                   {1}                             ; 0 : MUSIC_NONE,   1 : MUSIC_MP3_ONLY,   2 : MUSIC_MOD_ONLY,     3 : MUSIC_MP3_MOD
nv_write call_form_style           {0}                             ; 0 Voicemail/Toll-Free, 1 Always, 2 Never
nv_write lg_wdc                      {0,0,0,0,0}
nv_write  mf_mru_chan                {4980}

nv_write vp_spkr_lvl                 {0x6}                          ; Low(Volume1)~ High(Volume8)
nv_write vp_lvl_shadow	             {0x6}	            	          ; Low(Volume1)~ High(Volume8)
nv_write vp_bt_lvl                   {0x6}	             	          ; Low(Volume1)~ High(Volume8)
nv_write vp_spkr_shadow_lvl          {0x6}	             	          ; Low(Volume1)~ High(Volume8)
nv_write vp_lvl	                     {0x6}	             	          ; Low(Volume1)~ High(Volume8)
nv_write dual_nam_set_enable         {1}                            ; Enable(1)/Disable(0)
nv_write vibrate_factory_test        {0}	             	            ; TRUE(1), FALSE(0)

nv_write music_only_mode             {0}                            ; 0 default OFF, 1 ON
nv_write display_set                 {0,0,0}                        ; 5009 (Sub Clock, Main Clock, Theme)

nv_write service_num                 {"611"}                        ; Up to 48 Digits
nv_write set_touch                   {1,0,0,1,0}                    ; 5097 - (Auto Lock, Sensitivity, Vib Type, Vib Level, Sound)
nv_write set_menu_fonts              {0}                            ; 5099
nv_write set_usb_auto_detection      {1}                            ; 5100
nv_write sound_alerts                {0,0,0,0}                      ; 5006 
nv_write charging_alert_onoff        {0}                            ; 5092 
nv_write screen_saver                {0,0}                          ; 5081 
nv_write emergency_tone_set			     {2}                          	; 5456 - 0(Alert) ,1(Vibrate) ,2(Off)
nv_write set_shortcut_type           {1}                            ; 5462 - 0 0ff, 1 On
nv_write avr_key_type                {1}                            ; 5463 - 0 off, 1 On
nv_write set_banner_color            {0}                            ; 5460 - 0 Black
nv_write handwriting_setup            {0,0,0,0}                            ; 5464 - handwriting
nv_write set_clock_position          {12, 220, 77, 286, 52, 142, 186, 276, 6, 240, 135, 311, 6, 240, 135, 311, 6, 255, 229, 309, 6, 255, 229, 309, 6, 215, 192, 311}
nv_write set_touch_shortcut          {0, 15, 1, 2, 3, 4, 5, 16, 7, 8, 9, 10, 11}
;=========================================================================

;=========================================================================
;F/W ITEM
;=========================================================================
;nv_write ftm_mode {1}                                               ; ystk 2003.10.06 - for Initial Booting Mode to DMSS mode!
;nv_write fm_rssi {0x2c, 0x7f}                                       ; modify {0x4a, 0x77} -> {0x2c, 0x7f};hkshin 200.10.28 - for hw request
nv_write rf_config {6}
;nv_write lcd {39}                                                   ; don't use for VX8100
;hkshin 200.10.28 - for hw request
nv_write vbatt {138, 210}
nv_write batt_threshold {142, 123, 106, 71, 22, 11}
nv_write charger_vbatt_complete {1, 15, 192}

;nv_write cdma_rx_comp_vs_freq { -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12, -12 }
;nv_write pcs_rx_comp_vs_freq  { -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10, -10 }
;nv_write elapsed_time {59}

; modified by Heo Si Hang
;nv_write qdsp_snd_ctrl {0,0,0,49149,1280,0,190,22,31,6,6,0,0,19,6,0};
;nv_write audio_adj_phone             {0, 0, 0, 0, 0, 0, 0, 0, 0}
;nv_write audio_adj_earjack {0, 0, 0, 0, 0, 0, 0, 0, 0}
;nv_write audio_adj_spk {0,0,0,0,0,0,0,0,0}
;nv_write rx_pcm_filter_ctrl {0x7, 0x2, 0xFFF9, 0x213, 0x742, 0x1020, 0x3120}
;nv_write tx_pcm_filter_ctrl {0xb, 0xFFF4, 0xFFA6, 0xFF2B, 0xFD31, 0xF883, 0x48C3}
;nv_write qdsp_agc_ctrl{ 0x2000,0x0,0x780,0xFF52,0x1D00,0xF333,0,0,0x2000,0x0,0x780,0xFF52,0x2580,0xF333}
;nv_write charging_bypass_boot {0}

nv_write AUDIO_CODEC_GAIN {0,0,0,0,0,0,0,0,0}; 
nv_write AUDIO_VOC_GAIN {0,0,0,0,0,0,0,0,0,0}; 
nv_write AUDIO_AGC {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0};
nv_write AUDIO_RX_FIR_PCM_FILTER {0,0,0,0,0,0,0,0};
nv_write AUDIO_TX_FIR_PCM_FILTER {0,0,0,0,0,0,0,0};
nv_write AUDIO_QDSP {0,0,0,0,0,0,20,0,7,7,0,0,0,0,0,0,0,0,1,1};	
;nv_write proximity_adc {220}
;nv_write AUDIO_ASE {0}  	;Adaptive Speech Enhancement
;nv_write touch_cal_data	{0,0,0,0}; set to all 0 for User Calibration start
;nv_write factory_mode {0}
nv_write proxi_disable{0};
nv_write manual_test_mode{0};

;FW GPS NV ITEMS
;nv_write gps1_capabilities {1}	; Verizon Requset for LBS
;nv_write GPS1_DYNAMIC_MODE {0}	
;=========================================================================

;=========================================================================
;BREW ITEM modified by Kim sungkung
;=========================================================================
nv_write brew_bkey {0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00} 
nv_write brew_download_flags {0x0004}                           ; 
nv_write brew_auth_policy {1}                             ; 
nv_write brew_privacy_policy {3}                            ;
nv_write brew_carrier_id {200}                          ; 
nv_write brew_server    {"apps.myvzw.com,apps2.myvzw.com"}      ; 64 byte character
nv_write brew_platform_id {1233}			;VX9700 PID
;nv_write brew_disallow_dormancy {1}			; TRUE
nv_write brew_sid_length {32}		
;nv_write mflo_enable {1}                                             ; 0:OFF, 1:ON //lej 2006.10.26
nv_write testmode_alc     {0}    ;  0: high en false   1 : high en true
nv_write ALC_CONTROL {0,0,28,4,0,5,5,13,4 }
;=========================================================================


;lej 2006.09.07 default img efs·Î
;=========================================================================
;WALLPAPER DEFAULT IMAGE ITEM
;=========================================================================
;efs write "dload/default_img/wallpaper_3_320x204.bmp"
;efs write "dload/default_img/wallpaper_4_320x204.bmp"
;efs write "dload/default_img/wallpaper_5_320x204.bmp"
;efs write "dload/default_img/wallpaper_6_320x204.bmp"
;efs write "dload/default_img/wallpaper_7_320x204.bmp"
;efs write "dload/default_img/wallpaper_8_320x204.bmp"
;efs write "dload/default_img/wallpaper_3_240x284.bmp"
;efs write "dload/default_img/wallpaper_4_240x284.bmp"
;efs write "dload/default_img/wallpaper_5_240x284.bmp"
;efs write "dload/default_img/wallpaper_6_240x284.bmp"
;efs write "dload/default_img/wallpaper_7_240x284.bmp"
;efs write "dload/default_img/wallpaper_8_240x284.bmp"

;lkg 031002 added eri sound.
;=========================================================================
;ERI SOUND ITEM
;=========================================================================
efs write "eri_sound/extendednetwork.qcp"
efs write "eri_sound/lossofservice.qcp"
efs write "eri_sound/roaming.qcp"
efs write "eri_sound/verizonwireless.qcp"

;HKSHIN 2003.12.19
;=========================================================================
;MMS IMAGE ITEM
;=========================================================================

;HKSHIN 2003.12.19
;=========================================================================
;MMS SOUND ITEM
;=========================================================================

;Kim HyunWoo 2005.02.12
;=========================================================================
;ANIMATION IMAGE ITEM
;=========================================================================
;efs write "dload/mainOpening1.jpg"
;efs write "dload/mainOpening2.jpg"
;efs write "dload/subOpening1.jpg"
;efs write "dload/subOpening2.jpg"
;efs write "dload/mainClosing1.jpg"
;efs write "dload/mainClosing2.jpg"
;efs write "dload/subClosing1.jpg"
;efs write "dload/subClosing2.jpg"


;=========================================================================
; DCAMERA ITEM
;=========================================================================
efs write "dload/dcammenu.dat"
efs write "dload/default_img/DecodeErrorAnimation.jpg"
efs write "dload/default_img/DecodeErrorImage.jpg"
efs write "dload/default_img/NotSupportedImage_UnknownImage.jpg"
efs write "dload/default_img/phoneOnConversation.jpg"
efs write "dload/default_img/TooBigErrorImage.jpg"
efs write "dload/default_img/video_FirstFrame_PMD.jpg"
efs write "dload/default_img/video_FirstFrame_SVG.jpg"
efs write "dload/default_img/VideoImageSymbol.jpg"



;=========================================================================

;=========================================================================
; SHUTTER SOUND 
;=========================================================================
;efs write "dload/shutter1.wav"
;efs write "dload/shutter2.wav"
;efs write "dload/saycheese.wav"
;efs write "dload/ready123.wav"
;=========================================================================

;=========================================================================
; VIDEO SOUND 
;=========================================================================
;efs write "dload/videostart.wav"
;efs write "dload/videoend.wav"

;=========================================================================
; 2005.06.02 thunder - TTS 
;=========================================================================
; TTS ITEM  2008.03.11 Deleted by Red : moved to the resource partition
;=========================================================================
;efs write "mTalk/sms_etts.cnt"
;efs write "mTalk/sms_etts.dat"
;efs write "mTalk/sms_etts.etc"
;efs write "mTalk/sms_etts.hdx"
;efs write "mTalk/sms_etts.idx"
;efs write "mTalk/sms_etts.key"
;=========================================================================

; AVR SEARCHING PLAY NAME	;2008.01.07 Red
efs write "mVoice/dict/dict_en.080213.dat"
efs write "mVoice/dict/dictinfo_en.080213.dat"

;=========================================================================
;GPSONE ITEM added in 2005-03-04
;=========================================================================
nv_write gps1_lock {3}

nv_write gps1_pde_address {0,0,0,0}
nv_write gps1_pde_port {0}
;=========================================================================


;=========================================================================
; Flash UI ITEM
;=========================================================================
efs write "flash/ui/wallpaper/wallpaperType1.swf"
efs write "flash/ui/wallpaper/wallpaperType2.swf"
efs write "flash/ui/wallpaper/wallpaperType3.swf"
efs write "flash/ui/wallpaper/wallpaperType4.swf"
efs write "flash/ui/wallpaper/wallpaperType5.swf"
efs write "flash/ui/wallpaper/wallpaperType6.swf"
efs write "flash/ui/wallpaper/wallpaperType7.swf"
;efs write "flash/ui/tools/ezTipType1Main.swf"
efs write "flash/ui/tools/ezTipType1.swf"
;efs write "flash/ui/tools/worldClockType1Main.swf"
efs write "flash/ui/tools/worldClockType1.swf"
;efs write "flash/ui/menu/topMenuType1Color1Sub.swf"
;efs write "flash/ui/menu/topMenuType1Color2Sub.swf"
;efs write "flash/ui/menu/subMenuType1Color1Sub.swf"
;efs write "flash/ui/menu/subMenuType1Color2Sub.swf"
;efs write "flash/ui/widget/widget.swf"
;efs write "flash/ui/widget/widget1.swf"
;efs write "flash/ui/widget/widget2.swf"
;efs write "flash/ui/widget/widget3.swf"
;efs write "flash/ui/widget/widgetCalandar1.swf"
;efs write "flash/ui/startup/startUpType1.swf"


;=========================================================================
; UIEngine ITEM
;=========================================================================
efs write "uiengine/bg_gray_1.lki"
efs write "uiengine/bg_gray_2.lki"
efs write "uiengine/bg_gray_3.lki"
;
;  [Mainmenu Resource]
;
efs write "uiengine/reset.lki"
efs write "uiengine/reset_span.lki"
efs write "uiengine/select.lkt"
efs write "uiengine/select_bk.lkt"
efs write "uiengine/browser.lki"
efs write "uiengine/browser_span.lki"
efs write "uiengine/browser_bk.lki"
efs write "uiengine/browser_bk_span.lki"
efs write "uiengine/contacts.lki"
efs write "uiengine/contacts_span.lki"
efs write "uiengine/contacts_bk.lki"
efs write "uiengine/contacts_bk_span.lki"
efs write "uiengine/mediacenter.lki"
efs write "uiengine/mediacenter_span.lki"
efs write "uiengine/mediacenter_bk.lki"
efs write "uiengine/mediacenter_bk_span.lki"
efs write "uiengine/messaging.lki"
efs write "uiengine/messaging_span.lki"
efs write "uiengine/messaging_bk.lki"
efs write "uiengine/messaging_bk_span.lki"
efs write "uiengine/music.lki"
efs write "uiengine/music_span.lki"
efs write "uiengine/music_bk.lki"
efs write "uiengine/music_bk_span.lki"
efs write "uiengine/navigator.lki"
efs write "uiengine/navigator_span.lki"
efs write "uiengine/navigator_bk.lki"
efs write "uiengine/navigator_bk_span.lki"
efs write "uiengine/recentcalls.lki"
efs write "uiengine/recentcalls_span.lki"
efs write "uiengine/recentcalls_bk.lki"
efs write "uiengine/recentcalls_bk_span.lki"
efs write "uiengine/settingstools.lki"
efs write "uiengine/settingstools_span.lki"
efs write "uiengine/settingstools_bk.lki"
efs write "uiengine/settingstools_bk_span.lki"
efs write "uiengine/vcast.lki"
efs write "uiengine/vcast_span.lki"
efs write "uiengine/vcast_bk.lki"
efs write "uiengine/vcast_bk_span.lki"
;
;  [Favorite Resource]
;
efs write "uiengine/bottom_bar.lki"
efs write "uiengine/fav_notice_en.lki"
efs write "uiengine/fav_notice_sp.lki"
efs write "uiengine/friend_frame.lkt"
efs write "uiengine/fav_btn_call.lki"
efs write "uiengine/fav_btn_call_ds.lki"
efs write "uiengine/fav_btn_sms.lki"
efs write "uiengine/fav_btn_sms_ds.lki"
efs write "uiengine/fav_btn_contact.lki"
efs write "uiengine/fav_btn_contact_ds.lki"
efs write "uiengine/fav_btn_plus.lki"
efs write "uiengine/fav_btn_plus_ds.lki"
efs write "uiengine/fav_btn_minus.lki"
efs write "uiengine/fav_btn_minus_ds.lki"
;
;  [MP3 Resource]
;
efs write "uiengine/mp3_album_up.lkt"
efs write "uiengine/mp3_album_down.lkt"
efs write "uiengine/background_horizontal1.lki"
efs write "uiengine/background_horizontal2.lki"
efs write "uiengine/background_horizontal3.lki"
efs write "uiengine/background_horizontal4.lki"
efs write "uiengine/background_reverse_horizontal1.lki"
efs write "uiengine/background_reverse_horizontal2.lki"
efs write "uiengine/background_reverse_horizontal3.lki"
efs write "uiengine/background_reverse_horizontal4.lki"
efs write "uiengine/background_vertical1.lki"
efs write "uiengine/background_vertical2.lki"
efs write "uiengine/background_vertical3.lki"
efs write "uiengine/background_vertical4.lki"
efs write "uiengine/background_reverse_vertical1.lki"
efs write "uiengine/background_reverse_vertical2.lki"
efs write "uiengine/background_reverse_vertical3.lki"
efs write "uiengine/background_reverse_vertical4.lki"

;=========================================================================
;FOTA mgmttree files / cert
;=========================================================================
efs write "otadm/mgmttree.bin"
efs write "otadm/omadlc.ini"
efs write "cert/Verisign_Public_Primary.cer"
;=========================================================================


mode reset
