MIPT_SET_PULSE_TRAIN_REQ
  device DEC 4 pulse_train_id DEC 4 ser_no UDEC 1 high_priority UDEC 1 UNUSED PAD 2  0
MIPT_SET_ICON_REQ
  icon_id DEC 4 icon_state DEC 4 high_priority UDEC 1 UNUSED PAD 3  0
MIPT_ANIMATION_CONTROL_REQ
  Param1{ animation_spec{ code UDEC 2 font UDEC 1 UNUSED PAD 1 } animation_type DEC 4 
  command DEC 4 }  0
PTMI_PULSE_TRAIN_COMPLETE_IND
  ser_no UDEC 1  0
PTMI_ANIMATION_COMPLETE_IND
  animation_spec{ code UDEC 2 font UDEC 1 UNUSED PAD 1 } animation_type DEC 4  0
PTCMAN_PTCLED_PT_REQ
  pulse_train_id DEC 4 ser_no UDEC 1 high_priority UDEC 1 UNUSED PAD 2  0
PTCLED_PTCMAN_PT_COMPLETE_IND
  Param1{ ser_no UDEC 1 }  0
PTCMAN_PTCVIB_PT_REQ
  pulse_train_id DEC 4 ser_no UDEC 1 high_priority UDEC 1 UNUSED PAD 2  0
PTCVIB_PTCMAN_PT_COMPLETE_IND
  Param1{ ser_no UDEC 1 }  0
PTCMAN_PTCBLT_PT_REQ
  pulse_train_id DEC 4 ser_no UDEC 1 high_priority UDEC 1 UNUSED PAD 2  0
PTCBLT_PTCMAN_PT_COMPLETE_IND
  Param1{ ser_no UDEC 1 }  0
PTCMAN_PTCLCD_PT_REQ
  pulse_train_id DEC 4 ser_no UDEC 1 high_priority UDEC 1 UNUSED PAD 2  0
PTCMAN_PTCLCD_FLASH_ITEM_REQ
  flash_icon DEC 4 flash_off_to DEC 4 flash UDEC 1 UNUSED PAD 3  0
PTCLCD_PTCMAN_PT_COMPLETE_IND
  Param1{ ser_no UDEC 1 }  0
PTCMAN_PTCBAT_ANIMATION_REQ
  Param1{ animation_spec{ code UDEC 2 font UDEC 1 UNUSED PAD 1 } animation_type DEC 4 
  command DEC 4 }  0
z00N_AUST_AUDIO_INFORMATION
  Param1{ hfk_speaker DEC 4 hfk_mic DEC 4 hfk_no_echo DEC 4 hfk_volume DEC 4 
  hfk_alert DEC 4 }  0
z00O_AUL1_AUDIO_INFORMATION
  Param1{ tone_volume DEC 4 tone_action DEC 4 audconf DEC 4 side_shift DEC 4 
  freq1_sin DEC 4 freq1_cos DEC 4 freq2_sin DEC 4 freq2_cos DEC 4 
  tone_timing{ A ARRAY 6 [ TONE_TIMING DEC 4 ] } }  0
MMI_TUNE_ENDED
  Param1{ tuneid DEC 4 }  0
AU_CONTROL_CONNECTION
  Param1{ dir DEC 4 dnvol DEC 4 dev DEC 4 aec UDEC 1 UNUSED PAD 3 }  0
AU_DEVICE_CONFIG
  Param1{ dev DEC 4 part DEC 4 }  0
AU_ICO_CONTROL
  Param1{ ICOPseudoDedicatedMode UDEC 1 }  0
AU_CONTROL_TUNE
  Param1{ tuneid DEC 4 tunevol DEC 4 dev DEC 4 mix UDEC 1 UNUSED PAD 3 auxvol DEC 4 }  0
AU_CONTROL_LOOPBACK
  Param1{ src DEC 4 dest DEC 4 dnvol DEC 4 }  0
EFCE_RESPONSE
  src DEC 4 dest DEC 4 dnvol DEC 4  0
BMSM_SET_CHARGE_MODE_NTF
  Param1{ ChargeCommand DEC 4 }  0
SMBM_HFK_STATUS_IND
  Param1{ Status DEC 4 identity DEC 4 }  0
SMBM_CHARGING_STATE_IND
  Param1{ ChargingStatus DEC 4 }  0
HHBM_A_D_READINGS
  Param1{ ReadMask UDEC 1 UNUSED PAD 1 Readings{ A ARRAY 5 [ READINGS UDEC 2 ] } }  0
BMMI_BATTERY_STATUS
  Param1{ Status DEC 4 }  0
BMMI_BATTERY_LEVEL
  Param1{ ChargeLevel DEC 4 }  0
BMMI_CHARGING_PROGRESS
  Param1{ ChargingLevel DEC 4 }  0
PSSICC_ALERT_REQ
  Param1 LIB 1  0
PSSICC_CALL_CONF_REQ
  Param1 LIB 1  0
PSSICC_DISC_REQ
  Param1 LIB 1  0
PSSICC_FACILITY_REQ
  Param1 LIB 1  0
PSSICC_HOLD_REQ
  Param1 LIB 1  0
PSSICC_RETRIEVE_REQ
  Param1 LIB 1  0
PSSICC_MODIFY_ACCEPT
  Param1 LIB 1  0
PSSICC_MODIFY_REQ
  Param1 LIB 1  0
PSSICC_NOTIFY_REQ
  Param1 LIB 1  0
PSSICC_REJ_REQ
  Param1 LIB 1  0
PSSICC_REL_REQ
  Param1 LIB 1  0
PSSICC_REL_RSP
  Param1 LIB 1  0
PSSICC_SETUP_REQ
  Param1 DEC 4 Param2 LIB 1  0
PSSICC_SETUP_RSP
  Param1 LIB 1  0
PSSICC_START_DTMF_REQ
  Param1 LIB 1  0
PSSICC_STOP_DTMF_REQ
  Param1 LIB 1  0
PSSICC_START_CC_REQ
  Param1 LIB 1  0
PSSICC_CC_EST_CONF_REQ
  Param1 LIB 1  0
PSSICC_USER_INFO_REQ
  Param1 LIB 1  0
PSSICC_ALERT_IND
  Param1 LIB 1  0
PSSICC_CALL_PROC_IND
  Param1 LIB 1  0
PSSICC_DISC_IND
  Param1 LIB 1 Param2 DEC 4  0
PSSICC_FACILITY_IND
  Param1 LIB 1  0
PSSICC_HOLD_CNF
  Param1 LIB 1  0
PSSICC_HOLD_REJ
  Param1 LIB 1 Param2 DEC 4  0
PSSICC_MODIFY_CNF
  Param1 LIB 1 Param2 DEC 4  0
PSSICC_MODIFY_IND
  Param1 LIB 1  0
PSSICC_NOTIFY_IND
  Param1 LIB 1  0
PSSICC_PROGRESS_IND
  Param1 LIB 1  0
PSSICC_REJ_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
PSSICC_REL_CNF
  Param1 LIB 1 Param2 DEC 4  0
PSSICC_REL_IND
  Param1 LIB 1 Param2 DEC 4  0
PSSICC_RETRIEVE_CNF
  Param1 LIB 1 Param2 DEC 4  0
PSSICC_SETUP_COMPLETE_IND
  Param1 DEC 4  0
PSSICC_SETUP_CNF
  Param1 LIB 1  0
PSSICC_SETUP_IND
  Param1 LIB 1  0
PSSICC_START_DTMF_CNF
  Param1 LIB 1 Param2 DEC 4  0
PSSICC_STOP_DTMF_CNF
  Param1 LIB 1 Param2 DEC 4  0
PSSICC_SYNC_IND
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1  0
PSSICC_STATUS_IND
  Param1 DEC 4 Param2 DEC 4  0
PSSICC_PROMPT_IND
  Param1 DEC 4  0
PSSICC_CC_EST_IND
  Param1 LIB 1  0
PSSICC_RECALL_IND
  Param1 LIB 1  0
PSSICC_USER_INFO_IND
  Param1 LIB 1  0
PSSICC_CONG_CON_IND
  Param1 LIB 1  0
L1_READ_DCCH
  Param1 UDEC 1  0
L1_READ_SACCH
  Param1 UDEC 1  0
L1_RADIO_FRAME
  Param1{ A ARRAY 23 [ RADIO_FRAME UDEC 1 ] }  0
PH_CONNECT_IND
  Param1 UDEC 1  0
PH_DATA_IND
  Param1{ A ARRAY 23 [ RADIO_FRAME UDEC 1 ] }  0
OML1_CLOSE_TCH_LOOP_REQ
  sub_channel UDEC 1 loop_mode UDEC 1  0
OML1_START_DAI_TEST_REQ
  tested_device UDEC 1  0
MPH_MEAS_REPORT
  dtx_used UDEC 1 meas_valid UDEC 1 rxlev_full UDEC 1 rxlev_sub UDEC 1 
  rxqual_full UDEC 1 rxqual_sub UDEC 1 no_of_ncell_meas UDEC 1 
  UNUSED PAD 1 ncell_meas{ A ARRAY 6 [ A{ bcch_freq UDEC 2 bsic UDEC 1 rxlev UDEC 1 } ] } 
  no_of_fdd_ncell_meas UDEC 1 
  fdd_ncell_meas{ A ARRAY 6 [ A{ index_into_3g_ba_list UDEC 1 reported_value UDEC 1 } ] } UNUSED PAD 1  0
MPH_ENH_MEAS_REPORT
  dtx_used UDEC 1 scell_meas_valid UDEC 1 rxlev_val UDEC 1 rxqual_full UDEC 1 
  mean_bep DEC 4 cv_bep DEC 4 nbr_rcvd_blocks DEC 4 
  ncell_enh_meas{ BaUsed DEC 4 ThreeGBaUsed DEC 4 BsicSeen UDEC 1 scale UDEC 1 NumRepInvBSICInfo UDEC 1 
  UNUSED PAD 1 RepInvBSICInfoFreqs{ A ARRAY 9 [ A{ bcch_freq UDEC 2 bsic UDEC 1 rxlev UDEC 1 } ] } 
  NumRepeatedQty UDEC 1 NumRepValBSICInfo UDEC 1 
  ReportingQty{ A ARRAY 24 [ A{ radio_freq_no UDEC 2 rxlev UDEC 1 UNUSED PAD 1 } ] } 
  FddMeas{ A ARRAY 24 [ A{ index_into_3g_ba_list UDEC 1 reported_value UDEC 1 } ] } 
  FddMeasCnt UDEC 1 UNUSED PAD 1 }  0
MPH_DED_EXT_MEAS_REPORT_CNF
  Param1 UDEC 1 Param2 UDEC 1 Param3 UDEC 1 
  UNUSED PAD 1 Param4{ A ARRAY 32 [ A{ bcch_freq UDEC 2 bsic UDEC 1 rxlev UDEC 1 } ] }  0
MPH_BLIND_HO_REJ
  Param1 UDEC 1  0
MPH_ADD_CHN_ASSIGN_REQ
  channel_desc{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  frequency_list{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  starting_time{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } }  0
MPH_ASYNC_HO_COMPLETE
  timing_advance UDEC 1  0
MPH_ASYNC_HO_REQ
  handover_command{ cell_description{ ncc UDEC 1 bcc UDEC 1 bcch_carrier UDEC 2 } 
  channel_desc_1{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_mode_1 UDEC 1 
  starting_time{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } } 
  ho_acc UDEC 1 txpwr UDEC 1 report_time_diff UDEC 1 
  frequency_list{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  channel_desc_2{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_mode_2 UDEC 1 
  UNUSED PAD 1 frequency_list_bef_sti{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  channel_desc_1_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_desc_2_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  cipher_mode UDEC 1 a5_algorithm UDEC 1 }  0
MPH_CHANGE_FREQUENCY
  channel_desc{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  frequency_list{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  starting_time{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } }  0
MPH_CHANNEL_ASSIGN_REQ
  channel_desc_1{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_mode_1 UDEC 1 txpwr UDEC 1 
  frequency_list{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  starting_time{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } } 
  channel_desc_2{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_mode_2 UDEC 1 
  UNUSED PAD 1 frequency_list_bef_sti{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  channel_desc_1_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_desc_2_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  cipher_mode UDEC 1 a5_algorithm UDEC 1  0
MPH_CHANNEL_MODE_MODIFY_REQ
  subchannel UDEC 1 channel_mode UDEC 1  0
MPH_CHN_REL_REQ
  Param1 UDEC 1 UNUSED PAD 1 Param2 UDEC 2  0
MPH_IMMED_ASSIGN_REQ
  channel_desc{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  timing_advance UDEC 1 
  UNUSED PAD 1 frequency_list{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  plmn_permitted UDEC 1 
  starting_time{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } } 
  UNUSED PAD 1 frequency_list_bef_sti{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  maio_bef_sti UDEC 1 power_control_ind UDEC 1 dtx_allowed UDEC 1 
  radio_link_timeout UDEC 1  0
MPH_PART_CHN_REL_REQ
  subchannel UDEC 1  0
MPH_PRE_SYNC_HO_REQ
  handover_command{ cell_description{ ncc UDEC 1 bcc UDEC 1 bcch_carrier UDEC 2 } 
  channel_desc_1{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_mode_1 UDEC 1 
  starting_time{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } } 
  ho_acc UDEC 1 txpwr UDEC 1 report_time_diff UDEC 1 
  frequency_list{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  channel_desc_2{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_mode_2 UDEC 1 
  UNUSED PAD 1 frequency_list_bef_sti{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  channel_desc_1_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_desc_2_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  cipher_mode UDEC 1 a5_algorithm UDEC 1 } 
  nci UDEC 1 timing_advance_valid UDEC 1 timing_advance UDEC 1 UNUSED PAD 1  0
MPH_PSEUDO_SYNC_HO_REQ
  handover_command{ cell_description{ ncc UDEC 1 bcc UDEC 1 bcch_carrier UDEC 2 } 
  channel_desc_1{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_mode_1 UDEC 1 
  starting_time{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } } 
  ho_acc UDEC 1 txpwr UDEC 1 report_time_diff UDEC 1 
  frequency_list{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  channel_desc_2{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_mode_2 UDEC 1 
  UNUSED PAD 1 frequency_list_bef_sti{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  channel_desc_1_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_desc_2_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  cipher_mode UDEC 1 a5_algorithm UDEC 1 } 
  nci UDEC 1 real_time_difference UDEC 1  0
MPH_SET_CIPHERING_REQ
  cipher_mode UDEC 1 a5_algorithm UDEC 1 
  new_ciph_param{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] }  0
MPH_SYNC_HO_REQ
  handover_command{ cell_description{ ncc UDEC 1 bcc UDEC 1 bcch_carrier UDEC 2 } 
  channel_desc_1{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_mode_1 UDEC 1 
  starting_time{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } } 
  ho_acc UDEC 1 txpwr UDEC 1 report_time_diff UDEC 1 
  frequency_list{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  channel_desc_2{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_mode_2 UDEC 1 
  UNUSED PAD 1 frequency_list_bef_sti{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  channel_desc_1_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  channel_desc_2_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  cipher_mode UDEC 1 a5_algorithm UDEC 1 } 
  nci UDEC 1 UNUSED PAD 1  0
MPH_DED_EXT_MEAS_REPORT_REQ
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ num_of_chans UDEC 2 chan_number{ A ARRAY 32 [ CHAN_LIST UDEC 2 ] } }  0
MPH_DED_ENH_MEAS_REQ
  Param1{ ba_ind UDEC 1 three_g_ba_ind UDEC 1 ba_list_present UDEC 1 
  UNUSED PAD 1 bcch_bsic_list{ num_of_chans UDEC 2 
  chan{ A ARRAY 32 [ A{ arfcn UDEC 2 valid_bsic UDEC 1 UNUSED PAD 1 } ] } } 
  UNUSED PAD 2 abs_idx_start_emr DEC 4 serving_band_rpt DEC 4 scale_ord DEC 4 
  rep_priority UDEC 1 reporting_rate UDEC 1 invalid_bsic_allowed UDEC 1 
  UNUSED PAD 1 rpt_priority_list{ A ARRAY 96 [ REP_PRIORITY_LIST DEC 4 ] } 
  rpt_900_fields{ offset DEC 4 threshold DEC 4 } 
  rpt_1800_fields{ offset DEC 4 threshold DEC 4 } 
  rpt_1900_fields{ offset DEC 4 threshold DEC 4 } 
  rpt_fdd_fields{ offset DEC 4 threshold DEC 4 } network_ctrl_order UDEC 1 
  ncc_permitted UDEC 1 UNUSED PAD 2 }  0
MPH_RTD_REQ
  Param1{ rtd6_list{ num_of_chans UDEC 2 
  chan_rtd6_list{ A ARRAY 32 [ A{ arfcn UDEC 2 rtd6 UDEC 1 UNUSED PAD 1 } ] } } 
  rtd12_list{ num_of_chans UDEC 2 chan_rtd12_list{ A ARRAY 32 [ A{ arfcn UDEC 2 rtd12 UDEC 2 } ] } } }  0
MPH_UPDATE_BA_LIST
  bcch_allocation{ num_of_chans UDEC 2 chan_number{ A ARRAY 32 [ CHAN_LIST UDEC 2 ] } } 
  pwrc UDEC 1 radio_link_timeout UDEC 1 plmn_permitted UDEC 1 full_rate_dtx_allowed UDEC 1 
  multi_band_report UDEC 1 half_rate_dtx_allowed UDEC 1 multi_rat_report UDEC 1 
  search_priority_3g UDEC 1  0
MPH_SYNC_HO_CNF
  observed_time_diff UDEC 4  0
MPH_ASYNC_HO_CNF
  observed_time_diff UDEC 4  0
L2_CONNECT_IND
  Param1 UDEC 1  0
L2_DATA_IND
  Param1{ A ARRAY 23 [ RADIO_FRAME UDEC 1 ] }  0
DL_UNIT_DATA_IND
  Param1{ A ARRAY 23 [ RADIO_FRAME UDEC 1 ] } UNUSED PAD 1 Param2 DEC 4  0
DL_DATA_IND
  Param1 LIB 1  0
DL_ESTABLISH_IND
  Param1 DEC 4  0
DL_ESTABLISH_CON
  Param1 DEC 4  0
DL_RELEASE_IND
  Param1 DEC 4 Param2 DEC 4  0
DL_RELEASE_CON
  Param1 DEC 4  0
MDL_ERROR_IND
  Param1 DEC 4 Param2 DEC 4  0
DL_UNIT_DATA_REQ
  Param1 LIB 1 Param2 DEC 4  0
DL_DATA_REQ
  Param1 LIB 1  0
DL_ESTABLISH_REQ
  Param1 LIB 1  0
DL_RELEASE_REQ
  Param1 DEC 4 Param2 DEC 4  0
DL_RECONNECT_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 LIB 1  0
DL_RESUME_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 LIB 1  0
MDL_INFO_REQ
  Param1 DEC 4  0
PSSIMM_ATTACH_CNF
  Param1{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } Param2 DEC 4 Param3 DEC 4 
  Param4 DEC 4 Param5 DEC 4  0
PSSIMM_ATTACH_REJ
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1 Param4 UDEC 1 UNUSED PAD 2 Param5 DEC 4 
  Param6 DEC 4 Param7 UDEC 1 Param8 UDEC 1 
  Param9{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } UNUSED PAD 2 Param10 DEC 4 
  Param11 DEC 4  0
PSSIMM_DETACH_CNF
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
PSSIMM_DETACH_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
PSSIMM_SERVICE_IND
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1 Param4 UDEC 1 UNUSED PAD 2 Param5 DEC 4 
  Param6 DEC 4 Param7 UDEC 1 Param8 UDEC 1 
  Param9{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } UNUSED PAD 2 Param10 DEC 4 
  Param11 DEC 4 Param12 UDEC 1  0
PSSIMM_CS_CIPHER_IND
  Param1 UDEC 1  0
PSSIMM_PS_CIPHER_IND
  Param1 UDEC 1  0
PSSIMM_PLMN_LIST_CNF
  Param1{ num DEC 4 info_ptr HEX 4 } Param2 UDEC 1  0
PSSIMM_PLMN_LIST_REJ
  Param1 DEC 4  0
PSSIMM_SIM_BCCH_INFO_IND
  Param1{ A ARRAY 16 [ NEIGHBOUR_CELL_LIST UDEC 1 ] }  0
PSSIMM_SIM_FORB_PLMN_IND
  Param1{ A ARRAY 20 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] }  0
PSSIMM_CS_INFORMATION_IND
  Param1 HEX 4 Param2 HEX 4 Param3 UDEC 1 Param4 UDEC 1 Param5 UDEC 1 
  Param6{ A ARRAY 7 [ TIME_ZONE_AND_TIME UDEC 1 ] } Param7 UDEC 1 
  Param8{ length UDEC 1 lsa_id{ A ARRAY 3 [ LSA_ID UDEC 1 ] } } Param9 UDEC 1 
  Param10{ length UDEC 1 value UDEC 1 }  0
PSSIMM_PS_INFORMATION_IND
  Param1 HEX 4 Param2 HEX 4 Param3 UDEC 1 Param4 UDEC 1 Param5 UDEC 1 
  Param6{ A ARRAY 7 [ TIME_ZONE_AND_TIME UDEC 1 ] } Param7 UDEC 1 
  Param8{ length UDEC 1 lsa_id{ A ARRAY 3 [ LSA_ID UDEC 1 ] } } Param9 UDEC 1 
  Param10{ length UDEC 1 value UDEC 1 }  0
PSSIMM_SIM_CS_ALG_IND
  Param1{ A ARRAY 16 [ RAND_VALUE UDEC 1 ] } Param2 UDEC 1 
  Param3{ A ARRAY 17 [ AUTN_VALUE UDEC 1 ] }  0
PSSIMM_SIM_PS_ALG_IND
  Param1{ A ARRAY 16 [ RAND_VALUE UDEC 1 ] } Param2 UDEC 1 
  Param3{ A ARRAY 17 [ AUTN_VALUE UDEC 1 ] }  0
PSSIMM_SIM_CS_LOC_INFO_IND
  Param1{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param2{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } 
  Param3 UDEC 1  0
PSSIMM_SIM_PS_LOC_INFO_IND
  Param1{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param2{ A ARRAY 3 [ PTMSI_SIGNATURE UDEC 1 ] } 
  UNUSED PAD 1 Param3{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param4 UDEC 1  0
PSSIMM_SIM_CS_KEYS_IND
  Param1{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 }  0
PSSIMM_SIM_PS_KEYS_IND
  Param1{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 }  0
PSSIMM_EQ_PLMN_LIST_IND
  Param1{ length DEC 4 eq_plmn{ A ARRAY 6 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } }  0
PSSIMM_HO_IND
  Param1 DEC 4 Param2 DEC 4  0
PSSIMM_START_REQ
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4 
  Param4{ class2_field{ revision_level UDEC 1 es_ind UDEC 1 a51_supported UDEC 1 a52_supported UDEC 1 
  a53_supported UDEC 1 ps_capability UDEC 1 ss_screen UDEC 1 sm_capability UDEC 1 
  vbs UDEC 1 vgcs UDEC 1 fc UDEC 1 cm3 UDEC 1 lcsva UDEC 1 ucs2_supported UDEC 1 
  solsa_capability UDEC 1 cmsp UDEC 1 } 
  class3_field{ a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 multi_slot_class UDEC 1 ucs2_supported UDEC 1 
  ext_measurement UDEC 1 sms_value UDEC 1 sm_value UDEC 1 ms_positioning_method_cap UDEC 1 
  egprs_multi_slot_class UDEC 1 modulation_capability UDEC 1 edge_rf_power_cap_1 UDEC 1 
  edge_rf_power_cap_2 UDEC 1 umts_fdd_rat_cap UDEC 1 umts_tdd_supported UDEC 1 
  cdma_2000_supported UDEC 1 dtm_gprs_supported UDEC 1 dtm_gprs_multi_slot_subclass UDEC 1 
  mac_mode_supported UDEC 1 dtm_egprs_supported UDEC 1 dtm_egprs_multi_slot_subclass UDEC 1 
  gsm_400_radio_cap UDEC 1 gsm_850_radio_cap UDEC 1 gsm_1900_radio_cap UDEC 1 } 
  band_info_field{ p_gsm_available UDEC 1 e_gsm_available UDEC 1 dcs_available UDEC 1 
  pcs_available UDEC 1 r_gsm_available UDEC 1 gsm_400_available UDEC 1 
  gsm_850_available UDEC 1 p_gsm_pwr_class UDEC 1 e_gsm_pwr_class UDEC 1 
  dcs_pwr_class UDEC 1 pcs_pwr_class UDEC 1 r_gsm_pwr_class UDEC 1 
  gsm_400_pwr_class UDEC 1 gsm_850_pwr_class UDEC 1 gsm_band UDEC 1 
  gsm_400_bands_supported UDEC 1 } 
  UNUSED PAD 3 gprs_caps{ ms_class DEC 4 paging_channels UDEC 1 
  drx{ split_pg_cycle_code UDEC 1 split_on_ccch UDEC 1 timer_val UDEC 1 
  drx_cycle_length_coef UDEC 1 } 
  gea1_supported UDEC 1 gea2_supported UDEC 1 gea3_supported UDEC 1 
  gea4_supported UDEC 1 gea5_supported UDEC 1 gea6_supported UDEC 1 
  gea7_supported UDEC 1 sm_gprs UDEC 1 sm_cap_via_dedicated UDEC 1 
  revi_level_indicator UDEC 1 pfc_feature_mode UDEC 1 multi_slot_class UDEC 1 
  ecsd_multi_slot_class UDEC 1 ext_dyn_alloc UDEC 1 egprs_extended_dynamic_allocation_cap UDEC 1 
  compact_interference_meas UDEC 1 UNUSED PAD 3 } 
  gprs_services UDEC 1 cs_services UDEC 1 UNUSED PAD 2 gsm_release DEC 4 } 
  Param5 UDEC 1 Param6 UDEC 1 
  Param7{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param8{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param9 UDEC 1 
  UNUSED PAD 1 Param10{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 } 
  Param11{ length DEC 4 eq_plmn{ A ARRAY 6 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } } 
  Param12{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param13{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param14{ A ARRAY 3 [ PTMSI_SIGNATURE UDEC 1 ] } Param15 UDEC 1 
  Param16{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } Param17 UDEC 1 Param18 UDEC 1 
  Param19{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } }  0
PSSIMM_ATTACH_REQ
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4 
  Param4{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } Param5 DEC 4 Param6 DEC 4 
  Param7 DEC 4 Param8 DEC 4 Param9 UDEC 1 Param10 UDEC 1 UNUSED PAD 2 Param11 DEC 4 
  Param12 UDEC 1 Param13 UDEC 1 
  Param14{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } } 
  Param15 UDEC 1 Param16{ A ARRAY 16 [ NEIGHBOUR_CELL_LIST UDEC 1 ] } 
  Param17 UDEC 2 Param18{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param19{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } 
  Param20 UDEC 1 Param21 UDEC 1 Param22{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param23{ A ARRAY 3 [ PTMSI_SIGNATURE UDEC 1 ] } 
  UNUSED PAD 1 Param24{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param25 UDEC 1 Param26 UDEC 1  0
PSSIMM_DETACH_REQ
  Param1 DEC 4 Param2 UDEC 1 Param3 UDEC 1  0
PSSIMM_SIM_INFO_REQ
  Param1{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 } 
  Param2 UDEC 1 
  Param3{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 } 
  Param4 UDEC 1 Param5 UDEC 2 Param6 UDEC 1 
  UNUSED PAD 1 Param7{ A ARRAY 20 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } 
  Param8 UDEC 1 
  UNUSED PAD 1 Param9{ length DEC 4 list{ A ARRAY 30 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } } 
  Param10 UDEC 1 
  UNUSED PAD 3 Param11{ length DEC 4 
  list{ A ARRAY 30 [ A{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } act_id UDEC 2 } ] } } 
  Param12 UDEC 1 
  UNUSED PAD 3 Param13{ length DEC 4 
  list{ A ARRAY 30 [ A{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } act_id UDEC 2 } ] } } 
  Param14 UDEC 1 
  UNUSED PAD 3 Param15{ length DEC 4 
  list{ A ARRAY 30 [ A{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } act_id UDEC 2 } ] } } 
  Param16 UDEC 1 Param17 UDEC 1 Param18 UDEC 1 Param19 UDEC 1  0
PSSIMM_SIM_USER_PLMN_CHANGE_REQ
  Param1 DEC 4 
  Param2{ length DEC 4 list{ A ARRAY 30 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } } 
  Param3{ length DEC 4 
  list{ A ARRAY 30 [ A{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } act_id UDEC 2 } ] } }  0
PSSIMM_CLASSMARK_REQ
  Param1 UDEC 1 
  UNUSED PAD 3 Param2{ class2_field{ revision_level UDEC 1 es_ind UDEC 1 a51_supported UDEC 1 a52_supported UDEC 1 
  a53_supported UDEC 1 ps_capability UDEC 1 ss_screen UDEC 1 sm_capability UDEC 1 
  vbs UDEC 1 vgcs UDEC 1 fc UDEC 1 cm3 UDEC 1 lcsva UDEC 1 ucs2_supported UDEC 1 
  solsa_capability UDEC 1 cmsp UDEC 1 } 
  class3_field{ a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 multi_slot_class UDEC 1 ucs2_supported UDEC 1 
  ext_measurement UDEC 1 sms_value UDEC 1 sm_value UDEC 1 ms_positioning_method_cap UDEC 1 
  egprs_multi_slot_class UDEC 1 modulation_capability UDEC 1 edge_rf_power_cap_1 UDEC 1 
  edge_rf_power_cap_2 UDEC 1 umts_fdd_rat_cap UDEC 1 umts_tdd_supported UDEC 1 
  cdma_2000_supported UDEC 1 dtm_gprs_supported UDEC 1 dtm_gprs_multi_slot_subclass UDEC 1 
  mac_mode_supported UDEC 1 dtm_egprs_supported UDEC 1 dtm_egprs_multi_slot_subclass UDEC 1 
  gsm_400_radio_cap UDEC 1 gsm_850_radio_cap UDEC 1 gsm_1900_radio_cap UDEC 1 } 
  band_info_field{ p_gsm_available UDEC 1 e_gsm_available UDEC 1 dcs_available UDEC 1 
  pcs_available UDEC 1 r_gsm_available UDEC 1 gsm_400_available UDEC 1 
  gsm_850_available UDEC 1 p_gsm_pwr_class UDEC 1 e_gsm_pwr_class UDEC 1 
  dcs_pwr_class UDEC 1 pcs_pwr_class UDEC 1 r_gsm_pwr_class UDEC 1 
  gsm_400_pwr_class UDEC 1 gsm_850_pwr_class UDEC 1 gsm_band UDEC 1 
  gsm_400_bands_supported UDEC 1 } 
  UNUSED PAD 3 gprs_caps{ ms_class DEC 4 paging_channels UDEC 1 
  drx{ split_pg_cycle_code UDEC 1 split_on_ccch UDEC 1 timer_val UDEC 1 
  drx_cycle_length_coef UDEC 1 } 
  gea1_supported UDEC 1 gea2_supported UDEC 1 gea3_supported UDEC 1 
  gea4_supported UDEC 1 gea5_supported UDEC 1 gea6_supported UDEC 1 
  gea7_supported UDEC 1 sm_gprs UDEC 1 sm_cap_via_dedicated UDEC 1 
  revi_level_indicator UDEC 1 pfc_feature_mode UDEC 1 multi_slot_class UDEC 1 
  ecsd_multi_slot_class UDEC 1 ext_dyn_alloc UDEC 1 egprs_extended_dynamic_allocation_cap UDEC 1 
  compact_interference_meas UDEC 1 UNUSED PAD 3 } 
  gprs_services UDEC 1 cs_services UDEC 1 UNUSED PAD 2 gsm_release DEC 4 } 
  Param3 UDEC 1 Param4 UDEC 1 
  Param5{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param6{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param7 UDEC 1 
  UNUSED PAD 1 Param8{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 }  0
PSSIMM_SIM_CS_ALG_RSP
  Param1 DEC 4 
  Param2{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 } 
  Param3 UDEC 1 Param4{ A ARRAY 17 [ RES UDEC 1 ] } 
  Param5{ A ARRAY 4 [ SRES UDEC 1 ] } Param6 UDEC 1 
  Param7{ A ARRAY 15 [ AUTS_VALUE UDEC 1 ] }  0
PSSIMM_SIM_PS_ALG_RSP
  Param1 DEC 4 
  Param2{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 } 
  Param3 UDEC 1 Param4{ A ARRAY 17 [ RES UDEC 1 ] } 
  Param5{ A ARRAY 4 [ SRES UDEC 1 ] } Param6 UDEC 1 
  Param7{ A ARRAY 15 [ AUTS_VALUE UDEC 1 ] }  0
MMSV_NVM_UPDATE_IND
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param3 UDEC 1 Param4{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } Param5 UDEC 1 
  Param6{ A ARRAY 3 [ PTMSI_SIGNATURE UDEC 1 ] } Param7 UDEC 1 Param8 UDEC 1 
  Param9 UDEC 1 Param10{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } Param11 UDEC 1 
  Param12 UDEC 1 Param13 UDEC 1 Param14 UDEC 1  0
MMSV_IMSI_IND
  Param1{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } }  0
MMSV_LAST_RAT_IND
  Param1 DEC 4  0
PSSIADP_RSMP_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
PSSIADP_SIM_ACCESS_IND
  Param1 DEC 4 Param2{ A ARRAY 2 [ EF_ID UDEC 1 ] } UNUSED PAD 2 Param3 DEC 4 
  Param4 HEX 4  0
PSSIADP_CS_RAB_Establish_ind
  Param1 DEC 4 
  Param2{ A ARRAY 16 [ A{ rab_id{ Present{ RAB_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 12 [ RAB_Identity UDEC 1 ] } 
  l2entity_pid DEC 4 rb_id DEC 4 relocation_from_GSM UDEC 1 UNUSED PAD 3 } ] }  0
PSSIADP_CS_RAB_Release_ind
  Param1 DEC 4 
  Param2{ A ARRAY 16 [ A{ rab_id{ Present{ RAB_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 12 [ RAB_Identity UDEC 1 ] } } ] }  0
z05G_PSSIADP_CS_Uchannel_ind
  Param1 DEC 4 
  Param2{ A ARRAY 16 [ A{ rab_id{ Present{ RAB_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 12 [ RAB_Identity UDEC 1 ] } 
  uch_id UDEC 1 UNUSED PAD 3 } ] }  0
z05H_PSSIADP_PS_Uchannel_ind
  Param1 DEC 4 
  Param2{ A ARRAY 16 [ A{ rab_id{ Present{ RAB_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 12 [ RAB_Identity UDEC 1 ] } 
  uch_id UDEC 1 UNUSED PAD 3 } ] }  0
PSSIADP_RSMP_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
z05J_PSSIADP_SIM_ACCESS_RSP
  Param1 DEC 4 Param2 DEC 4 Param3{ A ARRAY 2 [ EF_ID UDEC 1 ] } UNUSED PAD 2 Param4 DEC 4 
  Param5 HEX 4  0
z05K_PSSIADP_SIM_UPDATE_REQ
  Param1{ A ARRAY 2 [ EF_ID UDEC 1 ] } UNUSED PAD 2 Param2 DEC 4 Param3 HEX 4  0
z05L_PSSIADP_CS_Uchannel_res
  Param1 DEC 4 
  Param2{ A ARRAY 16 [ A{ rab_id{ Present{ RAB_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 12 [ RAB_Identity UDEC 1 ] } 
  uch_id UDEC 1 UNUSED PAD 3 } ] }  0
PSSIADP_PS_Uchannel_res
  Param1 DEC 4 
  Param2{ A ARRAY 16 [ A{ rab_id{ Present{ RAB_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 12 [ RAB_Identity UDEC 1 ] } 
  uch_id UDEC 1 UNUSED PAD 3 } ] }  0
z05N_PSSIADP_CS_RAB_Release_rsp
  Param1 DEC 4 
  Param2{ A ARRAY 16 [ A{ rab_id{ Present{ RAB_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 12 [ RAB_Identity UDEC 1 ] } 
  l2entity_pid DEC 4 rb_id DEC 4 relocation_from_GSM UDEC 1 UNUSED PAD 3 } ] }  0
PSSISMS_DATA_IND
  Param1 LIB 1  0
PSSISMS_ERROR_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
PSSISMS_EST_IND
  Param1 LIB 1  0
PSSISMS_REL_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
PSSISMS_EST_CNF
  Param1 DEC 4  0
PSSISMS_REL_CNF
  Param1 DEC 4  0
PSSISMS_ABORT_REQ
  Param1 DEC 4  0
PSSISMS_DATA_REQ
  Param1 LIB 1  0
PSSISMS_EST_REQ
  Param1 LIB 1 Param2 UDEC 1  0
PSSISMS_REL_REQ
  Param1 DEC 4  0
PSSISS_BEGIN_IND
  Param1 LIB 1  0
PSSISS_END_IND
  Param1 LIB 1 Param2 DEC 4  0
PSSISS_FACILITY_IND
  Param1 LIB 1  0
PSSISS_BEGIN_REQ
  Param1 LIB 1  0
PSSISS_END_REQ
  Param1 LIB 1  0
PSSISS_FACILITY_REQ
  Param1 LIB 1  0
MIOM_BATT_CHECK_IND
  Param1 DEC 4  0
TAMMI_START_CALL
  Bc_Repeat_Ind UDEC 2 Bearer_Cap1{ A ARRAY 10 [ PACKED_BC UDEC 1 ] } 
  Bearer_Cap2{ A ARRAY 10 [ PACKED_BC UDEC 1 ] } 
  Packed_Called_BCD_No{ A ARRAY 14 [ PACKED_CALL_BCD_NUM UDEC 1 ] } 
  Called_Sub_Address{ A ARRAY 23 [ PACKED_CALL_PARTY_SUB_ADDRESS UDEC 1 ] } 
  UNUSED PAD 1 Llc_Repeat_Ind UDEC 2 Llc1{ A ARRAY 15 [ LLC UDEC 1 ] } 
  Llc2{ A ARRAY 15 [ LLC UDEC 1 ] } Hlc_Repeat_Ind UDEC 2 
  Hlc1{ A ARRAY 5 [ HLC UDEC 1 ] } Hlc2{ A ARRAY 5 [ HLC UDEC 1 ] }  0
TAMMI_ACCEPT_CALL
  Bc_Repeat_Ind UDEC 2 Bearer_Cap1{ A ARRAY 10 [ PACKED_BC UDEC 1 ] } 
  Bearer_Cap2{ A ARRAY 10 [ PACKED_BC UDEC 1 ] } Llc_Repeat_Ind UDEC 2 
  Llc1{ A ARRAY 15 [ LLC UDEC 1 ] } Llc2{ A ARRAY 15 [ LLC UDEC 1 ] } 
  Hlc_Repeat_Ind UDEC 2 Hlc1{ A ARRAY 5 [ HLC UDEC 1 ] } 
  Hlc2{ A ARRAY 5 [ HLC UDEC 1 ] }  0
TAMMI_ANSWER_CALL
  Bc_Repeat_Ind UDEC 2 Bearer_Cap1{ A ARRAY 10 [ PACKED_BC UDEC 1 ] } 
  Bearer_Cap2{ A ARRAY 10 [ PACKED_BC UDEC 1 ] }  0
TAMMI_MODE_REQ
  Param1{ Te_Mode UDEC 1 Ms_Mode UDEC 1 SMS_Indication UDEC 1 SMS_Delivery UDEC 1 }  0
TAMMI_MODE_ACK
  Param1{ Te_Mode UDEC 1 Ms_Mode UDEC 1 SMS_Indication UDEC 1 SMS_Delivery UDEC 1 }  0
TAMMI_DISCONNECT_CALL
  Param1{ Prop_Error_Value UDEC 1 }  0
MMITA_CHANNEL_MODE_MOD_REQ
  Param1{ Channel_Mode UDEC 1 Prop_Error_Value UDEC 1 }  0
TAMMI_CHANNEL_MODE_MOD_RESP
  Param1{ Channel_Mode UDEC 1 Prop_Error_Value UDEC 1 }  0
MMITA_CALL_PROCEEDING
  Bc_Repeat_Ind UDEC 2 Bearer_Cap1{ A ARRAY 10 [ PACKED_BC UDEC 1 ] } 
  Bearer_Cap2{ A ARRAY 10 [ PACKED_BC UDEC 1 ] }  0
MMITA_RECEIVED_CALL
  Bc_Repeat_Ind UDEC 2 Bearer_Cap1{ A ARRAY 10 [ PACKED_BC UDEC 1 ] } 
  Bearer_Cap2{ A ARRAY 10 [ PACKED_BC UDEC 1 ] } Calling_BCD_No_Valid UDEC 1 
  Calling_BCD_No{ A ARRAY 14 [ PACKED_CALL_BCD_NUM UDEC 1 ] } Calling_SA_Valid UDEC 1 
  Calling_Sub_Address{ A ARRAY 23 [ PACKED_CALL_PARTY_SUB_ADDRESS UDEC 1 ] } 
  UNUSED PAD 1 Llc_Repeat_Ind UDEC 2 Llc1{ A ARRAY 15 [ LLC UDEC 1 ] } 
  Llc2{ A ARRAY 15 [ LLC UDEC 1 ] } Hlc_Repeat_Ind UDEC 2 
  Hlc1{ A ARRAY 5 [ HLC UDEC 1 ] } Hlc2{ A ARRAY 5 [ HLC UDEC 1 ] }  0
MMITA_CONNECTED_CALL
  Bc_Repeat_Ind UDEC 2 Bearer_Cap1{ A ARRAY 10 [ PACKED_BC UDEC 1 ] } 
  Bearer_Cap2{ A ARRAY 10 [ PACKED_BC UDEC 1 ] } Called_BCD_No_Valid UDEC 1 
  Called_BCD_No{ A ARRAY 14 [ PACKED_CALL_BCD_NUM UDEC 1 ] } Called_SA_Valid UDEC 1 
  Called_Sub_Address{ A ARRAY 23 [ PACKED_CALL_PARTY_SUB_ADDRESS UDEC 1 ] } UNUSED PAD 1  0
MMITA_DISCONNECT_CALL
  Prop_Error_Value UDEC 1  0
MMITA_MODE_ACK
  Param1{ Te_Mode UDEC 1 Ms_Mode UDEC 1 SMS_Indication UDEC 1 SMS_Delivery UDEC 1 }  0
MMITA_MESSAGE_ARRIVED
  Param1{ Sms_Length UDEC 1 SmsMessage{ A ARRAY 50 [ SMS_MESSAGE UDEC 1 ] } }  0
MMITA_INC_MESSAGE
  Param1{ Sms_Length UDEC 1 SmsMessage{ A ARRAY 50 [ SMS_MESSAGE UDEC 1 ] } }  0
MMITA_END_SMS_MODE
  Cause UDEC 1  0
MMITA_SMS_BLOCK_MESSAGE
  Sms_Length UDEC 1 SmsMessage{ A ARRAY 50 [ SMS_MESSAGE UDEC 1 ] }  0
SISH_RESET_SIM
  Param1 DEC 4  0
SISH_SIM_COMMAND
  Param1{ CommandHeader{ CLA UDEC 1 INS UDEC 1 P1 UDEC 1 P2 UDEC 1 P3 UDEC 1 } 
  UNUSED PAD 3 ResDataLength DEC 4 DataLength DEC 4 
  CommandData{ A ARRAY 256 [ BYTE_ARRAY UDEC 1 ] } }  0
SISH_T_ONE_SIM_COMMAND
  Param1{ DataLength DEC 4 Le DEC 4 LeFlg UDEC 1 
  TOneCapduData{ A ARRAY 299 [ BYTE_ARRAY_CAPDU UDEC 1 ] } }  0
SISH_ADJUST_CLOCK
  Param1 DEC 4  0
SHSI_RESET_SIM_RESPONSE
  Param1{ ResetResult DEC 4 Reset_Volt DEC 4 Protocol DEC 4 Length UDEC 1 
  ATRContent{ A ARRAY 33 [ BYTE_ARRAY_ATR UDEC 1 ] } UNUSED PAD 2 }  0
SHSI_SIM_RESPONSE
  Param1{ CommandResult DEC 4 ShCond1 UDEC 1 ShCond2 UDEC 1 UNUSED PAD 2 ShRxState DEC 4 
  ShNoBytesExpected DEC 4 DataLength DEC 4 
  APDUResponse{ SW1 UDEC 1 SW2 UDEC 1 ResponseData{ A ARRAY 256 [ BYTE_ARRAY UDEC 1 ] } } UNUSED PAD 2 }  0
SHSI_T_ONE_SIM_RESPONSE
  Param1{ CommandResult DEC 4 ShCond1 UDEC 1 ShCond2 UDEC 1 UNUSED PAD 2 ShRxState DEC 4 
  ShNoBytesExpected DEC 4 DataLength DEC 4 
  APDUResponse{ SW1 UDEC 1 SW2 UDEC 1 ResponseData{ A ARRAY 256 [ BYTE_ARRAY UDEC 1 ] } } UNUSED PAD 2 }  0
SH_RX_ATR
  Param1 UDEC 1  0
SH_TX_RESPONSE
  Param1{ SW1 UDEC 1 SW2 UDEC 1 }  0
SH_FRAME_T1
  Param1{ Nad UDEC 1 Pcb UDEC 1 Len UDEC 1 } 
  Param2{ A ARRAY 256 [ BYTE_ARRAY UDEC 1 ] } UNUSED PAD 1 Param3 DEC 4  0
SH_RX_ERR_IRQ
  Param1{ ShDiag1 UDEC 1 ShDiag2 UDEC 1 UNUSED PAD 2 ShNoBytesReceived DEC 4 
  ShNoBytesSent DEC 4 }  0
SH_RX_OVFL_IRQ
  Param1{ ShDiag1 UDEC 1 ShDiag2 UDEC 1 UNUSED PAD 2 ShNoBytesReceived DEC 4 
  ShNoBytesSent DEC 4 }  0
SH_TX_ERR_IRQ
  Param1{ ShDiag1 UDEC 1 ShDiag2 UDEC 1 UNUSED PAD 2 ShNoBytesReceived DEC 4 
  ShNoBytesSent DEC 4 }  0
SH_INVALID_BYTE
  Param1{ ShDiag1 UDEC 1 ShDiag2 UDEC 1 UNUSED PAD 2 ShNoBytesReceived DEC 4 
  ShNoBytesSent DEC 4 }  0
SH_WWT_TIMER_IRQ
  Param1{ ShDiag1 UDEC 1 ShDiag2 UDEC 1 UNUSED PAD 2 ShNoBytesReceived DEC 4 
  ShNoBytesSent DEC 4 }  0
SH_BWT_TIMER_IRQ
  Param1{ ShDiag1 UDEC 1 ShDiag2 UDEC 1 UNUSED PAD 2 ShNoBytesReceived DEC 4 
  ShNoBytesSent DEC 4 }  0
SH_SEND_I_FRAME
  Param1 UDEC 1 Param2 UDEC 1 Param3{ A ARRAY 256 [ BYTE_ARRAY UDEC 1 ] }  0
SH_SEND_R_FRAME
  Param1 UDEC 1  0
SH_SEND_S_FRAME
  Param1 UDEC 1 Param2 UDEC 1  0
SHEF_RESET_SIM_RESPONSE
  Param1{ ResetResult DEC 4 Length UDEC 1 ATRContent{ A ARRAY 33 [ BYTE_ARRAY_ATR UDEC 1 ] } UNUSED PAD 2 }  0
SHEF_SIM_RESPONSE
  Param1{ CommandResult DEC 4 SW1 UDEC 1 SW2 UDEC 1 UNUSED PAD 2 }  0
EFSH_RESET_SIM
  Param1 DEC 4  0
EFSM_PWORD_CONFIRMATION_REQ
  Param1{ accessLevel UDEC 1 UNUSED PAD 1 accessCode UDEC 2 }  0
SMEF_PWORD_CONFIRMATION_RSP
  Param1 UDEC 1  0
STEF_ENG_FUNC_REQ
  Param1{ RequestParams{ A ARRAY 1100 [ EF_REQUEST_ARRAY UDEC 1 ] } }  0
EFST_ENG_FUNC_RSP
  Param1{ Response{ A ARRAY 1100 [ EF_RESPONSE_ARRAY UDEC 1 ] } }  0
L1EF_NON_SUSP_CMD_RSP
  Param1{ Response{ A ARRAY 1100 [ EF_RESPONSE_ARRAY UDEC 1 ] } }  0
L1EF_SUSP_CMD_RSP
  Param1{ Response{ A ARRAY 1100 [ EF_RESPONSE_ARRAY UDEC 1 ] } }  0
L1EF_STATUS_RSP
  Param1{ FunctionID UDEC 1 UNUSED PAD 3 ErrorCode DEC 4 }  0
EFL1_NON_SUSP_CMD_REQ
  Param1{ RequestParams{ A ARRAY 1100 [ EF_REQUEST_ARRAY UDEC 1 ] } }  0
EFL1_SUSP_CMD_REQ
  Param1{ RequestParams{ A ARRAY 1100 [ EF_REQUEST_ARRAY UDEC 1 ] } }  0
EFPS_OSCILLATOR_REQ
  Param1 DEC 4  0
PSEF_OSCILLATOR_RSP
  Param1 UDEC 1 UNUSED PAD 3 Param2 UDEC 4  0
L1PS_CAL_RPT
  Param1 DEC 4  0
EFPD_PWR_DWN_REQ
  Param1{ EFPwrDwn DEC 4 }  0
PUMI_PWR_UP_REASON
  Param1{ PowerUpReason DEC 4 }  0
PUMI_PWR_UP_ENVIRON
  Param1{ hw_config{ Charger_Connected UDEC 1 PCMCIA_Connected UDEC 1 } 
  results{ ROM_Checksum_Test_Ok UDEC 1 Ramtest_Ok UDEC 1 L1_Checksum_Ok UDEC 1 
  Battery_Checksum_Ok UDEC 1 ADC_Ok UDEC 1 Keypad_Ok UDEC 1 DSP_Mask_Ok UDEC 1 
  Bad_battery UDEC 1 } }  0
PDMI_PWR_DWN
  Param1{ PowerDwn DEC 4 }  0
MIPU_PWR_UP_TYPE
  Param1{ PowerUp DEC 4 }  0
MIPD_PWR_DWN_REQ
  Param1{ PowerDwn DEC 4 }  0
TH_TEST
  Param1 DEC 4 Param2 DEC 4  0
TH_TEST_SIM_RESET
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
TH_TEST_SIM_COM
  Param1 DEC 4  0
TH_TEST_CLOCK_STOP
  Param1 DEC 4  0
TH_RESPONSE
  Param1 DEC 4  0
TH_RESPONSE_SIM_RESET
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4 Param4 DEC 4  0
TH_RESPONSE_SIM_COM
  Param1 DEC 4  0
TH_RESPONSE_CLOCK_STOP
  Param1 DEC 4  0
ATV24_DATA_RECEIVED
  Param1{ A ARRAY 256 [ AT_CMD UDEC 1 ] }  0
IPT_LISTEN_TO_SOCKETS_IND
  Param1{ ClientId DEC 4 ConnId DEC 4 Socket DEC 4 
  ClientAddr{ A ARRAY 30 [ IPT_ADDR_PARAM UDEC 1 ] } UNUSED PAD 2 }  0
IPT_STOP_LISTENING_TO_SOCKETS_IND
  Param1{ ClientId DEC 4 ConnId DEC 4 Socket DEC 4 
  ClientAddr{ A ARRAY 30 [ IPT_ADDR_PARAM UDEC 1 ] } UNUSED PAD 2 }  0
IPR_LISTEN_TO_SOCKETS_CNF
  Param1{ ListenStatus DEC 4 }  0
GMM_ATTACH_REQ
  Param1 DEC 4 Param2 UDEC 1  0
GMM_CELL_REQ
  Param1{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param2 UDEC 2 Param3 UDEC 2 Param4 UDEC 1 Param5 UDEC 1 Param6 UDEC 1 
  UNUSED PAD 1 Param7 DEC 4 Param8 DEC 4  0
GMM_DETACH_REQ
  Param1 DEC 4 Param2 DEC 4  0
GMM_NO_CELL_REQ
  Param1 DEC 4  0
GMM_NREG_REQ
  Param1 DEC 4 Param2 UDEC 1  0
GMM_PLMN_SEL_REQ
  Param1 UDEC 1  0
GMM_PLMN_SEARCH_REQ
  Param1 UDEC 1  0
GMM_RU_REQ
  Param1 DEC 4 Param2 UDEC 1  0
GMM_SERVICE_REQ
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1 Param4 UDEC 1 UNUSED PAD 2 Param5 DEC 4 
  Param6 DEC 4  0
GMM_SIM_INFO_REQ
  Param1{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } } 
  Param2 UDEC 1 Param3{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param4{ A ARRAY 3 [ PTMSI_SIGNATURE UDEC 1 ] } 
  UNUSED PAD 1 Param5{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param6 UDEC 1 
  Param7{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 }  0
GMM_PS_CONN_RSP
  Param1{ Present{ InitialUE_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 68 [ InitialUE_Identity UDEC 1 ] }  0
GMM_CELL_CNF
  Param1 DEC 4  0
GMM_CS_CONN_CNF
  Param1 DEC 4  0
GMM_DETACH_CNF
  Param1 DEC 4  0
GMM_DETACH_IND
  Param1 DEC 4 Param2 UDEC 1 Param3 UDEC 1  0
GMM_NREG_IND
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1 Param4 UDEC 1 Param5 UDEC 1 
  Param6 UDEC 1 Param7 UDEC 1  0
GMM_REG_IND
  Param1{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param2 UDEC 1 Param3 UDEC 1 
  Param4{ id_len UDEC 1 id{ A ARRAY 9 [ MS_ID_OCTETS UDEC 1 ] } } 
  Param5 UDEC 1 Param6 UDEC 1 Param7 UDEC 1 Param8 UDEC 1 
  Param9{ length DEC 4 eq_plmn{ A ARRAY 6 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } }  0
GMM_RU_NEEDED
  Param1 DEC 4  0
GMM_PTMSI_IND
  Param1{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] }  0
GMM_PS_CONN_IND
  Param1 UDEC 1  0
MMCS_CELL_REQ
  Param1{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } 
  Param2 UDEC 2 Param3 UDEC 2 Param4 UDEC 1 UNUSED PAD 1 Param5 DEC 4 
  Param6 UDEC 1 UNUSED PAD 3 Param7 DEC 4 Param8 DEC 4 Param9 DEC 4  0
MMCS_CS_CONN_RSP
  Param1{ Present{ InitialUE_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 68 [ InitialUE_Identity UDEC 1 ] }  0
MMCS_DETACH_INITIATED
  Param1 UDEC 1  0
MMCS_DETACH_REQ
  Param1 DEC 4 Param2 UDEC 1  0
MMCS_LU_INITIATED
  Param1 UDEC 1  0
MMCS_LU_REQ
  Param1 DEC 4  0
MMCS_LU_RESULT
  Param1 DEC 4 Param2{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } 
  Param3 UDEC 1 Param4{ id_len UDEC 1 id{ A ARRAY 9 [ MS_ID_OCTETS UDEC 1 ] } } 
  Param5 UDEC 1 Param6 UDEC 1  0
MMCS_NO_CELL_REQ
  Param1 DEC 4  0
MMCS_NREG_REQ
  Param1 DEC 4  0
MMCS_PLMN_SEL_REQ
  Param1 UDEC 1  0
MMCS_PLMN_SEARCH_REQ
  Param1 UDEC 1  0
MMCS_SERVICE_REQ
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4 Param4 DEC 4  0
MMCS_SIM_INFO_REQ
  Param1{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } } 
  Param2{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  UNUSED PAD 1 Param3{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } 
  Param4 UDEC 1 
  Param5{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 }  0
MMCS_CELL_CNF
  Param1 DEC 4 Param2 UDEC 1  0
MMCS_CS_CONN_REL_IND
  Param1 DEC 4 Param2 UDEC 1  0
MMCS_CS_CONN_IND
  Param1 DEC 4 Param2 UDEC 1  0
MMCS_DETACH_CNF
  Param1 DEC 4  0
MMCS_LU_NEEDED
  Param1 DEC 4  0
MMCS_NREG_IND
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1 Param4 UDEC 1 Param5 UDEC 1  0
MMCS_REG_IND
  Param1{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } 
  Param2 UDEC 1 Param3 UDEC 1 Param4 UDEC 1 
  UNUSED PAD 3 Param5{ length DEC 4 eq_plmn{ A ARRAY 6 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } }  0
MMCS_TMSI_IND
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] }  0
SME_PDP_IND
  Param1 HEX 4 Param2 DEC 4  0
SME_ASSIGN_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
SME_REL_IND
  Param1 DEC 4 Param2 DEC 4  0
GMMSME_ESTABLISH_CNF
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
GMMSME_ESTABLISH_REJ
  Param1 DEC 4  0
GMMSME_UNITDATA_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  Param2{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
GMMSME_CHANGE_SYSTEM_IND
  Param1 DEC 4 Param2 DEC 4  0
PSSISME_PDP_ACTIVATE_REQ
  Param1 UDEC 1 
  UNUSED PAD 3 Param2{ version DEC 4 
  r97{ delay_class UDEC 1 reliability_class UDEC 1 precedence_class UDEC 1 
  peak_throughput UDEC 1 mean_throughput UDEC 1 } 
  r99{ Traffic_class UDEC 1 Delivery_order UDEC 1 Delivery_of_erroneous_SDU UDEC 1 
  Maximum_SDU_size UDEC 1 Maximum_bit_rate_for_uplink UDEC 1 Maximum_bit_rate_for_downlink UDEC 1 
  Residual_BER UDEC 1 SDU_error_ratio UDEC 1 Transfer_delay UDEC 1 
  Traffic_handling_priority UDEC 1 Guaranteed_bit_rate_for_uplink UDEC 1 
  Guaranteed_bit_rate_for_downlink UDEC 1 } UNUSED PAD 3 } 
  Param3{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } 
  Param4{ A ARRAY 101 [ APN UDEC 1 ] } 
  Param5{ A ARRAY 252 [ PROT_CONFIG_OPTION UDEC 1 ] } 
  Param6{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 }  0
PSSISME_PDP_ACTIVATE_SEC_REQ
  Param1 UDEC 1 
  UNUSED PAD 3 Param2{ version DEC 4 
  r97{ delay_class UDEC 1 reliability_class UDEC 1 precedence_class UDEC 1 
  peak_throughput UDEC 1 mean_throughput UDEC 1 } 
  r99{ Traffic_class UDEC 1 Delivery_order UDEC 1 Delivery_of_erroneous_SDU UDEC 1 
  Maximum_SDU_size UDEC 1 Maximum_bit_rate_for_uplink UDEC 1 Maximum_bit_rate_for_downlink UDEC 1 
  Residual_BER UDEC 1 SDU_error_ratio UDEC 1 Transfer_delay UDEC 1 
  Traffic_handling_priority UDEC 1 Guaranteed_bit_rate_for_uplink UDEC 1 
  Guaranteed_bit_rate_for_downlink UDEC 1 } UNUSED PAD 3 } 
  Param3 HEX 4 Param4{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 }  0
PSSISME_PDP_ACTIVATE_RSP
  Param1{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } Param2 UDEC 1  0
PSSISME_PDP_DEACTIVATE_REQ
  Param1 UDEC 1 Param2 UDEC 1 Param3{ length UDEC 1 value UDEC 1 }  0
PSSISME_PDP_MODIFY_RSP
  Param1 UDEC 1  0
PSSISME_PDP_MODIFY_REQ
  Param1 UDEC 1 Param2 UDEC 1 
  UNUSED PAD 2 Param3{ version DEC 4 
  r97{ delay_class UDEC 1 reliability_class UDEC 1 precedence_class UDEC 1 
  peak_throughput UDEC 1 mean_throughput UDEC 1 } 
  r99{ Traffic_class UDEC 1 Delivery_order UDEC 1 Delivery_of_erroneous_SDU UDEC 1 
  Maximum_SDU_size UDEC 1 Maximum_bit_rate_for_uplink UDEC 1 Maximum_bit_rate_for_downlink UDEC 1 
  Residual_BER UDEC 1 SDU_error_ratio UDEC 1 Transfer_delay UDEC 1 
  Traffic_handling_priority UDEC 1 Guaranteed_bit_rate_for_uplink UDEC 1 
  Guaranteed_bit_rate_for_downlink UDEC 1 } UNUSED PAD 3 } 
  Param4 HEX 4  0
SNSME_ACTIVATE_RSP
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  UNUSED PAD 3 Param3{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 } 
  Param4{ length UDEC 1 value UDEC 1 }  0
SNSME_DEACTIVATE_RSP
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
SNSME_MODIFY_RSP
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
SNSME_STATUS_REQ
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } UNUSED PAD 3 Param3 DEC 4  0
RABMSME_ACTIVATE_RSP
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
RABMSME_DEACTIVATE_RSP
  Param1 UDEC 1  0
RABMSME_MODIFY_RSP
  Param1 UDEC 1  0
RABMSME_STATUS_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
RABMSME_DEACTIVATE_REQ
  Param1 UDEC 1  0
SME_DELETE_REQ
  Param1{ ti_pd UDEC 1 ti_ext UDEC 1 }  0
SME_TERM_REQ
  Param1{ ti_pd UDEC 1 ti_ext UDEC 1 }  0
SME_RELEASE_TDI_IND
  Param1{ ti_pd UDEC 1 ti_ext UDEC 1 } 
  Param2{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] }  0
RAB_INFORM_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
RAB_INFORM_CNF
  Param1 UDEC 1  0
RAB_DEACTIVATE_CNF
  Param1 UDEC 1  0
RAB_RECOVER_REQ
  Param1 UDEC 1 UNUSED PAD 1 Param2 UDEC 2 Param3 UDEC 2 Param4 UDEC 2  0
RAB_SEQUENCE_RSP
  Param1 UDEC 1 UNUSED PAD 1 Param2 UDEC 2 Param3 UDEC 2  0
RAB_INACTIVE_REQ
  Param1 UDEC 1  0
GMRGMS_FORW_GSMS_ASSIGN_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
GMRGMS_FORW_GSMS_UNITDATA_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  Param2{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
GMRGMS_FORW_GSMS_REL_IND
  Param1 DEC 4  0
GMRGMS_FORW_PSSIGSMS_ABORT_REQ
  Param1 DEC 4  0
GMRGMS_FORW_PSSIGSMS_DATA_REQ
  Param1 LIB 1  0
GMRGMS_FORW_PSSIGSMS_EST_REQ
  Param1 LIB 1  0
GMRGMS_FORW_PSSIGSMS_REL_REQ
  Param1 DEC 4  0
GMRGMS_FORW_GSMS_EST_CNF
  Param1 DEC 4  0
GMRGMS_FORW_GMMSMS_CHANGE_PENDING_IND
  Param1 DEC 4  0
GMRGMS_FORW_GMMSMS_CHANGE_SYSTEM_IND
  Param1 DEC 4  0
GMRGMS_FORW_GMMSMS_CANCEL_SYSTEM_IND
  Param1 DEC 4  0
GMRGMS_INIT_IND
  Param1 DEC 4 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } Param3 UDEC 1 UNUSED PAD 3 Param4 DEC 4 
  Param5 UDEC 1  0
GMRGMS_END_IND
  Param1 DEC 4  0
MMCC_DATA_IND
  Param1 LIB 1  0
MMCC_ERR_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
MMCC_EST_CNF
  Param1 DEC 4  0
MMCC_EST_IND
  Param1 LIB 1  0
MMCC_REEST_CNF
  Param1 DEC 4  0
MMCC_REL_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
MMCC_REL_CNF
  Param1 DEC 4  0
MMCC_SYNC_IND
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1  0
MMCC_PROMPT_IND
  Param1 DEC 4  0
MMCC_TI_IND
  Param1 DEC 4 Param2 DEC 4  0
MMCC_SECURITY_IND
  Param1 UDEC 1  0
MMCC_DATA_REQ
  Param1 LIB 1  0
MMCC_EST_REQ
  Param1 DEC 4 Param2 DEC 4  0
MMCC_REEST_REQ
  Param1 DEC 4  0
MMCC_REL_REQ
  Param1 DEC 4 Param2 DEC 4  0
MMCC_START_CC_REQ
  Param1 LIB 1  0
MMCC_CHECK_IF_EMERG_REQ
  Param1 DEC 4 Param2 DEC 4  0
MMSMS_INFO_IND
  Param1 DEC 4 Param2 DEC 4  0
MMSMS_DATA_IND
  Param1 LIB 1  0
MMSMS_ERR_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
MMSMS_EST_CNF
  Param1 DEC 4  0
MMSMS_EST_IND
  Param1 LIB 1  0
MMSMS_REL_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
MMSMS_REL_CNF
  Param1 DEC 4  0
MMSMS_TI_IND
  Param1 DEC 4 Param2 DEC 4  0
MMSMS_DATA_REQ
  Param1 LIB 1  0
MMSMS_EST_REQ
  Param1 DEC 4  0
MMSMS_REL_REQ
  Param1 DEC 4  0
MMSS_DATA_IND
  Param1 LIB 1  0
MMSS_ERR_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
MMSS_EST_CNF
  Param1 DEC 4  0
MMSS_EST_IND
  Param1 LIB 1  0
MMSS_REL_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
MMSS_REL_CNF
  Param1 DEC 4  0
MMSS_TI_IND
  Param1 DEC 4  0
MMSS_DATA_REQ
  Param1 LIB 1  0
MMSS_EST_REQ
  Param1 DEC 4  0
MMSS_REL_REQ
  Param1 DEC 4  0
BMC2RRC_SETUP_IND
  Param1 DEC 4  0
IPR_PDP_CONFIG
  Param1{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } Param2 UDEC 1 
  Param3{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } 
  Param4{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] }  0
IPR_PDP_DEACTIVATE
  Param1 UDEC 1 Param2 UDEC 1  0
PPP_LINK_ACTIVATE
  Param1{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } Param2 UDEC 1 
  Param3{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } 
  Param4{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] }  0
GMMDCM_CHANGE_SYSTEM_IND
  Param1 DEC 4  0
GMMDCM_CHANGE_PENDING_IND
  Param1 DEC 4  0
GMMDCM_CANCEL_CHANGE_IND
  Param1 DEC 4  0
GMMRABM_REESTABLISH_REQ
  Param1 DEC 4  0
GMMRABM_REESTABLISH_REJ
  Param1 DEC 4  0
GMMSM_SEQUENCE_RSP
  Param1{ no_of_nsapi DEC 4 
  list{ A ARRAY 11 [ A{ nsapi UDEC 1 receive_npdu_no UDEC 1 } ] } UNUSED PAD 2 }  0
GMMSM_UNITDATA_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  Param2{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] } Param3 DEC 4  0
GMMSM_STATUS_RSP
  Param1 UDEC 1 Param2 UDEC 1  0
GMMSM_ASSIGN_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
z0E5_GMMSM_ESTABLISH_CNF
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
GMMSM_ESTABLISH_REJ
  Param1 DEC 4  0
GMMSM_RELEASE_IND
  Param1 DEC 4 Param2 DEC 4  0
GMMSM_SEQUENCE_IND
  Param1{ no_of_nsapi DEC 4 
  list{ A ARRAY 11 [ A{ nsapi UDEC 1 receive_npdu_no UDEC 1 } ] } UNUSED PAD 2 }  0
GMMSM_UNITDATA_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  Param2{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
GMMSM_MS_VERSION_IND
  Param1 DEC 4  0
GMMSM_NW_VERSION_IND
  Param1 DEC 4  0
GMMSM_CHANGE_SYSTEM_IND
  Param1 DEC 4 Param2 DEC 4  0
GMMSM_CHANGE_PENDING_IND
  Param1 DEC 4  0
GMMSM_CANCEL_CHANGE_IND
  Param1 DEC 4  0
GMMSMS_EST_REQ
  Param1 DEC 4  0
GMMSMS_UNITDATA_REQ
  Param1{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
GMMSMS_REG_STATE_RSP
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1 Param4{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
GMMSMS_ASSIGN_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
GMMSMS_RELEASE_IND
  Param1 DEC 4  0
GMMSMS_EST_CNF
  Param1 DEC 4  0
GMMSMS_UNITDATA_IND
  Param1{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
GMMSMS_CHANGE_SYSTEM_IND
  Param1 DEC 4  0
GMMSMS_CHANGE_PENDING_IND
  Param1 DEC 4  0
GMMSMS_CANCEL_CHANGE_IND
  Param1 DEC 4  0
GRR_RRC_UPDATE_SHARED_DATA_REQ
  Param1{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 HEX 4 
  Param4 HEX 4 Param5 HEX 4  0
GRR_RRC_CLASSMARK_IND
  Param1{ class2_field{ revision_level UDEC 1 es_ind UDEC 1 a51_supported UDEC 1 a52_supported UDEC 1 
  a53_supported UDEC 1 ps_capability UDEC 1 ss_screen UDEC 1 sm_capability UDEC 1 
  vbs UDEC 1 vgcs UDEC 1 fc UDEC 1 cm3 UDEC 1 lcsva UDEC 1 ucs2_supported UDEC 1 
  solsa_capability UDEC 1 cmsp UDEC 1 } 
  class3_field{ a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 multi_slot_class UDEC 1 ucs2_supported UDEC 1 
  ext_measurement UDEC 1 sms_value UDEC 1 sm_value UDEC 1 ms_positioning_method_cap UDEC 1 
  egprs_multi_slot_class UDEC 1 modulation_capability UDEC 1 edge_rf_power_cap_1 UDEC 1 
  edge_rf_power_cap_2 UDEC 1 umts_fdd_rat_cap UDEC 1 umts_tdd_supported UDEC 1 
  cdma_2000_supported UDEC 1 dtm_gprs_supported UDEC 1 dtm_gprs_multi_slot_subclass UDEC 1 
  mac_mode_supported UDEC 1 dtm_egprs_supported UDEC 1 dtm_egprs_multi_slot_subclass UDEC 1 
  gsm_400_radio_cap UDEC 1 gsm_850_radio_cap UDEC 1 gsm_1900_radio_cap UDEC 1 } 
  band_info_field{ p_gsm_available UDEC 1 e_gsm_available UDEC 1 dcs_available UDEC 1 
  pcs_available UDEC 1 r_gsm_available UDEC 1 gsm_400_available UDEC 1 
  gsm_850_available UDEC 1 p_gsm_pwr_class UDEC 1 e_gsm_pwr_class UDEC 1 
  dcs_pwr_class UDEC 1 pcs_pwr_class UDEC 1 r_gsm_pwr_class UDEC 1 
  gsm_400_pwr_class UDEC 1 gsm_850_pwr_class UDEC 1 gsm_band UDEC 1 
  gsm_400_bands_supported UDEC 1 } 
  UNUSED PAD 3 gprs_caps{ ms_class DEC 4 paging_channels UDEC 1 
  drx{ split_pg_cycle_code UDEC 1 split_on_ccch UDEC 1 timer_val UDEC 1 
  drx_cycle_length_coef UDEC 1 } 
  gea1_supported UDEC 1 gea2_supported UDEC 1 gea3_supported UDEC 1 
  gea4_supported UDEC 1 gea5_supported UDEC 1 gea6_supported UDEC 1 
  gea7_supported UDEC 1 sm_gprs UDEC 1 sm_cap_via_dedicated UDEC 1 
  revi_level_indicator UDEC 1 pfc_feature_mode UDEC 1 multi_slot_class UDEC 1 
  ecsd_multi_slot_class UDEC 1 ext_dyn_alloc UDEC 1 egprs_extended_dynamic_allocation_cap UDEC 1 
  compact_interference_meas UDEC 1 UNUSED PAD 3 } 
  gprs_services UDEC 1 cs_services UDEC 1 UNUSED PAD 2 gsm_release DEC 4 } 
  Param2{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param3{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param4{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 }  0
GRR_RRC_UPDATE_PARAM_REQ
  Param1{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] }  0
GRR_RRC_ASSIGN_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
GRR_RRC_EST_REQ
  Param1 LIB 1 Param2 UDEC 1  0
GRR_RRC_PDCH_ASSIGN_RES
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
GRR_RRC_CELL_CHANGE_RES
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
GRR_RRC_ERROR_IND
  Param1 DEC 4  0
GRR_RRCS_HANDOVER_DECODE_RSP
  Param1 DEC 4 Param2 DEC 4  0
GRR_RRCS_FORWARD_UAS_INFO_IND
  Param1{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 }  0
RRC_GRR_EST_CNF
  Param1 DEC 4  0
RRC_GRR_EST_FAIL
  Param1 DEC 4  0
RRC_GRR_PDCH_ASSIGN_IND
  Param1 DEC 4 
  Param2{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  Param3{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  Param4{ length UDEC 1 content{ A ARRAY 247 [ PACKET_CONSTRUCT_CONTENT UDEC 1 ] } } 
  Param5{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } } 
  Param6{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  Param7{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } }  0
RRC_GRR_CELL_CHANGE_IND
  Param1 UDEC 2 Param2 UDEC 1 UNUSED PAD 1 Param3 DEC 4  0
RRC_GRR_CHN_REL_IND
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1 Param4 UDEC 1 UNUSED PAD 2 Param5 DEC 4  0
RRCS_GRR_HANDOVER_CNF
  Param1 DEC 4 Param2 DEC 4  0
RRCS_GRR_MEAS_INFO_IND
  Param1{ reporting{ Present{ REPORTING_TO_GSMpresent ENUM 1 } UNUSED PAD 3 union ARRAY 12 [ REPORTING_TO_GSM UDEC 1 ] } 
  reportingPresent UDEC 1 
  UNUSED PAD 3 resel_to_umts{ Present{ RESEL_TO_UMTSpresent ENUM 1 } UNUSED PAD 3 union ARRAY 24 [ RESEL_TO_UMTS UDEC 1 ] } 
  resel_to_umtsPresent UDEC 1 
  UNUSED PAD 3 cell_list{ A ARRAY 3 [ A{ arfcn DEC 4 sc_pscg UDEC 1 sc_pscgPresent UDEC 1 
  UNUSED PAD 2 sc_list{ A ARRAY 32 [ SCRAMBLING_CODE_LIST DEC 4 ] } 
  sc_listPresent UDEC 1 UNUSED PAD 3 } ] } 
  cell_listPresent UDEC 1 UNUSED PAD 3 }  0
RRCS_GRR_CELL_CHANGE_ORDER_IND
  Param1{ uarfcn DEC 4 diversity UDEC 1 UNUSED PAD 3 scrambling_code DEC 4 
  bandwidth_present UDEC 1 UNUSED PAD 3 bandwidth DEC 4 }  0
RRCS_GRR_EVENT_NOTIFY_IND
  Param1 DEC 4  0
GRR_MAC_CLASSMARK_IND
  Param1{ class2_field{ revision_level UDEC 1 es_ind UDEC 1 a51_supported UDEC 1 a52_supported UDEC 1 
  a53_supported UDEC 1 ps_capability UDEC 1 ss_screen UDEC 1 sm_capability UDEC 1 
  vbs UDEC 1 vgcs UDEC 1 fc UDEC 1 cm3 UDEC 1 lcsva UDEC 1 ucs2_supported UDEC 1 
  solsa_capability UDEC 1 cmsp UDEC 1 } 
  class3_field{ a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 multi_slot_class UDEC 1 ucs2_supported UDEC 1 
  ext_measurement UDEC 1 sms_value UDEC 1 sm_value UDEC 1 ms_positioning_method_cap UDEC 1 
  egprs_multi_slot_class UDEC 1 modulation_capability UDEC 1 edge_rf_power_cap_1 UDEC 1 
  edge_rf_power_cap_2 UDEC 1 umts_fdd_rat_cap UDEC 1 umts_tdd_supported UDEC 1 
  cdma_2000_supported UDEC 1 dtm_gprs_supported UDEC 1 dtm_gprs_multi_slot_subclass UDEC 1 
  mac_mode_supported UDEC 1 dtm_egprs_supported UDEC 1 dtm_egprs_multi_slot_subclass UDEC 1 
  gsm_400_radio_cap UDEC 1 gsm_850_radio_cap UDEC 1 gsm_1900_radio_cap UDEC 1 } 
  band_info_field{ p_gsm_available UDEC 1 e_gsm_available UDEC 1 dcs_available UDEC 1 
  pcs_available UDEC 1 r_gsm_available UDEC 1 gsm_400_available UDEC 1 
  gsm_850_available UDEC 1 p_gsm_pwr_class UDEC 1 e_gsm_pwr_class UDEC 1 
  dcs_pwr_class UDEC 1 pcs_pwr_class UDEC 1 r_gsm_pwr_class UDEC 1 
  gsm_400_pwr_class UDEC 1 gsm_850_pwr_class UDEC 1 gsm_band UDEC 1 
  gsm_400_bands_supported UDEC 1 } 
  UNUSED PAD 3 gprs_caps{ ms_class DEC 4 paging_channels UDEC 1 
  drx{ split_pg_cycle_code UDEC 1 split_on_ccch UDEC 1 timer_val UDEC 1 
  drx_cycle_length_coef UDEC 1 } 
  gea1_supported UDEC 1 gea2_supported UDEC 1 gea3_supported UDEC 1 
  gea4_supported UDEC 1 gea5_supported UDEC 1 gea6_supported UDEC 1 
  gea7_supported UDEC 1 sm_gprs UDEC 1 sm_cap_via_dedicated UDEC 1 
  revi_level_indicator UDEC 1 pfc_feature_mode UDEC 1 multi_slot_class UDEC 1 
  ecsd_multi_slot_class UDEC 1 ext_dyn_alloc UDEC 1 egprs_extended_dynamic_allocation_cap UDEC 1 
  compact_interference_meas UDEC 1 UNUSED PAD 3 } 
  gprs_services UDEC 1 cs_services UDEC 1 UNUSED PAD 2 gsm_release DEC 4 } 
  Param2{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param3{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param4{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 }  0
GRR_MAC_UPDATE_PARAM_REQ
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ prach_ctrl_param{ acc_contrl_class UDEC 2 max_retrans{ A ARRAY 4 [ PERS_LEVEL UDEC 1 ] } 
  tx_int UDEC 1 s UDEC 1 
  persistence_level{ valid UDEC 1 pers_level{ A ARRAY 4 [ PERS_LEVEL UDEC 1 ] } } UNUSED PAD 1 } 
  rach_ctrl_param{ acc_contrl_class UDEC 2 max_retrans UDEC 1 tx_int UDEC 1 } } 
  Param3 UDEC 2 Param4 UDEC 2 Param5 UDEC 1 UNUSED PAD 3 Param6 DEC 4 
  Param7 UDEC 1 Param8 UDEC 1 Param9 UDEC 1 Param10 UDEC 1  0
GRR_MAC_FREQ_UPDATE_REQ
  Param1{ Present{ FREQ_UPDATEpresent ENUM 1 } union ARRAY 14 [ FREQ_UPDATE UDEC 1 ] }  0
GRR_MAC_DOWNLINK_PDCH_REQ
  Param1{ Present{ PACKET_DOWNL_ASSIGNMENTpresent ENUM 1 } UNUSED PAD 3 union ARRAY 528 [ PACKET_DOWNL_ASSIGNMENT UDEC 1 ] }  0
GRR_MAC_UPLINK_PDCH_REQ
  Param1{ chn_description_aft_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  mobile_allocation_aft_sti{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  packet_construct{ length UDEC 1 content{ A ARRAY 247 [ PACKET_CONSTRUCT_CONTENT UDEC 1 ] } } 
  starting_time{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } } 
  chn_description_bef_sti{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  mobile_allocation_bef_sti{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } }  0
GRR_MAC_UPLINK_PDCH_FAIL
  Param1 DEC 4  0
GRR_MAC_CIRCUIT_REQ
  Param1 DEC 4 Param2 UDEC 1 Param3 UDEC 1  0
MAC_GRR_DOWNLINK_PDCH_FAIL
  Param1 DEC 4  0
MAC_GRR_UPLINK_PDCH_FAIL
  Param1 DEC 4  0
MAC_GRR_UPLINK_PDCH_IND
  Param1 DEC 4  0
MAC_GRR_CIRCUIT_IND
  Param1{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  Param2 UDEC 1 
  UNUSED PAD 1 Param3{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  Param4{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } } 
  Param5{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  Param6 UDEC 1 UNUSED PAD 1 Param7 DEC 4 Param8 DEC 4 Param9 UDEC 1 
  UNUSED PAD 3 Param10 DEC 4 Param11 DEC 4 Param12 DEC 4 Param13 UDEC 1 
  UNUSED PAD 1 Param14 UDEC 2 Param15 UDEC 1 Param16 UDEC 1 Param17 UDEC 1  0
MAC_GRR_CIRCUIT_CNF
  Param1{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  Param2 UDEC 1 
  UNUSED PAD 1 Param3{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  Param4{ start_time_present UDEC 1 start_time{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 } } 
  Param5{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  Param6 UDEC 1  0
MAC_GRR_CIRCUIT_FAIL
  Param1 DEC 4  0
MAC_GRR_START_T3122
  Param1 UDEC 1  0
MAC_GRR_PROHIBIT_PACKET_ACCESS
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
MAC_GRR_DATA_IND
  Param1 UDEC 4 Param2 HEX 4 Param3 UDEC 1  0
MAC_GRR_FREQ_UPDATE_REQ
  Param1{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } }  0
MAC_GRR_PAGE_MODE_IND
  Param1 UDEC 1  0
MAC_GRR_PERS_LEVEL_IND
  Param1{ valid UDEC 1 pers_level{ A ARRAY 4 [ PERS_LEVEL UDEC 1 ] } }  0
GRR_RLC_RESUME_REQ
  Param1 UDEC 1  0
GRR_RLC_UPDATE_PARAM_REQ
  Param1 UDEC 2 Param2 UDEC 1 Param3 UDEC 1 Param4 UDEC 1 Param5 UDEC 1 
  Param6 UDEC 1 Param7 UDEC 1  0
GRR_RLC_ACCESS_REJ
  Param1 DEC 4  0
GRR_RLC_REL_PDCH_REQ
  Param1 DEC 4  0
GRR_RLC_UPLINK_PDCH_REQ
  Param1 DEC 4 
  Param2{ block_format DEC 4 pdch_block ARRAY 56 [ PDCH_BLOCK UDEC 1 ] }  0
GRR_RLC_DATA_REQ
  Param1 DEC 4 
  Param2{ block_format DEC 4 pdch_block ARRAY 56 [ PDCH_BLOCK UDEC 1 ] }  0
GRR_RLC_STATUS_IND
  Param1 DEC 4  0
GRR_RLC_CELL_CHANGE_IND
  Param1 UDEC 1 Param2 UDEC 1  0
GRR_RLC_CLASSMARK_IND
  Param1{ class2_field{ revision_level UDEC 1 es_ind UDEC 1 a51_supported UDEC 1 a52_supported UDEC 1 
  a53_supported UDEC 1 ps_capability UDEC 1 ss_screen UDEC 1 sm_capability UDEC 1 
  vbs UDEC 1 vgcs UDEC 1 fc UDEC 1 cm3 UDEC 1 lcsva UDEC 1 ucs2_supported UDEC 1 
  solsa_capability UDEC 1 cmsp UDEC 1 } 
  class3_field{ a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 multi_slot_class UDEC 1 ucs2_supported UDEC 1 
  ext_measurement UDEC 1 sms_value UDEC 1 sm_value UDEC 1 ms_positioning_method_cap UDEC 1 
  egprs_multi_slot_class UDEC 1 modulation_capability UDEC 1 edge_rf_power_cap_1 UDEC 1 
  edge_rf_power_cap_2 UDEC 1 umts_fdd_rat_cap UDEC 1 umts_tdd_supported UDEC 1 
  cdma_2000_supported UDEC 1 dtm_gprs_supported UDEC 1 dtm_gprs_multi_slot_subclass UDEC 1 
  mac_mode_supported UDEC 1 dtm_egprs_supported UDEC 1 dtm_egprs_multi_slot_subclass UDEC 1 
  gsm_400_radio_cap UDEC 1 gsm_850_radio_cap UDEC 1 gsm_1900_radio_cap UDEC 1 } 
  band_info_field{ p_gsm_available UDEC 1 e_gsm_available UDEC 1 dcs_available UDEC 1 
  pcs_available UDEC 1 r_gsm_available UDEC 1 gsm_400_available UDEC 1 
  gsm_850_available UDEC 1 p_gsm_pwr_class UDEC 1 e_gsm_pwr_class UDEC 1 
  dcs_pwr_class UDEC 1 pcs_pwr_class UDEC 1 r_gsm_pwr_class UDEC 1 
  gsm_400_pwr_class UDEC 1 gsm_850_pwr_class UDEC 1 gsm_band UDEC 1 
  gsm_400_bands_supported UDEC 1 } 
  UNUSED PAD 3 gprs_caps{ ms_class DEC 4 paging_channels UDEC 1 
  drx{ split_pg_cycle_code UDEC 1 split_on_ccch UDEC 1 timer_val UDEC 1 
  drx_cycle_length_coef UDEC 1 } 
  gea1_supported UDEC 1 gea2_supported UDEC 1 gea3_supported UDEC 1 
  gea4_supported UDEC 1 gea5_supported UDEC 1 gea6_supported UDEC 1 
  gea7_supported UDEC 1 sm_gprs UDEC 1 sm_cap_via_dedicated UDEC 1 
  revi_level_indicator UDEC 1 pfc_feature_mode UDEC 1 multi_slot_class UDEC 1 
  ecsd_multi_slot_class UDEC 1 ext_dyn_alloc UDEC 1 egprs_extended_dynamic_allocation_cap UDEC 1 
  compact_interference_meas UDEC 1 UNUSED PAD 3 } 
  gprs_services UDEC 1 cs_services UDEC 1 UNUSED PAD 2 gsm_release DEC 4 } 
  Param2{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param3{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param4{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 }  0
RLC_GRR_ACCESS_REQ
  Param1 UDEC 1  0
RLC_GRR_UPLINK_PDCH_FAIL
  Param1 DEC 4  0
RLC_GRR_ERROR_IND
  Param1 DEC 4  0
RLC_GRR_REL_PDCH_IND
  Param1 DEC 4  0
RLC_GRR_STATUS_IND
  Param1 DEC 4  0
MPH_RXLEV_REQ
  rf_list{ num_of_chans UDEC 2 chan_number{ A ARRAY 32 [ CHAN_LIST UDEC 2 ] } } 
  UNUSED PAD 2 no_samples_rqd DEC 4 min_duration DEC 4 PGSM_rqd UDEC 1 
  EGSM_rqd UDEC 1 PCN1800_rqd UDEC 1 PCS1900_rqd UDEC 1  0
MPH_SYNC_REQ
  Param1 UDEC 2  0
MPH_SYSINFO_REQ
  Param1 UDEC 2 UNUSED PAD 2 Param2 DEC 4 Param3 UDEC 1 Param4 UDEC 1 
  Param5{ psi1_repeat_period UDEC 1 bs_pbcch_blks UDEC 1 pb UDEC 1 tsc UDEC 1 
  tn UDEC 1 
  UNUSED PAD 1 chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  mobile_allocation{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } }  0
MPH_IDLE_MODE_REQ
  Param1 UDEC 2 Param2 UDEC 1 
  UNUSED PAD 1 Param3{ valid UDEC 1 
  UNUSED PAD 1 paging_par{ Present{ PAGING_PARpresent ENUM 1 } UNUSED PAD 1 union ARRAY 142 [ PAGING_PAR UDEC 1 ] } } 
  Param4{ valid UDEC 1 
  UNUSED PAD 1 paging_par{ Present{ PAGING_PARpresent ENUM 1 } UNUSED PAD 1 union ARRAY 142 [ PAGING_PAR UDEC 1 ] } } 
  Param5 DEC 4 Param6{ txpwr UDEC 1 UNUSED PAD 3 page_mode DEC 4 } 
  Param7{ alpha UDEC 1 UNUSED PAD 3 pc_meas_chan DEC 4 t_avg_w UDEC 1 t_avg_t UDEC 1 
  n_avg_i UDEC 1 pb UDEC 1 page_mode DEC 4 bs_prach_blks UDEC 1 multiband_report UDEC 1 
  txpwr UDEC 1 UNUSED PAD 1 nmo DEC 4 } 
  Param8{ num_of_chans UDEC 2 chan_number{ A ARRAY 32 [ CHAN_LIST UDEC 2 ] } } 
  Param9{ chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  channel_type UDEC 1 subchannel UDEC 1 timeslot_no UDEC 1 tsc UDEC 1 } 
  Param10{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } }  0
MPH_UPD_CELL_PARAM_REQ
  Param1 UDEC 1 Param2 UDEC 1 UNUSED PAD 2 Param3 DEC 4 Param4 UDEC 1 
  UNUSED PAD 1 Param5{ num_of_chans UDEC 2 chan_number{ A ARRAY 32 [ CHAN_LIST UDEC 2 ] } } 
  Param6 UDEC 1 Param7 UDEC 1 Param8 UDEC 1 Param9 UDEC 1 Param10 DEC 4 
  Param11 UDEC 1 Param12 UDEC 1  0
MPH_EXTENDED_PAGING_REQ
  Param1 DEC 4  0
MPH_PAGING_REORG_REQ
  Param1 DEC 4  0
MPH_NON_DRX_REQ
  Param1 DEC 4  0
MPH_UPDATE_PAGING_PARAMS
  Param1 DEC 4 
  Param2{ valid UDEC 1 
  UNUSED PAD 1 paging_par{ Present{ PAGING_PARpresent ENUM 1 } UNUSED PAD 1 union ARRAY 142 [ PAGING_PAR UDEC 1 ] } } 
  UNUSED PAD 2 Param3 DEC 4  0
MPH_START_NC_MEAS_REQ
  Param1 UDEC 4 Param2 UDEC 4 Param3 UDEC 1 
  UNUSED PAD 1 Param4{ num_of_chans UDEC 2 chan_number{ A ARRAY 32 [ CHAN_LIST UDEC 2 ] } }  0
MPH_START_EXT_MEAS_REQ
  Param1 UDEC 4 Param2 DEC 4 Param3 UDEC 1 UNUSED PAD 1 Param4 UDEC 2 
  Param5{ num_of_chans UDEC 2 chan_number{ A ARRAY 32 [ CHAN_LIST UDEC 2 ] } }  0
MPH_START_IFLEV_REQ
  Param1{ no_of_chn_groups UDEC 1 
  UNUSED PAD 1 chn_group_list{ A ARRAY 32 [ A{ timeslot_allocation UDEC 1 
  UNUSED PAD 1 chan_sel{ Present{ CHN_SELpresent ENUM 1 } UNUSED PAD 1 union ARRAY 2 [ CHN_SEL UDEC 1 ] } 
  ma_number UDEC 1 UNUSED PAD 1 } ] } }  0
MPH_START_ENH_MEAS_REQ
  Param1 UDEC 4 Param2 UDEC 4 Param3 UDEC 1 Param4 UDEC 1 Param5 UDEC 1 
  UNUSED PAD 1 Param6{ ba_ind UDEC 1 three_g_ba_ind UDEC 1 ba_list_present UDEC 1 
  UNUSED PAD 1 bcch_bsic_list{ num_of_chans UDEC 2 
  chan{ A ARRAY 32 [ A{ arfcn UDEC 2 valid_bsic UDEC 1 UNUSED PAD 1 } ] } } 
  UNUSED PAD 2 abs_idx_start_emr DEC 4 serving_band_rpt DEC 4 scale_ord DEC 4 
  rep_priority UDEC 1 reporting_rate UDEC 1 invalid_bsic_allowed UDEC 1 
  UNUSED PAD 1 rpt_priority_list{ A ARRAY 96 [ REP_PRIORITY_LIST DEC 4 ] } 
  rpt_900_fields{ offset DEC 4 threshold DEC 4 } 
  rpt_1800_fields{ offset DEC 4 threshold DEC 4 } 
  rpt_1900_fields{ offset DEC 4 threshold DEC 4 } 
  rpt_fdd_fields{ offset DEC 4 threshold DEC 4 } network_ctrl_order UDEC 1 
  ncc_permitted UDEC 1 UNUSED PAD 2 }  0
MPH_CLASSMARK_IND
  Param1{ class2_field{ revision_level UDEC 1 es_ind UDEC 1 a51_supported UDEC 1 a52_supported UDEC 1 
  a53_supported UDEC 1 ps_capability UDEC 1 ss_screen UDEC 1 sm_capability UDEC 1 
  vbs UDEC 1 vgcs UDEC 1 fc UDEC 1 cm3 UDEC 1 lcsva UDEC 1 ucs2_supported UDEC 1 
  solsa_capability UDEC 1 cmsp UDEC 1 } 
  class3_field{ a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 multi_slot_class UDEC 1 ucs2_supported UDEC 1 
  ext_measurement UDEC 1 sms_value UDEC 1 sm_value UDEC 1 ms_positioning_method_cap UDEC 1 
  egprs_multi_slot_class UDEC 1 modulation_capability UDEC 1 edge_rf_power_cap_1 UDEC 1 
  edge_rf_power_cap_2 UDEC 1 umts_fdd_rat_cap UDEC 1 umts_tdd_supported UDEC 1 
  cdma_2000_supported UDEC 1 dtm_gprs_supported UDEC 1 dtm_gprs_multi_slot_subclass UDEC 1 
  mac_mode_supported UDEC 1 dtm_egprs_supported UDEC 1 dtm_egprs_multi_slot_subclass UDEC 1 
  gsm_400_radio_cap UDEC 1 gsm_850_radio_cap UDEC 1 gsm_1900_radio_cap UDEC 1 } 
  band_info_field{ p_gsm_available UDEC 1 e_gsm_available UDEC 1 dcs_available UDEC 1 
  pcs_available UDEC 1 r_gsm_available UDEC 1 gsm_400_available UDEC 1 
  gsm_850_available UDEC 1 p_gsm_pwr_class UDEC 1 e_gsm_pwr_class UDEC 1 
  dcs_pwr_class UDEC 1 pcs_pwr_class UDEC 1 r_gsm_pwr_class UDEC 1 
  gsm_400_pwr_class UDEC 1 gsm_850_pwr_class UDEC 1 gsm_band UDEC 1 
  gsm_400_bands_supported UDEC 1 } 
  UNUSED PAD 3 gprs_caps{ ms_class DEC 4 paging_channels UDEC 1 
  drx{ split_pg_cycle_code UDEC 1 split_on_ccch UDEC 1 timer_val UDEC 1 
  drx_cycle_length_coef UDEC 1 } 
  gea1_supported UDEC 1 gea2_supported UDEC 1 gea3_supported UDEC 1 
  gea4_supported UDEC 1 gea5_supported UDEC 1 gea6_supported UDEC 1 
  gea7_supported UDEC 1 sm_gprs UDEC 1 sm_cap_via_dedicated UDEC 1 
  revi_level_indicator UDEC 1 pfc_feature_mode UDEC 1 multi_slot_class UDEC 1 
  ecsd_multi_slot_class UDEC 1 ext_dyn_alloc UDEC 1 egprs_extended_dynamic_allocation_cap UDEC 1 
  compact_interference_meas UDEC 1 UNUSED PAD 3 } 
  gprs_services UDEC 1 cs_services UDEC 1 UNUSED PAD 2 gsm_release DEC 4 } 
  Param2{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param3{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param4{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 }  0
MPH_AVAIL_PLMN_REQ
  NumSamplesReqd DEC 4 min_duration DEC 4 PGSMReqd UDEC 1 EGSMReqd UDEC 1 
  PCNReqd UDEC 1 PCSReqd UDEC 1  0
MPH_DM_BUILD_IN_3G_MEAS_REQ
  Param1{ fdd_ncell_meas_list{ A ARRAY 64 [ A{ index_into_3g_ba_list UDEC 1 reported_value UDEC 1 rssi_present UDEC 1 } ] } 
  num_of_fdd_meas UDEC 1 ba_used_3g UDEC 1 }  0
MPH_DM_START_MEAS_REQ
  Param1{ num_of_chans UDEC 2 chan_number{ A ARRAY 32 [ CHAN_LIST UDEC 2 ] } }  0
MPH_DM_SYNC_CELLS_REQ
  Param1{ num_of_chans UDEC 2 chan_number{ A ARRAY 32 [ CHAN_LIST UDEC 2 ] } }  0
MPH_GET_ALL_PLMNS_REQ
  Param1{ num_of_chans UDEC 2 chan_number{ A ARRAY 70 [ PLMN_CHAN_LIST UDEC 2 ] } }  0
RRGLL1_CS_BEARER_INFO_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
MPH_RXLEV_CNF
  rxlev_list{ A ARRAY 548 [ RXLEV_LIST UDEC 1 ] }  0
MPH_SYNC_CNF
  Param1 UDEC 2 Param2 UDEC 1  0
MPH_SYNC_REJ
  Param1 UDEC 2 Param2 UDEC 1  0
MPH_SYSINFO_CNF
  Param1 UDEC 2 Param2 UDEC 1 Param3 UDEC 1 
  Param4{ block_format DEC 4 radio_block{ A ARRAY 54 [ R_BLOCK UDEC 1 ] } UNUSED PAD 2 } 
  Param5 UDEC 1 Param6 UDEC 1  0
MPH_DATA_IND
  Param1 UDEC 2 Param2 UDEC 1 Param3 UDEC 1 
  Param4{ block_format DEC 4 radio_block{ A ARRAY 54 [ R_BLOCK UDEC 1 ] } UNUSED PAD 2 } 
  Param5 UDEC 1 Param6 UDEC 1 UNUSED PAD 2 Param7 UDEC 4  0
MPH_SYSINFO_REJ
  Param1 UDEC 2 Param2 UDEC 1  0
MPH_SCELL_RXLEV_IND
  serv_cell_meas{ bcch_freq UDEC 2 bsic UDEC 1 rxlev UDEC 1 }  0
MPH_NCELL_RXLEV_IND
  ncell_meas{ A ARRAY 32 [ A{ bcch_freq UDEC 2 bsic UDEC 1 rxlev UDEC 1 } ] }  0
MPH_ERROR_IND
  cause UDEC 1  0
MPH_NC_MEAS_REPORT_IND
  Param1{ bcch_freq UDEC 2 bsic UDEC 1 rxlev UDEC 1 } Param2 UDEC 1 
  UNUSED PAD 1 Param3{ A ARRAY 6 [ A{ bcch_freq UDEC 2 bsic UDEC 1 rxlev UDEC 1 } ] } 
  Param4 UDEC 1 Param5 UDEC 1 
  Param6{ A ARRAY 6 [ A{ index_into_3g_ba_list UDEC 1 reported_value UDEC 1 } ] }  0
MPH_EXT_MEAS_REPORT_IND
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ A ARRAY 32 [ A{ bcch_freq UDEC 2 bsic UDEC 1 rxlev UDEC 1 } ] } 
  Param3{ A ARRAY 8 [ IF_LEVEL_LIST UDEC 1 ] }  0
MPH_ENH_MEAS_REPORT_IND
  PmoUsed UDEC 1 PbcchPresent UDEC 1 Psi3ChangeMark UDEC 1 ServCellDataPresent UDEC 1 
  ServCellMeas{ bcch_freq UDEC 2 bsic UDEC 1 rxlev UDEC 1 } InterfServCellPresent UDEC 1 
  scellIfLevel UDEC 1 
  UNUSED PAD 2 ncell_enh_meas{ BaUsed DEC 4 ThreeGBaUsed DEC 4 BsicSeen UDEC 1 scale UDEC 1 NumRepInvBSICInfo UDEC 1 
  UNUSED PAD 1 RepInvBSICInfoFreqs{ A ARRAY 9 [ A{ bcch_freq UDEC 2 bsic UDEC 1 rxlev UDEC 1 } ] } 
  NumRepeatedQty UDEC 1 NumRepValBSICInfo UDEC 1 
  ReportingQty{ A ARRAY 24 [ A{ radio_freq_no UDEC 2 rxlev UDEC 1 UNUSED PAD 1 } ] } 
  FddMeas{ A ARRAY 24 [ A{ index_into_3g_ba_list UDEC 1 reported_value UDEC 1 } ] } 
  FddMeasCnt UDEC 1 UNUSED PAD 1 }  0
MM_ABORT_IND
  Param1 DEC 4  0
MM_CONN_ABORT_IND
  Param1 DEC 4 Param2 DEC 4  0
MM_DATA_IND
  Param1 LIB 1  0
MM_REL_IND
  Param1 DEC 4 Param2 DEC 4  0
MM_SERV_CNF
  Param1 DEC 4  0
MM_SERV_REJ
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
MM_SYNC_IND
  Param1 DEC 4 Param2 UDEC 1  0
MM_SECURITY_IND
  Param1 UDEC 1  0
MM_RAT_INFO_IND
  Param1 DEC 4  0
MM_MS_VERSION_IND
  Param1 DEC 4  0
MM_NW_VERSION_IND
  Param1 DEC 4  0
MM_PROMPT_IND
  Param1 DEC 4 Param2 DEC 4  0
MM_DATA_REQ
  Param1 LIB 1  0
MM_SERV_ABORT_REQ
  Param1 DEC 4 Param2 DEC 4  0
MM_SERV_REQ
  Param1 DEC 4 Param2 DEC 4  0
MM_REEST_REQ
  Param1 DEC 4 Param2 DEC 4  0
MM_PROMPT_REJ
  Param1 DEC 4  0
MM_EMERGENCY_IND
  Param1 DEC 4  0
GPRS_ATTACH_CNF
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 UDEC 1  0
GPRS_CLASS_QUERY_CNF
  Param1 DEC 4  0
ATPC_STATUS_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
PDP_CONTEXT_CNF
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
PDP_CONTEXT_MODIFY_CNF
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
PDP_ON_LINE_CNF
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
PDP_OFF_LINE_IND
  Param1 DEC 4 Param2 DEC 4  0
PDP_CONTEXT_QUERY_CNF
  Param1 DEC 4 Param2 UDEC 1  0
PDP_ACTIVE_CONTEXTS_CNF
  Param1{ A ARRAY 10 [ CID_ARRAY DEC 4 ] }  0
MT_PDP_CONTEXT_IND
  Param1 DEC 4 Param2{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } UNUSED PAD 1 Param3 DEC 4  0
GPRS_ATTACH_REQ
  Param1 UDEC 1  0
ATPC_STATUS_REQ
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
PDP_CONTEXT_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2{ A ARRAY 10 [ CID_ARRAY DEC 4 ] }  0
PDP_CONTEXT_MODIFY_REQ
  Param1{ A ARRAY 10 [ CID_ARRAY DEC 4 ] }  0
PDP_ON_LINE_REQ
  Param1 DEC 4 Param2{ A ARRAY 10 [ CID_ARRAY DEC 4 ] }  0
PDP_CONTEXT_QUERY_REQ
  Param1 DEC 4  0
MT_PDP_CONTEXT_RSP
  Param1 UDEC 1 UNUSED PAD 3 Param2{ A ARRAY 10 [ CID_ARRAY DEC 4 ] } 
  Param3 DEC 4  0
PDP_CONTEXT_UPDATE_REQ
  Param1 DEC 4  0
RLC_MAC_UPLINK_PDCH_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 DEC 4 Param3 DEC 4 Param4 DEC 4 
  Param5 UDEC 1 Param6 UDEC 1 Param7 UDEC 1 UNUSED PAD 1 Param8 UDEC 2 
  Param9{ length UDEC 1 value UDEC 1 }  0
RLC_MAC_REL_PDCH_REQ
  Param1 DEC 4 Param2 DEC 4  0
RLC_MAC_TLLI_ASSIGN_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
RLC_MAC_MEASUREMENT_REPORT
  Param1{ block_format DEC 4 pdch_block ARRAY 56 [ PDCH_BLOCK UDEC 1 ] }  0
RLC_MAC_DATA_REQ
  Param1{ block_format DEC 4 pdch_block ARRAY 56 [ PDCH_BLOCK UDEC 1 ] }  0
MAC_RLC_UPLINK_PDCH_IND
  Param1 DEC 4 Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4 Param4 UDEC 1 
  UNUSED PAD 3 Param5 DEC 4 
  Param6{ mac_mode DEC 4 number_of_ts UDEC 1 
  UNUSED PAD 3 info{ tbf_type DEC 4 rlc_data_blocks_granted DEC 4 } }  0
MAC_RLC_UPLINK_PDCH_FAIL
  Param1 DEC 4  0
MAC_RLC_REL_PDCH_CNF
  Param1 DEC 4  0
MAC_RLC_UPLINK_PDCH_CNF
  Param1 DEC 4  0
MAC_RLC_DOWNLINK_PDCH_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 DEC 4 Param3 DEC 4 Param4 DEC 4  0
MAC_RLC_DATA_IND
  Param1 UDEC 4 Param2{ A ARRAY 8 [ RADIO_BLOCK_ARRAY HEX 4 ] }  0
MAC_RLC_UPLINK_DATA_IND
  Param1 UDEC 4 Param2 HEX 4 Param3 UDEC 1  0
MAC_RLC_ERROR_IND
  Param1 DEC 4 Param2 DEC 4  0
MAC_RLC_STATUS_IND
  Param1 DEC 4  0
MAC_RLC_TLLI_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
PH_CHN_REL_CNF
  Param1 DEC 4  0
PH_CHN_REL_REQ
  Param1 DEC 4 Param2 DEC 4  0
PH_CONNECT_CNF
  Param1 DEC 4  0
PH_CONNECT_REJ
  Param1 DEC 4 Param2 UDEC 1  0
PH_CONNECT_REQ
  Param1 DEC 4 Param2 DEC 4 
  Param3{ physical_pars_aft_sti{ hopping UDEC 1 UNUSED PAD 1 arfcn UDEC 2 maio UDEC 1 hsn UDEC 1 
  mobile_allocation{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  tsc UDEC 1 UNUSED PAD 1 } 
  power_cntrl_pars{ alpha UDEC 1 gamma_ch_list{ A ARRAY 8 [ GAMMA_VALUE_ARRAY UDEC 1 ] } } 
  dl_power_cntrl_pars{ present UDEC 1 p0 UDEC 1 bts_pwr_ctrl_mode UDEC 1 pr_mode UDEC 1 } 
  starting_time_present UDEC 1 
  starting_time{ Present{ STARTING_FRAME_NUMBERpresent ENUM 1 } UNUSED PAD 3 union ARRAY 8 [ STARTING_FRAME_NUMBER UDEC 1 ] } 
  min_starting_time DEC 4 
  mac_mode_pars{ mac_mode DEC 4 dl_control_timeslot_valid UDEC 1 downlink_control_timeslot UDEC 1 
  UNUSED PAD 2 usf_granularity DEC 4 
  usf{ A ARRAY 8 [ USF_VALUE_ARRAY DEC 4 ] } } } 
  Param4{ ul_timing_advance{ contents DEC 4 value DEC 4 index DEC 4 timeslot UDEC 1 UNUSED PAD 3 } 
  dl_timing_advance{ contents DEC 4 value DEC 4 index DEC 4 timeslot UDEC 1 UNUSED PAD 3 } 
  ul_timeslot_allocation UDEC 1 dl_timeslot_allocation UDEC 1 bef_sti_pars_present UDEC 1 
  UNUSED PAD 1 physical_pars_bef_sti{ hopping UDEC 1 UNUSED PAD 1 arfcn UDEC 2 maio UDEC 1 hsn UDEC 1 
  mobile_allocation{ rf_chan_cnt UDEC 2 rf_chan_no{ A ARRAY 64 [ MA_FIELD UDEC 2 ] } } 
  tsc UDEC 1 UNUSED PAD 1 } UNUSED PAD 2 } 
  Param5{ valid UDEC 1 
  UNUSED PAD 3 starting_time{ Present{ STARTING_FRAME_NUMBERpresent ENUM 1 } UNUSED PAD 3 union ARRAY 8 [ STARTING_FRAME_NUMBER UDEC 1 ] } 
  bitmap UDEC 1 UNUSED PAD 3 interval DEC 4 }  0
PH_MAC_DATA_IND
  Param1 UDEC 4 Param2{ A ARRAY 8 [ RADIO_BLOCK_ARRAY HEX 4 ] } 
  Param3{ A ARRAY 8 [ TIMESLOT_NUMBER_ARRAY UDEC 1 ] } Param4 UDEC 1 
  Param5 UDEC 1  0
PH_RA_CNF
  Param1 UDEC 2 Param2{ n32 UDEC 1 n51 UDEC 1 n26 UDEC 1 }  0
PH_RA_REQ
  Param1 UDEC 2 UNUSED PAD 2 Param2 DEC 4 Param3 DEC 4 Param4 UDEC 1 
  Param5 UDEC 1  0
PH_TA_PWRC_INFO
  Param1{ gamma{ A ARRAY 8 [ GAMMA_VALUE_ARRAY UDEC 1 ] } global_power_control_parameters_present UDEC 1 
  power_control_parameters_present UDEC 1 alpha UDEC 1 t_avg_w UDEC 1 
  t_avg_t UDEC 1 pb UDEC 1 UNUSED PAD 2 pc_meas_chan DEC 4 n_avg_i UDEC 1 
  UNUSED PAD 3 uplink_tbf_timing_advance{ contents DEC 4 value DEC 4 index DEC 4 timeslot UDEC 1 UNUSED PAD 3 } 
  downlink_tbf_timing_advance{ contents DEC 4 value DEC 4 index DEC 4 timeslot UDEC 1 UNUSED PAD 3 } }  0
MAC_MAC_DATA_IND
  Param1 HEX 4 Param2 UDEC 1 UNUSED PAD 3 Param3 HEX 4 Param4 UDEC 1  0
LLGMM_ASSIGN_REQ
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  Param3{ A ARRAY 4 [ TLLI UDEC 1 ] } Param4 UDEC 1 
  Param5{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] }  0
LLGMM_SUSPEND_REQ
  Param1 DEC 4  0
LLGMM_TRIGGER_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 DEC 4  0
LLGMM_UNITDATA_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
LLGMM_STATUS_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
LLGMM_TRIGGER_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
LLGMM_UNITDATA_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  Param2{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
SNPDU_AVAIL_REQ
  Param1 DEC 4  0
z0KK_SNPDU_DEL_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
z0KL_SNPDU_DEL_RSP
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
LL_ESTABLISH_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ length DEC 4 data{ A ARRAY 150 [ SNDCP_XID_ARRAY UDEC 1 ] } UNUSED PAD 2 }  0
LL_ESTABLISH_RSP
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ length DEC 4 data{ A ARRAY 150 [ SNDCP_XID_ARRAY UDEC 1 ] } UNUSED PAD 2 }  0
LL_RELEASE_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 Param3 UDEC 1  0
LL_DATA_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ version DEC 4 
  r97{ delay_class UDEC 1 reliability_class UDEC 1 precedence_class UDEC 1 
  peak_throughput UDEC 1 mean_throughput UDEC 1 } 
  r99{ Traffic_class UDEC 1 Delivery_order UDEC 1 Delivery_of_erroneous_SDU UDEC 1 
  Maximum_SDU_size UDEC 1 Maximum_bit_rate_for_uplink UDEC 1 Maximum_bit_rate_for_downlink UDEC 1 
  Residual_BER UDEC 1 SDU_error_ratio UDEC 1 Transfer_delay UDEC 1 
  Traffic_handling_priority UDEC 1 Guaranteed_bit_rate_for_uplink UDEC 1 
  Guaranteed_bit_rate_for_downlink UDEC 1 } UNUSED PAD 3 } 
  Param4 UDEC 1 Param5 UDEC 1 Param6{ length UDEC 1 value UDEC 1 } 
  Param7{ length UDEC 2 data ARRAY 128 [ SNPDU UDEC 1 ] }  0
LL_UNITDATA_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ version DEC 4 
  r97{ delay_class UDEC 1 reliability_class UDEC 1 precedence_class UDEC 1 
  peak_throughput UDEC 1 mean_throughput UDEC 1 } 
  r99{ Traffic_class UDEC 1 Delivery_order UDEC 1 Delivery_of_erroneous_SDU UDEC 1 
  Maximum_SDU_size UDEC 1 Maximum_bit_rate_for_uplink UDEC 1 Maximum_bit_rate_for_downlink UDEC 1 
  Residual_BER UDEC 1 SDU_error_ratio UDEC 1 Transfer_delay UDEC 1 
  Traffic_handling_priority UDEC 1 Guaranteed_bit_rate_for_uplink UDEC 1 
  Guaranteed_bit_rate_for_downlink UDEC 1 } UNUSED PAD 3 } 
  Param4 UDEC 1 Param5{ length UDEC 1 value UDEC 1 } 
  UNUSED PAD 1 Param6{ length UDEC 2 data ARRAY 128 [ SNPDU UDEC 1 ] }  0
LL_XID_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ length DEC 4 data{ A ARRAY 150 [ SNDCP_XID_ARRAY UDEC 1 ] } UNUSED PAD 2 }  0
LL_XID_RSP
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ length DEC 4 data{ A ARRAY 150 [ SNDCP_XID_ARRAY UDEC 1 ] } UNUSED PAD 2 }  0
SNPDU_AVAIL_IND
  Param1 DEC 4  0
z0KU_SNPDU_DEL_CNF
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
z0KV_SNPDU_DEL_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
LL_ESTABLISH_CNF
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ length DEC 4 data{ A ARRAY 150 [ SNDCP_XID_ARRAY UDEC 1 ] } UNUSED PAD 2 } 
  Param4 UDEC 2 Param5 UDEC 2  0
LL_ESTABLISH_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ length DEC 4 data{ A ARRAY 150 [ SNDCP_XID_ARRAY UDEC 1 ] } UNUSED PAD 2 } 
  Param4 UDEC 2 Param5 UDEC 2  0
LL_RELEASE_CNF
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1  0
LL_RELEASE_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
LL_STATUS_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
LL_RESET_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
LL_DATA_CNF
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 Param3 UDEC 1  0
LL_DATA_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 1 Param3{ length UDEC 2 data ARRAY 128 [ SNPDU UDEC 1 ] }  0
LL_UNITDATA_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 1 Param3{ length UDEC 2 data ARRAY 128 [ SNPDU UDEC 1 ] }  0
LL_XID_CNF
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ length DEC 4 data{ A ARRAY 150 [ SNDCP_XID_ARRAY UDEC 1 ] } UNUSED PAD 2 } 
  Param4 UDEC 2 Param5 UDEC 2  0
LL_XID_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ length DEC 4 data{ A ARRAY 150 [ SNDCP_XID_ARRAY UDEC 1 ] } UNUSED PAD 2 } 
  Param4 UDEC 2 Param5 UDEC 2  0
LLSMS_UNITDATA_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
LLSMS_UNITDATA_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  Param2{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
RLC_DATA_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ ll_buf_id DEC 4 ll_buf_idx UDEC 1 UNUSED PAD 3 pdu_length DEC 4 } 
  Param4 UDEC 1 Param5 UDEC 1 Param6 UDEC 1 UNUSED PAD 1 Param7 DEC 4 
  Param8{ length UDEC 1 value UDEC 1 }  0
RLC_UNITDATA_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ ll_buf_id DEC 4 ll_buf_idx UDEC 1 UNUSED PAD 3 pdu_length DEC 4 } 
  Param4 UDEC 1 Param5 UDEC 1 Param6{ length UDEC 1 value UDEC 1 }  0
RLC_CLEAR_QUEUE_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
LL_RLC_RESUME_MM_REQ
  Param1 DEC 4  0
RLC_ASSIGN_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
RLC_DATA_CNF
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 HEX 4  0
RLC_UNITDATA_CNF
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4 
  Param4 UDEC 1  0
RLC_DATA_IND
  Param1 HEX 4  0
RLC_UNITDATA_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  Param2{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
RLC_CLEAR_QUEUE_CNF
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
RLC_CLEAR_QUEUE_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 DEC 4  0
DCMSN_DATA_IND
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 mode UDEC 1 fc UDEC 1 num_pdu UDEC 1 UNUSED PAD 1 }  0
DCMSN_DATA_CNF
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 result UDEC 1 UNUSED PAD 1 }  0
SN_NPDU_DEL_IND
  Param1 DEC 4  0
SN_NPDU_AVAIL_REQ
  Param1 DEC 4  0
SN_NPDU_AVAIL_IND
  Param1 DEC 4  0
DCMSN_SQ_HANDOVER_RSP
  Param1{ A ARRAY 11 [ A{ nsapi UDEC 1 UNUSED PAD 1 Oldest_Unconfirmed_SN UDEC 2 UL_Send_SN UDEC 2 
  DL_Receive_SN UDEC 2 } ] }  0
DCMSN_BUFFER_STATE_RSP
  Param1 UDEC 1  0
DCMSN_DATA_REQ
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 mode UDEC 1 num_pdu UDEC 1 }  0
DCMSN_DATA_RES
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 result UDEC 1 UNUSED PAD 1 }  0
DCMSN_SQ_RETRIEVE_RSP
  Param1{ A ARRAY 11 [ A{ nsapi UDEC 1 UNUSED PAD 1 Oldest_Unconfirmed_SN UDEC 2 UL_Send_SN UDEC 2 
  DL_Receive_SN UDEC 2 } ] }  0
MCDCM_CS_CHANGE_SYSTEM_IND
  Param1{ rat{ E_MCDM_CS_CHANGE_SYSTEM_IND_RAT ENUM 1 } }  0
PSSISN_XID_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 }  0
SNSM_ACTIVATE_IND
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  UNUSED PAD 3 Param3{ version DEC 4 
  r97{ delay_class UDEC 1 reliability_class UDEC 1 precedence_class UDEC 1 
  peak_throughput UDEC 1 mean_throughput UDEC 1 } 
  r99{ Traffic_class UDEC 1 Delivery_order UDEC 1 Delivery_of_erroneous_SDU UDEC 1 
  Maximum_SDU_size UDEC 1 Maximum_bit_rate_for_uplink UDEC 1 Maximum_bit_rate_for_downlink UDEC 1 
  Residual_BER UDEC 1 SDU_error_ratio UDEC 1 Transfer_delay UDEC 1 
  Traffic_handling_priority UDEC 1 Guaranteed_bit_rate_for_uplink UDEC 1 
  Guaranteed_bit_rate_for_downlink UDEC 1 } UNUSED PAD 3 } 
  Param4 UDEC 1 Param5 UDEC 1 Param6{ length UDEC 1 value UDEC 1 } 
  Param7{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 }  0
SNSM_ASSIGN_IND
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
SNSM_DEACTIVATE_IND
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } UNUSED PAD 3 Param3 DEC 4  0
SNSM_MODIFY_IND
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  UNUSED PAD 3 Param3{ version DEC 4 
  r97{ delay_class UDEC 1 reliability_class UDEC 1 precedence_class UDEC 1 
  peak_throughput UDEC 1 mean_throughput UDEC 1 } 
  r99{ Traffic_class UDEC 1 Delivery_order UDEC 1 Delivery_of_erroneous_SDU UDEC 1 
  Maximum_SDU_size UDEC 1 Maximum_bit_rate_for_uplink UDEC 1 Maximum_bit_rate_for_downlink UDEC 1 
  Residual_BER UDEC 1 SDU_error_ratio UDEC 1 Transfer_delay UDEC 1 
  Traffic_handling_priority UDEC 1 Guaranteed_bit_rate_for_uplink UDEC 1 
  Guaranteed_bit_rate_for_downlink UDEC 1 } UNUSED PAD 3 } 
  Param4 UDEC 1 Param5 UDEC 1 Param6{ length UDEC 1 value UDEC 1 }  0
SNSM_RECOVERY_IND
  Param1{ nsapi_array{ A ARRAY 15 [ A{ nsapi UDEC 1 
  UNUSED PAD 3 qos{ version DEC 4 
  r97{ delay_class UDEC 1 reliability_class UDEC 1 precedence_class UDEC 1 
  peak_throughput UDEC 1 mean_throughput UDEC 1 } 
  r99{ Traffic_class UDEC 1 Delivery_order UDEC 1 Delivery_of_erroneous_SDU UDEC 1 
  Maximum_SDU_size UDEC 1 Maximum_bit_rate_for_uplink UDEC 1 Maximum_bit_rate_for_downlink UDEC 1 
  Residual_BER UDEC 1 SDU_error_ratio UDEC 1 Transfer_delay UDEC 1 
  Traffic_handling_priority UDEC 1 Guaranteed_bit_rate_for_uplink UDEC 1 
  Guaranteed_bit_rate_for_downlink UDEC 1 } UNUSED PAD 3 } 
  sapi UDEC 1 radio_priority UDEC 1 
  UNUSED PAD 2 sndcp_compression{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 } } ] } 
  len DEC 4 }  0
SNSM_SEQUENCE_IND
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } UNUSED PAD 3 Param3 DEC 4  0
SNSM_ACTIVATE_RSP
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  UNUSED PAD 3 Param3{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 }  0
SNSM_DEACTIVATE_RSP
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
SNSM_MODIFY_RSP
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
SNSM_SEQUENCE_RSP
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } UNUSED PAD 3 Param3 DEC 4  0
SNSM_STATUS_REQ
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] } UNUSED PAD 3 Param3 DEC 4  0
PSSISM_PDP_ACTIVATE_CNF
  Param1 UDEC 1 
  Param2{ reliability_class UDEC 1 precedence_class UDEC 1 mean_throughput UDEC 1 
  delivery_of_erroneous_sdu UDEC 1 maximum_sdu_size UDEC 1 maximum_bit_rate_for_uplink UDEC 1 
  maximum_bit_rate_for_downlink UDEC 1 sdu_error_ratio UDEC 1 traffic_handling_priority UDEC 1 
  guaranteed_bit_rate_for_uplink UDEC 1 guaranteed_bit_rate_for_downlink UDEC 1 } 
  Param3 UDEC 1 Param4{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } 
  Param5{ A ARRAY 252 [ PROT_CONFIG_OPTION UDEC 1 ] } 
  Param6{ length UDEC 1 value UDEC 1 } UNUSED PAD 2 Param7 DEC 4 
  Param8{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 }  0
PSSISM_PDP_ACTIVATE_IND
  Param1{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } 
  Param2{ A ARRAY 101 [ APN UDEC 1 ] }  0
PSSISM_PDP_ACTIVATE_REJ
  Param1 UDEC 1 Param2 UDEC 1 Param3{ A ARRAY 252 [ PROT_CONFIG_OPTION UDEC 1 ] } 
  UNUSED PAD 2 Param4 DEC 4  0
PSSISM_PDP_DEACTIVATE_CNF
  Param1 UDEC 1  0
PSSISM_PDP_DEACTIVATE_IND
  Param1 UDEC 1 Param2 UDEC 1 Param3 UDEC 1 Param4{ length UDEC 1 value UDEC 1 } 
  UNUSED PAD 3 Param5 DEC 4  0
PSSISM_PDP_MODIFY_IND
  Param1 UDEC 1 
  Param2{ reliability_class UDEC 1 precedence_class UDEC 1 mean_throughput UDEC 1 
  delivery_of_erroneous_sdu UDEC 1 maximum_sdu_size UDEC 1 maximum_bit_rate_for_uplink UDEC 1 
  maximum_bit_rate_for_downlink UDEC 1 sdu_error_ratio UDEC 1 traffic_handling_priority UDEC 1 
  guaranteed_bit_rate_for_uplink UDEC 1 guaranteed_bit_rate_for_downlink UDEC 1 } 
  Param3{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } 
  Param4{ length UDEC 1 value UDEC 1 } UNUSED PAD 3 Param5 DEC 4  0
PSSISM_PDP_MODIFY_CNF
  Param1 UDEC 1 Param2 UDEC 1 
  Param3{ reliability_class UDEC 1 precedence_class UDEC 1 mean_throughput UDEC 1 
  delivery_of_erroneous_sdu UDEC 1 maximum_sdu_size UDEC 1 maximum_bit_rate_for_uplink UDEC 1 
  maximum_bit_rate_for_downlink UDEC 1 sdu_error_ratio UDEC 1 traffic_handling_priority UDEC 1 
  guaranteed_bit_rate_for_uplink UDEC 1 guaranteed_bit_rate_for_downlink UDEC 1 } 
  Param4{ length UDEC 1 value UDEC 1 }  0
PSSISM_PDP_MODIFY_REJ
  Param1 UDEC 1 Param2 UDEC 1 UNUSED PAD 2 Param3 DEC 4  0
PSSISM_PDP_ACTIVATE_SEC_CNF
  Param1 UDEC 1 Param2{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } 
  Param3{ reliability_class UDEC 1 precedence_class UDEC 1 mean_throughput UDEC 1 
  delivery_of_erroneous_sdu UDEC 1 maximum_sdu_size UDEC 1 maximum_bit_rate_for_uplink UDEC 1 
  maximum_bit_rate_for_downlink UDEC 1 sdu_error_ratio UDEC 1 traffic_handling_priority UDEC 1 
  guaranteed_bit_rate_for_uplink UDEC 1 guaranteed_bit_rate_for_downlink UDEC 1 } 
  Param4{ length UDEC 1 value UDEC 1 } UNUSED PAD 3 Param5 DEC 4 
  Param6{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 }  0
PSSISM_PDP_ACTIVATE_SEC_REJ
  Param1 UDEC 1 Param2 UDEC 1 UNUSED PAD 2 Param3 DEC 4  0
PSSISM_PDP_ACTIVATE_REQ
  Param1 UDEC 1 
  Param2{ reliability_class UDEC 1 precedence_class UDEC 1 mean_throughput UDEC 1 
  delivery_of_erroneous_sdu UDEC 1 maximum_sdu_size UDEC 1 maximum_bit_rate_for_uplink UDEC 1 
  maximum_bit_rate_for_downlink UDEC 1 sdu_error_ratio UDEC 1 traffic_handling_priority UDEC 1 
  guaranteed_bit_rate_for_uplink UDEC 1 guaranteed_bit_rate_for_downlink UDEC 1 } 
  Param3{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } 
  Param4{ A ARRAY 101 [ APN UDEC 1 ] } 
  Param5{ A ARRAY 252 [ PROT_CONFIG_OPTION UDEC 1 ] } 
  Param6{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 }  0
PSSISM_PDP_ACTIVATE_REJ_RSP
  Param1{ A ARRAY 19 [ PDP_ADDRESS UDEC 1 ] } Param2 UDEC 1 
  Param3{ A ARRAY 101 [ APN UDEC 1 ] }  0
PSSISM_PDP_DEACTIVATE_REQ
  Param1 UDEC 1 Param2 UDEC 1 Param3{ length UDEC 1 value UDEC 1 }  0
PSSISM_PDP_ACTIVATE_SEC_REQ
  Param1 UDEC 1 
  Param2{ reliability_class UDEC 1 precedence_class UDEC 1 mean_throughput UDEC 1 
  delivery_of_erroneous_sdu UDEC 1 maximum_sdu_size UDEC 1 maximum_bit_rate_for_uplink UDEC 1 
  maximum_bit_rate_for_downlink UDEC 1 sdu_error_ratio UDEC 1 traffic_handling_priority UDEC 1 
  guaranteed_bit_rate_for_uplink UDEC 1 guaranteed_bit_rate_for_downlink UDEC 1 } 
  Param3 UDEC 1 UNUSED PAD 3 Param4 HEX 4 
  Param5{ SNDCP_HC_Algorithm DEC 4 SNDCP_DC_Algorithm DEC 4 }  0
PSSISM_PDP_MODIFY_RSP
  Param1 UDEC 1  0
PSSISM_PDP_MODIFY_REQ
  Param1 UDEC 1 Param2 UDEC 1 
  Param3{ reliability_class UDEC 1 precedence_class UDEC 1 mean_throughput UDEC 1 
  delivery_of_erroneous_sdu UDEC 1 maximum_sdu_size UDEC 1 maximum_bit_rate_for_uplink UDEC 1 
  maximum_bit_rate_for_downlink UDEC 1 sdu_error_ratio UDEC 1 traffic_handling_priority UDEC 1 
  guaranteed_bit_rate_for_uplink UDEC 1 guaranteed_bit_rate_for_downlink UDEC 1 } 
  UNUSED PAD 3 Param4 HEX 4  0
SIEF_GET_SIM_INFO_RSP
  Param1 HEX 4  0
PSSIGSMS_ALLOC_CNF
  Param1 DEC 4  0
PSSIGSMS_ALLOC_REJ
  Param1 DEC 4  0
PSSIGSMS_DATA_IND
  Param1 LIB 1  0
PSSIGSMS_ERROR_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
PSSIGSMS_EST_IND
  Param1 LIB 1  0
PSSIGSMS_REL_IND
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
PSSIGSMS_ABORT_REQ
  Param1 DEC 4  0
PSSIGSMS_DATA_REQ
  Param1 LIB 1  0
PSSIGSMS_EST_REQ
  Param1 LIB 1  0
PSSIGSMS_REL_REQ
  Param1 DEC 4  0
CPMMNG_ATTACH_RSP
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1 Param4 UDEC 1 UNUSED PAD 2 Param5 DEC 4 
  Param6 DEC 4 Param7 UDEC 1 Param8 UDEC 1 
  Param9{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } UNUSED PAD 2 Param10 DEC 4 
  Param11 DEC 4  0
CPMMNG_ATTACH_IND
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1 Param4 UDEC 1 UNUSED PAD 2 Param5 DEC 4 
  Param6 DEC 4 Param7 UDEC 1 Param8 UDEC 1 
  Param9{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } UNUSED PAD 2 Param10 DEC 4 
  Param11 DEC 4  0
CPMMNG_DETACH_CNF
  Param1 DEC 4 Param2 DEC 4  0
CPMMNG_DETACH_IND
  Param1 DEC 4 Param2 DEC 4  0
CPMMNG_PLMN_LIST_CNF
  Param1{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } rat DEC 4 forbidden_indicator DEC 4 
  placement_indicator DEC 4 }  0
CPMMNG_INTER_RAT_HO_IND
  Param1 DEC 4 Param2 DEC 4  0
CPMMNG_ATTACH_REQ
  Param1 DEC 4 Param2 DEC 4 Param3{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } 
  Param4 DEC 4 Param5 DEC 4 Param6 UDEC 1 Param7 UDEC 1  0
CPMMNG_DETACH_REQ
  Param1 DEC 4 Param2 UDEC 1 Param3 UDEC 1  0
CPMMNG_USER_PLMN_CHANGE_REQ
  Param1 DEC 4  0
HWMI_KEYPRESS_IND
  Param1 DEC 4 Param2 DEC 4  0
HWMI_KEYREL_IND
  Param1 DEC 4 Param2 DEC 4  0
GTCPMM_CS_DATA_IND
  Param1 LIB 1  0
GTCPMM_PS_DATA_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } 
  Param2{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
GTCPMM_CS_DATA_REQ
  Param1 LIB 1  0
TCRABC_TEST_REQ
  Param1 UDEC 1  0
TCRABC_TEST_LOOP_REQ
  Param1 UDEC 1 Param2 UDEC 1 
  Param3{ A ARRAY 4 [ A{ rlc_sdu_size UDEC 2 rbid UDEC 1 UNUSED PAD 1 } ] }  0
TCRABC_TEST_LOOP_CNF
  Param1 UDEC 1  0
TCMMC_TEST_REQ
  Param1 UDEC 1  0
TCMME_TEST_REQ
  Param1 UDEC 1  0
TCMM_DATA_REQ
  Param1 LIB 1  0
TCMM_DATA_IND
  Param1 LIB 1  0
TCGMM_TEST_REQ
  Param1 UDEC 1  0
TCGMM_UNITDATA_REQ
  Param1{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
TCGMM_UNITDATA_IND
  Param1{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
L1F_HANDOVER_PARAMS
  Param1 UDEC 4 Param2 DEC 4 Param3 DEC 4 Param4 UDEC 4 Param5 UDEC 1 
  UNUSED PAD 1 Param6 UDEC 2 Param7 UDEC 1 UNUSED PAD 3 Param8 UDEC 4 
  Param9 UDEC 1 UNUSED PAD 1 Param10 UDEC 2 Param11 UDEC 1 Param12 UDEC 1 
  UNUSED PAD 2 Param13 UDEC 4 Param14 UDEC 4 Param15 UDEC 4  0
L1F_FCB_DETECTED
  Param1 UDEC 2  0
L1F_SB_DETECTED
  Param1 UDEC 2 Param2 UDEC 1  0
L1F_BSIC_RECONF_DONE
  Param1 UDEC 2  0
L1F_BSIC_RECONF
  success UDEC 1 UNUSED PAD 1 arfcn UDEC 2 timing_offset DEC 4 fn_offset UDEC 4 
  freq_corr DEC 4 bsic UDEC 1 search_state UDEC 1 UNUSED PAD 2  0
L1F_SYNC_FAILURE
  Param1 UDEC 2  0
L1F_BSIC_RECONF_FAIL
  Param1 UDEC 2  0
L1F_BCCH_DATA_IND
  Param1 UDEC 2 Param2 UDEC 1 Param3 UDEC 1 
  Param4{ A ARRAY 23 [ RADIO_FRAME UDEC 1 ] } Param5 UDEC 1 Param6 UDEC 1  0
L1F_FRMS_TO_NEXT_ACT
  Param1 DEC 4 Param2 DEC 4  0
L1F_EXT_MEASUREMENTS_EVENT
  Param1 DEC 4  0
L1F_PLMN_DELAY_INSERT
  Param1 UDEC 1 Param2 UDEC 1  0
L1C_SYNC_STATUS_RPT
  arfcn UDEC 2 fcb_status UDEC 1 sb_status UDEC 1 sb_data0 DEC 4 sb_data1 DEC 4 
  tim_offset DEC 4  0
L1F_INSERT_ULL1_ALLOC
  Param1{ Start_FN DEC 4 Start_mfrm DEC 4 Num_Frames DEC 4 a_list DEC 4 }  0
DTN_ABORT
  Param1 UDEC 1  0
DTN_DISC_REQ
  Param1 UDEC 1  0
DTN_REMAP
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4  0
DTN_SUSPEND_REQ
  Param1 UDEC 1  0
DTN_RESUME_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4  0
DTN_SYNC_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4 Param4 DEC 4 
  Param5{ rlp_vers DEC 4 rlp_kim DEC 4 rlp_kmi DEC 4 rlp_t1 DEC 4 rlp_n2 DEC 4 
  rlp_t2 DEC 4 } 
  Param6{ direction DEC 4 max_dict UDEC 4 max_string DEC 4 } 
  Param7{ direction DEC 4 max_dict UDEC 4 max_string DEC 4 } Param8 DEC 4 
  Param9{ pending_td DEC 4 pending_rd DEC 4 max_time DEC 4 }  0
DTN_STATUS_REQ
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
DTN_ABORT_CNF
  Param1 UDEC 1  0
DTN_DISC_CNF
  Param1 UDEC 1  0
DTN_DISC_IND
  Param1 UDEC 1  0
DTN_SYNC_CNF
  Param1 UDEC 1 UNUSED PAD 3 Param2{ direction DEC 4 max_dict UDEC 4 max_string DEC 4 }  0
DTN_SYNC_REJ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
DTN_STATUS_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4 Param4 DEC 4  0
DTN_SYNC_ACC
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
DTN_SUSPEND_ACC
  Param1 UDEC 1  0
DTN_RESUME_ACC
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
DTT_ABORT
  Param1 UDEC 1  0
DTT_DISC_REQ
  Param1 UDEC 1  0
DTT_SUSPEND_REQ
  Param1 UDEC 1  0
DTT_RESUME_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4  0
DTT_SYNC_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4 
  Param4{ pending_td DEC 4 pending_rd DEC 4 max_time DEC 4 }  0
DTT_STATUS_REQ
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
DTT_ABORT_CNF
  Param1 UDEC 1  0
DTT_DISC_CNF
  Param1 UDEC 1  0
DTT_SYNC_CNF
  Param1 UDEC 1  0
DTT_SYNC_REJ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
DTT_STATUS_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4 Param4 DEC 4  0
DTT_SYNC_ACC
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
DTT_SUSPEND_ACC
  Param1 UDEC 1  0
DTT_RESUME_ACC
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
DTT_DISC_IND
  Param1 UDEC 1  0
CSD_START_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4 Param4 DEC 4 
  Param5 DEC 4 Param6{ pending_td DEC 4 pending_rd DEC 4 max_time DEC 4 } 
  Param7{ rlp_vers DEC 4 rlp_kim DEC 4 rlp_kmi DEC 4 rlp_t1 DEC 4 rlp_n2 DEC 4 
  rlp_t2 DEC 4 } 
  Param8{ direction DEC 4 max_dict UDEC 4 max_string DEC 4 } Param9 DEC 4  0
CSD_STOP_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
CSD_RESUME_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4  0
CSD_SUSPEND_REQ
  Param1 UDEC 1  0
CSD_STATUS_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
CSD_START_CNF
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
CSD_STOP_CNF
  Param1 UDEC 1  0
CSD_SUSPEND_CNF
  Param1 UDEC 1  0
CSD_DISC_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
CSD_CONNECT_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
CSD_SYNC_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2{ direction DEC 4 max_dict UDEC 4 max_string DEC 4 } 
  Param3 DEC 4  0
CSD_RESUME_CNF
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4  0
DRL_UI_IND
  Param1{ A ARRAY 67 [ DRL_FRAME UDEC 1 ] }  0
DRL_XID_IND
  Param1{ rlp_vers DEC 4 rlp_kim DEC 4 rlp_kmi DEC 4 rlp_t1 DEC 4 rlp_n2 DEC 4 
  rlp_t2 DEC 4 } 
  Param2 DEC 4 Param3{ direction DEC 4 max_dict UDEC 4 max_string DEC 4 }  0
DRL_REMAP_CNF
  Param1 DEC 4  0
DRL_ATTACH_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 Param3 DEC 4 
  Param4{ rlp_vers DEC 4 rlp_kim DEC 4 rlp_kmi DEC 4 rlp_t1 DEC 4 rlp_n2 DEC 4 
  rlp_t2 DEC 4 } 
  Param5 DEC 4 Param6{ direction DEC 4 max_dict UDEC 4 max_string DEC 4 }  0
DRL_TEST_REQ
  Param1{ A ARRAY 67 [ DRL_FRAME UDEC 1 ] }  0
DRL_UI_REQ
  Param1{ A ARRAY 67 [ DRL_FRAME UDEC 1 ] }  0
DRL_XID_REQ
  Param1{ rlp_vers DEC 4 rlp_kim DEC 4 rlp_kmi DEC 4 rlp_t1 DEC 4 rlp_n2 DEC 4 
  rlp_t2 DEC 4 } 
  Param2 DEC 4 Param3{ direction DEC 4 max_dict UDEC 4 max_string DEC 4 }  0
DRL_REMAP_REQ
  Param1 DEC 4  0
RBH_MAC_DATA_BLOCKS_SENT
  Param1 UDEC 1  0
RBH_MAC_RESOURCES_LOST
  Param1 UDEC 1  0
RBH_MAC_DBLK_POLL_RESP_SENT
  Param1 UDEC 1 Param2 UDEC 1  0
RBH_MAC_UL_ESTABLISH_SENT
  Param1 UDEC 1  0
PSSIBMC_START_REQ
  Param1{ msg_id_filter_flag UDEC 1 UNUSED PAD 3 msg_id_filter DEC 4 } 
  Param2{ alphabet_flag UDEC 1 UNUSED PAD 3 alphabet_list{ A ARRAY 13 [ CB_ALPHABET_ARR DEC 4 ] } } 
  Param3{ language_flag UDEC 1 UNUSED PAD 3 language_list{ A ARRAY 13 [ CB_LANGUAGE_ARR DEC 4 ] } } 
  Param4{ power_sav_flag UDEC 1 UNUSED PAD 3 power_sav_duration DEC 4 power_sav_durationPresent UDEC 1 UNUSED PAD 3 } 
  Param5{ max_pages_flag UDEC 1 UNUSED PAD 3 max_pages DEC 4 max_pagesPresent UDEC 1 UNUSED PAD 3 } 
  Param6{ max_messages_flag UDEC 1 UNUSED PAD 3 max_messages DEC 4 max_messagesPresent UDEC 1 UNUSED PAD 3 } 
  Param7{ repeat_ind_flag UDEC 1 UNUSED PAD 3 repeat_ind DEC 4 repeat_indPresent UDEC 1 UNUSED PAD 3 }  0
PSSIBMC_ACTIVATE_REQ
  Param1{ msg_id_flag UDEC 1 UNUSED PAD 3 msg_id_len DEC 4 
  msg_id_list{ A ARRAY 255 [ CB_MSG_ID_LIST DEC 4 ] } } 
  Param2{ msg_id_flag UDEC 1 UNUSED PAD 3 msg_id_len DEC 4 
  msg_id_list{ A ARRAY 255 [ CB_MSG_ID_LIST DEC 4 ] } } 
  Param3{ msg_id_flag UDEC 1 UNUSED PAD 3 msg_id_len DEC 4 
  msg_id_list{ A ARRAY 255 [ A{ low_msg_id DEC 4 high_msg_id DEC 4 } ] } }  0
PSSIBMC_DEACTIVATE_REQ
  Param1{ msg_id_flag UDEC 1 UNUSED PAD 3 msg_id_len DEC 4 
  msg_id_list{ A ARRAY 255 [ CB_MSG_ID_LIST DEC 4 ] } } 
  Param2{ msg_id_flag UDEC 1 UNUSED PAD 3 msg_id_len DEC 4 
  msg_id_list{ A ARRAY 255 [ CB_MSG_ID_LIST DEC 4 ] } } 
  Param3{ msg_id_flag UDEC 1 UNUSED PAD 3 msg_id_len DEC 4 
  msg_id_list{ A ARRAY 255 [ A{ low_msg_id DEC 4 high_msg_id DEC 4 } ] } }  0
PSSIBMC_FILTER_REQ
  Param1{ msg_id_filter_flag UDEC 1 UNUSED PAD 3 msg_id_filter DEC 4 } 
  Param2{ alphabet_flag UDEC 1 UNUSED PAD 3 alphabet_list{ A ARRAY 13 [ CB_ALPHABET_ARR DEC 4 ] } } 
  Param3{ language_flag UDEC 1 UNUSED PAD 3 language_list{ A ARRAY 13 [ CB_LANGUAGE_ARR DEC 4 ] } } 
  Param4{ power_sav_flag UDEC 1 UNUSED PAD 3 power_sav_duration DEC 4 power_sav_durationPresent UDEC 1 UNUSED PAD 3 } 
  Param5{ max_pages_flag UDEC 1 UNUSED PAD 3 max_pages DEC 4 max_pagesPresent UDEC 1 UNUSED PAD 3 } 
  Param6{ max_messages_flag UDEC 1 UNUSED PAD 3 max_messages DEC 4 max_messagesPresent UDEC 1 UNUSED PAD 3 } 
  Param7{ repeat_ind_flag UDEC 1 UNUSED PAD 3 repeat_ind DEC 4 repeat_indPresent UDEC 1 UNUSED PAD 3 }  0
PSSIBMC_DATA_IND
  Param1{ serial_no DEC 4 msg_id DEC 4 
  dcs{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } pages DEC 4 
  msg{ A ARRAY 15 [ A{ cbMessageInformationPage{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } 
  cbMessageInformationPadding{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } 
  cbMessageInformationPaddingPresent UDEC 1 UNUSED PAD 3 } ] } }  0
PSSIDCM_PS_UCH_CONN_REQ
  Param1 UDEC 1 Param2 UDEC 1 UNUSED PAD 2 Param3 DEC 4 Param4 UDEC 1  0
PSSIDCM_PS_UCH_DISC_REQ
  Param1 UDEC 1  0
PSSIDCM_CS_UCH_CONN_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
PSSIDCM_CS_UCH_DISC_REQ
  Param1 UDEC 1  0
PSSIDCM_PS_UCH_CONN_CNF
  Param1 UDEC 1  0
PSSIDCM_PS_UCH_CONN_REJ
  Param1 UDEC 1  0
PSSIDCM_PS_UCH_DISC_CNF
  Param1 UDEC 1  0
PSSIDCM_CS_UCH_CONN_CNF
  Param1 UDEC 1  0
PSSIDCM_CS_UCH_CONN_REJ
  Param1 UDEC 1  0
PSSIDCM_CS_UCH_DISC_CNF
  Param1 UDEC 1  0
L1BMC_CBCH_DATA_IND
  Param1{ A ARRAY 23 [ RADIO_FRAME UDEC 1 ] }  0
LLTOM_UNITDATA_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 Param3 UDEC 1 
  UNUSED PAD 2 Param4{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
LLTOM_UNITDATA_IND
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 1 
  UNUSED PAD 3 Param3{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
PSSIMMR_ALLOC_CNF
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4 Param4 DEC 4  0
PSSIMMR_ALLOC_REJ
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4  0
PSSIMMR_ALLOC_REQ
  Param1 DEC 4 Param2 DEC 4  0
PSSIMMR_REJ_REQ
  Param1 DEC 4  0
DCMRABM_DATA_IND
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 mode UDEC 1 fc UDEC 1 num_pdu UDEC 1 UNUSED PAD 1 }  0
DCMRABM_DATA_CNF
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 result UDEC 1 UNUSED PAD 1 }  0
DCMRABM_SQ_HANDOVER_RSP
  Param1{ A ARRAY 11 [ A{ nsapi UDEC 1 UNUSED PAD 1 Oldest_Unconfirmed_SN UDEC 2 UL_Send_SN UDEC 2 
  DL_Receive_SN UDEC 2 } ] }  0
DCMRABM_SQ_RETRIEVE_REQ
  Param1{ len DEC 4 
  pid_update{ A ARRAY 11 [ A{ nsapi UDEC 1 UNUSED PAD 3 rabe_pid DEC 4 } ] } }  0
DCMRABM_RELEASE_IND
  Param1 UDEC 1  0
DCMRABM_DATA_REQ
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 mode UDEC 1 num_pdu UDEC 1 }  0
DCMRABM_DATA_RES
  Param1 UDEC 1 
  UNUSED PAD 1 Param2{ uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 result UDEC 1 UNUSED PAD 1 }  0
DCMRABM_SQ_RETRIEVE_RSP
  Param1{ A ARRAY 11 [ A{ nsapi UDEC 1 UNUSED PAD 1 Oldest_Unconfirmed_SN UDEC 2 UL_Send_SN UDEC 2 
  DL_Receive_SN UDEC 2 } ] }  0
DCMRABM_RELEASE_RES
  Param1 UDEC 1  0
RABMSM_ESTABLISH_IND
  Param1 UDEC 1  0
RABMSM_ACTIVATE_IND
  Param1 UDEC 1 Param2 UDEC 1  0
RABMSM_DEACTIVATE_IND
  Param1 UDEC 1  0
RABMSM_MODIFY_IND
  Param1 UDEC 1 Param2 UDEC 1  0
RABMSM_RECOVERY_IND
  Param1{ nsapi_array{ A ARRAY 15 [ A{ nsapi UDEC 1 traffic_class UDEC 1 } ] } 
  UNUSED PAD 2 len DEC 4 }  0
RABMSM_ACTIVATE_RSP
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
RABMSM_DEACTIVATE_RSP
  Param1 UDEC 1  0
RABMSM_DEACTIVATE_REQ
  Param1 UDEC 1  0
RABMSM_MODIFY_RSP
  Param1 UDEC 1  0
RABMSM_STATUS_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
RATMBMC_CELL_INFO_IND
  Param1 DEC 4 Param2 UDEC 2 UNUSED PAD 2 Param3 UDEC 4 
  Param4{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 }  0
MMRATM_CS_CIPHER_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
MMRATM_PS_CIPHER_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
MMRATM_PAGE_IND
  Param1 UDEC 1  0
MMRATM_CS_ABORT_IND
  Param1 DEC 4 Param2 DEC 4  0
MMRATM_PS_ABORT_IND
  Param1 DEC 4  0
MMRATM_ACT_CNF
  Param1 DEC 4 
  Param2{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param3 UDEC 2 
  Param4{ valid UDEC 1 ncell_list{ A ARRAY 16 [ NEIGHBOUR_CELL_LIST UDEC 1 ] } } 
  Param5 UDEC 1 Param6 UDEC 2 UNUSED PAD 2 Param7 DEC 4 Param8 UDEC 1 
  UNUSED PAD 3 Param9 DEC 4 Param10 UDEC 1 UNUSED PAD 3 Param11 DEC 4 
  Param12 DEC 4 Param13 UDEC 1  0
MMRATM_ACT_REJ
  Param1 DEC 4  0
MMRATM_ACT_FAIL
  Param1 DEC 4 Param2 UDEC 1  0
MMRATM_ACT_IND
  Param1 DEC 4 
  Param2{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param3 UDEC 2 
  Param4{ valid UDEC 1 ncell_list{ A ARRAY 16 [ NEIGHBOUR_CELL_LIST UDEC 1 ] } } 
  Param5 UDEC 1 Param6 UDEC 2 UNUSED PAD 2 Param7 DEC 4 Param8 UDEC 1 
  UNUSED PAD 3 Param9 DEC 4 Param10 UDEC 1 UNUSED PAD 3 Param11 DEC 4 
  Param12 DEC 4 Param13 UDEC 1  0
MMRATM_CS_DATA_IND
  Param1 LIB 1  0
MMRATM_PS_DATA_IND
  Param1{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] }  0
MMRATM_CS_EST_CNF
  Param1 DEC 4  0
MMRATM_EST_IND
  Param1 DEC 4  0
MMRATM_PLMN_CNF
  Param1 DEC 4 Param2{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } Param3 UDEC 1 
  UNUSED PAD 3 Param4 DEC 4 Param5 DEC 4 Param6 UDEC 1  0
MMRATM_PLMN_IND
  Param1 DEC 4 Param2{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } Param3 UDEC 1 
  UNUSED PAD 3 Param4 DEC 4 Param5 DEC 4 Param6 UDEC 1  0
MMRATM_STATUS_IND
  Param1 DEC 4  0
MMRATM_CS_REL_IND
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1 
  UNUSED PAD 3 Param4{ Present{ ScReleasepresent ENUM 1 } UNUSED PAD 3 union ARRAY 8 [ ScRelease UDEC 1 ] }  0
MMRATM_PS_REL_IND
  Param1{ Present{ ScReleasepresent ENUM 1 } UNUSED PAD 3 union ARRAY 8 [ ScRelease UDEC 1 ] }  0
MMRATM_SYNC_IND
  Param1 DEC 4 Param2 UDEC 1  0
MMRATM_HO_IND
  Param1 DEC 4 Param2 DEC 4  0
MMRATM_CS_NOTIFICATION_IND
  Param1 DEC 4 Param2 DEC 4 
  Param3{ Present{ CN_PagedUE_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 16 [ CN_PagedUE_Identity UDEC 1 ] }  0
MMRATM_PS_NOTIFICATION_IND
  Param1 DEC 4 Param2 DEC 4 
  Param3{ Present{ CN_PagedUE_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 16 [ CN_PagedUE_Identity UDEC 1 ] }  0
MMRATM_CONFIG_REQ
  Param1 DEC 4 Param2 DEC 4  0
MMRATM_SIM_STATUS_REQ
  Param1 UDEC 1  0
MMRATM_EQ_PLMN_LIST_REQ
  Param1{ length DEC 4 eq_plmn{ A ARRAY 6 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } }  0
MMRATM_ASSIGN_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param3{ A ARRAY 4 [ TLLI UDEC 1 ] } Param4{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] }  0
MMRATM_INFO_REQ
  Param1 DEC 4 Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
MMRATM_ACT_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4 
  Param3{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } Param4 DEC 4 
  Param5{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } } 
  Param6{ valid UDEC 1 ncell_list{ A ARRAY 16 [ NEIGHBOUR_CELL_LIST UDEC 1 ] } } 
  Param7 UDEC 2 
  Param8{ length DEC 4 lac{ A ARRAY 15 [ LAC_ARRAY UDEC 2 ] } UNUSED PAD 2 } 
  Param9 DEC 4 
  Param10{ ps_service UDEC 1 cs_service UDEC 1 UNUSED PAD 2 preferred_service DEC 4 }  0
MMRATM_CLASSMARK_IND
  Param1{ class2_field{ revision_level UDEC 1 es_ind UDEC 1 a51_supported UDEC 1 a52_supported UDEC 1 
  a53_supported UDEC 1 ps_capability UDEC 1 ss_screen UDEC 1 sm_capability UDEC 1 
  vbs UDEC 1 vgcs UDEC 1 fc UDEC 1 cm3 UDEC 1 lcsva UDEC 1 ucs2_supported UDEC 1 
  solsa_capability UDEC 1 cmsp UDEC 1 } 
  class3_field{ a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 multi_slot_class UDEC 1 ucs2_supported UDEC 1 
  ext_measurement UDEC 1 sms_value UDEC 1 sm_value UDEC 1 ms_positioning_method_cap UDEC 1 
  egprs_multi_slot_class UDEC 1 modulation_capability UDEC 1 edge_rf_power_cap_1 UDEC 1 
  edge_rf_power_cap_2 UDEC 1 umts_fdd_rat_cap UDEC 1 umts_tdd_supported UDEC 1 
  cdma_2000_supported UDEC 1 dtm_gprs_supported UDEC 1 dtm_gprs_multi_slot_subclass UDEC 1 
  mac_mode_supported UDEC 1 dtm_egprs_supported UDEC 1 dtm_egprs_multi_slot_subclass UDEC 1 
  gsm_400_radio_cap UDEC 1 gsm_850_radio_cap UDEC 1 gsm_1900_radio_cap UDEC 1 } 
  band_info_field{ p_gsm_available UDEC 1 e_gsm_available UDEC 1 dcs_available UDEC 1 
  pcs_available UDEC 1 r_gsm_available UDEC 1 gsm_400_available UDEC 1 
  gsm_850_available UDEC 1 p_gsm_pwr_class UDEC 1 e_gsm_pwr_class UDEC 1 
  dcs_pwr_class UDEC 1 pcs_pwr_class UDEC 1 r_gsm_pwr_class UDEC 1 
  gsm_400_pwr_class UDEC 1 gsm_850_pwr_class UDEC 1 gsm_band UDEC 1 
  gsm_400_bands_supported UDEC 1 } 
  UNUSED PAD 3 gprs_caps{ ms_class DEC 4 paging_channels UDEC 1 
  drx{ split_pg_cycle_code UDEC 1 split_on_ccch UDEC 1 timer_val UDEC 1 
  drx_cycle_length_coef UDEC 1 } 
  gea1_supported UDEC 1 gea2_supported UDEC 1 gea3_supported UDEC 1 
  gea4_supported UDEC 1 gea5_supported UDEC 1 gea6_supported UDEC 1 
  gea7_supported UDEC 1 sm_gprs UDEC 1 sm_cap_via_dedicated UDEC 1 
  revi_level_indicator UDEC 1 pfc_feature_mode UDEC 1 multi_slot_class UDEC 1 
  ecsd_multi_slot_class UDEC 1 ext_dyn_alloc UDEC 1 egprs_extended_dynamic_allocation_cap UDEC 1 
  compact_interference_meas UDEC 1 UNUSED PAD 3 } 
  gprs_services UDEC 1 cs_services UDEC 1 UNUSED PAD 2 gsm_release DEC 4 } 
  Param2 UDEC 1 
  Param3{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param4{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  UNUSED PAD 3 Param5{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 }  0
MMRATM_CS_DATA_REQ
  Param1 LIB 1 Param2 DEC 4  0
MMRATM_PS_DATA_REQ
  Param1{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] } Param2 DEC 4  0
MMRATM_CS_EST_REQ
  Param1 DEC 4 Param2 LIB 1 Param3 DEC 4 
  Param4{ Present{ InitialUE_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 68 [ InitialUE_Identity UDEC 1 ] } 
  Param5{ version{ Present{ IntraDomainNasNodeSelector_INLINE_0present ENUM 1 } UNUSED PAD 3 union ARRAY 24 [ IntraDomainNasNodeSelector_INLINE_0 UDEC 1 ] } }  0
MMRATM_PS_EST_REQ
  Param1{ pdu_length DEC 4 pdu ARRAY 128 [ GPDU UDEC 1 ] } Param2 DEC 4 
  Param3{ Present{ InitialUE_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 68 [ InitialUE_Identity UDEC 1 ] } 
  Param4{ version{ Present{ IntraDomainNasNodeSelector_INLINE_0present ENUM 1 } UNUSED PAD 3 union ARRAY 24 [ IntraDomainNasNodeSelector_INLINE_0 UDEC 1 ] } }  0
MMRATM_HPLMN_ACT_REQ
  Param1 DEC 4 Param2{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 }  0
MMRATM_PLMN_REQ
  Param1 DEC 4  0
MMRATM_UPDATE_FORB_LAC_REQ
  Param1{ length DEC 4 lac{ A ARRAY 15 [ LAC_ARRAY UDEC 2 ] } UNUSED PAD 2 } 
  Param2{ length DEC 4 
  lai{ A ARRAY 15 [ A{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } ] } UNUSED PAD 2 }  0
MMRATM_CS_UPDATE_PARAM_REQ
  Param1 UDEC 1 
  Param2{ identity_len UDEC 1 type_of_identity UDEC 1 
  tmsi{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } } 
  UNUSED PAD 1 Param3 DEC 4 Param4{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  Param5 UDEC 1 UNUSED PAD 3 Param6{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } 
  Param7{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 }  0
MMRATM_PS_UPDATE_PARAM_REQ
  Param1{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } 
  Param2{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 }  0
MMRATM_PAGING_CONTROL_REQ
  Param1{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } } 
  UNUSED PAD 3 Param2 DEC 4 
  Param3{ tmsi{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } 
  p_tmsi{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } }  0
MMRATM_EMERGENCY_IND
  Param1 DEC 4  0
RR_SUSPEND_REQ
  Param1 DEC 4  0
RR_MEASUREMENT_REPORT_REQ
  report{ A ARRAY 33 [ A{ object{ Present{ UMTS_OBJECTpresent ENUM 1 } UNUSED PAD 3 union ARRAY 8 [ UMTS_OBJECT UDEC 1 ] } 
  rxlev DEC 4 } ] }  0
RR_START_MEASUREMENT_REQ
  Present{ RR_START_MEASUREMENT_REQpresent ENUM 1 } UNUSED PAD 3 union ARRAY 604 [ RR_START_MEASUREMENT_REQ UDEC 1 ]  0
RR_STOP_MEASUREMENT_REQ
  Present{ RR_STOP_MEASUREMENT_REQpresent ENUM 1 } UNUSED PAD 3 union ARRAY 4 [ RR_STOP_MEASUREMENT_REQ UDEC 1 ]  0
RR_MEASUREMENT_CONFIG_IND
  reporting{ Present{ REPORTING_TO_GSMpresent ENUM 1 } UNUSED PAD 3 union ARRAY 12 [ REPORTING_TO_GSM UDEC 1 ] } 
  reportingPresent UDEC 1 
  UNUSED PAD 3 resel_to_umts{ Present{ RESEL_TO_UMTSpresent ENUM 1 } UNUSED PAD 3 union ARRAY 24 [ RESEL_TO_UMTS UDEC 1 ] } 
  resel_to_umtsPresent UDEC 1 
  UNUSED PAD 3 cell_list{ A ARRAY 3 [ A{ arfcn DEC 4 sc_pscg UDEC 1 sc_pscgPresent UDEC 1 
  UNUSED PAD 2 sc_list{ A ARRAY 32 [ SCRAMBLING_CODE_LIST DEC 4 ] } 
  sc_listPresent UDEC 1 UNUSED PAD 3 } ] } 
  cell_listPresent UDEC 1 UNUSED PAD 3  0
RR_MEASUREMENT_IND
  Present{ RR_MEASUREMENT_INDpresent ENUM 1 } UNUSED PAD 3 union ARRAY 528 [ RR_MEASUREMENT_IND UDEC 1 ]  0
RR_RESELECTION_REQ
  Param1 UDEC 2  0
RR_RESELECTION_CNF
  Param1 DEC 4  0
RR_CELL_CHANGE_ORDER_REQ
  Param1{ bsic{ ncc DEC 4 bcc DEC 4 } frequency_band DEC 4 bcch_ARFCN UDEC 2 
  ncMode_present UDEC 1 UNUSED PAD 1 ncMode{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } }  0
RR_CELL_CHANGE_ORDER_RSP
  Param1 DEC 4 Param2 DEC 4  0
RR_CELL_CHANGE_ORDER_CNF
  Param1 DEC 4 Param2 DEC 4  0
RR_CELL_CHANGE_ORDER_IND
  Param1{ uarfcn DEC 4 diversity UDEC 1 UNUSED PAD 3 scrambling_code DEC 4 
  bandwidth_present UDEC 1 UNUSED PAD 3 bandwidth DEC 4 }  0
RR_HANDOVER_DECODE_REQ
  Param1 DEC 4 Param2 LIB 1  0
RR_HANDOVER_DECODE_RSP
  Param1 DEC 4 Param2 DEC 4  0
RR_HANDOVER_RSP
  Param1 DEC 4 Param2 DEC 4  0
RR_HANDOVER_DECODE_CNF
  Param1 DEC 4 Param2 DEC 4 Param3 LIB 1  0
RR_HANDOVER_CNF
  Param1 DEC 4 Param2 DEC 4  0
RR_HANDOVER_DECODE_IND
  Param1 LIB 1  0
RR_EVENT_NOTIFY_REQ
  Param1 DEC 4  0
RR_EVENT_NOTIFY_RSP
  Param1 DEC 4  0
RR_EVENT_NOTIFY_CNF
  Param1 DEC 4  0
RR_EVENT_NOTIFY_IND
  Param1 DEC 4  0
RR_UMTS_CLASSMARK_CONTROL_REQ
  Param1{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 }  0
RR_UPDATE_STANDBY_PARAMS_REQ
  Param1{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } 
  Param2{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } } 
  UNUSED PAD 1 Param3 UDEC 2  0
RR_GSM_CLASSMARK_INFO_IND
  Param1{ classmark2{ A ARRAY 5 [ GSM_Classmark2 UDEC 1 ] } 
  classmark3{ A ARRAY 32 [ GSM_Classmark3 UDEC 1 ] } } 
  Param2{ a51_supported UDEC 1 a52_supported UDEC 1 a53_supported UDEC 1 
  a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 }  0
RRC_SUSPEND_REQ
  Param1 DEC 4  0
RRC_MEASUREMENT_REPORT_REQ
  meas_id DEC 4 
  event{ Present{ EVENT_ID_INTER_RATpresent ENUM 1 } UNUSED PAD 3 union ARRAY 4 [ EVENT_ID_INTER_RAT UDEC 1 ] } 
  cell_list{ A ARRAY 32 [ A{ arfcn UDEC 2 bsic UDEC 1 bsicPresent UDEC 1 rssi DEC 4 } ] }  0
RRC_MEASUREMENT_REQ
  reporting_control DEC 4 resel_control DEC 4 reporting_present UDEC 1 
  UNUSED PAD 3 reporting{ fdd_measure{ Present{ FDD_MEASURE_TYPEpresent ENUM 1 } UNUSED PAD 3 union ARRAY 4 [ FDD_MEASURE_TYPE UDEC 1 ] } 
  cell_list{ A ARRAY 3 [ A{ arfcn DEC 4 sc_pscg UDEC 1 sc_pscgPresent UDEC 1 
  UNUSED PAD 2 sc_list{ A ARRAY 32 [ SCRAMBLING_CODE_LIST DEC 4 ] } 
  sc_listPresent UDEC 1 UNUSED PAD 3 } ] } } 
  resel_to_umts_present UDEC 1 
  UNUSED PAD 3 resel_to_umts{ cell_list{ A ARRAY 3 [ A{ arfcn DEC 4 sc_pscg UDEC 1 sc_pscgPresent UDEC 1 
  UNUSED PAD 2 sc_list{ A ARRAY 32 [ SCRAMBLING_CODE_LIST DEC 4 ] } 
  sc_listPresent UDEC 1 UNUSED PAD 3 } ] } }  0
RRC_MEASUREMENT_CONFIG_IND
  Present{ RRC_MEASUREMENT_CONFIG_INDpresent ENUM 1 } UNUSED PAD 3 union ARRAY 560 [ RRC_MEASUREMENT_CONFIG_IND UDEC 1 ]  0
RRC_MEASUREMENT_IND
  Present{ RRC_MEASUREMENT_INDpresent ENUM 1 } UNUSED PAD 3 union ARRAY 16 [ RRC_MEASUREMENT_IND UDEC 1 ]  0
RRC_RESELECTION_REQ
  Param1{ arfcn DEC 4 scrambling_code DEC 4 }  0
RRC_RESELECTION_STATUS_IND
  Param1 DEC 4  0
RRC_RESELECTION_CNF
  Param1 DEC 4  0
RRC_CELL_CHANGE_ORDER_REQ
  Param1{ uarfcn DEC 4 diversity UDEC 1 UNUSED PAD 3 scrambling_code DEC 4 
  bandwidth_present UDEC 1 UNUSED PAD 3 bandwidth DEC 4 }  0
RRC_CELL_CHANGE_ORDER_RSP
  Param1 DEC 4 Param2 DEC 4  0
RRC_CELL_CHANGE_ORDER_CNF
  Param1 DEC 4 Param2 DEC 4  0
RRC_CELL_CHANGE_ORDER_IND
  Param1{ bsic{ ncc DEC 4 bcc DEC 4 } frequency_band DEC 4 bcch_ARFCN UDEC 2 
  ncMode_present UDEC 1 UNUSED PAD 1 ncMode{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } }  0
RRC_CONN_REDIRECTION_IND
  Param1 DEC 4  0
RRC_HANDOVER_DECODE_REQ
  Param1 LIB 1  0
RRC_HANDOVER_DECODE_RSP
  Param1 DEC 4 Param2 DEC 4 Param3 LIB 1  0
RRC_HANDOVER_RSP
  Param1 DEC 4 Param2 DEC 4  0
RRC_HANDOVER_CNF
  Param1 DEC 4 Param2 DEC 4  0
RRC_HANDOVER_DECODE_CNF
  Param1 DEC 4 Param2 DEC 4  0
RRC_HANDOVER_DECODE_IND
  Param1 DEC 4 Param2 LIB 1  0
RRC_EVENT_NOTIFY_REQ
  Param1 DEC 4  0
RRC_EVENT_NOTIFY_RSP
  Param1 DEC 4  0
RRC_EVENT_NOTIFY_CNF
  Param1 DEC 4  0
RRC_EVENT_NOTIFY_IND
  Param1 DEC 4  0
RRC_GSM_CLASSMARK_CONTROL_REQ
  Param1{ classmark2{ A ARRAY 5 [ GSM_Classmark2 UDEC 1 ] } 
  classmark3{ A ARRAY 32 [ GSM_Classmark3 UDEC 1 ] } } 
  Param2{ a51_supported UDEC 1 a52_supported UDEC 1 a53_supported UDEC 1 
  a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 }  0
RRC_UPDATE_PARAMS_REQ
  Param1 UDEC 1 
  UNUSED PAD 3 Param2{ mcc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } 
  mnc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } }  0
RRC_UMTS_CLASSMARK_INFO_IND
  Param1{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 }  0
PSSIRATM_RXSTAT_IND
  Param1 UDEC 1 Param2 UDEC 1 Param3 UDEC 1 
  UNUSED PAD 1 Param4{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 }  0
PSSIRATM_MEAS_REPORT_IND
  Param1 LIB 1 Param2 UDEC 1  0
PSSIRATM_CELL_INFO_IND
  Param1 DEC 4 Param2 UDEC 2 UNUSED PAD 2 Param3 UDEC 4 
  Param4{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 }  0
PSSIRATM_PERMISSION_IND
  Param1 UDEC 1 Param2 UDEC 1 UNUSED PAD 2 Param3 DEC 4  0
PSSIRATM_CHANNEL_IND
  Param1{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 }  0
PSSIRATM_CS_BEARER_INFO_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
RRC_Activation_req
  Param1 DEC 4  0
RRC_PLMN_Search_req
  Param1 DEC 4 
  Param2{ mcc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } 
  mnc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } }  0
RRC_PLMN_Search_cnf
  Param1 DEC 4 
  Param2{ mcc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } 
  mnc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } }  0
RRC_PLMN_List_cnf
  Param1 DEC 4 
  Param2{ n_plmn DEC 4 
  plmn{ A ARRAY 12 [ A{ mcc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } 
  mnc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } } ] } 
  rscp{ A ARRAY 12 [ RSCP_ArrayType UDEC 1 ] } }  0
RRC_PLMN_List_ind
  Param1 DEC 4 
  Param2{ n_plmn DEC 4 
  plmn{ A ARRAY 12 [ A{ mcc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } 
  mnc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } } ] } 
  rscp{ A ARRAY 12 [ RSCP_ArrayType UDEC 1 ] } }  0
RRC_Equivalent_List_req
  Param1{ n_plmn DEC 4 
  plmn{ A ARRAY 12 [ A{ mcc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } 
  mnc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } } ] } 
  rscp{ A ARRAY 12 [ RSCP_ArrayType UDEC 1 ] } }  0
RRC_Cell_Selection_Control_req
  Param1{ n_f_ra DEC 4 
  f_ra{ A ARRAY 12 [ A{ plmn_Identity{ mcc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } 
  mnc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } } 
  lac{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } } ] } }  0
RRC_System_Information_ind
  Param1 UDEC 4 
  Param2{ plmn{ mcc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } 
  mnc{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } } 
  plmnPresent UDEC 1 UNUSED PAD 3 common_info{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } 
  common_infoPresent UDEC 1 
  UNUSED PAD 3 cn_domain_info{ Present{ CnDomainSystemInformationListpresent ENUM 1 } UNUSED PAD 3 union ARRAY 16 [ CnDomainSystemInformationList UDEC 1 ] } 
  cn_domain_infoPresent UDEC 1 UNUSED PAD 3 }  0
RRC_Paging_Control_req
  Param1{ First HEX 4 Last HEX 4 Length DEC 4 IsAssigned DEC 4 } Param2 DEC 4 
  Param3{ tmsi{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } 
  p_tmsi{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } }  0
RRC_Notification_ind
  Param1 DEC 4 Param2 DEC 4 Param3 DEC 4 
  Param4{ Present{ CN_PagedUE_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 16 [ CN_PagedUE_Identity UDEC 1 ] }  0
RRC_SC_Establish_req
  Param1 DEC 4 
  Param2{ Present{ InitialUE_Identitypresent ENUM 1 } UNUSED PAD 3 union ARRAY 68 [ InitialUE_Identity UDEC 1 ] } 
  Param3 DEC 4 
  Param4{ version{ Present{ IntraDomainNasNodeSelector_INLINE_0present ENUM 1 } UNUSED PAD 3 union ARRAY 24 [ IntraDomainNasNodeSelector_INLINE_0 UDEC 1 ] } } 
  Param5{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 }  0
RRC_SC_Establish_cnf
  Param1 DEC 4 Param2 DEC 4  0
RRC_SC_Release_ind
  Param1 DEC 4 
  Param2{ Present{ CauseScReleaseIndpresent ENUM 1 } UNUSED PAD 3 union ARRAY 4 [ CauseScReleaseInd UDEC 1 ] }  0
RRC_SC_Release_cnf
  Param1 DEC 4 Param2 DEC 4  0
RRC_SC_Release_req
  Param1 DEC 4  0
RRC_SC_Abort_ind
  Param1 DEC 4  0
RRC_Data_req
  Param1 DEC 4 Param2 DEC 4 Param3{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 }  0
RRC_Data_ind
  Param1 DEC 4 Param2{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 }  0
RRC_Sync_ind
  Param1 DEC 4 Param2 DEC 4  0
RRC_KeyUpdate_ind
  Param1 DEC 4 Param2{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 } 
  Param3{  Length DEC 4 IsAssigned DEC 4 Bits HEX 4 }  0
RRC_UeCapability_info_req
  Param1 UDEC 1  0
RRC_Emergency_ind
  Param1 DEC 4  0
DCA_CONN_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
DCA_DISC_REQ
  Param1 UDEC 1  0
DCACSD_T_DATA_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 UDEC 4 Param3 UDEC 1 UNUSED PAD 3 Param4 DEC 4  0
DCACSD_NT_DATA_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 UDEC 4 Param3 UDEC 1 UNUSED PAD 3 Param4 DEC 4  0
DCACSD_T_UL_DATA_REQ_TRIGGER
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
DCACSD_NT_UL_DATA_REQ_TRIGGER
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
DCACSD_T_DATA_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 UDEC 4 Param3 DEC 4  0
DCACSD_NT_DATA_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 UDEC 4 Param3 DEC 4  0
L1DCM_GSM_UL_DATA_REQ_TRIGGER
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
L1DCM_DATA_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 UDEC 4 Param3 DEC 4  0
BRG_SYNC_DATA_REQ
  Param1{ T_W_Q UDEC 1 Uch UDEC 1 UNUSED PAD 2 pdu_desc UDEC 4 }  0
BRG_SYNC_DATA_IND
  Param1{ T_W_Q UDEC 1 Uch UDEC 1 UNUSED PAD 2 pdu_desc UDEC 4 }  0
URLCTM_DATA_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 UDEC 4  0
URLCTM_DATA_REQ
  Param1 UDEC 1 UNUSED PAD 3 Param2 UDEC 4  0
UP_DATA_REQ
  uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 mode UDEC 1 num_pdu UDEC 1  0
UP_DATA_RES
  uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 result UDEC 1 UNUSED PAD 1  0
UP_DATA_IND
  uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 mode UDEC 1 fc UDEC 1 num_pdu UDEC 1 UNUSED PAD 1  0
UP_DATA_CNF
  uchid UDEC 1 UNUSED PAD 1 opid UDEC 2 result UDEC 1 UNUSED PAD 1  0
ACMP_CONNECTION_INFO
  Param1{ uimf{ status DEC 4 } }  0
UIMP_EVENT_INFO
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  Param2{ event DEC 4 }  0
UIMP_APP_SELECT_INFO
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  Param2{ appIndn DEC 4 }  0
UIMP_C_APDU_REQ
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  count_of_commands UDEC 1  0
UIMP_UIM_LINK_REQ
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 }  0
UIMP_STATUS_INT_REQ
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  Param2{ interval DEC 4 }  0
UIMP_PASS_STATUS_INFO
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  Param2{ messagetype DEC 4 passwordClass DEC 4 
  retrycounter{ A ARRAY 2 [ TI_RETRY_COUNT UDEC 1 ] } UNUSED PAD 2 }  0
UIMP_EF_INFO
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  Param2{ efcondition DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  efID{ A ARRAY 2 [ TI_EF_ID UDEC 1 ] } 
  record_list{ A ARRAY 6 [ A{ A ARRAY 1 [ TI_RECORD_ID UDEC 1 ] } ] } 
  record_listPresent UDEC 1 count_of_record UDEC 1 count_of_recordPresent UDEC 1 UNUSED PAD 1 }  0
UIMP_MTF3G_EVENT_INFO
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  Param2{ event DEC 4 }  0
UIMP_MTF3G_APP_SELECT_INFO
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  Param2{ appIndn DEC 4 }  0
UIMP_C_APDU_RES
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  count_of_response UDEC 1  0
UIMP_UIM_LINK_RES
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  Param2{ result DEC 4 }  0
UIMP_STATUS_INT_RES
  Param1{ appIndn DEC 4 fileSelectInfo{ A ARRAY 8 [ TI_FILE_SELECT_INFO UDEC 1 ] } 
  msgid DEC 4 } 
  Param2{ result DEC 4 }  0
SIM_CALL_IND
  Param1 DEC 4  0
SIM_ACM_INCREASE_REQ
  Param1{ A ARRAY 3 [ SI_ARR_3 UDEC 1 ] }  0
SIM_CS_RUN_ALG_REQ
  Param1{ A ARRAY 16 [ RAND_VALUE UDEC 1 ] } Param2 UDEC 1 
  Param3{ A ARRAY 17 [ AUTN_VALUE UDEC 1 ] }  0
SIM_PS_RUN_ALG_REQ
  Param1{ A ARRAY 16 [ RAND_VALUE UDEC 1 ] } Param2 UDEC 1 
  Param3{ A ARRAY 17 [ AUTN_VALUE UDEC 1 ] }  0
SIM_READ_USER_PLMN_REQ
  Param1 DEC 4  0
SIM_UPDATE_CS_LOC_INFO_REQ
  Param1{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param2{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } 
  Param3 UDEC 1  0
SIM_UPDATE_PS_LOC_INFO_REQ
  Param1{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param2{ A ARRAY 3 [ PTMSI_SIGNATURE UDEC 1 ] } 
  UNUSED PAD 1 Param3{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param4 UDEC 1  0
SIM_UPDATE_CS_KEYS_REQ
  Param1{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 }  0
SIM_UPDATE_PS_KEYS_REQ
  Param1{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 }  0
SIM_UPDATE_BCCH_INFO_REQ
  Param1{ A ARRAY 16 [ NEIGHBOUR_CELL_LIST UDEC 1 ] }  0
SIM_UPDATE_FORB_PLMN_REQ
  Param1{ A ARRAY 20 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] }  0
SIM_UPDATE_START_INFO_REQ
  Param1{ start_cs{ A ARRAY 3 [ START_VALUE UDEC 1 ] } 
  start_ps{ A ARRAY 3 [ START_VALUE UDEC 1 ] } }  0
SIM_CONFIG_REQ
  Param1 DEC 4  0
SIM_USAT_REFRESH_IND
  Param1 DEC 4  0
SIM_UPDATE_CALL_TIMER_REQ
  Param1 UDEC 1 Param2{ A ARRAY 3 [ CALL_TIMER_VALUE UDEC 1 ] } Param3 UDEC 1 
  Param4{ A ARRAY 3 [ CALL_TIMER_VALUE UDEC 1 ] }  0
SIM_READ_ACM_INFO_CNF
  Param1 UDEC 1 Param2{ A ARRAY 3 [ SI_ARR_3 UDEC 1 ] } 
  Param3{ A ARRAY 3 [ SI_ARR_3 UDEC 1 ] }  0
SIM_ACM_INCREASE_CNF
  Param1 DEC 4 Param2{ A ARRAY 3 [ SI_ARR_3 UDEC 1 ] }  0
SIM_CS_RUN_ALG_CNF
  Param1 DEC 4 
  Param2{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 } 
  Param3 UDEC 1 Param4{ A ARRAY 17 [ RES UDEC 1 ] } 
  Param5{ A ARRAY 4 [ SRES UDEC 1 ] } Param6 UDEC 1 
  Param7{ A ARRAY 15 [ AUTS_VALUE UDEC 1 ] }  0
SIM_PS_RUN_ALG_CNF
  Param1 DEC 4 
  Param2{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 } 
  Param3 UDEC 1 Param4{ A ARRAY 17 [ RES UDEC 1 ] } 
  Param5{ A ARRAY 4 [ SRES UDEC 1 ] } Param6 UDEC 1 
  Param7{ A ARRAY 15 [ AUTS_VALUE UDEC 1 ] }  0
SIM_READ_CELL_INFO_CNF
  Param1{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } } 
  Param2 UDEC 1 Param3{ A ARRAY 16 [ NEIGHBOUR_CELL_LIST UDEC 1 ] } 
  Param4 UDEC 2 Param5{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param6{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } 
  Param7 UDEC 1 Param8 UDEC 1 Param9{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param10{ A ARRAY 3 [ PTMSI_SIGNATURE UDEC 1 ] } 
  UNUSED PAD 1 Param11{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param12 UDEC 1 
  Param13{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 } 
  Param14 UDEC 1 
  Param15{ gsm_key_present UDEC 1 gsm_ck{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  gsm_cksn UDEC 1 umts_keys_present UDEC 1 
  umts_ck{ A ARRAY 16 [ UMTS_CK UDEC 1 ] } 
  umts_ik{ A ARRAY 16 [ UMTS_IK UDEC 1 ] } umts_ksi UDEC 1 } 
  Param16 UDEC 1 Param17{ A ARRAY 3 [ START_VALUE UDEC 1 ] } Param18 UDEC 1 
  Param19{ start_cs{ A ARRAY 3 [ START_VALUE UDEC 1 ] } 
  start_ps{ A ARRAY 3 [ START_VALUE UDEC 1 ] } }  0
SIM_READ_SIM_INFO_CNF
  Param1 UDEC 1 UNUSED PAD 1 Param2 UDEC 2 Param3 UDEC 1 
  UNUSED PAD 1 Param4{ A ARRAY 20 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } 
  Param5 UDEC 1 
  UNUSED PAD 1 Param6{ length DEC 4 list{ A ARRAY 30 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } } 
  Param7 UDEC 1 
  UNUSED PAD 3 Param8{ length DEC 4 
  list{ A ARRAY 30 [ A{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } act_id UDEC 2 } ] } } 
  Param9 UDEC 1 
  UNUSED PAD 3 Param10{ length DEC 4 
  list{ A ARRAY 30 [ A{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } act_id UDEC 2 } ] } } 
  Param11 UDEC 1 
  UNUSED PAD 3 Param12{ length DEC 4 
  list{ A ARRAY 30 [ A{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } act_id UDEC 2 } ] } } 
  Param13 UDEC 1 Param14 UDEC 1 Param15 UDEC 1 Param16 UDEC 1  0
SIM_READ_USER_PLMN_CNF
  Param1 DEC 4 Param2 DEC 4 
  Param3{ length DEC 4 list{ A ARRAY 30 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } } 
  Param4{ length DEC 4 
  list{ A ARRAY 30 [ A{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } act_id UDEC 2 } ] } }  0
SIM_READ_CALL_TIMER_CNF
  Param1 UDEC 1 Param2{ A ARRAY 3 [ CALL_TIMER_VALUE UDEC 1 ] } Param3 UDEC 1 
  Param4{ A ARRAY 3 [ CALL_TIMER_VALUE UDEC 1 ] }  0
SIM_READ_EMERGENCY_INFO_CNF
  Param1{ Valid UDEC 1 NumberOfCodes UDEC 1 Codes{ A ARRAY 15 [ CODE_ARRAY UDEC 1 ] } } 
  UNUSED PAD 3 Param2{ operation_mode DEC 4 additional_info{ A ARRAY 2 [ AD_EXT_DATA UDEC 1 ] } 
  mnc_length UDEC 1 UNUSED PAD 1 }  0
SIM_FILE_UPDATE_IND
  Param1 DEC 4 
  Param2{ Present{ UPDATED_DATApresent ENUM 1 } UNUSED PAD 3 union ARRAY 184 [ UPDATED_DATA UDEC 1 ] }  0
SIM_FDN_MODE_IND
  Param1 DEC 4  0
SIM_STATUS_IND
  Param1 DEC 4 Param2 DEC 4  0
RRMM_CIPHER_IND
  Param1 UDEC 1  0
GMMRR_PAGE_IND
  Param1 UDEC 1  0
RR_ABORT_IND
  Param1 DEC 4  0
RR_ACT_CNF
  Param1{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param2 UDEC 2 
  Param3{ valid UDEC 1 ncell_list{ A ARRAY 16 [ NEIGHBOUR_CELL_LIST UDEC 1 ] } } 
  Param4 UDEC 1 Param5 UDEC 2 UNUSED PAD 2 Param6 DEC 4 Param7 UDEC 1 
  UNUSED PAD 3 Param8 DEC 4 Param9 UDEC 1 UNUSED PAD 3 Param10 DEC 4 
  Param11 DEC 4  0
RR_ACT_REJ
  Param1 DEC 4  0
RR_ACT_FAIL
  Param1 DEC 4 Param2 UDEC 1  0
RR_ACT_IND
  Param1{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param2 UDEC 2 
  Param3{ valid UDEC 1 ncell_list{ A ARRAY 16 [ NEIGHBOUR_CELL_LIST UDEC 1 ] } } 
  Param4 UDEC 1 Param5 UDEC 2 UNUSED PAD 2 Param6 DEC 4 Param7 UDEC 1 
  UNUSED PAD 3 Param8 DEC 4 Param9 UDEC 1 UNUSED PAD 3 Param10 DEC 4 
  Param11 DEC 4  0
RR_DATA_IND
  Param1 LIB 1  0
RR_EST_CNF
  Param1 DEC 4  0
RR_EST_IND
  Param1 DEC 4  0
RR_PLMN_CNF
  Param1{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } Param2 DEC 4 Param3 UDEC 1 
  Param4 UDEC 1 Param5 UDEC 1  0
RR_STATUS_IND
  Param1 DEC 4  0
RR_REL_IND
  Param1 DEC 4 Param2 DEC 4 Param3 UDEC 1  0
RR_SYNC_IND
  Param1 DEC 4 Param2 UDEC 1  0
RR_PERMISSION_IND
  Param1 UDEC 1 Param2 UDEC 1 UNUSED PAD 2 Param3 DEC 4  0
GMMRR_ASSIGN_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param3{ A ARRAY 4 [ TLLI UDEC 1 ] } Param4{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] }  0
GMMRR_INFO_REQ
  Param1 DEC 4 Param2 UDEC 1 UNUSED PAD 3 Param3 DEC 4  0
RR_ACT_REQ
  Param1{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } } 
  UNUSED PAD 1 Param2{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } 
  Param3{ valid UDEC 1 ncell_list{ A ARRAY 16 [ NEIGHBOUR_CELL_LIST UDEC 1 ] } } 
  UNUSED PAD 1 Param4 UDEC 2 
  UNUSED PAD 2 Param5{ length DEC 4 lac{ A ARRAY 15 [ LAC_ARRAY UDEC 2 ] } UNUSED PAD 2 } 
  Param6 DEC 4 Param7 DEC 4 
  Param8{ ps_service UDEC 1 cs_service UDEC 1 UNUSED PAD 2 preferred_service DEC 4 }  0
RR_CLASSMARK_IND
  Param1{ class2_field{ revision_level UDEC 1 es_ind UDEC 1 a51_supported UDEC 1 a52_supported UDEC 1 
  a53_supported UDEC 1 ps_capability UDEC 1 ss_screen UDEC 1 sm_capability UDEC 1 
  vbs UDEC 1 vgcs UDEC 1 fc UDEC 1 cm3 UDEC 1 lcsva UDEC 1 ucs2_supported UDEC 1 
  solsa_capability UDEC 1 cmsp UDEC 1 } 
  class3_field{ a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 multi_slot_class UDEC 1 ucs2_supported UDEC 1 
  ext_measurement UDEC 1 sms_value UDEC 1 sm_value UDEC 1 ms_positioning_method_cap UDEC 1 
  egprs_multi_slot_class UDEC 1 modulation_capability UDEC 1 edge_rf_power_cap_1 UDEC 1 
  edge_rf_power_cap_2 UDEC 1 umts_fdd_rat_cap UDEC 1 umts_tdd_supported UDEC 1 
  cdma_2000_supported UDEC 1 dtm_gprs_supported UDEC 1 dtm_gprs_multi_slot_subclass UDEC 1 
  mac_mode_supported UDEC 1 dtm_egprs_supported UDEC 1 dtm_egprs_multi_slot_subclass UDEC 1 
  gsm_400_radio_cap UDEC 1 gsm_850_radio_cap UDEC 1 gsm_1900_radio_cap UDEC 1 } 
  band_info_field{ p_gsm_available UDEC 1 e_gsm_available UDEC 1 dcs_available UDEC 1 
  pcs_available UDEC 1 r_gsm_available UDEC 1 gsm_400_available UDEC 1 
  gsm_850_available UDEC 1 p_gsm_pwr_class UDEC 1 e_gsm_pwr_class UDEC 1 
  dcs_pwr_class UDEC 1 pcs_pwr_class UDEC 1 r_gsm_pwr_class UDEC 1 
  gsm_400_pwr_class UDEC 1 gsm_850_pwr_class UDEC 1 gsm_band UDEC 1 
  gsm_400_bands_supported UDEC 1 } 
  UNUSED PAD 3 gprs_caps{ ms_class DEC 4 paging_channels UDEC 1 
  drx{ split_pg_cycle_code UDEC 1 split_on_ccch UDEC 1 timer_val UDEC 1 
  drx_cycle_length_coef UDEC 1 } 
  gea1_supported UDEC 1 gea2_supported UDEC 1 gea3_supported UDEC 1 
  gea4_supported UDEC 1 gea5_supported UDEC 1 gea6_supported UDEC 1 
  gea7_supported UDEC 1 sm_gprs UDEC 1 sm_cap_via_dedicated UDEC 1 
  revi_level_indicator UDEC 1 pfc_feature_mode UDEC 1 multi_slot_class UDEC 1 
  ecsd_multi_slot_class UDEC 1 ext_dyn_alloc UDEC 1 egprs_extended_dynamic_allocation_cap UDEC 1 
  compact_interference_meas UDEC 1 UNUSED PAD 3 } 
  gprs_services UDEC 1 cs_services UDEC 1 UNUSED PAD 2 gsm_release DEC 4 } 
  Param2{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param3{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param4{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 }  0
RR_DATA_REQ
  Param1 LIB 1  0
RR_EST_REQ
  Param1 DEC 4 Param2 LIB 1  0
RR_HPLMN_ACT_REQ
  Param1{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 }  0
RR_PLMN_REQ
  Param1 DEC 4  0
RR_UPDATE_FORB_LAC_REQ
  Param1{ length DEC 4 lac{ A ARRAY 15 [ LAC_ARRAY UDEC 2 ] } UNUSED PAD 2 }  0
RR_UPDATE_PARAM_REQ
  Param1 UDEC 1 
  Param2{ identity_len UDEC 1 type_of_identity UDEC 1 
  tmsi{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } } 
  UNUSED PAD 1 Param3 DEC 4 Param4{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } 
  Param5 UDEC 1  0
RR_EQ_PLMN_LIST_REQ
  Param1{ length DEC 4 eq_plmn{ A ARRAY 6 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } }  0
RR_CS_BEARER_INFO_IND
  Param1 UDEC 1 UNUSED PAD 3 Param2 DEC 4  0
TARR_PROPRIETARY_VER_DATA
  Serial_Interface_Support UDEC 1  0
RRMI_RXSTAT_IND
  Param1 UDEC 1 Param2 UDEC 1 Param3 UDEC 1 
  UNUSED PAD 1 Param4{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 }  0
RRMI_MEAS_REPORT_IND
  Param1 LIB 1 Param2 UDEC 1  0
MNRR_CELL_INFO_IND
  Param1 UDEC 2 Param2{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 }  0
RRMN_CHANNEL_IND
  Param1{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 }  0
CP_DATA_REQ
  da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 data ARRAY 2048 [ CP_DATA_REQ_C UDEC 1 ]  0
CP_DATA_IND
  da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 data ARRAY 2048 [ CP_DATA_IND_C UDEC 1 ]  0
SNSN_DEACTIVATE_IND
  Param1 UDEC 1 Param2{ A ARRAY 4 [ TLLI UDEC 1 ] }  0
GTCPL1_CLOSE_TCH_LOOP_REQ
  Param1 UDEC 1 Param2 UDEC 1  0
GTCPL1_START_DAI_TEST_REQ
  Param1 UDEC 1  0
GLUL_MEASUREMENT_REQ
  Param1 DEC 4 Param2{ Frame DEC 4 slot DEC 4 }  0
GLUL_STATE_IND
  Param1 DEC 4  0
GLUL_MEASUREMENT_CNF
  Param1 DEC 4  0
ULGL_STATE_IND
  Param1 DEC 4  0
ULGL_GAP_PATTERN_IND
  Param1 DEC 4 
  Param2{ Present{ ULL1_GP_STRUCTpresent ENUM 1 } UNUSED PAD 3 union ARRAY 40 [ ULL1_GP_STRUCT UDEC 1 ] }  0
ULGL_MEASUREMENT_REJ
  Param1 DEC 4  0
ULGL_MEASUREMENT_REQ
  Param1{ frame_count DEC 4 }  0
SIM_SET_UMTS_ACTIVE
  Param1 DEC 4  0
SIM_SET_ARB_TICK_OFFSET
  Param1 DEC 4  0
SIM_SET_DRX_GP
  Param1{ Present{ ULL1_GP_STRUCTpresent ENUM 1 } UNUSED PAD 3 union ARRAY 40 [ ULL1_GP_STRUCT UDEC 1 ] } 
  Param2{ tgsn DEC 4 tgl1 DEC 4 tgsfn DEC 4 }  0
SIM_SET_FACH_GP
  Param1{ Present{ ULL1_GP_STRUCTpresent ENUM 1 } UNUSED PAD 3 union ARRAY 40 [ ULL1_GP_STRUCT UDEC 1 ] }  0
SIM_SET_RSSI_DCH_GP
  Param1{ Present{ ULL1_GP_STRUCTpresent ENUM 1 } UNUSED PAD 3 union ARRAY 40 [ ULL1_GP_STRUCT UDEC 1 ] }  0
SIM_SET_INITSYNC_DCH_GP
  Param1{ Present{ ULL1_GP_STRUCTpresent ENUM 1 } UNUSED PAD 3 union ARRAY 40 [ ULL1_GP_STRUCT UDEC 1 ] }  0
SIM_SET_RECONF_DCH_GP
  Param1{ Present{ ULL1_GP_STRUCTpresent ENUM 1 } UNUSED PAD 3 union ARRAY 40 [ ULL1_GP_STRUCT UDEC 1 ] }  0
SIM_SET_UMTS_STATE
  Param1 DEC 4  0
SIM_WCDMA_EMULATE
  Param1 DEC 4  0
DULL1_START_MEAS_REQ
  Param1{ num_of_chans UDEC 2 chan_number{ A ARRAY 32 [ CHAN_LIST UDEC 2 ] } }  0
ADDRESS_ASSIGNMENT_RESPONSE
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CONNECTION_INFORMATION
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CONNECTION_STATE_REPORT_REQUEST
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ADDRESS_ASSIGNMENT_REQUEST
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CONNECTION_NOTIFICATION
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CONNECTION_RELEASE_NOTIFICATION
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CONNECTION_INFORMATION_REQUEST
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ALERTING_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CALL_CONFIRM_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
DISCONNECT_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
FACILITY_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
HOLD_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MODIFY_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MODIFY_RSP
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
NOTIFY_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
REJECT_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
RELEASE_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
RELEASE_RSP
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
RETRIEVE_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SETUP_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SETUP_RSP
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
START_DTMF_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
STOP_DTMF_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
USER_INFORMATION_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
START_CC_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CC_ESTABLISHMENTCONFIRM_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ALERTING_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CALL_PROCEEDING_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CONGESTION_CONTROL_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
DISCONNECT_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
FACILITY_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
HOLD_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MODIFY_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MODIFY_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
NOTIFY_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
REJECT_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
PROGRESS_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
RELEASE_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
RELEASE_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
RETRIEVE_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SETUP_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SETUP_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SETUP_COMPLETE_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
START_DTMF_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
STOP_DTMF_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
USER_INFORMATION_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CM_SERVICE_PROMPT_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CC_ESTABLISHMENT_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
RECALL_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_ACTIVATE_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_MODIFY_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_MODIFY_RSP
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_DEACTIVATE_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_ACTIVATE_REJ_RSP
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_ACTIVATE_SEC_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
GMMREG_ATTACH_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
GMMREG_DETACH_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_ACTIVATE_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_ACTIVATE_REJ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_ACTIVATE_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_MODIFY_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_MODIFY_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_DEACTIVATE_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_DEACTIVATE_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_MODIFY_REJ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_ACTIVATE_SEC_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SMREG_PDP_ACTIVATE_SEC_REJ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
GMMREG_ATTACH_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
GMMREG_ATTACH_REJ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
GMMREG_DETACH_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
GMMREG_DETACH_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SN_XID_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
OPERATOR_SELECT_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SELECT_WIRELESSNW_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
REESTSET_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SUPPORT_SYSTEM_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
OPERATOR_SELECT_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
OPERATOR_SELECT_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SELECT_WIRELESSNW_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
REESTSET_CNF
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SUPPORT_SYSTEM_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
AREA_STATUS_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
PERMISSION_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
RADIOQUALITY_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
SYSTEM_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CAUSE_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
RRCSTATE_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CIPHER_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MEAS_REPORT_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CELL_INFO_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
BEGIN_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
END_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
BEGIN_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
END_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
BATTERY_LEVEL_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MOBILE_STATION_CLASS_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
BATTERY_LEVEL_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MOBILE_STATION_CLASS_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MOBILE_MANAGEMENT_CAUSE_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MSERROR_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MOBILESTATION_POWER_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MTMP_INFORMATION_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ABORT_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
DATA_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ESTABLISH_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
DATA_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ESTABLISH_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ERROR_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
C_APDU_RES
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
AIN_AID_INFO
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
UIM_LINK_RES
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
EF_INFO
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
PASS_STATUS_INFO
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
STATUS_INT_RES
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ICC_RESET_RES
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ATR_REPORT_RES
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
APP_SELECT_INFO
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
C_APDU_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
UIM_LINK_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
STATUS_INT_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
EVENT_INFO
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ICC_RESET_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ATR_REPORT_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ATCOMMAND_INFORMATION
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ATRESPONSE_INFORMATION
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
ATINDICATION_INFORMATION
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CBSP_ACTIVATE_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CBSP_DEACTIVATE_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CBSP_FILTER_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CBSP_START_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CBSP_STOP_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CBSP_REFRESH_REQ
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
CBSP_DATA_IND
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
DCF_STATUS
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
PSSISV_START_REQ
  Param1{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param2{ identity_len UDEC 1 identity{ A ARRAY 9 [ IMEI_OCTETS UDEC 1 ] } } 
  Param3 DEC 4 Param4 DEC 4 
  Param5{ length DEC 4 eq_plmn{ A ARRAY 6 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } } 
  Param6{ class2_field{ revision_level UDEC 1 es_ind UDEC 1 a51_supported UDEC 1 a52_supported UDEC 1 
  a53_supported UDEC 1 ps_capability UDEC 1 ss_screen UDEC 1 sm_capability UDEC 1 
  vbs UDEC 1 vgcs UDEC 1 fc UDEC 1 cm3 UDEC 1 lcsva UDEC 1 ucs2_supported UDEC 1 
  solsa_capability UDEC 1 cmsp UDEC 1 } 
  class3_field{ a54_supported UDEC 1 a55_supported UDEC 1 a56_supported UDEC 1 
  a57_supported UDEC 1 multi_slot_class UDEC 1 ucs2_supported UDEC 1 
  ext_measurement UDEC 1 sms_value UDEC 1 sm_value UDEC 1 ms_positioning_method_cap UDEC 1 
  egprs_multi_slot_class UDEC 1 modulation_capability UDEC 1 edge_rf_power_cap_1 UDEC 1 
  edge_rf_power_cap_2 UDEC 1 umts_fdd_rat_cap UDEC 1 umts_tdd_supported UDEC 1 
  cdma_2000_supported UDEC 1 dtm_gprs_supported UDEC 1 dtm_gprs_multi_slot_subclass UDEC 1 
  mac_mode_supported UDEC 1 dtm_egprs_supported UDEC 1 dtm_egprs_multi_slot_subclass UDEC 1 
  gsm_400_radio_cap UDEC 1 gsm_850_radio_cap UDEC 1 gsm_1900_radio_cap UDEC 1 } 
  band_info_field{ p_gsm_available UDEC 1 e_gsm_available UDEC 1 dcs_available UDEC 1 
  pcs_available UDEC 1 r_gsm_available UDEC 1 gsm_400_available UDEC 1 
  gsm_850_available UDEC 1 p_gsm_pwr_class UDEC 1 e_gsm_pwr_class UDEC 1 
  dcs_pwr_class UDEC 1 pcs_pwr_class UDEC 1 r_gsm_pwr_class UDEC 1 
  gsm_400_pwr_class UDEC 1 gsm_850_pwr_class UDEC 1 gsm_band UDEC 1 
  gsm_400_bands_supported UDEC 1 } 
  UNUSED PAD 3 gprs_caps{ ms_class DEC 4 paging_channels UDEC 1 
  drx{ split_pg_cycle_code UDEC 1 split_on_ccch UDEC 1 timer_val UDEC 1 
  drx_cycle_length_coef UDEC 1 } 
  gea1_supported UDEC 1 gea2_supported UDEC 1 gea3_supported UDEC 1 
  gea4_supported UDEC 1 gea5_supported UDEC 1 gea6_supported UDEC 1 
  gea7_supported UDEC 1 sm_gprs UDEC 1 sm_cap_via_dedicated UDEC 1 
  revi_level_indicator UDEC 1 pfc_feature_mode UDEC 1 multi_slot_class UDEC 1 
  ecsd_multi_slot_class UDEC 1 ext_dyn_alloc UDEC 1 egprs_extended_dynamic_allocation_cap UDEC 1 
  compact_interference_meas UDEC 1 UNUSED PAD 3 } 
  gprs_services UDEC 1 cs_services UDEC 1 UNUSED PAD 2 gsm_release DEC 4 } 
  Param7 UDEC 1 Param8 UDEC 1 UNUSED PAD 2 Param9 DEC 4 Param10 UDEC 1 
  UNUSED PAD 3 Param11{ ms_channel_type DEC 4 ms_channel_mode UDEC 2 UNUSED PAD 2 } 
  Param12{ lai{ plmn{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } lac UDEC 2 } rac UDEC 1 UNUSED PAD 1 } 
  Param13{ A ARRAY 4 [ TMSI_OCTETS UDEC 1 ] } 
  Param14{ A ARRAY 3 [ PTMSI_SIGNATURE UDEC 1 ] } Param15 UDEC 1 
  Param16{ A ARRAY 8 [ ENCRYPTION_KEY UDEC 1 ] } Param17 UDEC 1 Param18 UDEC 1 
  Param19{ identity_len UDEC 1 identity{ A ARRAY 8 [ IMSI_OCTETS UDEC 1 ] } } 
  UNUSED PAD 1 Param20 DEC 4 Param21 DEC 4 Param22 UDEC 1 Param23 UDEC 1 
  Param24 UDEC 1  0
PSSISV_SELECT_WIRELESSNW_CNF
  Param1 DEC 4 
  Param2{ wirelessNW{ A ARRAY 32 [ TI_WIRELESSNW_LIST DEC 4 ] } wirelessNWPresent UDEC 1 
  count_of_wirelessNW UDEC 1 count_of_wirelessNWPresent UDEC 1 UNUSED PAD 1 }  0
PSSISV_SUPPORT_SYSTEM_IND
  Param1{ wirelessNW{ A ARRAY 32 [ TI_WIRELESSNW_LIST DEC 4 ] } wirelessNWPresent UDEC 1 
  count_of_wirelessNW UDEC 1 count_of_wirelessNWPresent UDEC 1 UNUSED PAD 1 }  0
PSSISV_EPLMN_SET_REQ
  Param1{ length DEC 4 eq_plmn{ A ARRAY 6 [ A{ mcc UDEC 2 mnc UDEC 1 UNUSED PAD 1 } ] } }  0
PSSISV_STATUS_REQ
  Param1{ mode UDEC 1 } Param2{ mode UDEC 1 } UNUSED PAD 2 Param3 HEX 4 
  Param4 HEX 4  0
PSSISV_SELECT_WIRELESSNW_REQ
  Param1 DEC 4 Param2 DEC 4  0
TCPSSI_TEST_REQ
  Param1 UDEC 1  0
GTCP_RLC_TEST_MODE_REQ
  Param1{ A ARRAY 4 [ TLLI UDEC 1 ] } Param2 UDEC 2 UNUSED PAD 2 Param3 DEC 4 
  Param4 UDEC 1 Param5 UDEC 1 Param6 UDEC 1 Param7 UDEC 1 Param8 DEC 4  0
MCPSSI_DETACH_REQ
  Param1 UDEC 1  0
MCPSSI_UIMP_MTF3G_APP_SELECT_INFO
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MCPSSI_UIMP_MTF3G_EVENT_INFO
  Param1{ da UDEC 1 sa UDEC 1 pd UDEC 1 UNUSED PAD 1 length UDEC 2 
  data{ A ARRAY 2048 [ TID_MSG_FIELD UDEC 1 ] } }  0
MCPSSI_EMER_ATTACH_CNF
  Param1 UDEC 1  0
MCPSSI_DETACH_CNF
  Param1 UDEC 1  0
TX_CONT_REQ
  Param1{ ptr_p_xtxreq UDEC 4 }  0
TX_CONT_CNF
  Param1{ ptr_p_xtxcnf UDEC 4 }  0
CMP_CONT_REQ
  Param1{ ptr_p_xcmpcontreq UDEC 4 }  0
CMP_CONT_CNF
  Param1{ ptr_p_xcmpcontcnf UDEC 4 }  0
OUTER_CONT_REQ
  Param1{ ptr_p_xoutercreq UDEC 4 }  0
OUTER_CONT_CNF
  Param1{ ptr_p_xouterccnf UDEC 4 }  0
TXPW_MEASURE_REQ
  Param1{ ptr_p_xtxpwmereq UDEC 4 }  0
TXPW_MEASURE_CNF
  Param1{ ptr_p_xtxpwmecnf UDEC 4 }  0
TXPW_MEASURE_IND
  Param1{ ptr_p_xtxpwmeind UDEC 4 }  0
DPCH_MEASURE_REQ
  Param1{ ptr_p_xdpchmereq UDEC 4 }  0
DPCH_MEASURE_CNF
  Param1{ ptr_p_xdpchmecnf UDEC 4 }  0
DPCH_MEASURE_IND
  Param1{ ptr_p_xdpchmeind UDEC 4 }  0
TRAFFIC_MEASURE_REQ
  Param1{ ptr_p_xtrfmereq UDEC 4 }  0
TRAFFIC_MEASURE_CNF
  Param1{ ptr_p_xtrfmecnf UDEC 4 }  0
TRAFFIC_MEASURE_IND
  Param1{ ptr_p_xtrfmeind UDEC 4 }  0
CMAC_CONFIG_REQ
  Param1{ ptr_p_xcmaccfgreq UDEC 4 }  0
CMAC_CONFIG_CNF
  Param1{ ptr_p_xcmaccfgcnf UDEC 4 }  0
CIPHER_CONT_REQ
  Param1{ ptr_p_xciphercntreq UDEC 4 }  0
CIPHER_CONT_CNF
  Param1{ ptr_p_xciphercntcnf UDEC 4 }  0
LCH_TEST_REQ
  Param1{ ptr_p_xlchtestreq UDEC 4 }  0
LCH_TEST_CNF
  Param1{ ptr_p_xlchtestcnf UDEC 4 }  0
MAC_PDU_PER_LCH_IND
  Param1{ ptr_p_xmacdataind UDEC 4 }  0
UMAC_DATA_END_INTERNAL
  Param1 UDEC 4 Param2 UDEC 4  0
UMAC_COMPUTE_TVM
  Param1{ ptr_p_xtrfmeind UDEC 4 } Param2 UDEC 4 Param3 UDEC 4  0
PCH_SET_REQ
  Param1{ ptr_p_xpchreq UDEC 4 }  0
PCH_SET_CNF
  Param1{ ptr_p_xpchcnf UDEC 4 }  0
PCH_ERROR_IND
  Param1{ ptr_p_xpcherrorind UDEC 4 }  0
FACH_SET_REQ
  Param1{ ptr_p_xfachreq UDEC 4 }  0
FACH_SET_CNF
  Param1{ ptr_p_xfachcnf UDEC 4 }  0
FACH_ERROR_IND
  Param1{ ptr_p_xfacherrorind UDEC 4 }  0
RACH_SET_REQ
  Param1{ ptr_p_xrachreq UDEC 4 }  0
RACH_SET_CNF
  Param1{ ptr_p_xrachcnf UDEC 4 }  0
RACH_ERROR_IND
  Param1{ ptr_p_xracherrorind UDEC 4 }  0
DCH_SET_REQ
  Param1{ ptr_p_xdchreq UDEC 4 }  0
DCH_SET_CNF
  Param1{ ptr_p_xdchcnf UDEC 4 }  0
DCH_ERROR_IND
  Param1{ ptr_p_xdcherrorind UDEC 4 }  0
RL_MODIFY_REQ
  Param1{ ptr_p_xrlmodifyreq UDEC 4 }  0
RL_MODIFY_CNF
  Param1{ ptr_p_xrlmodifycnf UDEC 4 }  0
PH_MODIFY_REQ
  Param1{ ptr_p_xphmodifyreq UDEC 4 }  0
PH_MODIFY_CNF
  Param1{ ptr_p_xphmodifycnf UDEC 4 }  0
TRCH_MODIFY_REQ
  Param1{ ptr_p_xtrchmodifyreq UDEC 4 }  0
TRCH_MODIFY_CNF
  Param1{ ptr_p_xtrchmodifycnf UDEC 4 }  0
BLER_MEASURE_REQ
  Param1{ ptr_p_xblermereq UDEC 4 }  0
BLER_MEASURE_CNF
  Param1{ ptr_p_xblermecnf UDEC 4 }  0
BLER_MEASURE_IND
  Param1{ ptr_p_xblermeind UDEC 4 }  0
TRCH_TEST_REQ
  Param1{ ptr_p_xtrchtestreq UDEC 4 }  0
TRCH_TEST_CNF
  Param1{ ptr_p_xtrchtestcnf UDEC 4 }  0
BAND_SEARCH_REQ
  Param1{ ptr_p_xbandsearchreq UDEC 4 }  0
BAND_SEARCH_CNF
  Param1{ ptr_p_xbandsearchcnf UDEC 4 }  0
BAND_SEARCH_IND
  Param1{ ptr_p_xbandsearchind UDEC 4 }  0
PCCPCH_DETECT_REQ
  Param1{ ptr_p_xpccpchdtreq UDEC 4 }  0
PCCPCH_DETECT_CNF
  Param1{ ptr_p_xpccpchdtcnf UDEC 4 }  0
PCCPCH_DETECT_IND
  Param1{ ptr_p_xpccpchdtind UDEC 4 }  0
PCCPCH_STATUS_REQ
  Param1{ ptr_p_xpcchchstreq UDEC 4 }  0
PCCPCH_STATUS_CNF
  Param1{ ptr_p_xpcchchstcnf UDEC 4 }  0
BCCH_GET_REQ
  Param1{ ptr_p_xbcchgetreq UDEC 4 }  0
BCCH_GET_CNF
  Param1{ ptr_p_xbcchgetcnf UDEC 4 }  0
FACH_MEASUREMENT_REQ
  Param1{ ptr_p_xfachmereq UDEC 4 }  0
FACH_MEASUREMENT_CNF
  Param1{ ptr_p_xfachmecnf UDEC 4 }  0
HOST_MAC_DATA_REQ
  Param1{ lcid UDEC 1 UNUSED PAD 1 opid UDEC 2 mode UDEC 1 
  UNUSED PAD 3 count_aum{ nr UDEC 1 
  UNUSED PAD 3 rev ARRAY 4 [ rev{ sn UDEC 2 UNUSED PAD 2 hfn UDEC 4 key_id UDEC 1 UNUSED PAD 3 } ] } 
  vta UDEC 2 size_pdu UDEC 2 num_pdu UDEC 1 kind_pdu UDEC 1 UNUSED PAD 2 }  0
HOST_MAC_DATA_IND
  Param1{ lcid UDEC 1 num_pdu UDEC 1 mode UDEC 1 status UDEC 1 opid UDEC 2 
  fn UDEC 2 }  0
HOST_INIT_TAD_REQ
  Param1{ rev{ scenario UDEC 1 UNUSED PAD 3 config UDEC 4 
  display{ nb_lch_bufferized UDEC 1 nb_lch_transmitted UDEC 1 } UNUSED PAD 2 } 
  fwd{ scenario UDEC 1 } UNUSED PAD 3 }  0
HOST_INIT_TAD_CNF
  Param1{ result UDEC 1 }  0
HOST_MAC_FC_IND
  Param1{ lcid UDEC 1 fc UDEC 1 }  0
HOST_MAC_DATA_CNF
  Param1{ lcid UDEC 1 UNUSED PAD 1 opid UDEC 2 fn UDEC 2 result UDEC 1 UNUSED PAD 1 }  0
HOST_MAC_STATUS_IND
  Param1{ result UDEC 1 tfci UDEC 1 beta_c UDEC 1 beta_d UDEC 1 fn UDEC 2 
  lch ARRAY 6 [ lch{ lchid UDEC 1 num_pdu UDEC 1 num_pdu_high_prio UDEC 1 } ] }  0
HOST_TAD_STATUS_IND
  Param1{ tad_status UDEC 1 lchid UDEC 1 
  mac_data_cnf{ opid UDEC 2 fn UDEC 2 result UDEC 1 UNUSED PAD 1 } 
  mac_fc_ind{ fc UDEC 1 } UNUSED PAD 1 }  0
HOST_PCH_SET_REQ
  Param1{ exe{ opid UDEC 1 mode UDEC 1 time UDEC 2 } 
  drx{ pch{ len UDEC 1 UNUSED PAD 1 gid UDEC 2 } pich{ gid UDEC 1 } UNUSED PAD 1 } 
  errdt{ sf UDEC 1 sr UDEC 1 } cctrch{ fwdch UDEC 1 } 
  UNUSED PAD 3 fwd_cctrch{ status UDEC 2 
  UNUSED PAD 2 cctrch ARRAY 1 [ cctrch{ trchid ARRAY 4 [ cctrch UDEC 1 ] rlid UDEC 1 phid UDEC 1 
  UNUSED PAD 2 tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 32 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 4 [ ST_CFWD_TFCS UDEC 1 ] } } ] 
  fwd_pich{ status UDEC 2 band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } 
  UNUSED PAD 2 rl ARRAY 1 [ rl{ txdiv UDEC 1 UNUSED PAD 3 srcd UDEC 4 frtm UDEC 2 relpw UDEC 1 
  UNUSED PAD 1 ph ARRAY 1 [ ph{ sformat UDEC 2 ccd UDEC 2 } ] } ] } 
  fwd_sccpch{ status UDEC 2 band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } psi UDEC 1 
  UNUSED PAD 1 rl ARRAY 1 [ rl{ txdiv UDEC 1 UNUSED PAD 3 srcd UDEC 4 frtm UDEC 2 
  chest{ ch UDEC 1 UNUSED PAD 1 scpich{ srcd UDEC 2 ccd UDEC 2 } } 
  ph ARRAY 1 [ ph{ sformat UDEC 2 ccd UDEC 2 } ] } ] } 
  fwd_trch{ status ARRAY 4 [ ST_CFWD_TRCH UDEC 1 ] 
  trch ARRAY 4 [ trch{ type UDEC 1 tti UDEC 1 ct UDEC 1 UNUSED PAD 1 rm UDEC 2 crc UDEC 1 
  UNUSED PAD 1 tf{ n UDEC 1 UNUSED PAD 1 set ARRAY 8 [ set{ tbn UDEC 2 tbs UDEC 2 } ] } } ] } } }  0
HOST_PCH_SET_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_PCH_ERROR_IND
  Param1{ fwd{ phid UDEC 1 rlid UDEC 1 } }  0
HOST_FACH_SET_REQ
  Param1{ exe{ opid UDEC 1 mode UDEC 1 time UDEC 2 } errdt{ sf UDEC 1 sr UDEC 1 } 
  cctrch{ fwdch UDEC 1 } 
  UNUSED PAD 1 fwd_cctrch{ status UDEC 2 
  UNUSED PAD 2 cctrch ARRAY 1 [ cctrch{ trchid ARRAY 4 [ cctrch UDEC 1 ] rlid UDEC 1 phid UDEC 1 
  UNUSED PAD 2 tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 32 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 4 [ ST_CFWD_TFCS UDEC 1 ] } } ] 
  fwd_pich{ status UDEC 2 band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } 
  UNUSED PAD 2 rl ARRAY 1 [ rl{ txdiv UDEC 1 UNUSED PAD 3 srcd UDEC 4 frtm UDEC 2 relpw UDEC 1 
  UNUSED PAD 1 ph ARRAY 1 [ ph{ sformat UDEC 2 ccd UDEC 2 } ] } ] } 
  fwd_sccpch{ status UDEC 2 band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } psi UDEC 1 
  UNUSED PAD 1 rl ARRAY 1 [ rl{ txdiv UDEC 1 UNUSED PAD 3 srcd UDEC 4 frtm UDEC 2 
  chest{ ch UDEC 1 UNUSED PAD 1 scpich{ srcd UDEC 2 ccd UDEC 2 } } 
  ph ARRAY 1 [ ph{ sformat UDEC 2 ccd UDEC 2 } ] } ] } 
  fwd_trch{ status ARRAY 4 [ ST_CFWD_TRCH UDEC 1 ] 
  trch ARRAY 4 [ trch{ type UDEC 1 tti UDEC 1 ct UDEC 1 UNUSED PAD 1 rm UDEC 2 crc UDEC 1 
  UNUSED PAD 1 tf{ n UDEC 1 UNUSED PAD 1 set ARRAY 8 [ set{ tbn UDEC 2 tbs UDEC 2 } ] } } ] } } }  0
HOST_FACH_SET_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_FACH_ERROR_IND
  Param1{ opid UDEC 1 fwd{ phid UDEC 1 rlid UDEC 1 } }  0
HOST_RACH_SET_REQ
  Param1{ exe{ opid UDEC 1 mode UDEC 1 time UDEC 2 } cctrch{ revch UDEC 1 } 
  UNUSED PAD 3 rev_cctrch{ status UDEC 2 
  UNUSED PAD 2 cctrch ARRAY 1 [ cctrch{ trchid ARRAY 4 [ cctrch UDEC 1 ] phid UDEC 1 
  UNUSED PAD 3 tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 16 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 1 [ ST_CREV_TFCS UDEC 1 ] UNUSED PAD 3 } } ] 
  fwd_aich{ status UDEC 2 band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } 
  UNUSED PAD 2 rl ARRAY 1 [ rl{ txdiv UDEC 1 UNUSED PAD 3 srcd UDEC 4 relpw UDEC 1 UNUSED PAD 1 ph ARRAY 1 [ ph{ ccd UDEC 2 } ] } ] } 
  rev_prach{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } pl UDEC 1 UNUSED PAD 3 srcd UDEC 4 
  frtm UDEC 2 
  pre{ phy{ np UDEC 1 } mac{ m UDEC 1 nboi_min UDEC 1 nboi_max UDEC 1 } } 
  cont{ sformat UDEC 2 } msg{ sformat UDEC 2 } UNUSED PAD 2 } 
  rev_trch{ status ARRAY 4 [ ST_CREV_TRCH UDEC 1 ] 
  trch ARRAY 1 [ trch{ type UDEC 1 tti UDEC 1 ct UDEC 1 UNUSED PAD 1 rm UDEC 2 crc UDEC 1 
  UNUSED PAD 1 tf{ n UDEC 1 UNUSED PAD 1 set ARRAY 8 [ set{ status UDEC 1 UNUSED PAD 1 tbn UDEC 2 tbs UDEC 2 } ] } } ] } UNUSED PAD 2 } }  0
HOST_RACH_SET_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_RACH_ERROR_IND
  Param1{ opid UDEC 1 rev{ cause UDEC 1 } }  0
HOST_DCH_SET_REQ
  Param1{ exe{ opid UDEC 1 mode UDEC 1 time UDEC 2 } 
  sync{ t312 UDEC 1 UNUSED PAD 1 n312 UDEC 2 } 
  errdt{ t313 UDEC 1 UNUSED PAD 1 n313 UDEC 2 n315 UDEC 2 } 
  cctrch{ fwdch UDEC 1 revch UDEC 1 } 
  fwd_cctrch{ status UDEC 2 
  UNUSED PAD 2 cctrch ARRAY 1 [ cctrch{ trchid ARRAY 4 [ cctrch UDEC 1 ] rlid UDEC 1 phid UDEC 1 
  UNUSED PAD 2 tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 48 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 6 [ ST_DFWD_TFCS UDEC 1 ] UNUSED PAD 2 } } ] 
  fwd_dpch{ status UDEC 2 band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } psi UDEC 1 
  txdiv{ fb{ mode UDEC 1 } ssdt{ mode UDEC 1 } } 
  UNUSED PAD 3 rl ARRAY 6 [ rl{ txdiv{ sttd{ mode UDEC 1 } fb{ adj UDEC 1 } ssdt{ id UDEC 1 } } 
  gate UDEC 1 tpc UDEC 1 UNUSED PAD 3 frtm UDEC 4 
  chest{ ch UDEC 1 UNUSED PAD 1 scpich{ srcd UDEC 2 ccd UDEC 2 } } 
  UNUSED PAD 2 ph ARRAY 3 [ ph{ sformat UDEC 2 UNUSED PAD 2 srcd UDEC 4 ccd UDEC 2 UNUSED PAD 2 } ] 
  rtd UDEC 4 } ] 
  cfnhandling UDEC 2 powerOffsetPilot_dpdch UDEC 1 UNUSED PAD 1 } 
  fwd_trch{ status ARRAY 4 [ ST_DFWD_TRCH UDEC 1 ] 
  trch ARRAY 6 [ trch{ type UDEC 1 tti UDEC 1 ct UDEC 1 UNUSED PAD 1 rm UDEC 2 crc UDEC 1 
  UNUSED PAD 1 tf{ n UDEC 1 UNUSED PAD 1 set ARRAY 8 [ set{ tbn UDEC 2 tbs UDEC 2 } ] } } ] } } 
  rev_cctrch{ status UDEC 2 
  UNUSED PAD 2 cctrch ARRAY 1 [ cctrch{ trchid ARRAY 4 [ cctrch UDEC 1 ] phid UDEC 1 
  UNUSED PAD 3 tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 64 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 6 [ ST_DREV_TFCS UDEC 1 ] UNUSED PAD 2 } } ] 
  rev_dpch{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } pl UDEC 1 gate UDEC 1 
  UNUSED PAD 2 srcd UDEC 4 cont{ sformat UDEC 2 } msg{ sformat UDEC 2 } } 
  rev_trch{ status ARRAY 4 [ ST_DREV_TRCH UDEC 1 ] 
  trch ARRAY 6 [ trch{ type UDEC 1 tti UDEC 1 ct UDEC 1 UNUSED PAD 1 rm UDEC 2 crc UDEC 1 
  UNUSED PAD 1 tf{ n UDEC 1 UNUSED PAD 1 set ARRAY 8 [ set{ status UDEC 1 UNUSED PAD 1 tbn UDEC 2 tbs UDEC 2 } ] } } ] } } }  0
HOST_DCH_SET_CNF
  Param1{ opid UDEC 1 UNUSED PAD 3 rev_dpch{ frtm UDEC 4 } result UDEC 1 UNUSED PAD 3 }  0
HOST_DCH_ERROR_IND
  Param1{ opid UDEC 1 }  0
HOST_PH_MODIFY_REQ
  Param1{ exe{ opid UDEC 1 mode ARRAY 2 [ exe UDEC 1 ] UNUSED PAD 1 time UDEC 2 } 
  sync{ t312 UDEC 1 UNUSED PAD 1 n312 UDEC 2 } 
  UNUSED PAD 2 dfwd_tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 48 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 6 [ ST_DFWD_TFCS UDEC 1 ] UNUSED PAD 2 } 
  drev_tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 64 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 6 [ ST_DREV_TFCS UDEC 1 ] UNUSED PAD 2 } 
  dfwd_dpch{ phid UDEC 1 
  UNUSED PAD 3 dpch{ status UDEC 2 band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } psi UDEC 1 
  txdiv{ fb{ mode UDEC 1 } ssdt{ mode UDEC 1 } } 
  UNUSED PAD 3 rl ARRAY 6 [ rl{ txdiv{ sttd{ mode UDEC 1 } fb{ adj UDEC 1 } ssdt{ id UDEC 1 } } 
  gate UDEC 1 tpc UDEC 1 UNUSED PAD 3 frtm UDEC 4 
  chest{ ch UDEC 1 UNUSED PAD 1 scpich{ srcd UDEC 2 ccd UDEC 2 } } 
  UNUSED PAD 2 ph ARRAY 3 [ ph{ sformat UDEC 2 UNUSED PAD 2 srcd UDEC 4 ccd UDEC 2 UNUSED PAD 2 } ] 
  rtd UDEC 4 } ] 
  cfnhandling UDEC 2 powerOffsetPilot_dpdch UDEC 1 UNUSED PAD 1 } } 
  drev_dpch{ phid UDEC 1 
  UNUSED PAD 3 dpch{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } pl UDEC 1 gate UDEC 1 
  UNUSED PAD 2 srcd UDEC 4 cont{ sformat UDEC 2 } msg{ sformat UDEC 2 } } } }  0
HOST_PH_MODIFY_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_TRCH_MODIFY_REQ
  Param1{ exe{ opid UDEC 1 mode ARRAY 2 [ exe UDEC 1 ] UNUSED PAD 1 time UDEC 2 } 
  UNUSED PAD 2 cfwd_tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 32 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 4 [ ST_CFWD_TFCS UDEC 1 ] } 
  crev_tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 16 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 1 [ ST_CREV_TFCS UDEC 1 ] UNUSED PAD 3 } 
  dfwd_tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 48 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 6 [ ST_DFWD_TFCS UDEC 1 ] UNUSED PAD 2 } 
  drev_tfcs{ n UDEC 2 UNUSED PAD 2 tfci ARRAY 64 [ tfci{ ctfc UDEC 4 } ] trchid ARRAY 6 [ ST_DREV_TFCS UDEC 1 ] UNUSED PAD 2 } 
  cfwd_trch{ trchid ARRAY 4 [ cfwd_trch UDEC 1 ] 
  trch{ status ARRAY 4 [ ST_CFWD_TRCH UDEC 1 ] 
  trch ARRAY 4 [ trch{ type UDEC 1 tti UDEC 1 ct UDEC 1 UNUSED PAD 1 rm UDEC 2 crc UDEC 1 
  UNUSED PAD 1 tf{ n UDEC 1 UNUSED PAD 1 set ARRAY 8 [ set{ tbn UDEC 2 tbs UDEC 2 } ] } } ] } } 
  crev_trch{ trchid ARRAY 4 [ crev_trch UDEC 1 ] 
  trch{ status ARRAY 4 [ ST_CREV_TRCH UDEC 1 ] 
  trch ARRAY 1 [ trch{ type UDEC 1 tti UDEC 1 ct UDEC 1 UNUSED PAD 1 rm UDEC 2 crc UDEC 1 
  UNUSED PAD 1 tf{ n UDEC 1 UNUSED PAD 1 set ARRAY 8 [ set{ status UDEC 1 UNUSED PAD 1 tbn UDEC 2 tbs UDEC 2 } ] } } ] } } 
  dfwd_trch{ trchid ARRAY 4 [ dfwd_trch UDEC 1 ] 
  trch{ status ARRAY 4 [ ST_DFWD_TRCH UDEC 1 ] 
  trch ARRAY 6 [ trch{ type UDEC 1 tti UDEC 1 ct UDEC 1 UNUSED PAD 1 rm UDEC 2 crc UDEC 1 
  UNUSED PAD 1 tf{ n UDEC 1 UNUSED PAD 1 set ARRAY 8 [ set{ tbn UDEC 2 tbs UDEC 2 } ] } } ] } } 
  drev_trch{ trchid ARRAY 4 [ drev_trch UDEC 1 ] 
  trch{ status ARRAY 4 [ ST_DREV_TRCH UDEC 1 ] 
  trch ARRAY 6 [ trch{ type UDEC 1 tti UDEC 1 ct UDEC 1 UNUSED PAD 1 rm UDEC 2 crc UDEC 1 
  UNUSED PAD 1 tf{ n UDEC 1 UNUSED PAD 1 set ARRAY 8 [ set{ status UDEC 1 UNUSED PAD 1 tbn UDEC 2 tbs UDEC 2 } ] } } ] } } UNUSED PAD 2 }  0
HOST_TRCH_MODIFY_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_RL_MODIFY_REQ
  Param1{ exe{ opid UDEC 1 mode UDEC 1 time UDEC 2 } 
  sync{ t312 UDEC 1 UNUSED PAD 1 n312 UDEC 2 } n UDEC 1 rl ARRAY 6 [ rl{ rlid UDEC 1 } ] 
  UNUSED PAD 1 fwd_dpch{ status UDEC 2 band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } psi UDEC 1 
  txdiv{ fb{ mode UDEC 1 } ssdt{ mode UDEC 1 } } 
  UNUSED PAD 3 rl ARRAY 6 [ rl{ txdiv{ sttd{ mode UDEC 1 } fb{ adj UDEC 1 } ssdt{ id UDEC 1 } } 
  gate UDEC 1 tpc UDEC 1 UNUSED PAD 3 frtm UDEC 4 
  chest{ ch UDEC 1 UNUSED PAD 1 scpich{ srcd UDEC 2 ccd UDEC 2 } } 
  UNUSED PAD 2 ph ARRAY 3 [ ph{ sformat UDEC 2 UNUSED PAD 2 srcd UDEC 4 ccd UDEC 2 UNUSED PAD 2 } ] 
  rtd UDEC 4 } ] 
  cfnhandling UDEC 2 powerOffsetPilot_dpdch UDEC 1 UNUSED PAD 1 } }  0
HOST_RL_MODIFY_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_BLER_MEASURE_REQ
  Param1{ event UDEC 1 exe{ opid UDEC 1 mode UDEC 1 } 
  UNUSED PAD 1 detect{ periodic{ trchid UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  event_5a{ trchid UDEC 1 UNUSED PAD 1 total_crc UDEC 2 bad_crc UDEC 2 ptat UDEC 2 } } }  0
HOST_BLER_MEASURE_CNF
  Param1{ event UDEC 1 opid UDEC 1 result UDEC 1 }  0
HOST_BLER_MEASURE_IND
  Param1{ event UDEC 1 opid UDEC 1 bler UDEC 1 UNUSED PAD 1 count{ total_crc UDEC 4 bad_crc UDEC 4 } }  0
HOST_TRCH_TEST_REQ
  Param1{ exe{ opid UDEC 1 mode UDEC 1 } 
  test{ mode1{ test_trch{ rev_trchid UDEC 1 pattern UDEC 1 n UDEC 2 rate ARRAY 300 [ test_trch UDEC 1 ] } 
  other_trch{ tfi UDEC 1 dummy UDEC 1 } } 
  mode2{ test_trch{ fwd_trchid UDEC 1 rev_trchid UDEC 1 tfi ARRAY 32 [ test_trch UDEC 1 ] } 
  other_trch{ tfi UDEC 1 dummy UDEC 1 } } 
  mode3{ test_trch{ fwd_trchid UDEC 1 rev_trchid UDEC 1 tfi ARRAY 32 [ test_trch UDEC 1 ] } 
  other_trch{ tfi UDEC 1 dummy UDEC 1 } } } }  0
HOST_TRCH_TEST_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_TX_CONT_REQ
  Param1{ exe{ mode UDEC 1 UNUSED PAD 1 time UDEC 2 } initial{ power UDEC 1 } 
  rang{ max UDEC 1 mini UDEC 1 } 
  UNUSED PAD 1 prach{ step{ p0 UDEC 1 } 
  UNUSED PAD 1 tfcs{ n UDEC 2 tfc ARRAY 16 [ tfc{ ppm UDEC 1 UNUSED PAD 1 gain UDEC 2 } ] } } 
  dpch{ pre UDEC 1 alg UDEC 1 step UDEC 1 
  UNUSED PAD 1 tfcs{ n UDEC 2 tfc ARRAY 64 [ tfc{ gain UDEC 2 } ] } } }  0
HOST_TX_CONT_CNF
  Param1{ result UDEC 1 }  0
HOST_CMP_CONT_REQ
  Param1{ exe{ opid UDEC 1 mode UDEC 1 time UDEC 2 } tgmp UDEC 1 dft UDEC 1 
  rdm{ fwd UDEC 1 rev UDEC 1 } 
  pattern{ tgprc UDEC 2 tgsn UDEC 1 UNUSED PAD 1 tgd UDEC 2 
  tgi{ tgl1 UDEC 1 tgl2 UDEC 1 } tgpl1 UDEC 2 tgpl2 UDEC 2 } 
  power{ itp UDEC 1 rpp UDEC 1 } 
  sir{ sir1 UDEC 1 siraft1 UDEC 1 sir2 UDEC 1 siraft2 UDEC 1 } 
  gsm{ bsic{ initial UDEC 1 reconf UDEC 1 } } }  0
HOST_CMP_CONT_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_OUTER_CONT_REQ
  Param1{ exe{ mode UDEC 1 UNUSED PAD 1 time UDEC 2 } 
  quality{ bler ARRAY 32 [ quality UDEC 1 ] } sir{ mode UDEC 1 } UNUSED PAD 1 }  0
HOST_OUTER_CONT_CNF
  Param1{ result UDEC 1 }  0
HOST_TXPW_MEASURE_REQ
  Param1{ event UDEC 1 exe{ opid UDEC 1 mode UDEC 1 } 
  UNUSED PAD 1 detect{ periodic{ filter UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  event_6a{ filter UDEC 1 UNUSED PAD 1 th UDEC 2 timer UDEC 2 amount UDEC 1 
  UNUSED PAD 1 intv UDEC 2 } 
  event_6b{ filter UDEC 1 UNUSED PAD 1 th UDEC 2 timer UDEC 2 amount UDEC 1 
  UNUSED PAD 1 intv UDEC 2 } 
  event_6c{ filter UDEC 1 UNUSED PAD 1 timer UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  event_6d{ filter UDEC 1 UNUSED PAD 1 timer UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } } }  0
HOST_TXPW_MEASURE_CNF
  Param1{ event UDEC 1 opid UDEC 1 result UDEC 1 }  0
HOST_TXPW_MEASURE_IND
  Param1{ event UDEC 1 opid UDEC 1 txinf{ power UDEC 1 } }  0
HOST_DPCH_MEASURE_REQ
  Param1{ exe{ opid UDEC 1 mode UDEC 1 } detect{ span UDEC 1 } }  0
HOST_DPCH_MEASURE_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_DPCH_MEASURE_IND
  Param1{ opid UDEC 1 UNUSED PAD 1 fn UDEC 2 dpchinf{ rscp UDEC 1 sir UDEC 1 } }  0
HOST_TRAFFIC_MEASURE_REQ
  Param1{ event UDEC 1 exe{ opid UDEC 1 mode UDEC 1 } 
  UNUSED PAD 1 detect{ periodic{ trchid UDEC 1 period UDEC 1 intv UDEC 2 } 
  event_4a{ trchid UDEC 1 period UDEC 1 quantify UDEC 1 UNUSED PAD 1 th UDEC 2 
  timer UDEC 2 ptat UDEC 2 txat UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  event_4b{ trchid UDEC 1 period UDEC 1 quantify UDEC 1 UNUSED PAD 1 th UDEC 2 
  timer UDEC 2 ptat UDEC 2 txat UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } } }  0
HOST_TRAFFIC_MEASURE_CNF
  Param1{ event UDEC 1 opid UDEC 1 result UDEC 1 }  0
HOST_TRAFFIC_MEASURE_IND
  Param1{ event UDEC 1 opid UDEC 1 n UDEC 1 
  UNUSED PAD 1 lch ARRAY 16 [ lch{ lchid UDEC 1 UNUSED PAD 1 occupancy UDEC 2 variance UDEC 2 average UDEC 2 } ] }  0
HOST_CMAC_CONFIG_REQ
  Param1{ n UDEC 1 
  UNUSED PAD 1 lch ARRAY 8 [ lch{ lcid UDEC 1 UNUSED PAD 1 exe{ mode UDEC 1 UNUSED PAD 1 time UDEC 2 } 
  bindinf{ fwd{ trch{ type UDEC 1 n UDEC 1 ch ARRAY 3 [ trch UDEC 1 ] } nm UDEC 1 
  mac ARRAY 2 [ mac{ n UDEC 1 head ARRAY 6 [ mac UDEC 1 ] } ] 
  rlc{ mode UDEC 1 } 
  UNUSED PAD 1 routing{ group UDEC 1 UNUSED PAD 1 task UDEC 2 crc UDEC 1 UNUSED PAD 1 } } 
  rev{ trch{ type UDEC 1 n UDEC 1 ch ARRAY 3 [ trch UDEC 1 ] } pri UDEC 1 
  asc{ pst UDEC 2 sg UDEC 2 subch UDEC 2 } 
  mac{ n UDEC 1 head ARRAY 6 [ mac UDEC 1 ] } rlc{ mode UDEC 1 } 
  routing{ group UDEC 1 UNUSED PAD 1 task UDEC 2 } } 
  uchinf{ uchid UDEC 2 syncinf UDEC 1 UNUSED PAD 1 pt UDEC 2 } } } ] }  0
HOST_CMAC_CONFIG_CNF
  Param1{ result UDEC 1 }  0
HOST_CIPHER_CONT_REQ
  Param1{ lcid UDEC 1 UNUSED PAD 1 exe{ mode UDEC 1 UNUSED PAD 1 time UDEC 2 } 
  rlc_mode UDEC 1 
  UNUSED PAD 1 rlc{ count_tm{ fwd{ hfn UDEC 4 key_id UDEC 1 UNUSED PAD 3 } 
  rev{ hfn UDEC 4 key_id UDEC 1 UNUSED PAD 3 } } 
  count_aum{ nf UDEC 1 
  UNUSED PAD 3 fwd ARRAY 4 [ fwd{ sn UDEC 2 UNUSED PAD 2 hfn UDEC 4 key_id UDEC 1 UNUSED PAD 3 } ] 
  nr UDEC 1 
  UNUSED PAD 3 rev ARRAY 4 [ rev{ sn UDEC 2 UNUSED PAD 2 hfn UDEC 4 key_id UDEC 1 UNUSED PAD 3 } ] } } 
  key ARRAY 4 [ key{ uea{ id UDEC 1 } ck{ n UDEC 1 data ARRAY 32 [ ck UDEC 1 ] } 
  bearer{ data UDEC 1 data2 UDEC 1 data3 UDEC 1 } } ] }  0
HOST_CIPHER_CONT_CNF
  Param1{ lcid UDEC 1 UNUSED PAD 1 exe{ time UDEC 2 } result UDEC 1 UNUSED PAD 1 }  0
HOST_LCH_TEST_REQ
  Param1{ exe{ opid UDEC 1 mode UDEC 1 } test{ mode1{ lcid UDEC 1 } } }  0
HOST_LCH_TEST_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_BAND_SEARCH_REQ
  Param1{ exe{ opid UDEC 1 mode UDEC 1 } report{ intv UDEC 2 } 
  detect{ crate UDEC 1 cfid ARRAY 38 [ detect UDEC 1 ] rssi UDEC 1 rscp UDEC 1 
  ecn UDEC 1 n UDEC 1 } 
  cell_info1{ codelist ARRAY 64 [ ST_CELL_INFO1 UDEC 1 ] } UNUSED PAD 1 }  0
HOST_BAND_SEARCH_CNF
  Param1{ opid UDEC 1 result UDEC 1 }  0
HOST_BAND_SEARCH_IND
  Param1{ opid UDEC 1 n UDEC 1 
  frq ARRAY 8 [ frq{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } rssi UDEC 1 n UDEC 1 
  cell ARRAY 1 [ cell{ srcd UDEC 2 rscp UDEC 1 ecn UDEC 1 } ] } ] }  0
HOST_PCCPCH_DETECT_REQ
  Param1{ event UDEC 1 exe{ opid UDEC 1 mode UDEC 1 } 
  UNUSED PAD 1 detect{ periodic{ filter UDEC 1 UNUSED PAD 1 intv UDEC 2 quantify UDEC 1 UNUSED PAD 1 } 
  select{ quantify UDEC 1 s_search{ intra UDEC 1 inter UDEC 1 hcs UDEC 1 } 
  hcs{ mobility UDEC 1 q_hyst UDEC 1 } t_reselt UDEC 1 } 
  UNUSED PAD 1 intra_1a{ filter UDEC 1 quantify UDEC 1 tgc UDEC 1 rprang UDEC 1 w UDEC 1 
  hysteresis UDEC 1 dath UDEC 1 UNUSED PAD 1 timer UDEC 2 amount UDEC 1 
  UNUSED PAD 1 intv UDEC 2 } 
  intra_1b{ filter UDEC 1 quantify UDEC 1 tgc UDEC 1 rprang UDEC 1 w UDEC 1 
  hysteresis UDEC 1 timer UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  intra_1c{ filter UDEC 1 quantify UDEC 1 hysteresis UDEC 1 ath UDEC 1 timer UDEC 2 
  amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  intra_1d{ filter UDEC 1 quantify UDEC 1 hysteresis UDEC 1 UNUSED PAD 1 timer UDEC 2 
  amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  intra_1e{ filter UDEC 1 quantify UDEC 1 th{ rscp UDEC 1 ecn UDEC 1 ptl UDEC 1 } 
  tgc UDEC 1 timer UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  intra_1f{ filter UDEC 1 quantify UDEC 1 th{ rscp UDEC 1 ecn UDEC 1 ptl UDEC 1 } 
  tgc UDEC 1 timer UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  inter_2a{ filter UDEC 1 quantify UDEC 1 w UDEC 1 th{ rscp UDEC 1 ecn UDEC 1 } 
  hysteresis UDEC 1 timer UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 
  n UDEC 1 
  UNUSED PAD 1 frq ARRAY 8 [ frq{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } w UDEC 1 
  th{ rscp UDEC 1 ecn UDEC 1 } UNUSED PAD 1 } ] } 
  inter_2b{ filter UDEC 1 quantify UDEC 1 w UDEC 1 th{ rscp UDEC 1 ecn UDEC 1 } 
  hysteresis UDEC 1 timer UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 
  n UDEC 1 
  UNUSED PAD 1 frq ARRAY 8 [ frq{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } w UDEC 1 
  th{ rscp UDEC 1 ecn UDEC 1 } UNUSED PAD 1 } ] } 
  inter_2c{ filter UDEC 1 quantify UDEC 1 hysteresis UDEC 1 UNUSED PAD 1 timer UDEC 2 
  amount UDEC 1 UNUSED PAD 1 intv UDEC 2 n UDEC 1 
  UNUSED PAD 1 frq ARRAY 8 [ frq{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } w UDEC 1 
  th{ rscp UDEC 1 ecn UDEC 1 } UNUSED PAD 1 } ] } 
  inter_2d{ filter UDEC 1 quantify UDEC 1 w UDEC 1 th{ rscp UDEC 1 ecn UDEC 1 } 
  hysteresis UDEC 1 timer UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  inter_2e{ filter UDEC 1 quantify UDEC 1 hysteresis UDEC 1 UNUSED PAD 1 timer UDEC 2 
  amount UDEC 1 UNUSED PAD 1 intv UDEC 2 n UDEC 1 
  UNUSED PAD 1 frq ARRAY 8 [ frq{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } w UDEC 1 
  th{ rscp UDEC 1 ecn UDEC 1 } UNUSED PAD 1 } ] } 
  inter_2f{ filter UDEC 1 quantify UDEC 1 w UDEC 1 th{ rscp UDEC 1 ecn UDEC 1 } 
  hysteresis UDEC 1 timer UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  inter_6e{ filter UDEC 1 UNUSED PAD 1 timer UDEC 2 amount UDEC 1 UNUSED PAD 1 intv UDEC 2 } 
  inter_6f{ filter UDEC 1 UNUSED PAD 1 th UDEC 2 timer UDEC 2 amount UDEC 1 
  UNUSED PAD 1 intv UDEC 2 } 
  inter_6g{ filter UDEC 1 UNUSED PAD 1 th UDEC 2 timer UDEC 2 amount UDEC 1 
  UNUSED PAD 1 intv UDEC 2 } } 
  cell_info2{ no UDEC 1 
  fdd_map{ n_rscp UDEC 1 
  rscp ARRAY 1 [ rscp{ type UDEC 1 upper{ q_meas UDEC 1 q_map UDEC 1 } 
  lower{ q_meas UDEC 1 q_map UDEC 1 } } ] 
  n_ecn UDEC 1 
  ecn ARRAY 1 [ ecn{ type UDEC 1 upper{ q_meas UDEC 1 q_map UDEC 1 } 
  lower{ q_meas UDEC 1 q_map UDEC 1 } } ] } 
  n UDEC 1 
  UNUSED PAD 2 frq ARRAY 3 [ frq{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } n UDEC 1 
  UNUSED PAD 3 cell ARRAY 5 [ cell{ pcpich{ srcd UDEC 2 } UNUSED PAD 2 rtd UDEC 4 dtxp UDEC 1 utxp UDEC 1 
  coff UDEC 1 q_qulmin UDEC 1 q_rxlmin UDEC 1 q_off UDEC 1 
  hcs{ q_hcs UDEC 1 hcs_prio UDEC 1 pen_time UDEC 1 temp_offset UDEC 1 } 
  sttd UDEC 1 rsfn UDEC 1 status ARRAY 6 [ cell UDEC 1 ] UNUSED PAD 2 } ] } ] } }  0
HOST_PCCPCH_DETECT_CNF
  Param1{ event UDEC 1 opid UDEC 1 result UDEC 1 }  0
HOST_PCCPCH_DETECT_IND
  Param1{ event UDEC 1 opid UDEC 1 n UDEC 1 
  UNUSED PAD 1 frq ARRAY 3 [ frq{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } rssi UDEC 1 n UDEC 1 
  UNUSED PAD 2 cell ARRAY 5 [ cell{ srcd UDEC 2 UNUSED PAD 2 sftm UDEC 4 rxlev{ rscp UDEC 1 map UDEC 1 s UDEC 2 } 
  qual{ ecn UDEC 1 map UDEC 1 s UDEC 2 } ptl UDEC 1 
  UNUSED PAD 1 hcs{ h UDEC 2 rank UDEC 2 pen_time UDEC 1 UNUSED PAD 1 } 
  status UDEC 1 UNUSED PAD 3 } ] } ] }  0
HOST_PCCPCH_STATUS_REQ
  Param1{ opid UDEC 1 quantify UDEC 1 }  0
HOST_PCCPCH_STATUS_CNF
  Param1{ opid UDEC 1 }  0
HOST_BCCH_GET_REQ
  Param1{ band{ crate UDEC 1 UNUSED PAD 1 fid UDEC 2 } srcd UDEC 2 exe{ time UDEC 2 } 
  detect{ rep UDEC 1 bchind ARRAY 128 [ detect UDEC 1 ] } 
  bcch{ tb ARRAY 32 [ tb{ bchinf UDEC 1 bch ARRAY 31 [ tb UDEC 1 ] } ] } UNUSED PAD 1 }  0
HOST_BCCH_GET_CNF
  Param1{ srcd UDEC 2 
  bcch{ tb ARRAY 32 [ tb{ bchinf UDEC 1 bch ARRAY 31 [ tb UDEC 1 ] } ] } }  0
HOST_FACH_MEASUREMENT_REQ
  Param1{ exe{ mode UDEC 1 } m_rep UDEC 1 c_rnti UDEC 2 }  0
HOST_FACH_MEASUREMENT_CNF
  Param1{ result UDEC 1 }  0
UBCAF_CPICH_OPENED
  Param1{ Result DEC 4 }  0
UMRTR_TIMER_EXPIRY
  Param1{ PoolId UDEC 1 UNUSED PAD 3 ListNb UDEC 4 List HEX 4 Obsolete UDEC 1 UNUSED PAD 3 }  0
UMRTR_DSP_CELL_IND
  Param1{ Mode DEC 4 CellIndTyp UDEC 1 UNUSED PAD 3 }  0
UEF_OMF2C_CALLBACK_IND
  Param1{ ServiceId DEC 4 pBuf HEX 4 }  0
UMRTR_DSP_UE_INT_MEAS_IND
  Param1{ Mode DEC 4 }  0
UMRTR_DSP_32K_CALIBRATE_CNF
  Param1{ Acceptance DEC 4 }  0
PSSV_ERROR_IND
  Param1{ factor UDEC 1 level UDEC 1 detectposition UDEC 1 UNUSED PAD 1 content UDEC 2 }  0
RIMP_DATA_IND
  Param1{ length UDEC 2 UNUSED PAD 2 ptr_data UDEC 4 }  0
START_MSG_cnf
  Param1{ mode UDEC 1 no UDEC 1 
  data{ class_a UDEC 2 class_b UDEC 2 class_c UDEC 2 class_d UDEC 2 class_e UDEC 2 
  class_f UDEC 2 class_g UDEC 2 class_h UDEC 2 } }  0
START_TIMEOUT
  Param1{ mode UDEC 1 no UDEC 1 
  data{ class_a UDEC 2 class_b UDEC 2 class_c UDEC 2 class_d UDEC 2 class_e UDEC 2 
  class_f UDEC 2 class_g UDEC 2 class_h UDEC 2 } }  0
STOP_MSG_cnf
  Param1{ mode UDEC 1 no UDEC 1 }  0
START_MSG_req
  Param1{ mode UDEC 1 no UDEC 1 }  0
DUM_CONNECT_IND
  Param1 DEC 4  0
L1DG_DED_SIG_LVL
  BcchRxLevel UDEC 1 BcchBsic UDEC 1 Rlc UDEC 1 TxLevel UDEC 1 TimingAdv UDEC 1 
  RxQuality UDEC 1 Arfcn UDEC 2 RxLevSub UDEC 1 RxLevFull UDEC 1 
  Ncells UDEC 1 
  UNUSED PAD 1 NcellData ARRAY 12 [ NcellData{ Arfcn UDEC 2 Bsic UDEC 1 BsicDecodeTryCnt UDEC 1 BsicReconfTryCnt UDEC 1 UNUSED PAD 1 } ] 
  BAListData ARRAY 32 [ BAListData{ Arfcn UDEC 2 RxLevel UDEC 1 CarrierState UDEC 1 InitBsicCnt UDEC 1 UNUSED PAD 1 } ]  0
L1DG_PTM_TA_PWR_LVL
  ptcch_in_use UDEC 1 UNUSED PAD 3 timing_advance_value DEC 4 timing_advance_index DEC 4 
  tx_pwr UDEC 1 UNUSED PAD 3 rxlev_pdch DEC 4 c UDEC 1 rxqual UDEC 1 
  sign_var UDEC 1  0
L1DG_PTM_SIG_LVL
  rx_lev DEC 4  0
L1DG_IDLE_SIG_LVL
  Dsc UDEC 1 RxLevel UDEC 1 Arfcn UDEC 2 Bsic UDEC 1 Ncells UDEC 1 
  NcellData ARRAY 6 [ NcellData{ Arfcn UDEC 2 Bsic UDEC 1 RxLevel UDEC 1 } ]  0
L1DG_SELECT_SYNC_CELL
  Arfcn UDEC 2 l1x_idle_frame_processing_start UDEC 2 l1x_idle_frame_processing_end UDEC 2  0
L1DG_PTM_SYNC_DIAG_ISYNC
  arfcn UDEC 2 tim_offset UDEC 2 stored_block_number UDEC 2 tn UDEC 1 
  l1c_ul_max_ts UDEC 1 l1c_dl_max_ts UDEC 1 l1x_gamma_time_slot UDEC 1 
  l1x_tx_to_sync_time UDEC 2  0
L1DG_PTM_SYNC_DIAG_RECONF
  arfcn UDEC 2 tim_offset UDEC 2 stored_block_number UDEC 2 l1c_ul_max_ts UDEC 1 
  l1c_dl_min_ts UDEC 1 l1c_dl_max_ts UDEC 1 l1x_gamma_time_slot UDEC 1 
  l1x_tx_to_sync_time UDEC 2  0
L1DG_PTM_SYNC_DIAG_RECONF2
  arfcn UDEC 2 l1c_tbf_active UDEC 1 blk_no UDEC 1 l1c_ul_max_ts UDEC 1 
  l1c_dl_min_ts UDEC 1 earliest_tn_SB_window_start UDEC 2 latest_tn_SB_window_start UDEC 2 
  temp_sync_offset UDEC 2  0
L1DG_SYNC_ACTION_ISYNC_DATA
  search_state UDEC 1 l1x_sync_started UDEC 1  0
RRDG_C1_C2_VALUES
  C1C2Data{ ServingCellArfcn UDEC 2 ServingCellCx1 DEC 2 ServingCellCx2 DEC 2 
  Ncells UDEC 1 UNUSED PAD 1 NcellCx1Cx2Data ARRAY 6 [ NcellCx1Cx2Data{ Arfcn UDEC 2 Cx1 DEC 2 Cx2 DEC 2 } ] 
  Resels DEC 4 Fails DEC 4 }  0
RRDG_C31_C32_VALUES
  C31C32Data{ ServingCellArfcn UDEC 2 ServingCellCx1 DEC 2 ServingCellCx2 DEC 2 
  Ncells UDEC 1 UNUSED PAD 1 NcellCx1Cx2Data ARRAY 6 [ NcellCx1Cx2Data{ Arfcn UDEC 2 Cx1 DEC 2 Cx2 DEC 2 } ] 
  Resels DEC 4 Fails DEC 4 }  0
RRDG_GPRS_INFO
  GprsIndicator UDEC 1 NetworkOpMode UDEC 1 NetworkControlOrder UDEC 1 
  DualBand UDEC 1 PbcchIndicator UDEC 1 
  CellData{ PBCCHData{ psi1_repeat_period UDEC 1 bs_pbcch_blks UDEC 1 bs_pag_blks_res UDEC 1 
  pb UDEC 1 tsc UDEC 1 tn UDEC 1 
  ChannelData{ hopping UDEC 1 single_rf UDEC 1 hopping_rf{ maio UDEC 1 hsn UDEC 1 } } 
  acc_burst_type UDEC 1 ctrl_ack_type UDEC 1 packet_psi_status UDEC 1 
  psi_count_lr UDEC 1 psi_count_hr UDEC 1 } 
  BCCHData{ Rac UDEC 1 PriorityAccessThr UDEC 1 spgc_ccch_sup UDEC 1 } }  0
SNP_DG_DATA_FLOW
  ul_sn_unitdata_req_no UDEC 2 ul_ll_unitdata_req_no UDEC 2 dl_sn_unitdata_ind_no UDEC 2 
  dl_ll_unitdata_ind_no UDEC 2 ul_sn_data_req_no UDEC 2 ul_ll_data_req_no UDEC 2 
  dl_sn_data_ind_no UDEC 2 dl_ll_data_ind_no UDEC 2  0
L1DG_SCELL_AFC_RTT_AGC_DIAG
  CurrentAFCCorrection DEC 2 LastPeriodAFCDelta DEC 2 CurrentTimeTrackingAdjust HEX 1 
  ValidCount UDEC 1 
  BurstInfo ARRAY 4 [ BurstInfo{ RawRSSI UDEC 2 VariableGain UDEC 1 UNUSED PAD 1 QualityEstimate UDEC 2 
  TimingError DEC 2 FreqError DEC 2 } ]  0
L1DG_NCELL_AFC_RTT_AGC_DIAG
  Arfcn UDEC 2 QuarterBitOffset DEC 2 
  BurstInfo{ RawRSSI UDEC 2 VariableGain UDEC 1 UNUSED PAD 1 QualityEstimate UDEC 2 
  TimingError DEC 2 FreqError DEC 2 }  0
L1DG_NCELL_A_SYNC_DIAG
  Arfcn UDEC 2 InitFreqCorr DEC 2  0
L1DG_NCELL_SCH_DIAG
  Arfcn UDEC 2 QuarterBitOffset DEC 2 FreqCorr DEC 2  0
L1DG_PCH_TIMERS_DIAG
  timer_code UDEC 2 pch_distance UDEC 2 bs_pa_mfrms UDEC 2 timer_tolerance UDEC 2 
  tolerance_x UDEC 2 unadjusted_time UDEC 2 adjusted_time UDEC 2  0
PSDG_SLEEP_METRICS
  SoftOffs UDEC 4 FramesInSoftOff UDEC 4 OkCcchDecAfterSfOff UDEC 4 
  FailCcchDecAfterSfOff UDEC 4 MfSleeps UDEC 4 FramesInMfSleep UDEC 4 
  OkCcchDecAfterMfs UDEC 4 FailCcchDecAfterMfs UDEC 4 EarlyWakeupCount UDEC 4 
  AverageFramesInSfOff UDEC 2 AverageFramesInMFS UDEC 1 PaMfms UDEC 1 
  SchOkNeighbours UDEC 1 PerCentInSoftOff UDEC 1 PercentInMfs UDEC 1 
  PercentInSleep UDEC 1 PercentTotalSleep UDEC 1  0
PSDG_UMTS_SLEEP_METRICS
  PercentInUSleep UDEC 1 UNUSED PAD 1 NumSleeps UDEC 2 NumFramesAsleep UDEC 2 
  AverageFramesInUSleep UDEC 2 PercentTotalSleep UDEC 1  0
PSDG_FAILURE_DIAG
  Num32kCals UDEC 4 BoardTempChecks UDEC 4 BoardTempDriftFail UDEC 4 
  ReCal32kHzDueToCcchFail UDEC 4 PreviousBoardTemp UDEC 1 CurrentBoardTemp UDEC 1 
  UNUSED PAD 2 CalCounter32kHz UDEC 4 TotTask UDEC 4 TotL1cQ UDEC 4 
  TotSDsp UDEC 4 TotSer UDEC 4 TotDat UDEC 4 TotLMfs UDEC 4 TotEFMfs UDEC 4 
  TotMFSn UDEC 4 TotEFSo UDEC 4 TotCry UDEC 4 TotCal UDEC 4 TotSOn UDEC 4 
  TotCSOD UDEC 4 TotATSOD UDEC 4 TotNOoz UDEC 4 TotSim UDEC 4 TotL1xS UDEC 4 
  Task UDEC 4 L1cQ UDEC 4 SDsp UDEC 4 Ser UDEC 4 Dat UDEC 4 LMfs UDEC 4 
  EFMfs UDEC 4 MFSn UDEC 4 EFSo UDEC 4 Cry UDEC 4 Cal UDEC 4 SOn UDEC 4 
  CSOD UDEC 4 ATSOD UDEC 4 NOoz UDEC 4 Sim UDEC 4 L1xS UDEC 4  0
L1_MON_RSSI_DISCARD_DIAG
  arfcn UDEC 2 margin_level UDEC 2 var_gain UDEC 1 rxlev UDEC 1 actual_discard UDEC 1  0
MMIDG_DISPLAY_DIAG
  display_data{ A ARRAY 0 [ DISPLAY_DATA UDEC 1 ] }  0
L1DG_DSP_DEBUG_INFO
  info ARRAY 10 [ L1DG_DSP_DEBUG_INFO UDEC 1 ]  0
MACDG_TBF_STATUS
  UplinkTfi UDEC 1 UplinkRlcMode UDEC 1 DownlinkTfi UDEC 1 DownlinkRlcMode UDEC 1  0
BINARY_DATA_DUMP
  msgID_hi UDEC 1 msgID_lo UDEC 1 MsgNo_hi UDEC 1 MsgNo_lo UDEC 1 
  TotNoMsg_hi UDEC 1 TotNoMsg_lo UDEC 1 DataSize_hi UDEC 1 DataSize_lo UDEC 1 
  TotDataSize_hi UDEC 1 TotDataSize_lo UDEC 1 hif_data ARRAY 0 [ BINARY_DATA_DUMP UDEC 1 ]  0
PH_MAC_DATA_REQ
  BlockFormat UDEC 1 PdchBlock{ A ARRAY 54 [ RB_DATA UDEC 1 ] }  0
PH_MAC_DATA_IND_DIAG
  TimeslotNo UDEC 1 BlockFormat UDEC 1 ChannelType UDEC 1 
  PdchBlock{ A ARRAY 54 [ RB_DATA UDEC 1 ] }  0
RLC_DATA_CNF_DIAG
  Tlli{ A ARRAY 4 [ DIAG_TLLI UDEC 1 ] } ValidNodes UDEC 1 
  UNUSED PAD 3 AckedPduInfo ARRAY 64 [ AckedPduInfo{ LlpduId{ ll_buf_id UDEC 1 ll_buf_idx UDEC 1 UNUSED PAD 2 pdu_length DEC 4 } 
  Sapi UDEC 1 UNUSED PAD 3 } ]  0
RLC_DATA_IND_HDR_DIAG
  Tlli{ A ARRAY 4 [ DIAG_TLLI UDEC 1 ] } PduLength DEC 4 
  PduData{ A ARRAY 20 [ PDU_HDR_DATA UDEC 1 ] }  0
RLC_DATA_IND_FULL_DIAG
  Tlli{ A ARRAY 4 [ DIAG_TLLI UDEC 1 ] } ContinuationBlock UDEC 1 
  UNUSED PAD 3 PduLength DEC 4 PduData{ A ARRAY 250 [ PDU_FULL_DATA UDEC 1 ] }  0
TEST_HARNESS_STEP3_SIG
  Data ARRAY 255 [ TEST_HARNESS_STEP3_SIG UDEC 1 ]  0
UIMP_C_APDU_REQ_COMMAND
  index UDEC 2 length UDEC 2 data ARRAY 300 [ UIMP_C_APDU_REQ_COMMAND UDEC 1 ]  0
UIMP_C_APDU_RES_RESPONSE
  index UDEC 2 length UDEC 2 data ARRAY 300 [ UIMP_C_APDU_RES_RESPONSE UDEC 1 ]  0
UP_DATA_PDU
  pdu_index UDEC 1 status UDEC 1 work UDEC 1 block_count UDEC 1 
  block{ block_index UDEC 1 UNUSED PAD 1 length UDEC 2 data ARRAY 80 [ UP_DATA_PDU_BLOCK UDEC 1 ] }  0
UP_DATA_PDU_CONT
  block{ block_index UDEC 1 UNUSED PAD 1 length UDEC 2 data ARRAY 80 [ UP_DATA_PDU_BLOCK UDEC 1 ] }  0
L1DG_ULL1_DRX_ALLOCATION
  AllocFrames UDEC 2  0
CSD_DATAFRAME_DIAG
  Uchid UDEC 1 TchFormat UDEC 1 RLPVersion UDEC 1 NonTransparent UDEC 1 
  UplinkDirection UDEC 1 CSDDataFrame{ A ARRAY 72 [ MaxCSDFrame UDEC 1 ] }  0
T_RCVS
  Param1 DEC 4 0
T3200
  Param1 DEC 4 0
T_PENALTY
  Param1 DEC 4 0
T3200_GRR
  Param1 DEC 4 0
TIME_REEST
  Param1 DEC 4 0
TIME_LL_UNITDATA_IND
  Param1 DEC 4 0
TIME_UACK_XOFF
  Param1 DEC 4 0
TIME_ACK_XOFF
  Param1 DEC 4 0
T201
  Param1 DEC 4 0
