[MCU Info #4B908293-59A4-11D5-AD5A-00508BCD726B]
V JP190V0700.nep&#0A13-01-06&#0ARM-97&#0A(c) NMP&#0A

[PPM Info #8473C5E7-AC0C-11D5-89FA-00C04FA0F3EA]
V JP190V0700.nep&#0A13-01-06&#0ARM-97&#0A(c)&#0ALOA

[ADSP Info #CB632B5D-19E8-4077-92AB-E728149CB7DA]
V JP190V0700_p_nok.ucp_oa\n13-01-06\nRM-97\n(c) NMP\n

[Simlock #87FFB2F0-A05F-11d5-ADC7-00B0D0116520]
SIMLOCK_IO_FILE_VERSION_V0.3

CONFIG_DATA="FFFFFFFFFFFFFFFF"
PROFILE_BITS="0000000000000000"

BLOCK
  BLOCK_STATE=NOT_DISCARD

LOCK
  STATE=CLOSED
  SIM_PATH="3F007F206F07FFFF"
  CRITERION=NIBBLEWISE_DISTINCT_EQ
  MASK=0b1111100000000000
  READ_SPECIFICATION=0x10000000
  UNIT_LENGTH=0
  DATA="00101F"
ENDLOCK

ENDBLOCK

[Settings Server Data #829803BD-D1AA-4077-93B4-767BD2203919]
FileFormat = 5.0
		; "T9 language state"
		Setting ID		= .1.1.1
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "T9 user database"
		Setting ID		= .1.1.2
		Setting type	= Binary
		Setting length	= 2012
		Setting value	= 07,d0,00,00,00,00,00,0f,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00

		; "Font size"
		Setting ID		= .1.1.3
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Grid state"
		Setting ID		= .1.2.3
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 1 (0x0001)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.0.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 1 (0x0001)

					; "Menu background"
					Setting ID		= .1.2.4.1.0.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 1 (0x0001)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.0.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.1.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 2 (0x0002)

					; "Menu background"
					Setting ID		= .1.2.4.1.1.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 2 (0x0002)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.1.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.2.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 3 (0x0003)

					; "Menu background"
					Setting ID		= .1.2.4.1.2.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 3 (0x0003)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.2.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.3.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 4 (0x0004)

					; "Menu background"
					Setting ID		= .1.2.4.1.3.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 4 (0x0004)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.3.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.4.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 5 (0x0005)

					; "Menu background"
					Setting ID		= .1.2.4.1.4.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 5 (0x0005)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.4.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.5.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 6 (0x0006)

					; "Menu background"
					Setting ID		= .1.2.4.1.5.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 6 (0x0006)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.5.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.6.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 7 (0x0007)

					; "Menu background"
					Setting ID		= .1.2.4.1.6.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 7 (0x0007)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.6.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.7.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 8 (0x0008)

					; "Menu background"
					Setting ID		= .1.2.4.1.7.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 8 (0x0008)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.7.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.8.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 9 (0x0009)

					; "Menu background"
					Setting ID		= .1.2.4.1.8.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 9 (0x0009)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.8.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.9.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 10 (0x000a)

					; "Menu background"
					Setting ID		= .1.2.4.1.9.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 10 (0x000a)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.9.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.10.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Menu background"
					Setting ID		= .1.2.4.1.10.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.10.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.11.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Menu background"
					Setting ID		= .1.2.4.1.11.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.11.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.12.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Menu background"
					Setting ID		= .1.2.4.1.12.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.12.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.13.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Menu background"
					Setting ID		= .1.2.4.1.13.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.13.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.14.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Menu background"
					Setting ID		= .1.2.4.1.14.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.14.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.15.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Menu background"
					Setting ID		= .1.2.4.1.15.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.15.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.16.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Menu background"
					Setting ID		= .1.2.4.1.16.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.16.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.17.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Menu background"
					Setting ID		= .1.2.4.1.17.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.17.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.18.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Menu background"
					Setting ID		= .1.2.4.1.18.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.18.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Wallpaper select"
					Setting ID		= .1.2.4.1.19.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Menu background"
					Setting ID		= .1.2.4.1.19.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Signal and battery bar"
					Setting ID		= .1.2.4.1.19.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

		; "Background light state"
		Setting ID		= .1.2.5
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Powersave clock timeout state"
		Setting ID		= .1.2.6
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 1 (0x0001)

		; "Brightness select state"
		Setting ID		= .1.2.7
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 5 (0x0005)

			; "Wake-up graphic switch"
			Setting ID		= .1.3.1.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Dealer welcome note"
			Setting ID		= .1.3.1.3
			Setting type	= ASCII
			Setting length	= 1
			Setting value	= ""

			; "User welcome note"
			Setting ID		= .1.3.1.4
			Setting type	= Unicode
			Setting length	= 2
			Setting value	= ""

			; "Display of Alpha Tag and MIN/MDN on Phone Power-up Options - PRI 681"
			Setting ID		= .1.3.1.5
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Banner Menu - PRI 103"
			Setting ID		= .1.3.1.6
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Automatic keyguard switch"
			Setting ID		= .1.3.2.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Automatic keyguard timeout"
			Setting ID		= .1.3.2.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 10 (0x000a)

			; "Automatic keyguard lock"
			Setting ID		= .1.3.2.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

				; "Headset default profile"
				Setting ID		= .1.3.3.1.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 6 (0x0006)

				; "Headset automatic answer switch"
				Setting ID		= .1.3.3.1.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Carkit default profile"
				Setting ID		= .1.3.3.2.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 6 (0x0006)

				; "Carkit automatic answer switch"
				Setting ID		= .1.3.3.2.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Carkit automatic light switch"
				Setting ID		= .1.3.3.2.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

		; "Phonebook view type"
		Setting ID		= .1.4.2
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Phonebook memory"
		Setting ID		= .1.4.4
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 1 (0x0001)

		; "Speed dial select state"
		Setting ID		= .1.4.6
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Phone Number Grouping Options - PRI 111"
		Setting ID		= .1.4.10
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Plus-code (+) to International Direct Dialing (IDD) Prefix Translation - PRI 980"
		Setting ID		= .1.4.11
		Setting type	= Binary
		Setting length	= 3
		Setting value	= 30,30,00

		; "Minimum Number of Digits for Caller ID/Phonebook Matching - PRI 1032"
		Setting ID		= .1.4.12
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 10 (0x000a)

			; "Signature select state"
			Setting ID		= .1.5.2.4
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Enhanced Voice Mail Notification - PRI 88"
			Setting ID		= .1.5.2.8
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

				; "Origination Address for MT SMS via Email Options - PRI 106"
				Setting ID		= .1.5.2.20.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Origination Address for MT SMS via E-mail Value - PRI 877"
				Setting ID		= .1.5.2.20.2
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "Validate Email Address For MO SMS - PRI 112"
				Setting ID		= .1.5.2.20.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "MO SMS Email Address Support - PRI 95"
				Setting ID		= .1.5.2.20.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Maximum Size of Callback Number - PRI 139"
				Setting ID		= .1.5.2.21.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 36 (0x0024)

				; "Maximum Size of Recipient Email Address - PRI 138"
				Setting ID		= .1.5.2.21.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 60 (0x003c)

				; "Maximum Size of Recipient Phone Number - PRI 137"
				Setting ID		= .1.5.2.21.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 36 (0x0024)

				; "Maximum Size for Submit Message - PRI 213"
				Setting ID		= .1.5.2.21.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 187 (0x00bb)

				; "Maximum Size for User Data in MO SMS Message (in bytes) - PRI 1081"
				Setting ID		= .1.5.2.21.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 140 (0x008c)

				; "Maximum Number of Characters for MO SMS Text - PRI 1291"
				Setting ID		= .1.5.2.21.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 160 (0x00a0)

				; "MO SMS Destination Address Format Options - PRI 87"
				Setting ID		= .1.5.2.21.7
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Message sending failed indication options - PRI 1024"
				Setting ID		= .1.5.2.22.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Send empty MO SMS message - PRI 976"
				Setting ID		= .1.5.2.22.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "MO SMS Traffic Channel Options for Multiple Recipients - PRI 679"
				Setting ID		= .1.5.2.22.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Force MO SMS Messages to be Sent over Traffic Channel - PRI 72"
				Setting ID		= .1.5.2.22.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Default Service Option for MO SMS Messages - PRI 438"
				Setting ID		= .1.5.2.22.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Transport Layer (Layer 3) Delivery Acknowledgement Timer - PRI 210"
				Setting ID		= .1.5.2.22.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 32 (0x0020)

				; "Language Indicator Subparameter in WMT MO SMS Message - PRI 908"
				Setting ID		= .1.5.2.23.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Network Support of 8-bit ASCII Characters in MO SMS - PRI 256"
				Setting ID		= .1.5.2.23.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Non-Standard MO & MT SMS Message Encoding (Vietnamese) Handling Feature - PRI 1265"
				Setting ID		= .1.5.2.23.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Destination Address Parameter in MT SMS Acknowledge Support - PRI 83"
				Setting ID		= .1.5.2.23.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Text Message Timestamp Options - PRI 108"
				Setting ID		= .1.5.2.24.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Urgent Message Priority Handling - PRI 1023"
				Setting ID		= .1.5.2.24.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Decoding of Octet Unspecified Encoding Assignment for SMS Message Options - PRI 511"
				Setting ID		= .1.5.2.24.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 2 (0x0002)

				; "Filter For Duplicate MT SMS - PRI 84"
				Setting ID		= .1.5.2.24.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Display and Storage of Delivery Acknowledgement Messages - PRI 518"
				Setting ID		= .1.5.2.24.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Send callback number Menu - PRI 1072"
				Setting ID		= .1.5.2.25.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Delivery note Menu - PRI 1071"
				Setting ID		= .1.5.2.25.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Smiley text"
				Setting ID		= .1.5.5.0.1
				Setting type	= Unicode
				Setting length	= 8
				Setting value	= ":-)"

				; "Smiley text"
				Setting ID		= .1.5.5.1.1
				Setting type	= Unicode
				Setting length	= 8
				Setting value	= ":-("

				; "Smiley text"
				Setting ID		= .1.5.5.2.1
				Setting type	= Unicode
				Setting length	= 8
				Setting value	= ":-/"

				; "Smiley text"
				Setting ID		= .1.5.5.3.1
				Setting type	= Unicode
				Setting length	= 8
				Setting value	= ";o)"

				; "Smiley text"
				Setting ID		= .1.5.5.4.1
				Setting type	= Unicode
				Setting length	= 8
				Setting value	= ";oD"

				; "Smiley text"
				Setting ID		= .1.5.5.5.1
				Setting type	= Unicode
				Setting length	= 14
				Setting value	= "(&#1601;&#1575;&#1585;&#1594;)"

				; "Smiley text"
				Setting ID		= .1.5.5.6.1
				Setting type	= Unicode
				Setting length	= 14
				Setting value	= "(&#1601;&#1575;&#1585;&#1594;)"

				; "Smiley text"
				Setting ID		= .1.5.5.7.1
				Setting type	= Unicode
				Setting length	= 14
				Setting value	= "(&#1601;&#1575;&#1585;&#1594;)"

				; "Template text"
				Setting ID		= .1.5.6.0.1
				Setting type	= Unicode
				Setting length	= 28
				Setting value	= "&#1571;&#1585;&#1580;&#1608; &#1575;&#1604;&#1575;&#1578;&#1589;&#1575;&#1604; "

				; "Template text"
				Setting ID		= .1.5.6.1.1
				Setting type	= Unicode
				Setting length	= 48
				Setting value	= "&#1571;&#1606;&#1575; &#1601;&#1610; &#1575;&#1604;&#1605;&#1606;&#1586;&#1604;. &#1575;&#1578;&#1589;&#1604; &#1576;&#1610; "

				; "Template text"
				Setting ID		= .1.5.6.2.1
				Setting type	= Unicode
				Setting length	= 46
				Setting value	= "&#1571;&#1606;&#1575; &#1601;&#1610; &#1575;&#1604;&#1593;&#1605;&#1604;. &#1575;&#1578;&#1589;&#1604; &#1576;&#1610; "

				; "Template text"
				Setting ID		= .1.5.6.3.1
				Setting type	= Unicode
				Setting length	= 86
				Setting value	= "&#1571;&#1606;&#1575; &#1601;&#1610; &#1575;&#1580;&#1578;&#1605;&#1575;&#1593;. &#1575;&#1578;&#1589;&#1604; &#1576;&#1610; &#1601;&#1610; &#1608;&#1602;&#1578; &#1604;&#1575;&#1581;&#1602; &#1575;&#1604;&#1587;&#1575;&#1593;&#1577; "

				; "Template text"
				Setting ID		= .1.5.6.4.1
				Setting type	= Unicode
				Setting length	= 38
				Setting value	= "&#1578;&#1605; &#1573;&#1604;&#1594;&#1575;&#1569; &#1575;&#1604;&#1575;&#1580;&#1578;&#1605;&#1575;&#1593;."

				; "Template text"
				Setting ID		= .1.5.6.5.1
				Setting type	= Unicode
				Setting length	= 62
				Setting value	= "&#1573;&#1606;&#1606;&#1610; &#1605;&#1578;&#1571;&#1582;&#1585;. &#1587;&#1571;&#1603;&#1608;&#1606; &#1607;&#1606;&#1575;&#1603; &#1575;&#1604;&#1587;&#1575;&#1593;&#1577; "

				; "Template text"
				Setting ID		= .1.5.6.6.1
				Setting type	= Unicode
				Setting length	= 26
				Setting value	= "&#1587;&#1608;&#1601; &#1571;&#1585;&#1575;&#1603; &#1601;&#1610; "

				; "Template text"
				Setting ID		= .1.5.6.7.1
				Setting type	= Unicode
				Setting length	= 34
				Setting value	= "&#1587;&#1608;&#1601; &#1571;&#1585;&#1575;&#1603; &#1575;&#1604;&#1587;&#1575;&#1593;&#1577; "

			; "Incoming multimedia messages Options - PRI 1027"
			Setting ID		= .1.5.9.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Maximum Size for MMS Message - PRI 1028"
			Setting ID		= .1.5.9.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 25600 (0x6400)

			; "Wireless Application Protocol Teleservice Support - PRI 204"
			Setting ID		= .1.5.9.4
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "MMS Message Processing - PRI 961"
			Setting ID		= .1.5.9.5
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Retry MMS Transfer for Temporary Failures - PRI 1038"
			Setting ID		= .1.5.9.6
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

				; "MMS Proxy Server Authentication Username - PRI 988"
				Setting ID		= .1.5.9.20.1
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "MMS Proxy Server Authentication Password - PRI 989"
				Setting ID		= .1.5.9.20.2
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "MMS Proxy Server Authentication Password Format Options - PRI 1311"
				Setting ID		= .1.5.9.20.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "MMS Proxy Server Connection Type Preference - PRI 990"
				Setting ID		= .1.5.9.20.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "MMS Proxy Server IP Address - PRI 987"
				Setting ID		= .1.5.9.20.5
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "MMSC URL (Primary) - PRI 860"
				Setting ID		= .1.5.9.20.6
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "Username (3G Packet) - PRI 1234"
				Setting ID		= .1.5.9.20.7
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "Password (3G Packet) - PRI 1236"
				Setting ID		= .1.5.9.20.8
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "PPP Authentication Options (3G Packet) - PRI 1238"
				Setting ID		= .1.5.9.20.9
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 3 (0x0003)

				; "PPP Authentication Options (3G Packet Data) - PRI 136"
				Setting ID		= .1.5.9.20.10
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 3 (0x0003)

				; "Simple/Mobile IP NAI - PRI 269"
				Setting ID		= .1.5.9.20.11
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "Simple/Mobile IP NAI Format Options - PRI 660"
				Setting ID		= .1.5.9.20.12
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Simple/Mobile IP NAI Customer Specified Text - PRI 666"
				Setting ID		= .1.5.9.20.13
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "Simple/Mobile IP NAI Length - PRI 268"
				Setting ID		= .1.5.9.20.14
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Simple/Mobile IP MN_AAA Shared Secret Data Format Options - PRI 1014"
				Setting ID		= .1.5.9.20.15
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Simple/Mobile IP MN_AAA Shared Secret Key - PRI 275"
				Setting ID		= .1.5.9.20.16
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "Simple/Mobile IP MN_AAA Shared Secret Key Length - PRI 274"
				Setting ID		= .1.5.9.20.17
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "International Dial Code - Country Code - PRI 947"
				Setting ID		= .1.5.9.21.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "MCC/IDC Options for Client ID in HTTP Header (MMS) - PRI 1077"
				Setting ID		= .1.5.9.21.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "MDN/MIN Options for Client ID in HTTP Header (MMS) - PRI 986"
				Setting ID		= .1.5.9.21.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Session Header ASCII String for HTTP Request Messages - PRI 948"
				Setting ID		= .1.5.9.21.4
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "User Agent Profile URL - PRI 853"
				Setting ID		= .1.5.9.21.5
				Setting type	= Binary
				Setting length	= 2
				Setting value	= 00,00

				; "MMS M_Notify Response Indication Message Transmission - PRI 1041"
				Setting ID		= .1.5.9.22.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Non-Standard Message Handling for MMS Messages Exceeding Maximum Supported Size - PRI 1241"
				Setting ID		= .1.5.9.22.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "WAP Push Message Decoding Options - PRI 934"
				Setting ID		= .1.5.9.23.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 2 (0x0002)

				; "Push Proxy Gateway ID Options - PRI 965"
				Setting ID		= .1.5.9.23.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

		; "Active profile"
		Setting ID		= .1.6.1
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

				; "Screen saver switch"
				Setting ID		= .1.6.2.0.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver timeout"
				Setting ID		= .1.6.2.0.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver graphics"
				Setting ID		= .1.6.2.0.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Backlight alert"
				Setting ID		= .1.6.2.0.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, notification"
				Setting ID		= .1.6.2.0.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Lights, coverage"
				Setting ID		= .1.6.2.0.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, alert"
				Setting ID		= .1.6.2.0.7
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Theme selection"
				Setting ID		= .1.6.2.0.8
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Profile ringing tone"
				Setting ID		= .1.6.2.0.9
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 130 (0x0082)

				; "Ringing volume"
				Setting ID		= .1.6.2.0.10
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 6 (0x0006)

				; "Vibrating alert"
				Setting ID		= .1.6.2.0.11
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Message alert"
				Setting ID		= .1.6.2.0.12
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Keypad tones"
				Setting ID		= .1.6.2.0.13
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 4 (0x0004)

				; "Warning tones"
				Setting ID		= .1.6.2.0.14
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver switch"
				Setting ID		= .1.6.2.1.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver timeout"
				Setting ID		= .1.6.2.1.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver graphics"
				Setting ID		= .1.6.2.1.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Backlight alert"
				Setting ID		= .1.6.2.1.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, notification"
				Setting ID		= .1.6.2.1.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, coverage"
				Setting ID		= .1.6.2.1.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, alert"
				Setting ID		= .1.6.2.1.7
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Theme selection"
				Setting ID		= .1.6.2.1.8
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Profile ringing tone"
				Setting ID		= .1.6.2.1.9
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 130 (0x0082)

				; "Ringing volume"
				Setting ID		= .1.6.2.1.10
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 3 (0x0003)

				; "Vibrating alert"
				Setting ID		= .1.6.2.1.11
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Message alert"
				Setting ID		= .1.6.2.1.12
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Keypad tones"
				Setting ID		= .1.6.2.1.13
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 255 (0x00ff)

				; "Warning tones"
				Setting ID		= .1.6.2.1.14
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 255 (0x00ff)

				; "Screen saver switch"
				Setting ID		= .1.6.2.2.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver timeout"
				Setting ID		= .1.6.2.2.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver graphics"
				Setting ID		= .1.6.2.2.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Backlight alert"
				Setting ID		= .1.6.2.2.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, notification"
				Setting ID		= .1.6.2.2.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, coverage"
				Setting ID		= .1.6.2.2.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, alert"
				Setting ID		= .1.6.2.2.7
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Theme selection"
				Setting ID		= .1.6.2.2.8
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Profile ringing tone"
				Setting ID		= .1.6.2.2.9
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 17 (0x0011)

				; "Ringing volume"
				Setting ID		= .1.6.2.2.10
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Vibrating alert"
				Setting ID		= .1.6.2.2.11
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Message alert"
				Setting ID		= .1.6.2.2.12
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 3 (0x0003)

				; "Keypad tones"
				Setting ID		= .1.6.2.2.13
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Warning tones"
				Setting ID		= .1.6.2.2.14
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 255 (0x00ff)

				; "Screen saver switch"
				Setting ID		= .1.6.2.3.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver timeout"
				Setting ID		= .1.6.2.3.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver graphics"
				Setting ID		= .1.6.2.3.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Backlight alert"
				Setting ID		= .1.6.2.3.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, notification"
				Setting ID		= .1.6.2.3.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Lights, coverage"
				Setting ID		= .1.6.2.3.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, alert"
				Setting ID		= .1.6.2.3.7
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Theme selection"
				Setting ID		= .1.6.2.3.8
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Profile ringing tone"
				Setting ID		= .1.6.2.3.9
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 130 (0x0082)

				; "Ringing volume"
				Setting ID		= .1.6.2.3.10
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 9 (0x0009)

				; "Vibrating alert"
				Setting ID		= .1.6.2.3.11
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Message alert"
				Setting ID		= .1.6.2.3.12
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 2 (0x0002)

				; "Keypad tones"
				Setting ID		= .1.6.2.3.13
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 9 (0x0009)

				; "Warning tones"
				Setting ID		= .1.6.2.3.14
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver switch"
				Setting ID		= .1.6.2.4.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver timeout"
				Setting ID		= .1.6.2.4.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver graphics"
				Setting ID		= .1.6.2.4.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Backlight alert"
				Setting ID		= .1.6.2.4.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Lights, notification"
				Setting ID		= .1.6.2.4.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Lights, coverage"
				Setting ID		= .1.6.2.4.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Lights, alert"
				Setting ID		= .1.6.2.4.7
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Theme selection"
				Setting ID		= .1.6.2.4.8
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Profile ringing tone"
				Setting ID		= .1.6.2.4.9
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 130 (0x0082)

				; "Ringing volume"
				Setting ID		= .1.6.2.4.10
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 3 (0x0003)

				; "Vibrating alert"
				Setting ID		= .1.6.2.4.11
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Message alert"
				Setting ID		= .1.6.2.4.12
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Keypad tones"
				Setting ID		= .1.6.2.4.13
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 255 (0x00ff)

				; "Warning tones"
				Setting ID		= .1.6.2.4.14
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 255 (0x00ff)

				; "Screen saver switch"
				Setting ID		= .1.6.2.5.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver timeout"
				Setting ID		= .1.6.2.5.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Screen saver graphics"
				Setting ID		= .1.6.2.5.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Backlight alert"
				Setting ID		= .1.6.2.5.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, notification"
				Setting ID		= .1.6.2.5.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, coverage"
				Setting ID		= .1.6.2.5.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Lights, alert"
				Setting ID		= .1.6.2.5.7
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Theme selection"
				Setting ID		= .1.6.2.5.8
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Profile ringing tone"
				Setting ID		= .1.6.2.5.9
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 130 (0x0082)

				; "Ringing volume"
				Setting ID		= .1.6.2.5.10
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 4 (0x0004)

				; "Vibrating alert"
				Setting ID		= .1.6.2.5.11
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Message alert"
				Setting ID		= .1.6.2.5.12
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Keypad tones"
				Setting ID		= .1.6.2.5.13
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 4 (0x0004)

				; "Warning tones"
				Setting ID		= .1.6.2.5.14
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

		; "Clock display"
		Setting ID		= .1.7.2
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Time format"
		Setting ID		= .1.7.3
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Auto update of date and time"
		Setting ID		= .1.7.4
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 2 (0x0002)

		; "Alarm state"
		Setting ID		= .1.7.5
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Alarm time"
		Setting ID		= .1.7.6
		Setting type	= ASCII
		Setting length	= 6
		Setting value	= "09:00"

		; "Alarm repeat"
		Setting ID		= .1.7.7
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Alarm tone type state"
		Setting ID		= .1.7.8
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Alarm tone type personal state"
		Setting ID		= .1.7.9
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 130 (0x0082)

		; "Calendar note tone type"
		Setting ID		= .1.7.10
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Calendar note tone"
		Setting ID		= .1.7.11
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 130 (0x0082)

		; "PLMN selection mode"
		Setting ID		= .1.8.1
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Voice mailbox number - PRI 433"
		Setting ID		= .1.8.2
		Setting type	= ASCII
		Setting length	= 1
		Setting value	= ""

		; "Send caller identity switch (CLIR switch)"
		Setting ID		= .1.8.4
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Automatic redial switch"
		Setting ID		= .1.8.8
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Voice Mail Box Options - PRI 260"
		Setting ID		= .1.8.21
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Display MDN/Emergency Number During Emergency Call - PRI 682"
		Setting ID		= .1.8.22
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Display Talkzone/Mobile Text During Call - PRI 243"
		Setting ID		= .1.8.23
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Allow Service Numbers to be Dialed while Phone Lock Active - PRI 507"
		Setting ID		= .1.8.24
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

		; "Menu language switch - PRI 231"
		Setting ID		= .1.9.1
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 16 (0x0010)

		; "Startup tone state"
		Setting ID		= .1.9.2
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 1 (0x0001)

		; "Light"
		Setting ID		= .1.14.1
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 1 (0x0001)

		; "Sound"
		Setting ID		= .1.14.2
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 1 (0x0001)

		; "Vibra"
		Setting ID		= .1.14.3
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 1 (0x0001)

		; "Exchange rate (used in the calculator)"
		Setting ID		= .1.17.1
		Setting type	= ASCII
		Setting length	= 2
		Setting value	= "1"

		; "Security level"
		Setting ID		= .1.20.1
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 17 (0x0011)

		; "Phone SW version etc."
		Setting ID		= .2.1.1
		Setting type	= ASCII
		Setting length	= 41
		Setting value	= "V JP190V0700.nep,13-01-06,RM-97,(c) NMP,"

		; "PRI Version String - PRI 247"
		Setting ID		= .2.1.20
		Setting type	= Binary
		Setting length	= 15
		Setting value	= 30,35,77,31,30,00,31,32,33,34,00,00,00,03,00

		; "PRI File Name - PRI 487"
		Setting ID		= .2.1.21
		Setting type	= Binary
		Setting length	= 11
		Setting value	= 35,33,32,34,37,35,72,30,30,31,00

			; "SPC Query For Flashing - PRI 359"
			Setting ID		= .2.2.1.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "SPC Query For PRL Downloading - PRI 360"
			Setting ID		= .2.2.1.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "SPC Query For Read Settings - PRI 361"
			Setting ID		= .2.2.1.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "SPC Query For Write Settings - PRI 362"
			Setting ID		= .2.2.1.4
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "SPC Query For Transfer User Data - PRI 363"
			Setting ID		= .2.2.1.5
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "SPC Query For Read Phonebook - PRI 364"
			Setting ID		= .2.2.1.6
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "SPC Query For Write Phonebook - PRI 365"
			Setting ID		= .2.2.1.7
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "SPC Query For Perform Diagnostics - PRI 366"
			Setting ID		= .2.2.1.8
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "SPC Query For Refurbishment - PRI 367"
			Setting ID		= .2.2.1.9
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

		; "Phone Lock Code - PRI 183"
		Setting ID		= .2.2.20
		Setting type	= Binary
		Setting length	= 5
		Setting value	= 31,32,33,34,00

		; "Security & Lock Codes Configuration Options - PRI 505"
		Setting ID		= .2.2.21
		Setting type	= Integer16
		Setting length	= 2
		Setting value	= 0 (0x0000)

			; "Handportable CDMA Earpiece Equalizer Coefficients - PRI 736"
			Setting ID		= .2.3.1.1
			Setting type	= Binary
			Setting length	= 63
			Setting value	= 00,03,00,11,ff,ff,00,00,e2,10,4e,da,ff,ff,00,00,bc,91,42,7b,00,00,00,00,9f,ac,39,4d,ff,fe,00,01,ca,b8,6c,fa,00,07,40,4f,8f,51,55,0f,25,78,c9,32,60,25,4a,75,d5,f1,65,bb,23,d1,ba,ac,27,9c,00

			; "Handportable CDMA Microphone Equalizer Coefficients - PRI 737"
			Setting ID		= .2.3.1.2
			Setting type	= Binary
			Setting length	= 35
			Setting value	= 00,01,00,09,ff,fe,00,00,d7,ff,7d,72,00,00,00,00,ce,5e,8b,fd,00,03,13,36,a0,3f,5c,c7,23,ad,3c,6d,61,f8,00

			; "Universal Headset CDMA Earpiece Equalizer Coefficients - PRI 740"
			Setting ID		= .2.3.1.3
			Setting type	= Binary
			Setting length	= 63
			Setting value	= 00,03,00,11,ff,ff,00,00,1e,2b,03,a3,ff,ff,00,00,54,40,03,53,00,02,00,00,ff,a2,01,27,ff,fd,00,01,d7,26,4b,9d,00,04,e6,0a,eb,86,50,1e,a9,3a,f2,43,77,d8,00,a9,f7,8e,60,cf,37,ef,97,55,59,05,00

			; "Universal Headset CDMA Microphone Equalizer Coefficients - PRI 741"
			Setting ID		= .2.3.1.4
			Setting type	= Binary
			Setting length	= 35
			Setting value	= 00,01,00,09,ff,fe,00,00,f9,3d,53,9b,ff,ff,00,01,e1,99,ad,a6,00,04,08,3f,b8,b9,47,9b,21,0c,5d,c2,41,70,00

			; "Mobile Directory Number (MDN) - PRI 152, 171"
			Setting ID		= .3.1.1.1
			Setting type	= Binary
			Setting length	= 16
			Setting value	= 30,30,30,30,30,30,30,30,30,30,30,30,30,30,30,00

			; "Mobile Identification Number (MIN) - PRI 156, 175"
			Setting ID		= .3.1.1.2
			Setting type	= Binary
			Setting length	= 11
			Setting value	= 30,30,30,30,30,30,38,34,36,38,00

			; "A-key code - PRI 439, 489"
			Setting ID		= .3.1.1.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Alpha Tag - PRI 918, 919"
			Setting ID		= .3.1.1.4
			Setting type	= Unicode
			Setting length	= 28
			Setting value	= "Yemen Telecom"

			; "Emergency Numbers - PRI 157, 176"
			Setting ID		= .3.1.1.5
			Setting type	= ASCII
			Setting length	= 18
			Setting value	= "911,*911,,,,,,,,"

			; "Service Numbers - PRI 158, 177"
			Setting ID		= .3.1.1.6
			Setting type	= ASCII
			Setting length	= 6
			Setting value	= ",,,,"

				; "Primary CDMA Channel A Band - PRI 159, 178"
				Setting ID		= .3.1.1.7.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 201 (0x00c9)

				; "Secondary CDMA Channel A Band - PRI 161, 180"
				Setting ID		= .3.1.1.7.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 283 (0x011b)

				; "Primary CDMA Channel B Band - PRI 160, 179"
				Setting ID		= .3.1.1.7.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 201 (0x00c9)

				; "Secondary CDMA Channel B Band - PRI 162, 181"
				Setting ID		= .3.1.1.7.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 777 (0x0309)

				; "Home SID - PRI 154, 173"
				Setting ID		= .3.1.1.8.1
				Setting type	= Binary
				Setting length	= 40
				Setting value	= 2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47,2c,47

				; "Home NID - PRI 153, 172"
				Setting ID		= .3.1.1.8.2
				Setting type	= Binary
				Setting length	= 40
				Setting value	= 00,01,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00

				; "Preferred SIDs - PRI 67, 69"
				Setting ID		= .3.1.1.8.3
				Setting type	= Binary
				Setting length	= 160
				Setting value	= 00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00

				; "Preferred NIDs - PRI 502, 504"
				Setting ID		= .3.1.1.8.4
				Setting type	= Binary
				Setting length	= 160
				Setting value	= ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff

				; "Forbidden SIDs - PRI 66, 68"
				Setting ID		= .3.1.1.8.5
				Setting type	= Binary
				Setting length	= 20
				Setting value	= 00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00

				; "Forbidden NIDs - PRI 501, 503"
				Setting ID		= .3.1.1.8.6
				Setting type	= Binary
				Setting length	= 20
				Setting value	= ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff,ff

				; "Country Code - PRI 151, 170"
				Setting ID		= .3.1.1.8.7
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 421 (0x01a5)

				; "Network Code - PRI 155, 174"
				Setting ID		= .3.1.1.8.8
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 3 (0x0003)

				; "Access Overload Class (ACCOLC) - PRI 146, 165"
				Setting ID		= .3.1.1.9.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 8 (0x0008)

				; "NAM x Slot Cycle Index - PRI 680, 677"
				Setting ID		= .3.1.1.9.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 2 (0x0002)

				; "NAM x Status - PRI 672, 673"
				Setting ID		= .3.1.1.9.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

			; "ACCOLC Updated by MIN Change - PRI 486"
			Setting ID		= .3.1.9.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Set MDN/MIN Equal Feature - PRI 488"
			Setting ID		= .3.1.9.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "NAM Programming Access Options - PRI 631"
			Setting ID		= .3.1.10.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "ACCOLC Menu - PRI 633"
			Setting ID		= .3.1.10.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Alpha Tag Menu - PRI 102"
			Setting ID		= .3.1.10.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Alpha Tag Protection by SPC - PRI 357"
			Setting ID		= .3.1.11.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "CDMA SID/NID Lists Menu Option in Long NAM Programming - PRI 640"
			Setting ID		= .3.1.11.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "IS-683 Support Options - PRI 1209"
			Setting ID		= .3.2.1.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Maximum SPC Failure Attempts - PRI 141"
			Setting ID		= .3.2.1.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 5 (0x0005)

			; "SPC Failure Handling Feature - PRI 261"
			Setting ID		= .3.2.1.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "NAM 1 SPASM Security For OTAPA - PRI 133"
			Setting ID		= .3.2.2.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "NAM 2 SPASM Security For OTAPA - PRI 143"
			Setting ID		= .3.2.2.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Automatic update of service (OTAPA) Menu - PRI 77"
			Setting ID		= .3.2.3.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Automatic update of service (OTAPA) Menu Status - PRI 922"
			Setting ID		= .3.2.3.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Allow OTASP Call In Cell Mode - PRI 75"
			Setting ID		= .3.2.4.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Mobile Station Firmware Revision Number - PRI 128"
			Setting ID		= .3.2.4.4
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 6 (0x0006)

			; "Mobile Station Manufacturer's Model Number - PRI 129"
			Setting ID		= .3.2.4.5
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 75 (0x004b)

			; "OTASP Feature Code Options - PRI 98"
			Setting ID		= .3.2.4.6
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "OTASP Status Messages Feature - PRI 99"
			Setting ID		= .3.2.4.7
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "SPC - PRI 214"
			Setting ID		= .3.2.5.1
			Setting type	= ASCII
			Setting length	= 7
			Setting value	= "000000"

			; "XTKSL - PRI 215"
			Setting ID		= .3.2.5.2
			Setting type	= ASCII
			Setting length	= 7
			Setting value	= "000000"

			; "X Value - PRI 142"
			Setting ID		= .3.2.5.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

					; "Automatic Menu Option - PRI 650"
					Setting ID		= .3.3.1.1.1.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 1 (0x0001)

					; "Home only Menu Option - PRI 657"
					Setting ID		= .3.3.1.1.1.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 1 (0x0001)

					; "Network Menu Default Setting - PRI 748"
					Setting ID		= .3.3.1.1.1.6
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

			; "Confirmation Tone for Acquisition of Roaming System - PRI 78"
			Setting ID		= .3.3.2.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Standard/Non-Standard Enhanced Roaming Indicator Options - PRI 368"
			Setting ID		= .3.3.2.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Short Distance Coverage Area (SDCA) Feature - PRI 935"
			Setting ID		= .3.3.2.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

					; "Acquire More/Most Preferred System in Another GEO during BSR - PRI 606"
					Setting ID		= .3.3.3.1.1.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 2 (0x0002)

					; "Maximum Number of Better Service Rescans While on Current System - PRI 626"
					Setting ID		= .3.3.3.1.1.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Allow Acquisition of Wildcard Systems during BSR - PRI 618"
					Setting ID		= .3.3.3.1.1.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "GEO Hopping during BSR - Non-Home System to Home System - PRI 617"
					Setting ID		= .3.3.3.1.1.4
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Allow Channel Repetition During Microscan - PRI 624"
					Setting ID		= .3.3.3.1.2.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Maximum Number of Channels per Better Service Rescan - PRI 396"
					Setting ID		= .3.3.3.1.2.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Maximum Number of Channels per Better Service Rescan Options - PRI 627"
					Setting ID		= .3.3.3.1.2.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

					; "Better Service Rescan Low Timer for CDMA Systems - PRI 758"
					Setting ID		= .3.3.3.1.3.1
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 180 (0x00b4)

					; "Better Service Rescan High Timer for CDMA Systems - PRI 759"
					Setting ID		= .3.3.3.1.3.2
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 900 (0x0384)

					; "Better Service Rescan High Timer in Seconds After Call Release - PRI 610"
					Setting ID		= .3.3.3.1.3.3
					Setting type	= Integer16
					Setting length	= 2
					Setting value	= 0 (0x0000)

				; "Delay Between Attempts while in Silent Retry Mode Timer - PRI 132"
				Setting ID		= .3.3.3.2.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 4 (0x0004)

				; "Silent Retry Configuration - PRI 431"
				Setting ID		= .3.3.3.2.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 3 (0x0003)

				; "Addition of PCS/CDMA Channels to RCL Options - PRI 405"
				Setting ID		= .3.3.3.3.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Cross Pollination  - PRI 752"
				Setting ID		= .3.3.3.3.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "GEO Confinement through Negative System Detection - PRI 418"
				Setting ID		= .3.3.3.3.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "GEO Scan List Options when System Loss Occurs - PRI 603"
				Setting ID		= .3.3.3.3.4
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "GSRM/Redirection Message (Ping-Pong) Feature - PRI 756"
				Setting ID		= .3.3.3.3.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Scan Second RCL Channel After Call Release - PRI 607"
				Setting ID		= .3.3.3.3.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Scan Second RCL Channel First during BSR - PRI 394"
				Setting ID		= .3.3.3.3.7
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Threshold Level for Acquisition of CDMA Systems after Scanning Entire PRL & NAM - PRI 417"
				Setting ID		= .3.3.3.3.8
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 2 (0x0002)

				; "Use CDMA Home SID/NID List for System Acquisition & Override Roaming Indicator Feature - PRI 757"
				Setting ID		= .3.3.3.3.9
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Add Primary Cellular Channel to All Scan Lists - PRI 601"
				Setting ID		= .3.3.3.3.10
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Ignore Comparison of Expected/Acquired NID When Wildcard SID - PRI 629"
				Setting ID		= .3.3.3.3.11
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Primary CDMA Channel Preferred over Secondary Channel - ER Mode - PRI 397"
				Setting ID		= .3.3.3.3.12
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Addition of Channels to RCL - PRI 404"
				Setting ID		= .3.3.3.3.13
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

			; "Out of Range Low Timer for SSPR Mode Iteration Counter - PRI 389"
			Setting ID		= .3.3.4.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "CDMA Call Release/System Lost Reacquisition Period - PRI 375"
			Setting ID		= .3.3.5.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 3 (0x0003)

			; "Out of Range Low Timer in Seconds for SSPR Mode - PRI 377"
			Setting ID		= .3.3.5.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 300 (0x012c)

			; "Out of Range High Timer in Seconds for SSPR Mode - PRI 379"
			Setting ID		= .3.3.5.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 900 (0x0384)

			; "Addition of Channels for Non-Preferred Systems to RCL - PRI 608"
			Setting ID		= .3.3.6.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Acquire Non-Preferred Systems Immediately - PRI 411"
			Setting ID		= .3.3.6.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Better Service Rescan High Timer in Secs for Non-Pref Systems - PRI 614"
			Setting ID		= .3.3.6.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Better Service Rescan Scan List for Non-Preferred Systems - PRI 615"
			Setting ID		= .3.3.6.4
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "CDMA Call Release/Digital System Lost Re-acq Period - PRI 613"
			Setting ID		= .3.3.6.5
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "CDMA Digital System Lost Re-acq Options for Non-Pref Systems - PRI 619"
			Setting ID		= .3.3.6.6
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "GEO-confinement due to Negative System Detection Counter - PRI 390"
			Setting ID		= .3.3.6.7
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "GEO Hopping during BSR - SID/NID Match Priority Preferred Over GEO Priority - PRI 753"
			Setting ID		= .3.3.6.8
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Ignore Out of Range State if Mobile is Charging - PRI 621"
			Setting ID		= .3.3.6.9
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Maximum Time for Power-up Scan Timer - PRI 382"
			Setting ID		= .3.3.6.10
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1200 (0x04b0)

			; "Multiple Non-Preferred Systems Preference Options - PRI 605"
			Setting ID		= .3.3.6.11
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Multiple Non-Preferred Systems (Same Band/Type) Acq Options - PRI 604"
			Setting ID		= .3.3.6.12
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Negative System Acquisition Options - PRI 602"
			Setting ID		= .3.3.6.13
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Inclusion of SSPR Menu via *#PRLSET# - PRI 258"
			Setting ID		= .3.3.6.20
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Enhanced Roaming Mode - PRI 398"
			Setting ID		= .3.3.7.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Non-Preferred System Acceptance while in ER Mode - PRI 422"
			Setting ID		= .3.3.7.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

				; "Voice Privacy Menu - PRI 185"
				Setting ID		= .3.4.1.1.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Manual Touch Tones - PRI 126"
				Setting ID		= .3.4.1.2.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 2 (0x0002)

				; "Touch Tone Length - PRI 134"
				Setting ID		= .3.4.1.2.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

			; "Call Timer Options - PRI 642"
			Setting ID		= .3.4.1.11
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

				; "EVRC On/HomeOnly/Off for Call Origination - PRI 402"
				Setting ID		= .3.4.2.1.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Inclusion of EVRC Menu for Call Origination via *#EVRC# - PRI 92"
				Setting ID		= .3.4.2.1.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Call Rejection Feature - PRI 878"
				Setting ID		= .3.4.2.2.1
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 1 (0x0001)

				; "Send Empty Flash Prior to Making Three-way Call Attempt - PRI 711"
				Setting ID		= .3.4.2.2.2
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Send Digits in Buffer when Answering Call Waiting/Three-way Call - PRI 932"
				Setting ID		= .3.4.2.2.3
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Display of In-Service Indicators during Initial BSR - PRI 609"
				Setting ID		= .3.4.2.2.5
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

				; "Display of In-Service Indicators for Non-Pref System Detection - PRI 616"
				Setting ID		= .3.4.2.2.6
				Setting type	= Integer16
				Setting length	= 2
				Setting value	= 0 (0x0000)

			; "DNS Retry Attempts Counter - PRI 936"
			Setting ID		= .3.5.5.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 3 (0x0003)

			; "DNS Retry Attempt Interval - PRI 937"
			Setting ID		= .3.5.5.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 5000 (0x1388)

			; "Report Pilot Phase Referenced to Lead Finger - PRI 1317"
			Setting ID		= .3.6.1.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Non-standard Datang R-UIM Feature - PRI 1059"
			Setting ID		= .3.6.2.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Access Handoff Feature Support - PRI 493"
			Setting ID		= .3.100.1.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Access Probe Handoff Feature Support - PRI 492"
			Setting ID		= .3.100.1.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Mobile Assisted Hard Handoff Feature Support - PRI 496"
			Setting ID		= .3.100.1.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "NDSS Feature Support - PRI 491"
			Setting ID		= .3.100.1.4
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Nokia Proprietary Access Handoff - PRI 110"
			Setting ID		= .3.100.1.5
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Nokia Proprietary PSMM Message Handling - PRI 109"
			Setting ID		= .3.100.1.6
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Pilot Ec/Io Threshold for Pseudo Pilot Acquisition Feature - PRI 881"
			Setting ID		= .3.100.1.7
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 17 (0x0011)

			; "Pilot Power Threshold for Pseudo Pilot Acquisition Feature - PRI 882"
			Setting ID		= .3.100.1.8
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 85 (0x0055)

			; "Quick Paging Channel (IS-2000) Feature Support - PRI 495"
			Setting ID		= .3.100.1.9
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "R_FCH 1/8 Rate Gating Feature Support - PRI 76"
			Setting ID		= .3.100.1.10
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Signaling Message Encryption Feature Support - PRI 494"
			Setting ID		= .3.100.1.11
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Slotted Timer Feature Support - PRI 497"
			Setting ID		= .3.100.1.12
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "SR_ID Patch - PRI 446"
			Setting ID		= .3.100.1.13
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Status Response Patch - PRI 447"
			Setting ID		= .3.100.1.14
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "TMSI Feature Support - PRI 490"
			Setting ID		= .3.100.1.15
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 0 (0x0000)

			; "Service Option 2 - PRI 573"
			Setting ID		= .3.100.2.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 3 - PRI 574"
			Setting ID		= .3.100.2.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 4 - PRI 575"
			Setting ID		= .3.100.2.4
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 5 - PRI 576"
			Setting ID		= .3.100.2.5
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 6 - PRI 577"
			Setting ID		= .3.100.2.6
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 7 - PRI 578"
			Setting ID		= .3.100.2.7
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 9 - PRI 579"
			Setting ID		= .3.100.2.9
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 12 - PRI 580"
			Setting ID		= .3.100.2.12
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 13 - PRI 581"
			Setting ID		= .3.100.2.13
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 14 - PRI 582"
			Setting ID		= .3.100.2.14
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 15 - PRI 583"
			Setting ID		= .3.100.2.15
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 17 - PRI 584"
			Setting ID		= .3.100.2.17
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 18 - PRI 585"
			Setting ID		= .3.100.2.18
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 19 - PRI 586"
			Setting ID		= .3.100.2.19
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 32 - PRI 587"
			Setting ID		= .3.100.2.32
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 33 - PRI 588"
			Setting ID		= .3.100.2.33
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 35 - PRI 589"
			Setting ID		= .3.100.2.35
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 36 - PRI 590"
			Setting ID		= .3.100.2.36
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 54 - PRI 591"
			Setting ID		= .3.100.2.54
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 55 - PRI 592"
			Setting ID		= .3.100.2.55
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 4100 - PRI 593"
			Setting ID		= .3.100.2.100
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 4101 - PRI 594"
			Setting ID		= .3.100.2.101
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 4103 - PRI 595"
			Setting ID		= .3.100.2.103
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 32768 - PRI 596"
			Setting ID		= .3.100.2.200
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 32798 - PRI 597"
			Setting ID		= .3.100.2.201
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Service Option 32799 - PRI 598"
			Setting ID		= .3.100.2.202
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Silent Retry Iteration Counter - PRI 432"
			Setting ID		= .3.100.3.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 3 (0x0003)

			; "Remain in Emergency Mode Timer - PRI 131"
			Setting ID		= .3.100.3.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 300 (0x012c)

			; "Better Service Rescan Low Timer Iteration Counter - PRI 385"
			Setting ID		= .3.100.3.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 4 (0x0004)

			; "Initial Better Service Rescan - PRI 392"
			Setting ID		= .3.100.3.4
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Threshold Level for CDMA System Acq Candidates in SSPR Mode - PRI 412"
			Setting ID		= .3.100.3.5
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 4 (0x0004)

			; "Maximum Time for Call Origination Attempt Timer - PRI 130"
			Setting ID		= .3.100.3.6
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 30 (0x001e)

			; "RSSI Update on User Interface Timer - PRI 383"
			Setting ID		= .3.100.3.7
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 6 (0x0006)

			; "Mobile Originated Short Message Service Support - PRI 200"
			Setting ID		= .3.100.5.1
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Mobile Terminated Short Message Support - PRI 201"
			Setting ID		= .3.100.5.2
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Mobile Originated Wireless Messaging Teleservice Support - PRI 202"
			Setting ID		= .3.100.5.3
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Mobile Terminated Wireless Messaging Teleservice Support - PRI 205"
			Setting ID		= .3.100.5.4
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

			; "Mobile Terminated Wireless Paging Teleservice Support - PRI 206"
			Setting ID		= .3.100.5.5
			Setting type	= Integer16
			Setting length	= 2
			Setting value	= 1 (0x0001)

