PRODUCT_PROFILE_PHONE_SETTINGS_V.1.0

PHONE
  TYPE 
    Model = "NPE-4"

  SETS
    Count = 1
  
  FEATURES
    0   "Codec order" COMBOBOX
        0b10100111 "EFR 1st, FR 2nd, HR last"
        0b10011011 "EFR 1st, HR 2nd, FR last"
        0b10100011 "EFR 1st, FR 2nd"
        0b10001011 "EFR 1st, HR 2nd"
        0b10000011 "EFR only"

        0b10110110 "FR 1st, EFR 2nd, HR last"
        0b10111001 "FR 1st, HR 2nd, EFR last"
        0b10110010 "FR 1st, EFR 2nd"
        0b10111000 "FR 1st, HR 2nd"
        0b10110000 "FR only"

        0b10011110 "HR 1st, EFR 2nd, FR last"
        0b10101101 "HR 1st, FR 2nd, EFR last"
        0b10001110 "HR 1st, EFR 2nd"
        0b10101100 "HR 1st, FR 2nd"
        0b10001100 "HR only"

        0b10000000 "No codecs supported"
/*      0b00100111 "14k4 Data off, EFR, FR, HR" */
;
/*  0   "Codec order" EDITFIELD 0 255; */
    1   "Alternate line service (ALS)" CHECKBOX ;
    2   "HSCSD multislot class" EDITFIELD 0 18;
    3   "Ciphering algorithm A52" CHECKBOX;
    4   "Automatic redial" COMBOBOX 0 "Normal" 1 "Continuous";
    5   "Redial tone" COMBOBOX 0 "Normal" 1 "Loud";
    6   "CSP support" CHECKBOX;
    7   "Games WAP download" CHECKBOX;
    8   "Games WAP score send" CHECKBOX;
    9   "Games WAP URL check" CHECKBOX;
    10  "Bluetooth support" CHECKBOX;
    11  "High priority PLMN scan" CHECKBOX;
    12  "Trad Chinese input method" COMBOBOX 0 "BoPoMoFo" 1 "Stroke";
    13  "PCCCH support" CHECKBOX;
    14  "GPRS auto attach" CHECKBOX;
    15  "GEA1 support" CHECKBOX;
    16  "Reserved" CHECKBOX;
    17  "Reserved" CHECKBOX;
    18  "GPRS always online" COMBOBOX 0 "Context" 1 "Attach";
