From kraze1984:

dumped from a factory reset device.
the NAND flash (made by Micron) has a large number of bitflips. So the device will correct the errors based on the ECC data, but without these corrections the actual dump is faulty.
You cannot currently write this dump back with RIFF, all compatible loaders give errors.