Product: cxc 132 8062 R2C
Packager: QPETPAU

This is the meflash flash USB kernel driver to be used for communicating
with Ericsson AB Mobile Platforms Mobile Equipment (ME:s).

Folders:

  x86\InstallDisk\ - this folder contains necessery files to install ME drivers,
	for processors: i386, i486, i586 (Pentium), i686 (Pentium II) etc.
  x64\InstallDisk\ - this folder contains necessery files to install ME drivers,
	for processors with 64bits instructions.

Files in both x86 and x64:

InstallDisk\InstallationGuide.txt  - Describes how to install the driver.
InstallDisk\Data\meflash.sys  - Windows kernel driver
InstallDisk\Data\meflash.inf  - Kernel driver information file for registration

The kernel driver can be installed by right-clicking the .inf file and choose
"install".

For developing applications using this driver you also need to obtain
product CYA 901 624 R1E which contains the API files (DLL) and headers.
