L	Loading device drivers
S	Starting comms server
C	Connecting to comms server
L	Loading IRCOM.CSY module
R	Comms server reports we have '5' comms modules loaded
A	emux_k1		has 	Multiplexed serial port 		available as	'AMUX::1' to 'AMUX::60'
A	ecacm		has 	USB Serial Port Emulation via ACM	available as	'ACM::0' to 'ACM::0'
A	'ecuart'	has 	'Built in Serial ports'			available as	'COMM::0 to COMM::3
A	'ircomm'	has	'IrCOMM 3 wire raw'			available as	'IrCOMM::0' to 'IrCOMM::0'
A	'btcomm'	has	'BT RFComm Serial Emulation'		available as	BTCOMM::0' to 'BTCOMM::63'
U	Using the lowest 'IRCOMM 3 wire raw' out of 'IrCOMM::0' to 'IrCOMM::0'
O	Opened		IrCOMM::0
C	Configuring Serial port for 19200 bps 8 bits no parity 1 stop
P	Powering up port
