;/*****************************************************************************
;*  Copyright Statement:
;*  --------------------
;*  This software is protected by Copyright and the information contained
;*  herein is confidential. The software may not be copied and the information
;*  contained herein may not be used or disclosed except with the written
;*  permission of MediaTek Inc. (C) 2007
;*
;*  BY OPENING THIS FILE, BUYER HEREBY UNEQUIVOCALLY ACKNOWLEDGES AND AGREES
;*  THAT THE SOFTWARE/FIRMWARE AND ITS DOCUMENTATIONS ("MEDIATEK SOFTWARE")
;*  RECEIVED FROM MEDIATEK AND/OR ITS REPRESENTATIVES ARE PROVIDED TO BUYER ON
;*  AN "AS-IS" BASIS ONLY. MEDIATEK EXPRESSLY DISCLAIMS ANY AND ALL WARRANTIES,
;*  EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE IMPLIED WARRANTIES OF
;*  MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE OR NONINFRINGEMENT.
;*  NEITHER DOES MEDIATEK PROVIDE ANY WARRANTY WHATSOEVER WITH RESPECT TO THE
;*  SOFTWARE OF ANY THIRD PARTY WHICH MAY BE USED BY, INCORPORATED IN, OR
;*  SUPPLIED WITH THE MEDIATEK SOFTWARE, AND BUYER AGREES TO LOOK ONLY TO SUCH
;*  THIRD PARTY FOR ANY WARRANTY CLAIM RELATING THERETO. MEDIATEK SHALL ALSO
;*  NOT BE RESPONSIBLE FOR ANY MEDIATEK SOFTWARE RELEASES MADE TO BUYER'S
;*  SPECIFICATION OR TO CONFORM TO A PARTICULAR STANDARD OR OPEN FORUM.
;*
;*  BUYER'S SOLE AND EXCLUSIVE REMEDY AND MEDIATEK'S ENTIRE AND CUMULATIVE
;*  LIABILITY WITH RESPECT TO THE MEDIATEK SOFTWARE RELEASED HEREUNDER WILL BE,
;*  AT MEDIATEK'S OPTION, TO REVISE OR REPLACE THE MEDIATEK SOFTWARE AT ISSUE,
;*  OR REFUND ANY SOFTWARE LICENSE FEES OR SERVICE CHARGE PAID BY BUYER TO
;*  MEDIATEK FOR SUCH MEDIATEK SOFTWARE AT ISSUE.
;*
;*  THE TRANSACTION CONTEMPLATED HEREUNDER SHALL BE CONSTRUED IN ACCORDANCE
;*  WITH THE LAWS OF THE STATE OF CALIFORNIA, USA, EXCLUDING ITS CONFLICT OF
;*  LAWS PRINCIPLES.  ANY DISPUTES, CONTROVERSIES OR CLAIMS ARISING THEREOF AND
;*  RELATED THERETO SHALL BE SETTLED BY ARBITRATION IN SAN FRANCISCO, CA, UNDER
;*  THE RULES OF THE INTERNATIONAL CHAMBER OF COMMERCE (ICC).
;*
;*****************************************************************************/
;
;/*****************************************************************************
; *
; * Filename:
; * ---------
; *   scatZTENJ25_09A.txt
; *
; * Project:
; * --------
; *   Maui_Software
; *
; * Description:
; * ------------
; *   defines the memory map for the validation board
; *
; * Author:
; * -------
; *   system auto generator v2.33 -> p2.41 -> p2.49 -> p2.45
; *
; * Auto Generated Date:
; * -------
; *   2010/12/21
; *
; * Revision History:
; * -------
; * $Log: scatZTENJ25_09A.txt system auto generator v2.33 -> p2.41 -> p2.49 -> p2.45 $
; * 
; ****************************************************************************/
;
;=========================================================================
; This scatter file is auto-generated and please DO NOT change the content at will
;=========================================================================
;
;--------------------
; SCHEME   : external 16MB flash memory and 8MB SRAM
; PLATFORM : MT6225
; FEATURES : 
;--------------------

ROM 0x00000000 0x01000000
{
    ROM 0x00000000 0x00400000
    {
         bootarm.obj (C$$code,+First)
         *.obj (LEADING_PART,+First)
         
         
         
         Regioninit_ads.obj (+RO-CODE)
         *l1_classb_g2.lib (+RO-CODE)
         *l1_g2.lib (+RO-CODE)
         *l1_classb_umts.lib (+RO-CODE)
         *l4_classb.lib (+RO-CODE)
         *l4misc.lib (+RO-CODE)
         *lcmmi.lib (+RO-CODE)
         *mmi_framework.lib (+RO-CODE)
         *mmi_app.lib (+RO-CODE)
         *conn_app.lib (+RO-CODE)
         *inet_app.lib (+RO-CODE)
         
         cpp_initialise.o(+RO)
         cpp_finalise.o(+RO)
         * (C$$pi_ctorvec)
         * (C$$pi_dtorvec)
         * (C$$ddtorvec)
         
         divrt_real.o (+RO-CODE)
         *f_t_p.l (+RO-CODE)
         
; moved from ITCM
         tct.obj (+RO)
    }
    ROM2 +0x0 0x00400000
    {
; WAP family
         *wapadp.lib (+RO-CODE)
         *wap.lib (+RO-CODE)
         *wae.lib (+RO-CODE)
         *jataayu.lib (+RO-CODE)
         *jataayuapp.lib (+RO-CODE)
         *wapapp.lib (+RO-CODE)
         *obigo05aadp.lib (+RO-CODE)
         *obigo05alib.lib (+RO-CODE)
         *obigo03capp.lib (+RO-CODE)
         *obigo03cadp.lib (+RO-CODE)
         *obigo03clib.lib (+RO-CODE)
; J2ME family
         *j2me_11.lib (+RO-CODE)
         *j2me_hi.lib (+RO-CODE)
         *jal.lib (+RO-CODE)
         *ijet_adp.lib (+RO-CODE)
         *jblendia.lib (+RO-CODE)
         j2me_custom_*.obj (+RO-CODE)
    }
    ROM3 +0x0 0x00400000
    {
         .ANY (+RO-CODE)
    }
    ROM4 +0x0 0x00400000
    {
         .ANY (+RO-CODE)
    }
    ROM5 +0x0 
    {
         .ANY (+RO-DATA)
    }
    EXTSRAM_LARGEPOOL_NORMAL 0x08000000
    {
; For MT6225 projects, app-based ASM always at first due to Java FBBR
         app_mem.obj (LARGEPOOL_FIRST_ZI)
         ScrMemMgr.obj (LARGEPOOL_ZI)
         j2me_custom_resource.obj (LARGEPOOL_ZI)
         med_main.obj (LARGEPOOL_ZI)
    }
    EXTSRAM +0x00 
    {
         * (+RW, +ZI)
    }
    DUMMY_END 0x08800000 0x04
    {
         bootarm.obj (DUMMY_POOL)
    }
    EMIINIT_CODE 0xA0000000 OVERLAY
    {
    	   * (EMIINITCODE, EMIINITCONST, EMIINITZI)
    }
    INTSRAM_CODE 0xA0000000 OVERLAY 0x6870
    {
         * (INTSRAM_ROCODE)
; system-realted CODE , SMALL set
         bootarm.obj (INTERNCODE)
         data_buff_pool.obj (INTERNCODE)
         ctrl_buff_pool.obj (INTERNCODE)
         stack_buff_pool.obj (INTERNCODE)
         stack_ltlcom.obj (INTERNCODE)
         stack_timer.obj (INTERNCODE)
         SST_intrCtrl.obj (INTERNCODE, INTERNCONST)
         idle_task.obj (INTERNCODE)
         cache.obj (INTERNCODE)
; Nucleus-related CODE , SMALL set
         tct.obj (INTERNCODE)
         tcc.obj (INTERNCODE)
         csc.obj (INTERNCODE)
         tmt.obj (+RO)
         smc.obj (INTERNCODE)
         evc.obj (INTERNCODE)
         pmc.obj (INTERNCODE)
         quc.obj (INTERNCODE)
         kal_nucleus_buff_mgr.obj (INTERNCODE)
         kal_nucleus_evshed_buff_mgr.obj (INTERNCODE)
         kal_nucleus_itc.obj (INTERNCODE)
         kal_nucleus_timer.obj (INTERNCODE)
; THREADX-related CODE , SMALL set
         ; UNDER CONSTRUCTION
         tx_thread_interrupt_disable.obj (+RO)
         tx_thread_interrupt_restore.obj (+RO)
         tx_thread_context_save.obj (+RO)
         tx_thread_context_restore.obj (+RO)
         tx_thread_irq_nesting_start.obj (+RO)
         tx_thread_irq_nesting_end.obj (+RO)
         tx_thread_system_return.obj (+RO)
         tx_thread_schedule.obj (+RO)
         tx_thread_resume.obj (+RO)
         tx_thread_system_resume.obj (+RO)
         tx_timer_interrupt.obj (+RO)
         tx_timer_thread_entry.obj (+RO)
         tx_block_allocate.obj (+RO)
         tx_block_release.obj (+RO)
         tx_event_flags_get.obj (+RO)
         tx_event_flags_set.obj (+RO)
         tx_mutex_get.obj (+RO)
         tx_mutex_put.obj (+RO)
         kal_threadx_tasks.obj (INTERNCODE)
         kal_threadx_buff_mgr.obj (INTERNCODE)
         kal_threadx_itc.obj (INTERNCODE)
         kal_threadx_timer.obj (INTERNCODE)
; common used C library
         memset.o (+RO)
         rt_memclr.o (+RO)
         callvia.o (+RO)
         _sprintf.o (+RO)
         rt_memcpy.o (+RO)
         lludiv10.o (+RO)
         rt_udiv.o (+RO)
         uread4.o (+RO)
         uwrite4.o (+RO)
; INTSRAM_CODE_OBJ_others_6225
         cam_module.obj (INTERNCODE)
         uart.obj (INTERNCODE)
         gdi_image_direct_gif.obj (INTERNCODE)
         gdi_mutex.obj (INTERNCODE)
         gpt.obj (INTERNCODE)
         * (SNORCODE_INT)
         * (SNORCONST_INT)

; Please Do Not Remove
         m12160.obj (INTERNCODE)
         m12170.obj (INTERNCODE)
    }
    INTSRAM_DATA 0xA0006870 0x5A00
    {
         * (INTSRAM_RODATA, INTSRAM_RW, INTSRAM_ZI)
; system-realted data
         bootarm.obj (STACK_POOL_INTSRAM)
         stack_init.obj (INTERNCONST, INTERNRW, INTERNZI)
         ctrl_buff_pool.obj (INTERNCONST, INTERNRW, INTERNZI)
         stack_ltlcom.obj (INTERNCONST, INTERNRW, INTERNZI)
         idle_task.obj (INTERNCONST, INTERNRW, INTERNZI)
; Nucleus-related data ; Standard set
         tst*.obj (INTERNCONST, INTERNRW, INTERNZI)
         tct.obj (+RW, +ZI)
         tcd.obj (INTERNCONST, INTERNRW, INTERNZI)
         tmd.obj (+RW, +ZI)
         evd.obj (+RW, +ZI)
         pmd.obj (+RW, +ZI)
         qud.obj (+RW, +ZI)
         smd.obj (+RW, +ZI)
; THREADX-related data ; Standard set
         tx_thread_initialize.obj (+RW, +ZI)
         tx_timer_initialize.obj (+RW, +ZI)
; INTSRAM_DATA_OBJ_others_6225
         gdi_image.obj (INTERNCONST, INTERNRW, INTERNZI)
         gdi.obj (INTERNZI)
         interpret.obj (INTERNZI)
         sw_jpeg_decoder.obj (INTERNRW1, INTERNZI1)
         jpeg_encoder.obj (INTERNRW, INTERNZI)
         drv_gfx_stack_switch_manager.obj (INTERNRW2, INTERNZI2)

; Please Do Not Remove
         m12160.obj (INTERNCONST, INTERNRW, INTERNZI)
         m12170.obj (INTERNCONST, INTERNRW, INTERNZI)
    }   
    DYNAMIC_CODE18 0xa000c270 OVERLAY 0x0d90
    {
         * (MP4DEC_DYNAMIC_CODE, MP4DEC_DYNAMIC_RO)
    }
    DYNAMIC_CODE19 0xa000c270 OVERLAY 0x0d90
    {
         * (MP4ENC_DYNAMIC_CODE, MP4ENC_DYNAMIC_RO)
    }
    DYNAMIC_CODE1 0xa000d000 OVERLAY 0x5000
    {
         * (AMR515_DYNAMIC_CODE, AMR515_DYNAMIC_ZI)
    }
    DYNAMIC_CODE11 0xa000d000 OVERLAY 0x5000
    {
         * (VRENGINE_DYNAMIC_CODE, VRENGINE_DYNAMIC_ZI)
    }
    DYNAMIC_CODE12 0xa000d000 OVERLAY 0x5000
    {
         * (MP4DEC2_DYNAMIC_ZI, MP4DEC2_DYNAMIC_RO)
    }
    DYNAMIC_CODE13 0xa000d000 OVERLAY 0x5000
    {
         * (MP4ENC2_DYNAMIC_ZI, MP4ENC2_DYNAMIC_RO)
    }
    DYNAMIC_CODE14 0xa000d000 OVERLAY 0x5000
    {
         * (264DEC2_DYNAMIC_ZI, 264DEC2_DYNAMIC_RO)
    }
    DYNAMIC_CODE3 0xa000d000 OVERLAY 0x5000
    {
         * (CTM_DYNAMIC_CODE, CTM_DYNAMIC_ZI)
    }
    DYNAMIC_CODE4 0xa000d000 OVERLAY 0x5000
    {
         * (G729_DYNAMIC_CODE, G729_DYNAMIC_ZI)
    }
    DYNAMIC_CODE5 0xa000d000 OVERLAY 0x5000
    {
         * (SBC_DYNAMIC_CODE, SBC_DYNAMIC_ZI)
    }
    INTSRAM_MULTIMEDIA 0x40000000  0xC000
    {
         med_main.obj (INTERNRW1, INTERNZI1)
         isp_comm.obj (INTERNRW1, INTERNZI1)
    }
}
