Compatibility Info MIDI Implementation Chart |

Model: Beatnik Platform Date: April 2, 2000 Software Wavetable Synthesizer Version: BAE 1.5.2
Function | Transmitted | Recognized | Remarks
Basic Channel | Default | x | 1 - 16 |
Changed | x | 1 - 16
Mode | Default | x | Mode 3 | Can't change
Messages | x | x
Altered | *********** |
Note Number |  | x | 0-127 |
True Voice | *********** | 0-127
Velocity | Note on | x | O |
Note off | x | x
After Touch | Key | x | x |
Channels | x | x
Pitch Bend | Pitch Bend | x | *1, *2 | Resolution 12 bit
Change Control | 0 | x | *1, *2 | Bank Select (MSB Only)
1 | x | *1, *2 | Modulation
6 | x | *1, *2 | Data Entry
7 | x | *1, *2 | Volume
10 | x | *1, *2 | Panpot
11 | x | *1, *2 | Expression
64 | x | *1, *2 | Hold1 (Sustain)
85, 86, 87 | x | *1, *2 | Beatnik Loop & Mute (files only)
90 | x | *1, *2 | Master Reverb Type
91 | x | *1, *2 | Reverb depth (>15 = on for reverb types 1-7)
93 | x | *1, *2 | Chorus Send
98, 99 | x | *1, *2 | NRPN (LSB, MSB)
100, 101 | x | *1, *2 | RPN (LSB, MSB) - Reserved
121 | x | *1, *2 | Reset All Controllers
123 | x | O | All Notes Off
Program Change |  | x | *1 |
True Number | *********** | 0-127
System Exclusive | x | x |
System Common | Song Position | x | x |
Song Select | x | x
Tune Request | x | x
System Real Time | Clock | x | x |
Commands | x | x
Aux. Messages | Local On/Off | x | x |
All Notes Off | x | O (123)
Active Sensing | x | x
System Reset | x | x
Notes | *1 O x can be selectable O : Yes x : No *2 See For Musicians for details on Beatnik's response to Controllers.
Mode 1: OMNI ON, POLY Mode 2: OMNI ON, MONO Mode 3: OMNI OFF, POLY Mode 4: OMNI OFF, MONO

Compatibility Info / MIDI Implementation Chart top |