<?xml version="1.0" encoding="Windows-1251"?>
<patch version="0.4">

<info title="SMS auf TF-Karte" id="F8540D59" group="ModExperten Option" version="1">
 <description short="The patch alters the memory path of the incoming SMS on the TF map. One must absolutely provide a folder called 'SMS' on the TF map. If of the SMS memory is full, one can rename the file sms.dat in the SMS folder simply to sms1.dat. Memory becomes thereby free to the SMS again, but one can restore the SMS to sms1.dat any time while one renames the file again in sms.dat...." />
    <author nickname="Grenf" fullname="" status="xxx" email="xxx" www="xxx" icq="" />
</info>
 <patchdata firmware="D600EXEFA1" >
  <changes>
   <nord offset="0x016FE003" from="2F612F" to="2F652F" />
   <nord offset="0x016FE00A" from="2F612F" to="2F652F" />
   <nord offset="0x016FE01B" from="2F612F" to="2F652F" />
   <nord offset="0x016FE026" from="2F612F" to="2F652F" />
   <nord offset="0x016FE037" from="2F612F" to="2F652F" />
   <nord offset="0x016FE044" from="2F612F" to="2F652F" />
   <nord offset="0x016FE057" from="2F612F" to="2F652F" />
   <nord offset="0x016FE719" from="2F612F" to="2F652F" />
  </changes>
 </patchdata>
</patch>
