DLL not found...
BB5 Easy Service Tool v1.14.1 (c) Infinity-Box Team Ready

Connect phone on selected interface...

DLL not found...
BB5 Easy Service Tool v1.14.1 (c) Infinity-Box Team Ready

Connect phone on selected interface...

UFS S/N 74898 boot - Ok

Connect phone on selected interface...

Phone found!
Series 40 Device detected!
read info...  - Ok

Reading Phone Info....
SW ver  : V 05wk47v61.1 09-07-08 RM-133 (c) Nokia.  
IMEI    :      352757013524094
PPM     :      
DSP Ver :      scarfe_mc.05wk46v50p2
PCode   :      0539343
BPCode  :      0527006
HWID    :      6012
LCDVer  :      
IMEI    :      352757013524094
Sl Conf  : --
Sl Prof  : -
Sl Aux   : 
Hw Sig   : 
Provider : Unknown providers

Lock info:

Done!

Backup Certificates now...
Backup CRT308
CRT308 Backup Created... :)
CRT308 Backup Created... :)
Setting FlashMode
FlashMode set Ok

1st boot Ok, C0

APE part info : 
APE ASICID   : 17100708
APE MODE ID : 00
APE PUB ID    : 183633F439D05E89C6F793B63267F064B6853C44
APE R_HASH  : 49A97E826B93BA20B7ED0B082475C005
APE ROM ID  : 1DFD66132C872FD4

CMT part info : 
CMT ASICID   : 000000010000022600010006010C192101003000
CMT EM0 ID  : 00000295
CMT EM1 ID  : 00000B21
CMT PUB ID  : 1DF001148A9401544FBF47B644A61365C98AD05F
CMT MODE ID : 00
CMT R_HASH  : BAF3A9C3DBFA8454937DB77F2B8852B1
CMT ROM ID  : 273F6D55DFAAF68F

CMT : Sending 2nd loader...
Use : RAP3Gv3_2nd.fg
CMT Loader sent, Boot Ok
MCU Configuration
FLASHID : 22E800EC , CMT , NOR
CMT Flash ID : 22E800EC < SAMSUNG [SEC] => K5G2829ATC
FLCNT   : 00000000000000000000000000000000000000
FLASHID : 0000FFFF , CMT , MMC , EXT
CMT Flash ID : 0000FFFF < Bad Flash Type , if MMC - It Ok
Sending ALGO....
Use : RAP3Gv3_algo.fg
CMT Algo sent
CMT PAPUB : 8D0D504A0902E261268C14FCD8A2C9093523BCBD00
Transmission mode :  Dual (Ddr, TX2) 

APE : Sending 2nd loader...
Use : helen3_2nd.fg
APE Loader sent, Boot Ok
FLASHID : 00A100EC , APE , NAND
APE Flash ID : 00A100EC < SAMSUNG [SEC] => K5E1G12ACM [NAND]
FLCNT : 00FFFFFFFFFFFFFFFFFFFFFFFFFFFF
Sending ALGO....
Use : h3_sam_nand_xsr.fg
APE Algo sent
APE PAPUB : 8D0D504A0902E261268C14FCD8A2C9093523BCBC00
Transmission mode :  Dual (Ddr, TX2) 

Boot Done!

CMT : Read NPC certificate...
Cert size : 30600 byte(s)
IMEI : 352757013524094
CMT : Read CCC certificate...
Cert size : 0 byte(s)
CMT : Read HWC certificate...
Cert size : 0 byte(s)
CMT : Read VARIANT certificate...
Cert size : 30600 byte(s)
APE : Read NPC certificate...
Cert size : 0 byte(s)
APE : Read CCC certificate...
Cert size : 0 byte(s)
APE : Read HWC certificate...
Cert size : 0 byte(s)
APE : Read VARIANT certificate...
Cert size : 0 byte(s)
Cert Read done!

NPC Certificate saved...

RPL saved : C:\Users\CHAMI\Desktop\BEST\Backup\Cert\352757013524094_2nd.rpl

Connect phone on selected interface...

Phone found!
Series 40 Device detected!
read info...  - Ok

Selected FlashSettings : FullFlash
Files Set for Flashing :
MCU : N73_4.0839.42.2.1_western_C00_PRD_cc.fpsx
PPM : N73_rofx_4.0839.42.2.1_PRD.V05
FlashFile verify disabled
-> SWversion check skipped : Manual mode selected

Backup enabled, Will read Certificates now...
Backup CRT308
CRT308 Backup Created... :)
CRT308 Backup Created... :)
Setting FlashMode
FlashMode set Ok

1st boot Ok, C0

APE part info : 
APE ASICID   : 17100708
APE MODE ID : 00
APE PUB ID    : 183633F439D05E89C6F793B63267F064B6853C44
APE R_HASH  : 49A97E826B93BA20B7ED0B082475C005
APE ROM ID  : 1DFD66132C872FD4

CMT part info : 
CMT ASICID   : 000000010000022600010006010C192101003000
CMT EM0 ID  : 00000295
CMT EM1 ID  : 00000B21
CMT PUB ID  : 1DF001148A9401544FBF47B644A61365C98AD05F
CMT MODE ID : 00
CMT R_HASH  : BAF3A9C3DBFA8454937DB77F2B8852B1
CMT ROM ID  : 273F6D55DFAAF68F

CMT : Sending 2nd loader...
Use : RAP3Gv3_2nd.fg
CMT Loader sent, Boot Ok
MCU Configuration
FLASHID : 22E800EC , CMT , NOR
CMT Flash ID : 22E800EC < SAMSUNG [SEC] => K5G2829ATC
FLCNT   : 00000000000000000000000000000000000000
FLASHID : 0000FFFF , CMT , MMC , EXT
CMT Flash ID : 0000FFFF < Bad Flash Type , if MMC - It Ok
Sending ALGO....
Use : RAP3Gv3_algo.fg
CMT Algo sent
CMT PAPUB : 8D0D504A0902E261268C14FCD8A2C9093523BCBD00
Transmission mode :  Dual (Ddr, TX2) 

APE : Sending 2nd loader...
Use : helen3_2nd.fg
APE Loader sent, Boot Ok
FLCNT : 
Sending ALGO....
Use : h3_xsr15_flash_alg.fg
Error on prepare stage - connection fail or HW error


RPL saved : C:\Users\CHAMI\Desktop\BEST\Backup\Cert\352757013524094_SIM.rpl

Setting FlashMode
FlashMode set Ok

1st boot Ok, C0

APE part info : 
APE ASICID   : 17100708
APE MODE ID : 00
APE PUB ID    : 183633F439D05E89C6F793B63267F064B6853C44
APE R_HASH  : 49A97E826B93BA20B7ED0B082475C005
APE ROM ID  : 1DFD66132C872FD4

CMT part info : 
CMT ASICID   : 000000010000022600010006010C192101003000
CMT EM0 ID  : 00000295
CMT EM1 ID  : 00000B21
CMT PUB ID  : 1DF001148A9401544FBF47B644A61365C98AD05F
CMT MODE ID : 00
CMT R_HASH  : BAF3A9C3DBFA8454937DB77F2B8852B1
CMT ROM ID  : 273F6D55DFAAF68F

CMT : Sending 2nd loader...
Use : RAP3Gv3_2nd.fg
CMT Loader sent, Boot Ok
MCU Configuration
FLASHID : 22E800EC , CMT , NOR
CMT Flash ID : 22E800EC < SAMSUNG [SEC] => K5G2829ATC
FLCNT   : 00000000000000000000000000000000000000
FLASHID : 0000FFFF , CMT , MMC , EXT
CMT Flash ID : 0000FFFF < Bad Flash Type , if MMC - It Ok
Sending ALGO....
Use : RAP3Gv3_algo.fg
CMT Algo sent
CMT PAPUB : 8D0D504A0902E261268C14FCD8A2C9093523BCBD00
Transmission mode :  Dual (Ddr, TX2) 

APE : Sending 2nd loader...
Use : helen3_2nd.fg
APE Loader sent, Boot Ok
FLASHID : 00A100EC , APE , NAND
APE Flash ID : 00A100EC < SAMSUNG [SEC] => K5E1G12ACM [NAND]
FLCNT : 00FFFFFFFFFFFFFFFFFFFFFFFFFFFF
Sending ALGO....
Use : h3_sam_nand_xsr.fg
APE Algo sent
APE PAPUB : 8D0D504A0902E261268C14FCD8A2C9093523BCBC00
Transmission mode :  Dual (Ddr, TX2) 

Boot Done!

Partitioning....
Partitioning Ok...
Transmission mode :  Dual (Ddr, TX2) 
Erase : Processing N73_4.0839.42.2.1_western_C00_PRD_cc.fpsx
Found 4 areas to erase, erase group
Asic : CMT , Sub : NOR
CMT , NOR , Area : 0x00080000 - 0x00731951
CMT , NOR , Area : 0x00000000 - 0x0005FFFF
CMT , NOR , Area : 0x001E0000 - 0x001FFFFF
CMT , NOR , Area : 0x00880000 - 0x00FEFFFF
Using TimeOut : 5 min ( 300 sec )
Erasing, wait.....
Erase error! Conection lost :(
Error on Erasing Phone!
Error... :(

Connect phone on selected interface...

Selected FlashSettings : Manual
Files Set for Flashing :
MCU : N73_4.0839.42.2.1_western_C00_PRD_cc.fpsx
PPM : N73_rofx_4.0839.42.2.1_PRD.V05
FlashFile verify disabled
-> SWversion check skipped : Dead mode selected

Backup enabled, Will read Certificates now...
Setting FlashMode
FlashMode set Ok

1st boot Ok, C0

APE part info : 
APE ASICID   : 17100708
APE MODE ID : 00
APE PUB ID    : 183633F439D05E89C6F793B63267F064B6853C44
APE R_HASH  : 49A97E826B93BA20B7ED0B082475C005
APE ROM ID  : 1DFD66132C872FD4

CMT part info : 
CMT ASICID   : 000000010000022600010006010C192101003000
CMT EM0 ID  : 00000295
CMT EM1 ID  : 00000B21
CMT PUB ID  : 1DF001148A9401544FBF47B644A61365C98AD05F
CMT MODE ID : 00
CMT R_HASH  : BAF3A9C3DBFA8454937DB77F2B8852B1
CMT ROM ID  : 273F6D55DFAAF68F

CMT : Sending 2nd loader...
Use : RAP3Gv3_2nd.fg
CMT Loader sent, Boot Ok
MCU Configuration
FLASHID : 22E800EC , CMT , NOR
CMT Flash ID : 22E800EC < SAMSUNG [SEC] => K5G2829ATC
FLCNT   : 00000000000000000000000000000000000000
FLASHID : 0000FFFF , CMT , MMC , EXT
CMT Flash ID : 0000FFFF < Bad Flash Type , if MMC - It Ok
Sending ALGO....
Use : RAP3Gv3_algo.fg
CMT Algo sent
PAPUBkeys blank (erased or HW failure)
Transmission mode :  Dual (Ddr, TX2) 

APE : Sending 2nd loader...
Use : helen3_2nd.fg
APE Loader sent, Boot Ok
FLASHID : 00A100EC , APE , NAND
APE Flash ID : 00A100EC < SAMSUNG [SEC] => K5E1G12ACM [NAND]
FLCNT : 00FFFFFFFFFFFFFFFFFFFFFFFFFFFF
Sending ALGO....
Use : h3_sam_nand_xsr.fg
APE Algo sent
APE PAPUB : 8D0D504A0902E261268C14FCD8A2C9093523BCBC00
Transmission mode :  Dual (Ddr, TX2) 

Boot Done!

CMT : Read NPC certificate...
Cert size : 0 byte(s)
CMT : Read CCC certificate...
Cert size : 0 byte(s)
CMT : Read HWC certificate...
Cert size : 0 byte(s)
CMT : Read VARIANT certificate...
Cert size : 0 byte(s)
APE : Read NPC certificate...
Cert size : 0 byte(s)
APE : Read CCC certificate...
Cert size : 0 byte(s)
APE : Read HWC certificate...
Cert size : 0 byte(s)
APE : Read VARIANT certificate...
Cert size : 0 byte(s)
No any CRT data (MCU damaged/CERT erased), skip saving

Init Service mode... Wait...

Init Service Mode Failed!
Setting FlashMode
FlashMode set Ok

1st boot Ok, C0

APE part info : 
APE ASICID   : 17100708
APE MODE ID : 00
APE PUB ID    : 183633F439D05E89C6F793B63267F064B6853C44
APE R_HASH  : 49A97E826B93BA20B7ED0B082475C005
APE ROM ID  : 1DFD66132C872FD4

CMT part info : 
CMT ASICID   : 000000010000022600010006010C192101003000
CMT EM0 ID  : 00000295
CMT EM1 ID  : 00000B21
CMT PUB ID  : 1DF001148A9401544FBF47B644A61365C98AD05F
CMT MODE ID : 00
CMT R_HASH  : BAF3A9C3DBFA8454937DB77F2B8852B1
CMT ROM ID  : 273F6D55DFAAF68F

CMT : Sending 2nd loader...
Use : RAP3Gv3_2nd.fg
CMT Loader sent, Boot Ok
MCU Configuration
FLASHID : 22E800EC , CMT , NOR
CMT Flash ID : 22E800EC < SAMSUNG [SEC] => K5G2829ATC
FLCNT   : 00000000000000000000000000000000000000
FLASHID : 0000FFFF , CMT , MMC , EXT
CMT Flash ID : 0000FFFF < Bad Flash Type , if MMC - It Ok
Sending ALGO....
Use : RAP3Gv3_algo.fg
CMT Algo sent
PAPUBkeys blank (erased or HW failure)
Transmission mode :  Dual (Ddr, TX2) 

APE : Sending 2nd loader...
Use : helen3_2nd.fg
APE Loader sent, Boot Ok
FLASHID : 00A100EC , APE , NAND
APE Flash ID : 00A100EC < SAMSUNG [SEC] => K5E1G12ACM [NAND]
FLCNT : 00FFFFFFFFFFFFFFFFFFFFFFFFFFFF
Sending ALGO....
Use : h3_sam_nand_xsr.fg
APE Algo sent
APE PAPUB : 8D0D504A0902E261268C14FCD8A2C9093523BCBC00
Transmission mode :  Dual (Ddr, TX2) 

Boot Done!

Partitioning....
Partitioning Ok...
Transmission mode :  Dual (Ddr, TX2) 
Erase : Processing N73_4.0839.42.2.1_western_C00_PRD_cc.fpsx
Found 4 areas to erase, erase group
Asic : CMT , Sub : NOR
CMT , NOR , Area : 0x00080000 - 0x00731951
CMT , NOR , Area : 0x00000000 - 0x0005FFFF
CMT , NOR , Area : 0x001E0000 - 0x001FFFFF
CMT , NOR , Area : 0x00880000 - 0x00FEFFFF
Using TimeOut : 5 min ( 300 sec )
Erasing, wait.....
CMT : Group erase Ok
Found 4 areas to erase, erase group
Asic : APE , Sub : NAND
APE , NAND , Area : 0x00000000 - 0x0007FFFF
APE , NAND , Area : 0x00080000 - 0x000FFFFF
APE , NAND , Area : 0x00100000 - 0x0025FFFF
APE , NAND , Area : 0x003C0000 - 0x04E1FFFF
Erasing, wait.....
APE : Group erase Ok
TIME : Erase time : 00:00:12
Transmission mode :  Dual (Ddr, TX2) 
Write : Processing N73_4.0839.42.2.1_western_C00_PRD_cc.fpsx
CMT: Writing Hash CERT [NOLO]
CMT: Writing Hash CERT [KEYS]
CMT: Writing Hash CERT [PRIMAPP]
CMT: Writing Hash CERT [PASUBTOC]
CMT: Writing Hash CERT [PAPUBKEYS]
CMT: Writing Hash CERT [UPDAPP]
CMT: Writing Hash CERT [ADL]
CMT: Writing Hash CERT [DSP0]
CMT: Writing Hash CERT [MCUSW]
APE: Writing Hash CERT [KEYS]
APE: Writing Hash CERT [X-LOADER]
APE: Writing Hash CERT [PRIMAPP]
APE: Writing Hash CERT [SOS+LOADER]
APE: Writing Hash CERT [SOS*UPDAPP]
APE: Writing Hash CERT [SOS+UZIP]
APE: Writing Hash CERT [PAPUBKEYS]
APE: Writing Hash CERT [PASUBTOC]
APE: Writing Hash CERT [ADL]
APE: Writing Hash CERT [SOS+XZIP]
APE: Writing Hash CERT [SOS*CORE]
APE: Writing Hash CERT [SOS+ROFS]
APE: Writing Hash CERT [SOS+ROFX]
Total writen 1770 blocks
TIME : Write time : 00:05:41 


Partitioning....
Partitioning Ok...
Transmission mode :  Dual (Ddr, TX2) 
Erase : Processing N73_rofx_4.0839.42.2.1_PRD.V05
Found 1 areas to erase, erase group
Asic : APE , Sub : NAND
APE , NAND , Area : 0x03920000 - 0x04E1FFFF
Erasing, wait.....
APE : Group erase Ok
TIME : Erase time : 00:00:00
Transmission mode :  Dual (Ddr, TX2) 
Write : Processing N73_rofx_4.0839.42.2.1_PRD.V05
APE: Writing Hash CERT [SOS+ROFX]
Total writen 2071 blocks
TIME : Write time : 00:02:47 


Init Service mode... Wait...

Reading Phone Info....
Connected phone -   Nokia N73
Software Info:     V 05wk47v61.1
09-07-08
RM-133
(c) Nokia.  
IMEI:  352757013524094
Product code:  0539343
Checking...
SimLock status : SimLock is Ok
Security status : Security is Ok
Read Info Done!
Settings After Flash Defaults...
ProductTuneSet...OK!
SwUpgradeSet...OK!
AfterFlash operations done... Reconnect, wait...
Connect phone on selected interface...

Phone found!
Series 40 Device detected!
read info...  - Ok

Phone disconected!

Connect phone on selected interface...

Phone found!
Series 40 Device detected!
read info...  - Ok

Phone disconected!

Connect phone on selected interface...

Phone found!
Series 40 Device detected!
read info...  - Ok

Reading Phone Info....
SW ver  : V 05wk47v61.1 09-07-08 RM-133 (c) Nokia.  
IMEI    :      352757013524094
PPM     :      
DSP Ver :      scarfe_mc.05wk46v50p2
PCode   :      0539343
BPCode  :      0527006
HWID    :      6012
LCDVer  :      
IMEI    :      352757013524094
Sl Conf  : --
Sl Prof  : -
Sl Aux   : 
Hw Sig   : 
Provider : Unknown providers

Lock info:

Done!

Resetting selected items...
Check phone mode...
Phone already in Test mode, skip change...
Settings Full Factory Defaults...
Set OK!

Elapsed: 00:00:00

Unlock procedure started...

UFS S/N 74898 boot - Ok

Connect phone on selected interface...

UFS S/N 74898 boot - Ok

Connect phone on selected interface...

DLL not found...
BB5 Easy Service Tool v1.14.1 (c) Infinity-Box Team Ready

Connect phone on selected interface...

UFS S/N 74898 boot - Ok

Connect phone on selected interface...

Phone found!
Series 40 Device detected!
read info...  - Ok

Reading Phone Info....
SW ver  : V 05wk47v61.1 09-07-08 RM-133 (c) Nokia.  
IMEI    :      352757013524094
PPM     :      
DSP Ver :      scarfe_mc.05wk46v50p2
PCode   :      0539343
BPCode  :      0527006
HWID    :      6012
LCDVer  :      
IMEI    :      352757013524094
Sl Conf  : --
Sl Prof  : -
Sl Aux   : 
Hw Sig   : 
Provider : Unknown providers

Lock info:

Done!

Initializing Tests...
IMEI : 352757013524094 , Phone : RM-133
Get keys...
PASSED | ST_TAHVOINT_TEST
PASSED | ST_UEM_CBUS_IF_TEST
PASSED | ST_EAR_DATA_LOOP_TEST
PASSED | ST_SIM_CLK_LOOP_TEST
PASSED | ST_SIM_IO_CTRL_LOOP_TEST
PASSED | ST_SIM_LOCK_TEST
PASSED | ST_SECURITY_TEST
PASSED | ST_PWR_KEY_TEST
PASSED | ST_CURRENT_CONS_TEST
PASSED | ST_BACKUP_BATT_TEST
PASSED | ST_CMT_APE_WAKEUP_TEST
PASSED | ST_SLEEPCLK_FREQ_TEST
PASSED | ST_RADIO_TEST
PASSED | ST_HOOKINT_TEST
PASSED | ST_BTEMP_TEST
->ERROR | ST_VIBRA_TEST
->ERROR | ST_MBUS_RX_TX_LOOP_TEST
PASSED | ST_EXT_DEVICE_TEST
PASSED | ST_IR_LOOP_TEST
PASSED | ST_KEYBOARD_STUCK_TEST
PASSED | ST_LPRF_IF_TEST
MINOR | ST_CAMERA_IF_TEST
MINOR | ST_CAMERA_ACCELERATOR_TEST
MINOR | ST_SEC_CAMERA_IF_TEST
MINOR | ST_CAMERA_AUTOFOCUS_TEST
MINOR | ST_LPRF_AUDIO_LINES_TEST
MINOR | ST_MAIN_LCD_IF_TEST
MINOR | ST_BT_WAKEUP_TEST
SelfTests end
Done!

Elapsed: 00:03:15

Phone disconected!

Connect phone on selected interface...

Phone found!
Series 40 Device detected!
read info...  - Ok

Read and Check phone data...
SimLock status : SimLock is Ok
Security status : Security is Ok
Setting FlashMode
FlashMode set Ok

1st boot Ok, C0

APE part info : 
APE ASICID   : 17100708
APE MODE ID : 00
APE PUB ID    : 183633F439D05E89C6F793B63267F064B6853C44
APE R_HASH  : 49A97E826B93BA20B7ED0B082475C005
APE ROM ID  : 1DFD66132C872FD4

CMT part info : 
CMT ASICID   : 000000010000022600010006010C192101003000
CMT EM0 ID  : 00000295
CMT EM1 ID  : 00000B21
CMT PUB ID  : 1DF001148A9401544FBF47B644A61365C98AD05F
CMT MODE ID : 00
CMT R_HASH  : BAF3A9C3DBFA8454937DB77F2B8852B1
CMT ROM ID  : 273F6D55DFAAF68F

CMT : Sending 2nd loader...
Use : RAP3Gv3_2nd.fg
CMT Loader sent, Boot Ok
MCU Configuration
FLASHID : 22E800EC , CMT , NOR
CMT Flash ID : 22E800EC < SAMSUNG [SEC] => K5G2829ATC
FLCNT   : 00000000000000000000000000000000000000
FLASHID : 0000FFFF , CMT , MMC , EXT
CMT Flash ID : 0000FFFF < Bad Flash Type , if MMC - It Ok
Sending ALGO....
Use : RAP3Gv3_algo.fg
CMT Algo sent
CMT PAPUB : 8D0D504A0902E261268C14FCD8A2C9093523BCBD00
Transmission mode :  Dual (Ddr, TX2) 

APE : Sending 2nd loader...
Use : helen3_2nd.fg
APE Loader sent, Boot Ok
FLASHID : 00A100EC , APE , NAND
APE Flash ID : 00A100EC < SAMSUNG [SEC] => K5E1G12ACM [NAND]
FLCNT : 00FFFFFFFFFFFFFFFFFFFFFFFFFFFF
Sending ALGO....
Use : h3_sam_nand_xsr.fg
APE Algo sent
APE PAPUB : 8D0D504A0902E261268C14FCD8A2C9093523BCBC00
Transmission mode :  Dual (Ddr, TX2) 

Boot Done!

Init Service mode... Wait...


Connect phone on selected interface...

Phone found!
Series 40 Device detected!
read info...  - Ok

Phone disconected!

Connect phone on selected interface...

Phone found!
Series 40 Device detected!
read info...  - Ok

Reading Phone Info....
SW ver  : V 05wk47v61.1 09-07-08 RM-133 (c) Nokia.  
IMEI    :      352757013524094
PPM     :      
DSP Ver :      scarfe_mc.05wk46v50p2
PCode   :      0539343
BPCode  :      0527006
HWID    :      6012
LCDVer  :      
IMEI    :      352757013524094
Sl Conf  : --
Sl Prof  : -
Sl Aux   : 
Hw Sig   : 
Provider : Unknown providers

Lock info:

Done!

Reading Phone Info....
SW ver  : V 05wk47v61.1 09-07-08 RM-133 (c) Nokia.  
IMEI    :      352757013524094
PPM     :      
DSP Ver :      scarfe_mc.05wk46v50p2
PCode   :      0539343
BPCode  :      0527006
HWID    :      6012
LCDVer  :      
IMEI    :      352757013524094
Sl Conf  : --
Sl Prof  : -
Sl Aux   : 
Hw Sig   : 
Provider : Unknown providers

Lock info:

Done!

Reading Product code...
Product code : 0539343
Done!

Reading Product code...
Product code : 0539343
Done!

Phone disconected!

Connect phone on selected interface...

