; Release: V JP175_04w47_29.nbr|21-03-06|RM-97|(c) NMP|
; This file contains 348 settings, 91 ordinary setting groups and 17 tables

Group ID          = .1
Group Description = Application

    Group ID          = .1.1
    Group Description = Queries and editors

        Setting ID          = .1.1.1
        Setting description = "T9 language state"
        Setting type	    = Integer16

        Setting ID          = .1.1.2
        Setting description = "T9 user database"
        Setting type	    = Binary

        Setting ID          = .1.1.3
        Setting description = "Font size"
        Setting type	    = Integer16

    Group ID          = .1.2
    Group Description = Windows and layouts

        Setting ID          = .1.2.1
        Setting description = "Wallpaper - PRI 1220"
        Setting type	    = Binary
        Setting Editor	    = Wallpaper[128, 128]

        Setting ID          = .1.2.2
        Setting description = "UI Theme"
        Setting type	    = Binary
        Setting Editor	    = Theme

        Setting ID          = .1.2.3
        Setting description = "Grid state"
        Setting type	    = Integer16

        Group ID          = .1.2.4
        Group Description = Themes

            Table ID          = .1.2.4.1
            Table Description = Themes
            Table Range       = 0, 21

                Index Description = Themes index
                Index ID          = .1.2.4.1.x

                    Setting ID          = .1.2.4.1.0.1
                    Setting description = "Wallpaper select"
                    Setting type	    = Integer16

                    Setting ID          = .1.2.4.1.0.2
                    Setting description = "Menu background"
                    Setting type	    = Integer16

                    Setting ID          = .1.2.4.1.0.3
                    Setting description = "Signal and battery bar"
                    Setting type	    = Integer16

        Setting ID          = .1.2.5
        Setting description = "Background light state"
        Setting type	    = Integer16

        Setting ID          = .1.2.6
        Setting description = "Powersave clock timeout state"
        Setting type	    = Integer16

        Setting ID          = .1.2.7
        Setting description = "Brightness select state"
        Setting type	    = Integer16

    Group ID          = .1.3
    Group Description = UI/Core interface

        Group ID          = .1.3.1
        Group Description = Wake-up graphic

            Setting ID          = .1.3.1.1
            Setting description = "Wake-up graphic switch"
            Setting type	    = Integer16

            Setting ID          = .1.3.1.2
            Setting description = "Wake-up graphic image - PRI 1214"
            Setting type	    = Binary
            Setting Editor	    = WUG[128, 128]

            Setting ID          = .1.3.1.3
            Setting description = "Dealer welcome note"
            Setting type	    = ASCII

            Setting ID          = .1.3.1.4
            Setting description = "User welcome note"
            Setting type	    = Unicode

            Setting ID          = .1.3.1.5
            Setting description = "Display of Alpha Tag and MIN/MDN on Phone Power-up Options - PRI 681"
            Setting type	    = Integer16
            Setting Editor	    = Range[None, Display MDN & Alpha Tag, Display MIN & Alpha Tag]

            Setting ID          = .1.3.1.6
            Setting description = "Banner Menu - PRI 103"
            Setting type	    = Integer16
            Setting Editor	    = Range[Excluded, Included]

        Group ID          = .1.3.2
        Group Description = Automatic keyguard

            Setting ID          = .1.3.2.1
            Setting description = "Automatic keyguard switch"
            Setting type	    = Integer16

            Setting ID          = .1.3.2.2
            Setting description = "Automatic keyguard timeout"
            Setting type	    = Integer16

            Setting ID          = .1.3.2.3
            Setting description = "Automatic keyguard lock"
            Setting type	    = Integer16

        Group ID          = .1.3.3
        Group Description = Accessory

            Group ID          = .1.3.3.1
            Group Description = Headset

                Setting ID          = .1.3.3.1.1
                Setting description = "Headset default profile"
                Setting type	    = Integer16

                Setting ID          = .1.3.3.1.2
                Setting description = "Headset automatic answer switch"
                Setting type	    = Integer16

            Group ID          = .1.3.3.2
            Group Description = Carkit (handsfree)

                Setting ID          = .1.3.3.2.1
                Setting description = "Carkit default profile"
                Setting type	    = Integer16

                Setting ID          = .1.3.3.2.2
                Setting description = "Carkit automatic answer switch"
                Setting type	    = Integer16

                Setting ID          = .1.3.3.2.3
                Setting description = "Carkit automatic light switch"
                Setting type	    = Integer16

    Group ID          = .1.4
    Group Description = Phonebook

        Setting ID          = .1.4.2
        Setting description = "Phonebook view type"
        Setting type	    = Integer16

        Group ID          = .1.4.3
        Group Description = Contacts

            Table ID          = .1.4.3.1
            Table Description = Contacts in mobile equipment (= phone without SIM)
            Table Range       = 1, 200

                Index Description = Contact index
                Index ID          = .1.4.3.1.x

                    Setting ID          = .1.4.3.1.1.1
                    Setting description = "Contact Name"
                    Setting type	    = Unicode
                    Setting Editor	    = @P

                    Setting ID          = .1.4.3.1.1.2
                    Setting description = "Contact Number"
                    Setting type	    = ASCII
                    Setting Editor	    = @P

                    Setting ID          = .1.4.3.1.1.3
                    Setting description = "Additional Numbers"
                    Setting type	    = ASCII
                    Setting Editor	    = @P

                    Setting ID          = .1.4.3.1.1.100
                    Setting description = "Contact Tone ID"
                    Setting type	    = Integer16

            Table ID          = .1.4.3.2
            Table Description = Contacts in SIM
            Table Range       = 1, 250

                Index Description = Contact index
                Index ID          = .1.4.3.2.x

                    Setting ID          = .1.4.3.2.1.100
                    Setting description = "Tone ID"
                    Setting type	    = Integer16

        Setting ID          = .1.4.4
        Setting description = "Phonebook memory"
        Setting type	    = Integer16

        Table ID          = .1.4.5
        Table Description = Speed dials
        Table Range       = 2, 8

            Index Description = Speed dial index
            Index ID          = .1.4.5.x

                Setting ID          = .1.4.5.2.1
                Setting description = "Speed dial location"
                Setting type	    = Integer16

                Setting ID          = .1.4.5.2.2
                Setting description = "Speed dial memory"
                Setting type	    = Integer16

        Setting ID          = .1.4.6
        Setting description = "Speed dial select state"
        Setting type	    = Integer16

        Setting ID          = .1.4.10
        Setting description = "Phone Number Grouping Options - PRI 111"
        Setting type	    = Integer16
        Setting Editor	    = Range[Non-NA Phone Number Grouping, NA Phone Number Grouping] @P

        Setting ID          = .1.4.11
        Setting description = "Plus-code (+) to International Direct Dialing (IDD) Prefix Translation - PRI 980"
        Setting type	    = ASCII
        Setting Editor	    = BCD[10]

        Setting ID          = .1.4.12
        Setting description = "Minimum Number of Digits for Caller ID/Phonebook Matching - PRI 1032"
        Setting type	    = Integer16
        Setting Editor	    = @P

    Group ID          = .1.5
    Group Description = Messaging

        Group ID          = .1.5.1
        Group Description = Message folders

            Table ID          = .1.5.1.1
            Table Description = Inbox
            Table Range       = 1, 60

                Index Description = Inbox message index
                Index ID          = .1.5.1.1.x

                    Setting ID          = .1.5.1.1.1.1
                    Setting description = "Inbox message type"
                    Setting type	    = Integer16

                    Setting ID          = .1.5.1.1.1.2
                    Setting description = "Inbox message version"
                    Setting type	    = Integer16

                    Setting ID          = .1.5.1.1.1.3
                    Setting description = "Inbox message content"
                    Setting type	    = Binary

            Table ID          = .1.5.1.3
            Table Description = Sent items
            Table Range       = 1, 25

                Index Description = Sent message index
                Index ID          = .1.5.1.3.x

                    Setting ID          = .1.5.1.3.1.1
                    Setting description = "Sent message type"
                    Setting type	    = Integer16

                    Setting ID          = .1.5.1.3.1.2
                    Setting description = "Sent message version"
                    Setting type	    = Integer16

                    Setting ID          = .1.5.1.3.1.3
                    Setting description = "Sent message content"
                    Setting type	    = Binary

            Table ID          = .1.5.1.4
            Table Description = Screened items
            Table Range       = 1, 25

                Index Description = Screened message index
                Index ID          = .1.5.1.4.x

                    Setting ID          = .1.5.1.4.1.1
                    Setting description = "Screened message type"
                    Setting type	    = Integer16

                    Setting ID          = .1.5.1.4.1.2
                    Setting description = "Screened message version"
                    Setting type	    = Integer16

                    Setting ID          = .1.5.1.4.1.3
                    Setting description = "Screened message content"
                    Setting type	    = Binary

        Group ID          = .1.5.2
        Group Description = SMS

            Setting ID          = .1.5.2.1
            Setting description = "Delivery reports"
            Setting type	    = Integer16

            Setting ID          = .1.5.2.4
            Setting description = "Signature select state"
            Setting type	    = Integer16

            Setting ID          = .1.5.2.5
            Setting description = "Signature"
            Setting type	    = Unicode

            Setting ID          = .1.5.2.6
            Setting description = "Screened sms filter list"
            Setting type	    = Binary

            Setting ID          = .1.5.2.8
            Setting description = "Enhanced Voice Mail Notification - PRI 88"
            Setting type	    = Binary
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .1.5.2.9
            Setting description = "Callback number"
            Setting type	    = ASCII
            Setting Editor	    = BCD[]

            Group ID          = .1.5.2.20
            Group Description = E-mail Message Settings

                Setting ID          = .1.5.2.20.1
                Setting description = "Origination Address for MT SMS via Email Options - PRI 106"
                Setting type	    = Integer16
                Setting Editor	    = Range[6245=0, <reserved>, Custom Origination Address=2, 0000000000=3]

                Setting ID          = .1.5.2.20.2
                Setting description = "Origination Address for MT SMS via E-mail Value - PRI 877"
                Setting type	    = ASCII

                Setting ID          = .1.5.2.20.3
                Setting description = "Validate Email Address For MO SMS - PRI 112"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .1.5.2.20.4
                Setting description = "MO SMS Email Address Support - PRI 95"
                Setting type	    = Integer16
                Setting Editor	    = Range[Excluded, Included]

            Group ID          = .1.5.2.21
            Group Description = Message Creation Settings

                Setting ID          = .1.5.2.21.1
                Setting description = "Maximum Size of Callback Number - PRI 139"
                Setting type	    = Integer16

                Setting ID          = .1.5.2.21.2
                Setting description = "Maximum Size of Recipient Email Address - PRI 138"
                Setting type	    = Integer16

                Setting ID          = .1.5.2.21.3
                Setting description = "Maximum Size of Recipient Phone Number - PRI 137"
                Setting type	    = Integer16

                Setting ID          = .1.5.2.21.4
                Setting description = "Maximum Size for Submit Message - PRI 213"
                Setting type	    = Integer16

                Setting ID          = .1.5.2.21.5
                Setting description = "Maximum Size for User Data in MO SMS Message (in bytes) - PRI 1081"
                Setting type	    = Integer16

                Setting ID          = .1.5.2.21.6
                Setting description = "Maximum Number of Characters for MO SMS Text - PRI 1291"
                Setting type	    = Integer16

                Setting ID          = .1.5.2.21.7
                Setting description = "MO SMS Destination Address Format Options - PRI 87"
                Setting type	    = Integer16
                Setting Editor	    = Range[Numbers and All Symbols (0-9, *, #, p, w, +), Numbers Only (0-9), Numbers and "+" Symbol only (0-9, +)]

            Group ID          = .1.5.2.22
            Group Description = Message Sending Settings

                Setting ID          = .1.5.2.22.1
                Setting description = "Message sending failed indication options - PRI 1024"
                Setting type	    = Integer16
                Setting Editor	    = Range[Notification message only, User confirmation & Cause code information]

                Setting ID          = .1.5.2.22.2
                Setting description = "Send empty MO SMS message - PRI 976"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .1.5.2.22.3
                Setting description = "MO SMS Traffic Channel Options for Multiple Recipients - PRI 679"
                Setting type	    = Integer16
                Setting Editor	    = Range[Send over one traffic channel, Send over multiple traffic channels]

                Setting ID          = .1.5.2.22.4
                Setting description = "Force MO SMS Messages to be Sent over Traffic Channel - PRI 72"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .1.5.2.22.5
                Setting description = "Default Service Option for MO SMS Messages - PRI 438"
                Setting type	    = Integer16
                Setting Editor	    = Range[<reserved>, SO 6, SO 14]

                Setting ID          = .1.5.2.22.6
                Setting description = "Transport Layer (Layer 3) Delivery Acknowledgement Timer - PRI 210"
                Setting type	    = Integer16

            Group ID          = .1.5.2.23
            Group Description = Miscellaneous Settings

                Setting ID          = .1.5.2.23.2
                Setting description = "Language Indicator Subparameter in WMT MO SMS Message - PRI 908"
                Setting type	    = Integer16
                Setting Editor	    = Range[Excluded, Included]

                Setting ID          = .1.5.2.23.3
                Setting description = "Network Support of 8-bit ASCII Characters in MO SMS - PRI 256"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .1.5.2.23.4
                Setting description = "Non-Standard MO & MT SMS Message Encoding (Vietnamese) Handling Feature - PRI 1265"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .1.5.2.23.5
                Setting description = "Destination Address Parameter in MT SMS Acknowledge Support - PRI 83"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

            Group ID          = .1.5.2.24
            Group Description = Message Receipt Settings

                Setting ID          = .1.5.2.24.1
                Setting description = "Text Message Timestamp Options - PRI 108"
                Setting type	    = Integer16
                Setting Editor	    = Range[GMT Time, Local Time, System Time]

                Setting ID          = .1.5.2.24.2
                Setting description = "Urgent Message Priority Handling - PRI 1023"
                Setting type	    = Integer16
                Setting Editor	    = Range[Normal and Urgent Messages handled identically, Display soft notification & Give higher priority to Urgent Message]

                Setting ID          = .1.5.2.24.3
                Setting description = "Decoding of Octet Unspecified Encoding Assignment for SMS Message Options - PRI 511"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disabled, Latin (ISO 8859-1), UTF-8, 7-bit ASCII]

                Setting ID          = .1.5.2.24.4
                Setting description = "Filter For Duplicate MT SMS - PRI 84"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .1.5.2.24.5
                Setting description = "Display and Storage of Delivery Acknowledgement Messages - PRI 518"
                Setting type	    = Integer16
                Setting Editor	    = Range[Store Delivery Acks in Inbox, Display Delivery Acks on idle screen]

            Group ID          = .1.5.2.25
            Group Description = Menu Settings

                Setting ID          = .1.5.2.25.1
                Setting description = "Send callback number Menu - PRI 1072"
                Setting type	    = Integer16
                Setting Editor	    = Range[Excluded, Included]

                Setting ID          = .1.5.2.25.2
                Setting description = "Delivery note Menu - PRI 1071"
                Setting type	    = Integer16
                Setting Editor	    = Range[Excluded, Included]

        Table ID          = .1.5.5
        Table Description = Smileys
        Table Range       = 0, 8

            Index Description = Smiley index
            Index ID          = .1.5.5.x

                Setting ID          = .1.5.5.0.1
                Setting description = "Smiley text"
                Setting type	    = Unicode

        Table ID          = .1.5.6
        Table Description = Templates
        Table Range       = 0, 8

            Index Description = Template index
            Index ID          = .1.5.6.x

                Setting ID          = .1.5.6.0.1
                Setting description = "Template text"
                Setting type	    = Unicode

        Table ID          = .1.5.7
        Table Description = Distribution lists
        Table Range       = 0, 6

            Index Description = Distribution list index
            Index ID          = .1.5.7.x

                Setting ID          = .1.5.7.0.1
                Setting description = "Distribution list name"
                Setting type	    = Unicode

                Setting ID          = .1.5.7.0.2
                Setting description = "Distribution list members"
                Setting type	    = Binary

        Group ID          = .1.5.9
        Group Description = MMS

            Setting ID          = .1.5.9.2
            Setting description = "Incoming multimedia messages Options - PRI 1027"
            Setting type	    = Integer16
            Setting Editor	    = Range[Retrieve, Ask first]

            Setting ID          = .1.5.9.3
            Setting description = "Maximum Size for MMS Message - PRI 1028"
            Setting type	    = Integer16

            Setting ID          = .1.5.9.4
            Setting description = "Wireless Application Protocol Teleservice Support - PRI 204"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .1.5.9.5
            Setting description = "MMS Message Processing - PRI 961"
            Setting type	    = Integer16
            Setting Editor	    = Range[Discard the message, Process the message upon arrival, Hold the message until mobile is in Idle Mode]

            Setting ID          = .1.5.9.6
            Setting description = "Retry MMS Transfer for Temporary Failures - PRI 1038"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Group ID          = .1.5.9.20
            Group Description = MMS Connection Parameters

                Setting ID          = .1.5.9.20.1
                Setting description = "MMS Proxy Server Authentication Username - PRI 988"
                Setting type	    = ASCII
                Setting Editor	    = @L

                Setting ID          = .1.5.9.20.2
                Setting description = "MMS Proxy Server Authentication Password - PRI 989"
                Setting type	    = ASCII
                Setting Editor	    = @L

                Setting ID          = .1.5.9.20.3
                Setting description = "MMS Proxy Server Authentication Password Format Options - PRI 1311"
                Setting type	    = Integer16
                Setting Editor	    = Range[Leave, HMAC-MD5 ((MDN | ESN (hexadecimal)) with 12 character output)]

                Setting ID          = .1.5.9.20.4
                Setting description = "MMS Proxy Server Connection Type Preference - PRI 990"
                Setting type	    = Integer16
                Setting Editor	    = Range[MMS Proxy Server IP Address, MultiMedia Service Centre (MMSC) URL] @L

                Setting ID          = .1.5.9.20.5
                Setting description = "MMS Proxy Server IP Address - PRI 987"
                Setting type	    = Binary
                Setting Editor	    = IPV4[] @L

                Setting ID          = .1.5.9.20.6
                Setting description = "MMSC URL (Primary) - PRI 860"
                Setting type	    = ASCII
                Setting Editor	    = T[128] @L

                Setting ID          = .1.5.9.20.7
                Setting description = "Username (3G Packet) - PRI 1234"
                Setting type	    = ASCII
                Setting Editor	    = T[72]

                Setting ID          = .1.5.9.20.8
                Setting description = "Password (3G Packet) - PRI 1236"
                Setting type	    = ASCII
                Setting Editor	    = T[64]

                Setting ID          = .1.5.9.20.9
                Setting description = "PPP Authentication Options (3G Packet) - PRI 1238"
                Setting type	    = Integer16
                Setting Editor	    = Range[No Authentication, PAP, CHAP, Both PAP and CHAP]

                Setting ID          = .1.5.9.20.10
                Setting description = "PPP Authentication Options (3G Packet Data) - PRI 136"
                Setting type	    = Integer16
                Setting Editor	    = Range[No Authentication, PAP, CHAP, Both PAP and CHAP]

                Setting ID          = .1.5.9.20.11
                Setting description = "Simple/Mobile IP NAI - PRI 269"
                Setting type	    = ASCII
                Setting Editor	    = T[72] @P

                Setting ID          = .1.5.9.20.12
                Setting description = "Simple/Mobile IP NAI Format Options - PRI 660"
                Setting type	    = Integer16
                Setting Editor	    = Range[Leave NAI Unchanged, <Customer Specified Text>, MIN@<Customer Specified Text>, MDN@<Customer Specified Text>, 1+MIN@<Customer Specified Text>, 1+MDN@<Customer Specified Text>, "ESN@<Customer Specified Text>, ESN in decimal", "ESN@<Customer Specified Text>, ESN in hexadecimal]" @P]

                Setting ID          = .1.5.9.20.13
                Setting description = "Simple/Mobile IP NAI Customer Specified Text - PRI 666"
                Setting type	    = ASCII
                Setting Editor	    = T[48] @P

                Setting ID          = .1.5.9.20.14
                Setting description = "Simple/Mobile IP NAI Length - PRI 268"
                Setting type	    = Integer16
                Setting Editor	    = @P

                Setting ID          = .1.5.9.20.15
                Setting description = "Simple/Mobile IP MN_AAA Shared Secret Data Format Options - PRI 1014"
                Setting type	    = Integer16
                Setting Editor	    = Range[Leave, MD5 (A-key|ESN), MIN, MDN, ESN (decimal), ESN (hexadecimal), MD5 ((A-key + checksum)|ESN)] @P

                Setting ID          = .1.5.9.20.16
                Setting description = "Simple/Mobile IP MN_AAA Shared Secret Key - PRI 275"
                Setting type	    = ASCII
                Setting Editor	    = T[32] @P

                Setting ID          = .1.5.9.20.17
                Setting description = "Simple/Mobile IP MN_AAA Shared Secret Key Length - PRI 274"
                Setting type	    = Integer16
                Setting Editor	    = @P

            Group ID          = .1.5.9.21
            Group Description = Hypertext Transfer Protocol (HTTP) Parameters

                Setting ID          = .1.5.9.21.1
                Setting description = "International Dial Code - Country Code - PRI 947"
                Setting type	    = Integer16
                Setting Editor	    = @L

                Setting ID          = .1.5.9.21.2
                Setting description = "MCC/IDC Options for Client ID in HTTP Header (MMS) - PRI 1077"
                Setting type	    = Integer16
                Setting Editor	    = Range[Exclude MCC & IDC from MMS HTTP Session Header String, Insert MCC in MMS HTTP Session Header String,Insert IDC in MMS HTTP Session Header String] @L

                Setting ID          = .1.5.9.21.3
                Setting description = "MDN/MIN Options for Client ID in HTTP Header (MMS) - PRI 986"
                Setting type	    = Integer16
                Setting Editor	    = Range[MIN, MDN] @L

                Setting ID          = .1.5.9.21.4
                Setting description = "Session Header ASCII String for HTTP Request Messages - PRI 948"
                Setting type	    = ASCII
                Setting Editor	    = T[64] @L

                Setting ID          = .1.5.9.21.5
                Setting description = "User Agent Profile URL - PRI 853"
                Setting type	    = ASCII
                Setting Editor	    = T[128]

            Group ID          = .1.5.9.22
            Group Description = MMS Features

                Setting ID          = .1.5.9.22.1
                Setting description = "MMS M_Notify Response Indication Message Transmission - PRI 1041"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .1.5.9.22.2
                Setting description = "Non-Standard Message Handling for MMS Messages Exceeding Maximum Supported Size - PRI 1241"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

            Group ID          = .1.5.9.23
            Group Description = Network Features

                Setting ID          = .1.5.9.23.1
                Setting description = "WAP Push Message Decoding Options - PRI 934"
                Setting type	    = Integer16
                Setting Editor	    = Range[<reserved for future use>, Decode using Single-decoding, Decode using Double-decoding, Decode as ASCII BREW string, Single/Double-Decoding per OOA Configuration] @L

                Setting ID          = .1.5.9.23.2
                Setting description = "Push Proxy Gateway ID Options - PRI 965"
                Setting type	    = Integer16
                Setting Editor	    = Range[WAP Standard, Openwave, 724, Comverse]

    Group ID          = .1.6
    Group Description = Profiles

        Setting ID          = .1.6.1
        Setting description = "Active profile"
        Setting type	    = Integer16

        Table ID          = .1.6.2
        Table Description = Profiles
        Table Range       = 0, 6

            Index Description = Profile index
            Index ID          = .1.6.2.x

                Setting ID          = .1.6.2.0.1
                Setting description = "Screen saver switch"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.2
                Setting description = "Screen saver timeout"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.3
                Setting description = "Screen saver graphics"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.4
                Setting description = "Backlight alert"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.5
                Setting description = "Lights, notification"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.6
                Setting description = "Lights, coverage"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.7
                Setting description = "Lights, alert"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.8
                Setting description = "Theme selection"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.9
                Setting description = "Profile ringing tone"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.10
                Setting description = "Ringing volume"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.11
                Setting description = "Vibrating alert"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.12
                Setting description = "Message alert"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.13
                Setting description = "Keypad tones"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.14
                Setting description = "Warning tones"
                Setting type	    = Integer16

                Setting ID          = .1.6.2.0.15
                Setting description = "Profile name"
                Setting type	    = Unicode

    Group ID          = .1.7
    Group Description = Clock

        Table ID          = .1.7.1
        Table Description = Calendar notes, e.g. reminders
        Table Range       = 0, 10

            Index Description = Calendar note index
            Index ID          = .1.7.1.x

                Setting ID          = .1.7.1.0.1
                Setting description = "Calendar note type"
                Setting type	    = Integer16

                Setting ID          = .1.7.1.0.2
                Setting description = "Calendar note subject"
                Setting type	    = Unicode

                Setting ID          = .1.7.1.0.3
                Setting description = "Calendar note date"
                Setting type	    = ASCII

                Setting ID          = .1.7.1.0.4
                Setting description = "Calendar note time"
                Setting type	    = ASCII

                Setting ID          = .1.7.1.0.5
                Setting description = "Calendar note alarm date"
                Setting type	    = ASCII

                Setting ID          = .1.7.1.0.6
                Setting description = "Calendar note alarm time"
                Setting type	    = ASCII

        Setting ID          = .1.7.2
        Setting description = "Clock display"
        Setting type	    = Integer16

        Setting ID          = .1.7.3
        Setting description = "Time format"
        Setting type	    = Integer16

        Setting ID          = .1.7.4
        Setting description = "Auto update of date and time"
        Setting type	    = Integer16

        Setting ID          = .1.7.5
        Setting description = "Alarm state"
        Setting type	    = Integer16

        Setting ID          = .1.7.6
        Setting description = "Alarm time"
        Setting type	    = ASCII

        Setting ID          = .1.7.7
        Setting description = "Alarm repeat"
        Setting type	    = Integer16

        Setting ID          = .1.7.8
        Setting description = "Alarm tone type state"
        Setting type	    = Integer16

        Setting ID          = .1.7.9
        Setting description = "Alarm tone type personal state"
        Setting type	    = Integer16

        Setting ID          = .1.7.10
        Setting description = "Calendar note tone type"
        Setting type	    = Integer16

        Setting ID          = .1.7.11
        Setting description = "Calendar note tone"
        Setting type	    = Integer16

    Group ID          = .1.8
    Group Description = Call management

        Setting ID          = .1.8.1
        Setting description = "PLMN selection mode"
        Setting type	    = Integer16

        Setting ID          = .1.8.2
        Setting description = "Voice mailbox number - PRI 433"
        Setting type	    = ASCII
        Setting Editor	    = @P

        Setting ID          = .1.8.4
        Setting description = "Send caller identity switch (CLIR switch)"
        Setting type	    = Integer16

        Setting ID          = .1.8.8
        Setting description = "Automatic redial switch"
        Setting type	    = Integer16

        Table ID          = .1.8.10
        Table Description = Calling Cards
        Table Range       = 1, 4

            Index Description = Card Index
            Index ID          = .1.8.10.x

                Setting ID          = .1.8.10.1.1
                Setting description = "Name"
                Setting type	    = Unicode

                Setting ID          = .1.8.10.1.2
                Setting description = "Access"
                Setting type	    = ASCII

                Setting ID          = .1.8.10.1.3
                Setting description = "ID"
                Setting type	    = ASCII

                Setting ID          = .1.8.10.1.4
                Setting description = "Prefix"
                Setting type	    = ASCII

                Setting ID          = .1.8.10.1.5
                Setting description = "Sequence"
                Setting type	    = Integer16
                Setting Editor	    = Range["Access nr, phone nr, card nr.", "Access nr, card nr, phone nr.", "Prefix, phone nr, card nr."]

            Setting ID          = .1.8.10.100
            Setting description = "Selected Card"
            Setting type	    = Integer16
            Setting Editor	    = Range[None=255, 1-4]

        Setting ID          = .1.8.21
        Setting description = "Voice Mail Box Options - PRI 260"
        Setting type	    = Integer16
        Setting Editor	    = Range[Blank, Dedicated VMN, MIN, MDN, MIN+1, MDN+1, MDN with User Customizability, MDN+1 with User Customizability] @P

        Setting ID          = .1.8.22
        Setting description = "Display MDN/Emergency Number During Emergency Call - PRI 682"
        Setting type	    = Integer16
        Setting Editor	    = Range[MDN, Emergency Number]

        Setting ID          = .1.8.23
        Setting description = "Display Talkzone/Mobile Text During Call - PRI 243"
        Setting type	    = Integer16
        Setting Editor	    = Range[Disable, Enable]

        Setting ID          = .1.8.24
        Setting description = "Allow Service Numbers to be Dialed while Phone Lock Active - PRI 507"
        Setting type	    = Integer16
        Setting Editor	    = Range[Disable, Enable]

    Group ID          = .1.9
    Group Description = Config

        Setting ID          = .1.9.1
        Setting description = "Menu language switch - PRI 231"
        Setting type	    = Integer16
        Setting Editor	    = Range[English (American)=35, French=38, Spanish=36, Portuguese=37, Hebrew=25, Chinese (Simplified)=22, Chinese (Traditional)=23, English (British)=1, Russian=15, Hindi (Indian)=41, Bahasa (Indonesia)=17, Thai=33, Vietnamese=34, Tagalog (Philippines)=40, Arabic=16, Marathi (Indian)=55, Gujarati (Indian)=56, Bengali (Indian)=57, Tamil (Indian)=54] @B@P

        Setting ID          = .1.9.2
        Setting description = "Startup tone state"
        Setting type	    = Integer16

    Group ID          = .1.14
    Group Description = Games

        Setting ID          = .1.14.1
        Setting description = "Light"
        Setting type	    = Integer16

        Setting ID          = .1.14.2
        Setting description = "Sound"
        Setting type	    = Integer16

        Setting ID          = .1.14.3
        Setting description = "Vibra"
        Setting type	    = Integer16

    Group ID          = .1.16
    Group Description = SIM ATK

        Setting ID          = .1.16.1
        Setting description = "SIM service actions confirmation switch"
        Setting type	    = Integer16

    Group ID          = .1.17
    Group Description = Voicedial etc.

        Setting ID          = .1.17.1
        Setting description = "Exchange rate (used in the calculator)"
        Setting type	    = ASCII

        Setting ID          = .1.17.2
        Setting description = "Daily spreadsheet"
        Setting type	    = Binary

        Setting ID          = .1.17.3
        Setting description = "Monthly spreadsheet"
        Setting type	    = Binary

    Group ID          = .1.20
    Group Description = Security

        Setting ID          = .1.20.1
        Setting description = "Security level"
        Setting type	    = Integer16

    Group ID          = .1.22
    Group Description = Radio

        Setting ID          = .1.22.1
        Setting description = "Audio Mode"
        Setting type	    = Integer16

        Group ID          = .1.22.3
        Group Description = FM Radio

            Setting ID          = .1.22.3.1
            Setting description = "Last Station"
            Setting type	    = Integer16

            Setting ID          = .1.22.3.2
            Setting description = "Last Name"
            Setting type	    = Unicode

            Table ID          = .1.22.3.3
            Table Description = FM Presets
            Table Range       = 1, 10

                Index Description = FM Presets index
                Index ID          = .1.22.3.3.x

                    Setting ID          = .1.22.3.3.1.1
                    Setting description = "Preset Name"
                    Setting type	    = Unicode

                    Setting ID          = .1.22.3.3.1.2
                    Setting description = "Frequency (kHz)"
                    Setting type	    = Integer32

    Table ID          = .1.23
    Table Description = NAI pool data
    Table Range       = 0, 101

        Index Description = Pool index
        Index ID          = .1.23.x

            Setting ID          = .1.23.0.1
            Setting description = "Pool data"
            Setting type	    = Binary

    Group ID          = .1.24
    Group Description = Converter

        Table ID          = .1.24.1
        Table Description = My Converter
        Table Range       = 0, 5

            Index Description = My Converter index
            Index ID          = .1.24.1.x

                Setting ID          = .1.24.1.0.1
                Setting description = "My Converter title"
                Setting type	    = Unicode

                Setting ID          = .1.24.1.0.2
                Setting description = "My Converter from name"
                Setting type	    = Unicode

                Setting ID          = .1.24.1.0.3
                Setting description = "My Converter to name"
                Setting type	    = Unicode

                Setting ID          = .1.24.1.0.4
                Setting description = "My Converter factor"
                Setting type	    = Unicode

Group ID          = .2
Group Description = Core

    Group ID          = .2.1
    Group Description = Basic phone information

        Setting ID          = .2.1.1
        Setting description = "Phone SW version etc."
        Setting type	    = ASCII
        Setting Editor	    = Hidden

        Setting ID          = .2.1.20
        Setting description = "PRI Version String - PRI 247"
        Setting type	    = ASCII

        Setting ID          = .2.1.21
        Setting description = "PRI File Name - PRI 487"
        Setting type	    = ASCII

    Group ID          = .2.3
    Group Description = Tuning Parameters

        Group ID          = .2.3.1
        Group Description = Audio EQ

            Setting ID          = .2.3.1.1
            Setting description = "Handportable CDMA Earpiece Equalizer Coefficients - PRI 736"
            Setting type	    = Integer16
            Setting Editor	    = List[31]

            Setting ID          = .2.3.1.2
            Setting description = "Handportable CDMA Microphone Equalizer Coefficients - PRI 737"
            Setting type	    = Integer16
            Setting Editor	    = List[17]

            Setting ID          = .2.3.1.3
            Setting description = "Universal Headset CDMA Earpiece Equalizer Coefficients - PRI 740"
            Setting type	    = Integer16
            Setting Editor	    = List[31]

            Setting ID          = .2.3.1.4
            Setting description = "Universal Headset CDMA Microphone Equalizer Coefficients - PRI 741"
            Setting type	    = Integer16
            Setting Editor	    = List[17]

Group ID          = .3
Group Description = Protocol

    Table ID          = .3.1
    Table Description = NAM Settings
    Table Range       = 1, 1

        Index Description = NAM
        Index ID          = .3.1.x

            Setting ID          = .3.1.1.1
            Setting description = "Mobile Directory Number (MDN) - PRI 152, 171"
            Setting type	    = ASCII
            Setting Editor	    = @B@P

            Setting ID          = .3.1.1.2
            Setting description = "Mobile Identification Number (MIN) - PRI 156, 175"
            Setting type	    = ASCII
            Setting Editor	    = @B@P

            Setting ID          = .3.1.1.3
            Setting description = "A-key code - PRI 439, 489"
            Setting type	    = Integer16
            Setting Editor	    = Range[Default A-key, Random A-key, Same as NAM 1] @B

            Setting ID          = .3.1.1.4
            Setting description = "Alpha Tag - PRI 918, 919"
            Setting type	    = Unicode
            Setting Editor	    = Length[20] @B@L

            Setting ID          = .3.1.1.5
            Setting description = "Emergency Numbers - PRI 157, 176"
            Setting type	    = ASCII
            Setting Editor	    = BCDList[10, 8] @P

            Setting ID          = .3.1.1.6
            Setting description = "Service Numbers - PRI 158, 177"
            Setting type	    = ASCII
            Setting Editor	    = BCDList[5, 11] @P

            Group ID          = .3.1.1.7
            Group Description = CDMA Settings

                Setting ID          = .3.1.1.7.1
                Setting description = "Primary CDMA Channel A Band - PRI 159, 178"
                Setting type	    = Integer16
                Setting Editor	    = @P

                Setting ID          = .3.1.1.7.2
                Setting description = "Secondary CDMA Channel A Band - PRI 161, 180"
                Setting type	    = Integer16
                Setting Editor	    = @P

                Setting ID          = .3.1.1.7.3
                Setting description = "Primary CDMA Channel B Band - PRI 160, 179"
                Setting type	    = Integer16
                Setting Editor	    = @P

                Setting ID          = .3.1.1.7.4
                Setting description = "Secondary CDMA Channel B Band - PRI 162, 181"
                Setting type	    = Integer16
                Setting Editor	    = @P

            Group ID          = .3.1.1.8
            Group Description = SID/NID Lists

                Setting ID          = .3.1.1.8.1
                Setting description = "Home SID - PRI 154, 173"
                Setting type	    = Binary
                Setting Editor	    = List[20] @B@P

                Setting ID          = .3.1.1.8.2
                Setting description = "Home NID - PRI 153, 172"
                Setting type	    = Binary
                Setting Editor	    = List[20] @B@P

                Setting ID          = .3.1.1.8.3
                Setting description = "Preferred SIDs - PRI 67, 69"
                Setting type	    = Binary
                Setting Editor	    = List[80] @B@P

                Setting ID          = .3.1.1.8.4
                Setting description = "Preferred NIDs - PRI 502, 504"
                Setting type	    = Binary
                Setting Editor	    = List[80] @B@P

                Setting ID          = .3.1.1.8.5
                Setting description = "Forbidden SIDs - PRI 66, 68"
                Setting type	    = Binary
                Setting Editor	    = List[10] @B@P

                Setting ID          = .3.1.1.8.6
                Setting description = "Forbidden NIDs - PRI 501, 503"
                Setting type	    = Binary
                Setting Editor	    = List[10] @B@P

                Setting ID          = .3.1.1.8.7
                Setting description = "Country Code - PRI 151, 170"
                Setting type	    = Integer16
                Setting Editor	    = @P

                Setting ID          = .3.1.1.8.8
                Setting description = "Network Code - PRI 155, 174"
                Setting type	    = Integer16
                Setting Editor	    = @P

            Group ID          = .3.1.1.9
            Group Description = Other Settings

                Setting ID          = .3.1.1.9.1
                Setting description = "Access Overload Class (ACCOLC) - PRI 146, 165"
                Setting type	    = Integer16
                Setting Editor	    = @P

                Setting ID          = .3.1.1.9.4
                Setting description = "NAM x Slot Cycle Index - PRI 680, 677"
                Setting type	    = Integer16
                Setting Editor	    = @L

                Setting ID          = .3.1.1.9.5
                Setting description = "NAM x Status - PRI 672, 673"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable] @L

        Group ID          = .3.1.9
        Group Description = NAM Programming Features

            Setting ID          = .3.1.9.1
            Setting description = "ACCOLC Updated by MIN Change - PRI 486"
            Setting type	    = Integer16
            Setting Editor	    = Range[Not Update, Update]

            Setting ID          = .3.1.9.3
            Setting description = "Set MDN/MIN Equal Feature - PRI 488"
            Setting type	    = Integer16
            Setting Editor	    = Range[MDN not equal to MIN, MDN equal to MIN, Set MIN equal to MDN, Set MIN equal to MDN if MCC = 0 or 310 and MNC = 0]

        Group ID          = .3.1.10
        Group Description = NAM Programming Menu

            Setting ID          = .3.1.10.1
            Setting description = "NAM Programming Access Options - PRI 631"
            Setting type	    = Integer16
            Setting Editor	    = Range[Accept *3001#12345# as the only access code, All access codes rejected and application not launched]

            Setting ID          = .3.1.10.2
            Setting description = "ACCOLC Menu - PRI 633"
            Setting type	    = Integer16
            Setting Editor	    = Range[Excluded, Included]

            Setting ID          = .3.1.10.3
            Setting description = "Alpha Tag Menu - PRI 102"
            Setting type	    = Integer16
            Setting Editor	    = Range[Excluded, Included]

        Group ID          = .3.1.11
        Group Description = NAM Programming Menu Features

            Setting ID          = .3.1.11.3
            Setting description = "CDMA SID/NID Lists Menu Option in Long NAM Programming - PRI 640"
            Setting type	    = Integer16
            Setting Editor	    = Range[Excluded, Included]

    Group ID          = .3.2
    Group Description = Mobile Provisioning (OTASP/OTAPA)

        Group ID          = .3.2.3
        Group Description = OTAPA Menu

            Setting ID          = .3.2.3.2
            Setting description = "Automatic update of service (OTAPA) Menu Status - PRI 922"
            Setting type	    = Integer16
            Setting Editor	    = Range[Default setting not yet applied, Default setting applied]

    Group ID          = .3.3
    Group Description = System Selection

        Group ID          = .3.3.1
        Group Description = UI & Menu Features

            Group ID          = .3.3.1.1
            Group Description = System Menu

                Group ID          = .3.3.1.1.1
                Group Description = Single Menu

                    Setting ID          = .3.3.1.1.1.1
                    Setting description = "Automatic Menu Option - PRI 650"
                    Setting type	    = Integer16
                    Setting Editor	    = Range[Excluded, Included]

                    Setting ID          = .3.3.1.1.1.2
                    Setting description = "Home only Menu Option - PRI 657"
                    Setting type	    = Integer16
                    Setting Editor	    = Range[Excluded, Included]

                    Setting ID          = .3.3.1.1.1.6
                    Setting description = "Network Menu Default Setting - PRI 748"
                    Setting type	    = Integer16
                    Setting Editor	    = Range[Automatic, Automatic A, Automatic B, Home only, IS95 Per Call=6, Digital Only]

        Group ID          = .3.3.2
        Group Description = Miscellaneous UI Features

            Setting ID          = .3.3.2.1
            Setting description = "Confirmation Tone for Acquisition of Roaming System - PRI 78"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.3.2.2
            Setting description = "Standard/Non-Standard Enhanced Roaming Indicator Options - PRI 368"
            Setting type	    = Integer16
            Setting Editor	    = Range[None, Verizon, Sprint, Alltel]

            Setting ID          = .3.3.2.3
            Setting description = "Short Distance Coverage Area (SDCA) Feature - PRI 935"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

        Group ID          = .3.3.3
        Group Description = System Selection Features

            Group ID          = .3.3.3.1
            Group Description = Better Service Rescan (BSR)

                Group ID          = .3.3.3.1.1
                Group Description = BSR Settings

                    Setting ID          = .3.3.3.1.1.1
                    Setting description = "Acquire More/Most Preferred System in Another GEO during BSR - PRI 606"
                    Setting type	    = Integer16
                    Setting Editor	    = Range[Disabled, More Preferred, Most Preferred]

                    Setting ID          = .3.3.3.1.1.2
                    Setting description = "Maximum Number of Better Service Rescans While on Current System - PRI 626"
                    Setting type	    = Integer16

                    Setting ID          = .3.3.3.1.1.3
                    Setting description = "Allow Acquisition of Wildcard Systems during BSR - PRI 618"
                    Setting type	    = Integer16
                    Setting Editor	    = Range[Disable, Enable]

                    Setting ID          = .3.3.3.1.1.4
                    Setting description = "GEO Hopping during BSR - Non-Home System to Home System - PRI 617"
                    Setting type	    = Integer16
                    Setting Editor	    = Range[Disable, Enable]

                Group ID          = .3.3.3.1.2
                Group Description = Microscan Settings

                    Setting ID          = .3.3.3.1.2.1
                    Setting description = "Allow Channel Repetition During Microscan - PRI 624"
                    Setting type	    = Integer16
                    Setting Editor	    = Range[Disable, Enable]

                    Setting ID          = .3.3.3.1.2.2
                    Setting description = "Maximum Number of Channels per Better Service Rescan - PRI 396"
                    Setting type	    = Integer16

                    Setting ID          = .3.3.3.1.2.3
                    Setting description = "Maximum Number of Channels per Better Service Rescan Options - PRI 627"
                    Setting type	    = Integer16
                    Setting Editor	    = Range[Less Preferred System, Non-Preferred System, Less & Non-Preferred System]

                Group ID          = .3.3.3.1.3
                Group Description = BSR Timers

                    Setting ID          = .3.3.3.1.3.1
                    Setting description = "Better Service Rescan Low Timer for CDMA Systems - PRI 758"
                    Setting type	    = Integer16

                    Setting ID          = .3.3.3.1.3.2
                    Setting description = "Better Service Rescan High Timer for CDMA Systems - PRI 759"
                    Setting type	    = Integer16

                    Setting ID          = .3.3.3.1.3.3
                    Setting description = "Better Service Rescan High Timer in Seconds After Call Release - PRI 610"
                    Setting type	    = Integer16

            Group ID          = .3.3.3.2
            Group Description = Silent Retry

                Setting ID          = .3.3.3.2.1
                Setting description = "Delay Between Attempts while in Silent Retry Mode Timer - PRI 132"
                Setting type	    = Integer16

                Setting ID          = .3.3.3.2.2
                Setting description = "Silent Retry Configuration - PRI 431"
                Setting type	    = Integer16
                Setting Editor	    = Range[<Reserved>, More Preferred, Less Preferred, Same System, Same System + Delay Timer]

            Group ID          = .3.3.3.3
            Group Description = Miscellaneous Features

                Setting ID          = .3.3.3.3.1
                Setting description = "Addition of PCS/CDMA Channels to RCL Options - PRI 405"
                Setting type	    = Integer16
                Setting Editor	    = Range[Algorithm Zero, Algorithm One]

                Setting ID          = .3.3.3.3.2
                Setting description = "Cross Pollination  - PRI 752"
                Setting type	    = Integer16
                Setting Editor	    = Range[Cross Pollination Disabled (no additional criteria applied), Cross Pollination Enabled, Cross Pollination Disabled (excact match criteria applied) ]

                Setting ID          = .3.3.3.3.3
                Setting description = "GEO Confinement through Negative System Detection - PRI 418"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .3.3.3.3.4
                Setting description = "GEO Scan List Options when System Loss Occurs - PRI 603"
                Setting type	    = Integer16
                Setting Editor	    = Range[Five-ping channel excluded, Five-ping channel included]

                Setting ID          = .3.3.3.3.5
                Setting description = "GSRM/Redirection Message (Ping-Pong) Feature - PRI 756"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disabled, Algorithm One, Algorithm Two]

                Setting ID          = .3.3.3.3.6
                Setting description = "Scan Second RCL Channel After Call Release - PRI 607"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .3.3.3.3.7
                Setting description = "Scan Second RCL Channel First during BSR - PRI 394"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .3.3.3.3.8
                Setting description = "Threshold Level for Acquisition of CDMA Systems after Scanning Entire PRL & NAM - PRI 417"
                Setting type	    = Integer16
                Setting Editor	    = Range[<reserved>, Excact SID/Excact NID, Exact SID/Wildcard NID, Wildcard SID/Exact NID, Wildcard SID/Wildcard NID]

                Setting ID          = .3.3.3.3.9
                Setting description = "Use CDMA Home SID/NID List for System Acquisition & Override Roaming Indicator Feature - PRI 757"
                Setting type	    = Integer16
                Setting Editor	    = Range[Acquire systems only listed in PRL, Override PRL roaming indicator only, Acquire systems if PREF_ONLY is F & Override PRL roaming indicator, Acquire systems regardless of PREF_ONLY configuration & Override PRL roaming indicator]

                Setting ID          = .3.3.3.3.10
                Setting description = "Add Primary Cellular Channel to All Scan Lists - PRI 601"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .3.3.3.3.11
                Setting description = "Ignore Comparison of Expected/Acquired NID When Wildcard SID - PRI 629"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disabled, Ignore Expected NID if GSRM contains Wildcard SID, Ignore Expected SID/NID Pair Confirmation]

                Setting ID          = .3.3.3.3.12
                Setting description = "Primary CDMA Channel Preferred over Secondary Channel - ER Mode - PRI 397"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .3.3.3.3.13
                Setting description = "Addition of Channels to RCL - PRI 404"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

        Group ID          = .3.3.4
        Group Description = System Selection Counters

            Setting ID          = .3.3.4.1
            Setting description = "Out of Range Low Timer for SSPR Mode Iteration Counter - PRI 389"
            Setting type	    = Integer16

        Group ID          = .3.3.5
        Group Description = System Selection Timers

            Setting ID          = .3.3.5.1
            Setting description = "CDMA Call Release/System Lost Reacquisition Period - PRI 375"
            Setting type	    = Integer16

            Setting ID          = .3.3.5.2
            Setting description = "Out of Range Low Timer in Seconds for SSPR Mode - PRI 377"
            Setting type	    = Integer16

            Setting ID          = .3.3.5.3
            Setting description = "Out of Range High Timer in Seconds for SSPR Mode - PRI 379"
            Setting type	    = Integer16

        Group ID          = .3.3.6
        Group Description = SSPR Specific Features

            Setting ID          = .3.3.6.1
            Setting description = "Addition of Channels for Non-Preferred Systems to RCL - PRI 608"
            Setting type	    = Integer16
            Setting Editor	    = Range[Never Add to RCL, Always Add to RCL, "If Registration Successful, Add to RCL"]

            Setting ID          = .3.3.6.2
            Setting description = "Acquire Non-Preferred Systems Immediately - PRI 411"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.3.6.3
            Setting description = "Better Service Rescan High Timer in Secs for Non-Pref Systems - PRI 614"
            Setting type	    = Integer16

            Setting ID          = .3.3.6.4
            Setting description = "Better Service Rescan Scan List for Non-Preferred Systems - PRI 615"
            Setting type	    = Integer16
            Setting Editor	    = Range[Miscellaneous Scan List (Last channel at end only), Power-up Scan List]

            Setting ID          = .3.3.6.5
            Setting description = "CDMA Call Release/Digital System Lost Re-acq Period - PRI 613"
            Setting type	    = Integer16

            Setting ID          = .3.3.6.6
            Setting description = "CDMA Digital System Lost Re-acq Options for Non-Pref Systems - PRI 619"
            Setting type	    = Integer16
            Setting Editor	    = Range[Scan Lost Channel Periodically, Do Not Scan Last Channel, Scan Last Channel at the End]

            Setting ID          = .3.3.6.7
            Setting description = "GEO-confinement due to Negative System Detection Counter - PRI 390"
            Setting type	    = Integer16

            Setting ID          = .3.3.6.8
            Setting description = "GEO Hopping during BSR - SID/NID Match Priority Preferred Over GEO Priority - PRI 753"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.3.6.9
            Setting description = "Ignore Out of Range State if Mobile is Charging - PRI 621"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.3.6.10
            Setting description = "Maximum Time for Power-up Scan Timer - PRI 382"
            Setting type	    = Integer16

            Setting ID          = .3.3.6.11
            Setting description = "Multiple Non-Preferred Systems Preference Options - PRI 605"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disabled, Enabled]

            Setting ID          = .3.3.6.12
            Setting description = "Multiple Non-Preferred Systems (Same Band/Type) Acq Options - PRI 604"
            Setting type	    = Integer16
            Setting Editor	    = Range[Initial Non-Preferred System, Most Recent Non-Preferred System]

            Setting ID          = .3.3.6.13
            Setting description = "Negative System Acquisition Options - PRI 602"
            Setting type	    = Integer16
            Setting Editor	    = Range[Emergency Calls Only, All Calls]

            Setting ID          = .3.3.6.20
            Setting description = "Inclusion of SSPR Menu via *#PRLSET# - PRI 258"
            Setting type	    = Integer16
            Setting Editor	    = Range[Excluded, Included]

        Group ID          = .3.3.7
        Group Description = ER Specific Features

            Setting ID          = .3.3.7.1
            Setting description = "Enhanced Roaming Mode - PRI 398"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.3.7.2
            Setting description = "Non-Preferred System Acceptance while in ER Mode - PRI 422"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

    Group ID          = .3.4
    Group Description = Call Processing (Voice & Data)

        Group ID          = .3.4.1
        Group Description = Call Processing (Voice) Menu Options

            Group ID          = .3.4.1.1
            Group Description = Network Service Menu

                Setting ID          = .3.4.1.1.1
                Setting description = "Call Forwarding for Forward all calls Activate Feature Code (NAM 1) - PRI 79"
                Setting type	    = ASCII

                Setting ID          = .3.4.1.1.2
                Setting description = "Call Forwarding for Forward all calls Cancel Feature Code (NAM 1) - PRI 65"
                Setting type	    = ASCII

                Setting ID          = .3.4.1.1.6
                Setting description = "Voice Privacy Menu - PRI 185"
                Setting type	    = Integer16
                Setting Editor	    = Range["VP Menu Not Included, Feature Off", "VP Menu Not Included, Feature On", "VP Menu Included, Feature Off", "VP Menu Included, Feature On"]

                Setting ID          = .3.4.1.1.7
                Setting description = "Call Forwarding divert if busy activate - PRI 1283"
                Setting type	    = ASCII

                Setting ID          = .3.4.1.1.8
                Setting description = "Call Forwarding divert if busy cancel - PRI 1284"
                Setting type	    = ASCII

                Setting ID          = .3.4.1.1.9
                Setting description = "Call Forwarding divert if not answered activate - PRI 1285"
                Setting type	    = ASCII

                Setting ID          = .3.4.1.1.10
                Setting description = "Call Forwarding divert if not answered cancel - PRI 1286"
                Setting type	    = ASCII

                Setting ID          = .3.4.1.1.11
                Setting description = "Call Forwarding call waiting activate- PRI 1287"
                Setting type	    = ASCII

                Setting ID          = .3.4.1.1.12
                Setting description = "Call Forwarding call waiting cancel- PRI 1288"
                Setting type	    = ASCII

                Setting ID          = .3.4.1.1.13
                Setting description = "Call Forwarding if out of reach activate- PRI 440"
                Setting type	    = ASCII

                Setting ID          = .3.4.1.1.14
                Setting description = "Call Forwarding if out of reach cancel- PRI 441"
                Setting type	    = ASCII

                Setting ID          = .3.4.1.1.15
                Setting description = "Read & write via mobile phone's native memory or RUIM card- PRI 442"
                Setting type	    = Integer16

            Group ID          = .3.4.1.2
            Group Description = Touch Tones Menu

                Setting ID          = .3.4.1.2.1
                Setting description = "Manual Touch Tones - PRI 126"
                Setting type	    = Integer16
                Setting Editor	    = Range[Off, Fixed, Continuous]

                Setting ID          = .3.4.1.2.2
                Setting description = "Touch Tone Length - PRI 134"
                Setting type	    = Integer16
                Setting Editor	    = Range[Short, Long]

            Setting ID          = .3.4.1.11
            Setting description = "Call Timer Options - PRI 642"
            Setting type	    = Integer16
            Setting Editor	    = Range[Off, On]

        Group ID          = .3.4.2
        Group Description = Call Processing (Voice) Features

            Group ID          = .3.4.2.1
            Group Description = EVRC

                Setting ID          = .3.4.2.1.1
                Setting description = "EVRC On/HomeOnly/Off for Call Origination - PRI 402"
                Setting type	    = Integer16
                Setting Editor	    = Range[<reserved>, EVRC On, EVRC Off, EVRC Home Only] @L

                Setting ID          = .3.4.2.1.2
                Setting description = "Inclusion of EVRC Menu for Call Origination via *#EVRC# - PRI 92"
                Setting type	    = Integer16
                Setting Editor	    = Range[Diable, Enable]

            Group ID          = .3.4.2.2
            Group Description = Generic Features

                Setting ID          = .3.4.2.2.1
                Setting description = "Call Rejection Feature - PRI 878"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .3.4.2.2.2
                Setting description = "Send Empty Flash Prior to Making Three-way Call Attempt - PRI 711"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .3.4.2.2.3
                Setting description = "Send Digits in Buffer when Answering Call Waiting/Three-way Call - PRI 932"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .3.4.2.2.5
                Setting description = "Display of In-Service Indicators during Initial BSR - PRI 609"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

                Setting ID          = .3.4.2.2.6
                Setting description = "Display of In-Service Indicators for Non-Pref System Detection - PRI 616"
                Setting type	    = Integer16
                Setting Editor	    = Range[Disable, Enable]

    Group ID          = .3.5
    Group Description = Internet Protocol (IP)

        Group ID          = .3.5.5
        Group Description = DNS Parameters

            Setting ID          = .3.5.5.1
            Setting description = "DNS Retry Attempts Counter - PRI 936"
            Setting type	    = Integer16

            Setting ID          = .3.5.5.2
            Setting description = "DNS Retry Attempt Interval - PRI 937"
            Setting type	    = Integer16

    Group ID          = .3.6
    Group Description = Miscellaneous

        Group ID          = .3.6.1
        Group Description = Field Performance

            Setting ID          = .3.6.1.2
            Setting description = "Report Pilot Phase Referenced to Lead Finger - PRI 1317"
            Setting type	    = Integer16
            Setting Editor	    = Range[Report pilot phase referenced to mobile's system time, Report pilot phase referenced to earliest arriving multipath]

        Group ID          = .3.6.2
        Group Description = R-UIM

            Setting ID          = .3.6.2.1
            Setting description = "Non-standard Datang R-UIM Feature - PRI 1059"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

    Group ID          = .3.100
    Group Description = R&D

        Group ID          = .3.100.1
        Group Description = IS-2000 Features

            Setting ID          = .3.100.1.1
            Setting description = "Access Handoff Feature Support - PRI 493"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.2
            Setting description = "Access Probe Handoff Feature Support - PRI 492"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.3
            Setting description = "Mobile Assisted Hard Handoff Feature Support - PRI 496"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.4
            Setting description = "NDSS Feature Support - PRI 491"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.5
            Setting description = "Nokia Proprietary Access Handoff - PRI 110"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.6
            Setting description = "Nokia Proprietary PSMM Message Handling - PRI 109"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.7
            Setting description = "Pilot Ec/Io Threshold for Pseudo Pilot Acquisition Feature - PRI 881"
            Setting type	    = Integer16

            Setting ID          = .3.100.1.8
            Setting description = "Pilot Power Threshold for Pseudo Pilot Acquisition Feature - PRI 882"
            Setting type	    = Integer16

            Setting ID          = .3.100.1.9
            Setting description = "Quick Paging Channel (IS-2000) Feature Support - PRI 495"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.10
            Setting description = "R_FCH 1/8 Rate Gating Feature Support - PRI 76"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.11
            Setting description = "Signaling Message Encryption Feature Support - PRI 494"
            Setting type	    = Integer16
            Setting Editor	    = Range[Basic Encryption only, Basic & Enhanced Encryption]

            Setting ID          = .3.100.1.12
            Setting description = "Slotted Timer Feature Support - PRI 497"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.13
            Setting description = "SR_ID Patch - PRI 446"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.14
            Setting description = "Status Response Patch - PRI 447"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.1.15
            Setting description = "TMSI Feature Support - PRI 490"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

        Group ID          = .3.100.2
        Group Description = Service Options

            Setting ID          = .3.100.2.2
            Setting description = "Service Option 2 - PRI 573"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.3
            Setting description = "Service Option 3 - PRI 574"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.4
            Setting description = "Service Option 4 - PRI 575"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.5
            Setting description = "Service Option 5 - PRI 576"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.6
            Setting description = "Service Option 6 - PRI 577"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.7
            Setting description = "Service Option 7 - PRI 578"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.9
            Setting description = "Service Option 9 - PRI 579"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.12
            Setting description = "Service Option 12 - PRI 580"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.13
            Setting description = "Service Option 13 - PRI 581"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.14
            Setting description = "Service Option 14 - PRI 582"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.15
            Setting description = "Service Option 15 - PRI 583"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.17
            Setting description = "Service Option 17 - PRI 584"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.18
            Setting description = "Service Option 18 - PRI 585"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.19
            Setting description = "Service Option 19 - PRI 586"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.32
            Setting description = "Service Option 32 - PRI 587"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.33
            Setting description = "Service Option 33 - PRI 588"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.35
            Setting description = "Service Option 35 - PRI 589"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.36
            Setting description = "Service Option 36 - PRI 590"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.54
            Setting description = "Service Option 54 - PRI 591"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.55
            Setting description = "Service Option 55 - PRI 592"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.100
            Setting description = "Service Option 4100 - PRI 593"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.101
            Setting description = "Service Option 4101 - PRI 594"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.103
            Setting description = "Service Option 4103 - PRI 595"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.200
            Setting description = "Service Option 32768 - PRI 596"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.201
            Setting description = "Service Option 32798 - PRI 597"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.2.202
            Setting description = "Service Option 32799 - PRI 598"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

        Group ID          = .3.100.3
        Group Description = System Selection

            Setting ID          = .3.100.3.1
            Setting description = "Silent Retry Iteration Counter - PRI 432"
            Setting type	    = Integer16

            Setting ID          = .3.100.3.2
            Setting description = "Remain in Emergency Mode Timer - PRI 131"
            Setting type	    = Integer16

            Setting ID          = .3.100.3.3
            Setting description = "Better Service Rescan Low Timer Iteration Counter - PRI 385"
            Setting type	    = Integer16

            Setting ID          = .3.100.3.4
            Setting description = "Initial Better Service Rescan - PRI 392"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.3.5
            Setting description = "Threshold Level for CDMA System Acq Candidates in SSPR Mode - PRI 412"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disabled, Exact SID/Exact NID, Exact SID/Wildcard NID, Wildcard SID/Exact NID, Wildcard SID/Wildcard NID]

            Setting ID          = .3.100.3.6
            Setting description = "Maximum Time for Call Origination Attempt Timer - PRI 130"
            Setting type	    = Integer16

            Setting ID          = .3.100.3.7
            Setting description = "RSSI Update on User Interface Timer - PRI 383"
            Setting type	    = Integer16

        Group ID          = .3.100.5
        Group Description = Messaging

            Setting ID          = .3.100.5.1
            Setting description = "Mobile Originated Short Message Service Support - PRI 200"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.5.2
            Setting description = "Mobile Terminated Short Message Support - PRI 201"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.5.3
            Setting description = "Mobile Originated Wireless Messaging Teleservice Support - PRI 202"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.5.4
            Setting description = "Mobile Terminated Wireless Messaging Teleservice Support - PRI 205"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]

            Setting ID          = .3.100.5.5
            Setting description = "Mobile Terminated Wireless Paging Teleservice Support - PRI 206"
            Setting type	    = Integer16
            Setting Editor	    = Range[Disable, Enable]


;{ZQNGMFIGGJDJGNLEASDKAIKIMRGEENFHLLAGHJCM@LBPFLBEGQGRNPEKDSHN@IBEEI@REHLSLLGJLPDE@RIIGFJOMLCGJMAKL}