# name,element,offset,size,signed,[value]
[RF]
PA_TEMP_0,0,0,2,-
CDMA_RX_DC_OFFSET_I,0,1,2,-
CDMA_RX_DC_OFFSET_Q,0,2,2,-
CDMA_RX_BB_FILTER,0,3,2,-
AMPS_RX_DC_OFFSET_Q,0,4,2,-
AMPS_RX_DC_OFFSET_Q,0,5,2,- 
AMPS_RX_BB_FILTER,0,6,2,-
VCTCXO,0,7,2,-
TX_RF_AGC_0,0,8,2,-
TX_RF_AGC_1,0,9,2,-
TX_RF_AGC_2,0,10,2,-
TX_RF_AGC_3,0,11,2,-
TX_RF_AGC_4,0,12,2,-
TX_RF_AGC_5,0,13,2,-
TX_RF_AGC_6,0,14,2,-
TX_RF_AGC_7,0,15,2,-
TX_RF_AGC_8,0,16,2,- 
PA_GAIN_0,0,17,2,-
PA_GAIN_1,0,18,2,-
PA_GAIN_2,0,19,2,-
PA_GAIN_3,0,20,2,-
PA_GAIN_4,0,21,2,-
PA_GAIN_5,0,22,2,-
PA_GAIN_6,0,23,2,-
PA_GAIN_7,0,24,2,-
PA_GAIN_8,0,25,2,-
TX_IF_AGC_0,0,26,2,-
TX_IF_AGC_1,0,27,2,-
TX_IF_AGC_2,0,28,2,-
TX_IF_AGC_3,0,29,2,-
TX_IF_AGC_4,0,30,2,-
TX_IF_AGC_5,0,31,2,-
TX_IF_AGC_6,0,32,2,-
TX_IF_AGC_7,0,33,2,-
TX_IF_AGC_8,0,34,2,-
TX_IF_AGC_9,0,35,2,-
TX_IF_AGC_10,0,36,2,-
TX_IF_AGC_11,0,37,2,-
TX_IF_AGC_12,0,38,2,-
TX_IF_AGC_13,0,39,2,-
TX_IF_AGC_14,0,40,2,-
TX_IF_AGC_15,0,41,2,-
TX_IF_AGC_16,0,42,2,-
AMPS_TX_DC_OFFSET_0,0,43,2,-
AMPS_TX_DC_OFFSET_1,0,44,2,-
TX_PHASE_OFFSET_0,0,45,2,-
TX_AMP_BAL_0,0,46,2,-
TX_AMP_BAL_1,0,47,2,-
RX_IF_AGC_0,0,48,2,-
RX_IF_AGC_1,0,49,2,-
RX_IF_AGC_2,0,50,2,-
RX_IF_AGC_3,0,51,2,-
RX_IF_AGC_4,0,52,2,-
RX_IF_AGC_5,0,53,2,-
RX_IF_AGC_6,0,54,2,-
RX_IF_AGC_7,0,55,2,-
RX_IF_AGC_8,0,56,2,-
RX_IF_AGC_9,0,57,2,-
RX_IF_AGC_10,0,58,2,-
RX_IF_AGC_11,0,59,2,-
RX_IF_AGC_12,0,60,2,-
RX_IF_AGC_13,0,61,2,-
RX_IF_AGC_14,0,62,2,-
RX_IF_AGC_15,0,63,2,-
RX_IF_AGC_16,0,64,2,-
AMPS_LNA_GAIN_0,0,65,2,-
AMPS_LNA_GAIN_1,0,66,2,-
AMPS_LNA_GAIN_2,0,67,2,-
AMPS_LNA_GAIN_3,0,68,2,-
AMPS_LNA_GAIN_4,0,69,2,-
CDMA_PCS_LNA_GAIN_0,0,70,2,-
CDMA_PCS_LNA_GAIN_1,0,71,2,-
CDMA_PCS_LNA_GAIN_2,0,72,2,-
CDMA_PCS_LNA_GAIN_3,0,73,2,-
CDMA_PCS_LNA_GAIN_4,0,74,2,-
CDMA_CELL_LNA_GAIN_0,0,75,2,-
CDMA_CELL_LNA_GAIN_1,0,76,2,-
CDMA_CELL_LNA_GAIN_2,0,77,2,-
CDMA_CELL_LNA_GAIN_3,0,78,2,-
CDMA_CELL_LNA_GAIN_4,0,79,2,-
CDMA_TX_DC_OFFSET_0,0,80,2,-
CDMA_TX_DC_OFFSET_1,0,81,2,-
PCS_TX_POWER_DETECTOR_0,0,82,2,-
PCS_TX_POWER_DETECTOR_1,0,83,2,-
PCS_TX_POWER_DETECTOR_2,0,84,2,-
PCS_TX_POWER_DETECTOR_3,0,85,2,-
PCS_TX_POWER_DETECTOR_4,0,86,2,-
PCS_TX_POWER_DETECTOR_5,0,87,2,-
PCS_TX_POWER_DETECTOR_6,0,88,2,-
PCS_TX_POWER_DETECTOR_7,0,89,2,-
PCS_TX_POWER_DETECTOR_8,0,90,2,-
PCS_TX_POWER_DETECTOR_9,0,91,2,-
PCS_TX_POWER_DETECTOR_10,0,92,2,-
PCS_TX_POWER_DETECTOR_11,0,93,2,-
PCS_TX_POWER_DETECTOR_12,0,94,2,-
PCS_TX_POWER_DETECTOR_13,0,95,2,-
PCS_TX_POWER_DETECTOR_14,0,96,2,-
PCS_TX_POWER_DETECTOR_15,0,97,2,-
PCS_TX_POWER_DETECTOR_16,0,98,2,-
PCS_TX_POWER_DETECTOR_17,0,99,2,-
AMPS_TX_POWER_LEVEL_0,0,100,2,-
AMPS_TX_POWER_LEVEL_1,0,101,2,-
AMPS_TX_POWER_LEVEL_2,0,102,2,-
AMPS_TX_POWER_LEVEL_3,0,103,2,-
AMPS_TX_POWER_LEVEL_4,0,104,2,-
AMPS_TX_POWER_LEVEL_5,0,105,2,-
AMPS_TX_POWER_LEVEL_6,0,106,2,-
AMPS_TX_POWER_LEVEL_7,0,107,2,-
AMPS_TX_POWER_LEVEL_8,0,108,2,-
AMPS_TX_POWER_LEVEL_9,0,109,2,-
AMPS_TX_POWER_LEVEL_10,0,110,2,-
AMPS_TX_POWER_LEVEL_11,0,111,2,-
AMPS_TX_POWER_LEVEL_12,0,112,2,-
AMPS_TX_POWER_LEVEL_13,0,113,2,-
AMPS_TX_POWER_LEVEL_14,0,114,2,-
AMPS_TX_POWER_LEVEL_15,0,115,2,-
AMPS_TX_POWER_LEVEL_16,0,116,2,-
AMPS_TX_POWER_LEVEL_17,0,117,2,-
CDMA_CELL_TX_LIMIT_0,0,118,2,-
CDMA_CELL_TX_LIMIT_1,0,119,2,-
CDMA_CELL_TX_LIMIT_2,0,120,2,-
CDMA_PCS_TX_LIMIT_0,0,121,2,-
CDMA_PCS_TX_LIMIT_1,0,122,2,-
CDMA_PCS_TX_LIMIT_2,0,123,2,-
CDMA_CELL_PA_GAIN_COMP_GOffset_0,0,124,2,-
CDMA_CELL_PA_GAIN_COMP_PaCmp_0,0,125,2,-
CDMA_PCS_PA_GAIN_COMP_RdrvCmp_0,0,126,2,-
CDMA_PCS_PA_GAIN_COMP_GOffset_0,0,127,2,-
CDMA_PCS_PA_GAIN_COMP_PaCmp_0,0,128,2,-
AMPS_PA_GAIN_COMP_RdrvCmp_0,0,129,2,-
AMPS_PA_GAIN_COMP_GOffset_0,0,130,2,-
AMPS_PA_GAIN_COMP_PaCmp_0,0,131,2,-
AMPS_PA_GAIN_COMP_RdrvCmp_0,0,132,2,-
PCS_PA_GAIN_0,0,133,2,-
PCS_PA_GAIN_1,0,134,2,-
PCS_PA_GAIN_2,0,135,2,-
PCS_PA_GAIN_3,0,136,2,-
PCS_PA_GAIN_4,0,137,2,-
PCS_PA_GAIN_5,0,138,2,-
PCS_PA_GAIN_6,0,139,2,-
PCS_PA_GAIN_7,0,140,2,-
PCS_PA_GAIN_8,0,141,2,-
TX_CHANNEL_PCS_0,0,142,2,-
TX_CHANNEL_CELL_0,0,143,2,-
RX_CHANNEL_PCS_0,0,144,2,-
RX_CHANNEL_CELL_0,0,145,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_0,0,146,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_1,0,147,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_2,0,148,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_3,0,149,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_4,0,150,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_5,0,151,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_6,0,152,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_7,0,153,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_8,0,154,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_9,0,155,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_10,0,156,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_11,0,157,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_12,0,158,2,-
CDMA_CELL_TX_LIMIT_FREQ_COMP_13,0,159,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_0,0,160,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_1,0,161,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_2,0,162,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_3,0,163,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_4,0,164,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_5,0,165,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_6,0,166,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_7,0,167,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_8,0,168,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_9,0,169,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_10,0,170,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_11,0,171,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_12,0,172,2,-
CDMA_PCS_TX_LIMIT_FREQ_COMP_13,0,173,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_0,0,174,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_1,0,175,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_2,0,176,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_3,0,177,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_4,0,178,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_5,0,179,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_6,0,180,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_7,0,181,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_8,0,182,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_9,0,183,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_10,0,184,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_11,0,185,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_12,0,186,2,-
AMPS_TX_POWER_LEVEL_FREQ_COMP_13,0,187,2,-
CDMA_CELL_RX_OFFSET_FCOMP_0,0,188,2,-
CDMA_CELL_RX_OFFSET_FCOMP_1,0,189,2,-
CDMA_CELL_RX_OFFSET_FCOMP_2,0,190,2,-
CDMA_CELL_RX_OFFSET_FCOMP_3,0,191,2,-
CDMA_CELL_RX_OFFSET_FCOMP_4,0,192,2,-
CDMA_CELL_RX_OFFSET_FCOMP_5,0,193,2,-
CDMA_CELL_RX_OFFSET_FCOMP_6,0,194,2,-
CDMA_CELL_RX_OFFSET_FCOMP_7,0,195,2,-
CDMA_CELL_RX_OFFSET_FCOMP_8,0,196,2,-
CDMA_CELL_RX_OFFSET_FCOMP_9,0,197,2,-
CDMA_CELL_RX_OFFSET_FCOMP_10,0,198,2,-
CDMA_CELL_RX_OFFSET_FCOMP_11,0,199,2,-
CDMA_CELL_RX_OFFSET_FCOMP_12,0,200,2,-
CDMA_CELL_RX_OFFSET_FCOMP_13,0,201,2,-
CDMA_PCS_RX_OFFSET_FCOMP_0,0,202,2,-
CDMA_PCS_RX_OFFSET_FCOMP_1,0,203,2,-
CDMA_PCS_RX_OFFSET_FCOMP_2,0,204,2,-
CDMA_PCS_RX_OFFSET_FCOMP_3,0,205,2,-
CDMA_PCS_RX_OFFSET_FCOMP_4,0,206,2,-
CDMA_PCS_RX_OFFSET_FCOMP_5,0,207,2,-
CDMA_PCS_RX_OFFSET_FCOMP_6,0,208,2,-
CDMA_PCS_RX_OFFSET_FCOMP_7,0,209,2,-
CDMA_PCS_RX_OFFSET_FCOMP_8,0,210,2,-
CDMA_PCS_RX_OFFSET_FCOMP_9,0,211,2,-
CDMA_PCS_RX_OFFSET_FCOMP_10,0,212,2,-
CDMA_PCS_RX_OFFSET_FCOMP_11,0,213,2,-
CDMA_PCS_RX_OFFSET_FCOMP_12,0,214,2,-
CDMA_PCS_RX_OFFSET_FCOMP_13,0,215,2,-
TX_OFFSET_TEMP_STEP_0,0,216,2,-
RX_OFFSET_TEMP_STEP_0,0,217,2,-
RX_OFFSET_TCOMP_0,0,218,2,-
RX_OFFSET_TCOMP_1,0,219,2,-
RX_OFFSET_TCOMP_2,0,220,2,-
RX_OFFSET_TCOMP_3,0,221,2,-
RX_OFFSET_TCOMP_4,0,222,2,-
RX_OFFSET_TCOMP_5,0,223,2,-
RX_OFFSET_TCOMP_6,0,224,2,-
RX_OFFSET_TCOMP_7,0,225,2,-
RX_OFFSET_TCOMP_8,0,226,2,-
RX_OFFSET_TCOMP_9,0,227,2,-
RX_OFFSET_TCOMP_10,0,228,2,-
RX_OFFSET_TCOMP_11,0,229,2,-
CELL_TX_OFFSET_TCOMP_0,0,230,2,-
CELL_TX_OFFSET_TCOMP_1,0,231,2,-
CELL_TX_OFFSET_TCOMP_2,0,232,2,-
CELL_TX_OFFSET_TCOMP_3,0,233,2,-
CELL_TX_OFFSET_TCOMP_4,0,234,2,-
CELL_TX_OFFSET_TCOMP_5,0,235,2,-
CELL_TX_OFFSET_TCOMP_6,0,236,2,-
CELL_TX_OFFSET_TCOMP_7,0,237,2,-
CELL_TX_OFFSET_TCOMP_8,0,238,2,-
CELL_TX_OFFSET_TCOMP_9,0,239,2,-
CELL_TX_OFFSET_TCOMP_10,0,240,2,-
CELL_TX_OFFSET_TCOMP_11,0,241,2,-
PCS_TX_OFFSET_TCOMP_0,0,242,2,-
PCS_TX_OFFSET_TCOMP_1,0,243,2,-
PCS_TX_OFFSET_TCOMP_2,0,244,2,-
PCS_TX_OFFSET_TCOMP_3,0,245,2,-
PCS_TX_OFFSET_TCOMP_4,0,246,2,-
PCS_TX_OFFSET_TCOMP_5,0,247,2,-
PCS_TX_OFFSET_TCOMP_6,0,248,2,-
PCS_TX_OFFSET_TCOMP_7,0,249,2,-
PCS_TX_OFFSET_TCOMP_8,0,250,2,-
PCS_TX_OFFSET_TCOMP_9,0,251,2,-
PCS_TX_OFFSET_TCOMP_10,0,252,2,-
PCS_TX_OFFSET_TCOMP_11,0,253,2,-
TX_RF_AGC_ROBIN_D_0,0,254,2,- 
TX_RF_AGC_ROBIN_D_1,0,255,2,-
TX_RF_AGC_ROBIN_D_2,0,256,2,-
TX_RF_AGC_ROBIN_D_3,0,257,2,- 
TX_RF_AGC_ROBIN_D_4,0,258,2,- 
TX_RF_AGC_ROBIN_D_5,0,259,2,- 
TX_RF_AGC_ROBIN_D_6,0,260,2,- 
TX_RF_AGC_ROBIN_D_7,0,261,2,- 
TX_RF_AGC_ROBIN_D_8,0,262,2,- 
TX_RF_AGC_ROBIN_D_9,0,263,2,- 
TX_RF_AGC_ROBIN_D_10,0,264,2,-
PCS_TX_RF_0,0,265,2,-
PCS_TX_RF_1,0,266,2,-
PCS_TX_RF_2,0,267,2,-
PCS_TX_RF_3,0,268,2,-
PCS_TX_RF_4,0,269,2,-
PCS_TX_RF_5,0,270,2,-
PCS_TX_RF_6,0,271,2,-
PCS_TX_RF_7,0,272,2,-
PCS_TX_RF_8,0,273,2,-
PCS_TX_RF_9,0,274,2,-
PCS_TX_RF_10,0,275,2,-
TUNE_CELL_TX_LIMIT_BOOST_0,0,276,2,-
TUNE_CELL_TX_LIMIT_BOOST_1,0,277,2,-
TUNE_CELL_TX_LIMIT_BOOST_2,0,278,2,-
TUNE_CELL_TX_LIMIT_BOOST_3,0,279,2,-
TUNE_CELL_TX_LIMIT_BOOST_4,0,280,2,-
TUNE_CELL_TX_LIMIT_BOOST_5,0,281,2,-
TUNE_CELL_TX_LIMIT_BOOST_6,0,282,2,-
TUNE_PCS_TX_LIMIT_BOOST_0,0,283,2,-
TUNE_PCS_TX_LIMIT_BOOST_1,0,284,2,-
TUNE_PCS_TX_LIMIT_BOOST_2,0,285,2,-
TUNE_PCS_TX_LIMIT_BOOST_3,0,286,2,-
TUNE_PCS_TX_LIMIT_BOOST_4,0,287,2,-
TUNE_PCS_TX_LIMIT_BOOST_5,0,288,2,-
TUNE_PCS_TX_LIMIT_BOOST_6,0,289,2,-
TUNE_CELL_TX_LO_PWR_FCOMP_0,0,290,2,-
TUNE_CELL_TX_LO_PWR_FCOMP_1,0,291,2,-
TUNE_CELL_TX_LO_PWR_FCOMP_2,0,292,2,-
TUNE_CELL_TX_LO_PWR_FCOMP_3,0,293,2,-
TUNE_CELL_TX_LO_PWR_FCOMP_4,0,294,2,-
TUNE_CELL_TX_LO_PWR_FCOMP_5,0,295,2,-
TUNE_CELL_TX_LO_PWR_FCOMP_6,0,296,2,-
TUNE_PCS_TX_LO_PWR_FCOMP_0,0,297,2,-
TUNE_PCS_TX_LO_PWR_FCOMP_1,0,298,2,-
TUNE_PCS_TX_LO_PWR_FCOMP_2,0,299,2,-
TUNE_PCS_TX_LO_PWR_FCOMP_3,0,300,2,-
TUNE_PCS_TX_LO_PWR_FCOMP_4,0,301,2,-
TUNE_PCS_TX_LO_PWR_FCOMP_5,0,302,2,-
TUNE_PCS_TX_LO_PWR_FCOMP_6,0,303,2,-
TUNE_CDMA_CELL_RX_OFFSET_FCOMP_H_0,0,304,2,-
TUNE_CDMA_CELL_RX_OFFSET_FCOMP_H_1,0,305,2,-
TUNE_CDMA_CELL_RX_OFFSET_FCOMP_H_2,0,306,2,-
TUNE_CDMA_CELL_RX_OFFSET_FCOMP_H_3,0,307,2,-
TUNE_CDMA_CELL_RX_OFFSET_FCOMP_H_4,0,308,2,-
TUNE_CDMA_CELL_RX_OFFSET_FCOMP_H_5,0,309,2,-
TUNE_CDMA_CELL_RX_OFFSET_FCOMP_H_6,0,310,2,-
TUNE_CDMA_PCS_RX_OFFSET_FCOMP_H_0,0,311,2,-
TUNE_CDMA_PCS_RX_OFFSET_FCOMP_H_1,0,312,2,-
TUNE_CDMA_PCS_RX_OFFSET_FCOMP_H_2,0,313,2,-
TUNE_CDMA_PCS_RX_OFFSET_FCOMP_H_3,0,314,2,-
TUNE_CDMA_PCS_RX_OFFSET_FCOMP_H_4,0,315,2,-
TUNE_CDMA_PCS_RX_OFFSET_FCOMP_H_5,0,316,2,-
TUNE_CDMA_PCS_RX_OFFSET_FCOMP_H_6,0,317,2,-
[SET]
lna_gain_enable,4,0,2,+
split_band_ch,4,2,2,+
rx_offset_comp,4,4,2,-
rx_gain_sw1_h_pcs,4,6,2,-
rx_gain_sw1_l_pcs,4,8,2,-
rx_gain_sw1_h_cell,4,10,2,-
rx_gain_sw1_l_cell,4,12,2,-
rx_pwr_logref,4,14,2,-
rx_pole1,4,16,2,-
rx_pole2,4,18,2,-
rx_bbamp_gain_mode_0,4,20,2,-
rx_bbamp_gain_mode_1,4,22,2,-
rx_bbamp_gain_mode_2,4,24,2,-
rx_bbamp_gain_mode_3,4,26,2,-
rx_bbamp_gain_comp_0,4,28,2,-
rx_bbamp_gain_comp_1,4,30,2,-
rx_bbamp_gain_comp_2,4,32,2,-
rx_bbamp_gain_comp_3,4,34,2,-
rx_bbamp_gain_comp_4,4,36,2,-
rx_bbamp_gain_comp_5,4,38,2,-
closed_loop_init,4,40,2,-
closed_loop_step,4,42,2,-
pa_switch_l_cell,4,44,2,-
pa_switch_h_cell,4,46,2,-
pa_switch_l_pcs,4,48,2,-
pa_switch_h_pcs,4,50,2,-
pa_gain_dist_cell,4,52,2,-
pa_gain_dist_pcs,4,54,2,-
pa_low_gain_cell,4,56,2,-
pa_low_gain_pcs,4,58,2,-
closed_loop_limit_h,4,60,2,-
closed_loop_limit_l,4,62,2,-
tx_agc_robin_dvr_h,4,64,2,-
tx_agc_robin_dvr_l,4,66,2,-
robin_dvr_comp,4,68,2,-
rf_switch_l_cell,4,70,2,-
rf_switch_l_pcs,4,72,2,-
rf_low_gain_cell,4,74,2,-
rf_low_gain_pcs,4,76,2,-
tx_gain_offset_cell,4,78,2,-
tx_gain_offset_pcs,4,80,2,-
pole_pwr_est,4,82,2,-
pole_open_loop,4,84,2,-
a_rx_offset_comp,4,86,2,-
a_rx_gain_sw1_h,4,88,2,-
a_rx_gain_sw1_l,4,90,2,-
a_rx_pwr_sw_logref_h,4,92,2,-
a_rx_pwr_sw_logref_l,4,94,2,-
a_rx_pwr_logref_h,4,96,2,-
a_rx_pwr_logref_l,4,98,2,-
a_rx_pole1,4,100,2,-
a_rx_pole2,4,102,2,-
a_rx_bbamp_gain_mode_0,4,104,2,-
a_rx_bbamp_gain_mode_1,4,106,2,-
a_rx_bbamp_gain_mode_2,4,108,2,-
a_rx_bbamp_gain_mode_3,4,110,2,-
a_pa_switch_l,4,112,2,-
a_pa_switch_h,4,114,2,-
a_pa_gain_dist,4,116,2,-
a_pa_low_gain,4,118,2,-
a_tx_agc_robin_dvr_h,4,120,2,-
a_tx_agc_robin_dvr_l,4,122,2,-
a_robin_dvr_comp,4,124,2,-
a_rf_switch_l,4,126,2,-
a_rf_low_gain,4,128,2,-
a_tx_gain_offset,4,130,2,-
a_pole_pwr_est,4,132,2,-
if_dip_offset,4,134,2,-
tx_channel_pcs,4,136,2,-
tx_channel_cell,4,138,2,-
rx_channel_pcs,4,140,2,-
rx_channel_cell,4,142,2,-
pwd_comp_slope_low_temp_cell_0,4,144,2,-
pwd_comp_slope_low_temp_cell_1,4,146,2,-
pwd_comp_slope_low_temp_cell_2,4,148,2,-
pwd_comp_slope_low_temp_cell_3,4,150,2,-
pwd_comp_slope_low_temp_cell_4,4,152,2,-
pwd_comp_slope_low_temp_cell_5,4,154,2,-
pwd_comp_slope_low_temp_cell_6,4,156,2,-
pwd_comp_slope_high_temp_cell_0,4,158,2,-
pwd_comp_slope_high_temp_cell_1,4,160,2,-
pwd_comp_slope_high_temp_cell_2,4,162,2,-
pwd_comp_slope_high_temp_cell_3,4,164,2,-
pwd_comp_slope_high_temp_cell_4,4,166,2,-
pwd_comp_slope_high_temp_cell_5,4,168,2,-
pwd_comp_slope_high_temp_cell_6,4,170,2,-
pwd_comp_slope_low_temp_pcs_0,4,172,2,-
pwd_comp_slope_low_temp_pcs_1,4,174,2,-
pwd_comp_slope_low_temp_pcs_2,4,176,2,-
pwd_comp_slope_low_temp_pcs_3,4,178,2,-
pwd_comp_slope_low_temp_pcs_4,4,180,2,-
pwd_comp_slope_low_temp_pcs_5,4,182,2,-
pwd_comp_slope_low_temp_pcs_6,4,184,2,-
pwd_comp_slope_high_temp_pcs_0,4,186,2,-
pwd_comp_slope_high_temp_pcs_1,4,188,2,-
pwd_comp_slope_high_temp_pcs_2,4,190,2,-
pwd_comp_slope_high_temp_pcs_3,4,192,2,-
pwd_comp_slope_high_temp_pcs_4,4,194,2,-
pwd_comp_slope_high_temp_pcs_5,4,196,2,-
pwd_comp_slope_high_temp_pcs_6,4,198,2,-
tx_offset_temp_step,4,200,2,-
rx_offset_temp_step,4,202,2,-
rx_offset_tcomp_0,4,204,2,-
rx_offset_tcomp_1,4,206,2,-
rx_offset_tcomp_2,4,208,2,-
rx_offset_tcomp_3,4,210,2,-
rx_offset_tcomp_4,4,212,2,-
rx_offset_tcomp_5,4,214,2,-
rx_offset_tcomp_6,4,216,2,-
rx_offset_tcomp_7,4,218,2,-
rx_offset_tcomp_8,4,220,2,-
rx_offset_tcomp_9,4,222,2,-
rx_offset_tcomp_10,4,224,2,-
rx_offset_tcomp_11,4,226,2,-
tx_offset_tcomp_0,4,228,2,-
tx_offset_tcomp_1,4,230,2,-
tx_offset_tcomp_2,4,232,2,-
tx_offset_tcomp_3,4,234,2,-
tx_offset_tcomp_4,4,236,2,-
tx_offset_tcomp_5,4,238,2,-
tx_offset_tcomp_6,4,240,2,-
tx_offset_tcomp_7,4,242,2,-
tx_offset_tcomp_8,4,244,2,-
tx_offset_tcomp_9,4,246,2,-
tx_offset_tcomp_10,4,248,2,-
tx_offset_tcomp_11,4,250,2,-
rf_temp_adc_0,4,252,2,-
rf_temp_adc_1,4,254,2,-
rf_temp_adc_2,4,256,2,-
rf_temp_adc_3,4,258,2,-
rf_temp_adc_4,4,260,2,-
rf_temp_adc_5,4,262,2,-
rf_temp_adc_6,4,264,2,-
rf_temp_adc_7,4,266,2,-
rf_temp_adc_8,4,268,2,-
rf_temp_adc_9,4,270,2,-
rf_temp_adc_10,4,272,2,-
rf_temp_adc_11,4,274,2,-
cell_pfs1_offset,4,276,2,-
cell_pdcch_offset,4,278,2,-
pcs_pf_offset,4,280,2,-
pcs_pfs1_offset,4,282,2,-
pcs_pdcch_offset,4,284,2,-
lna_gain_mode_switch_margin,4,286,2,-
spare_flag_6,4,288,2,-
spare_flag_7,4,290,2,-
[CAL]
ADC Offset,0,0,2,-
ADC Gain,0,2,2,+
VBAT_DIV Offset,1,0,2,-
VBAT_DIV Gain,1,4,4,+
VBAT_SCAL Offset,1,8,2,-
VBAT_SCAL Gain,1,12,4,+
VCHAR Offset,1,16,2,-
VCHAR Gain,1,20,4,+
ICHAR Offset,1,24,2,-
ICHAR Gain,1,28,4,+
PATEMP Offset,1,32,2,-
PATEMP Gain,1,36,4,+
BSI Gain,2,0,2,+
CTI Gain,2,2,2,+
BTEMP Gain,3,0,2,+
BTEMP b,3,2,2,+
VCXO_TEMP t_ref1,3,4,2,+
VCXO_TEMP gain,3,6,2,+
VCXO_TEMP b,3,8,2,+
VCXO_TEMP t_ref2,3,10,2,+
[PANEL:218]
contrast,0,0,1,-
