
NPE-4 Phone Data Package 5.0 Installation
==========================================


Note! AMS Phoenix release 03.72.002 or newer is required.

Close Phoenix before starting installation of the Data Package.

If some earlier version of NPE-4 Phone Data Package is already installed,
it can be uninstalled first, but uninstalling is not mandatory.

Close Phoenix before starting installation of the Data Package.


Changes in NPE-4 Phone Data Package 5.0 (compared to Data Package 4.20):

- MCU software release 04.31 + language packages (PPM)

- Updated NPE_4.ini

- New setting and ini-files:

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C D2 (0508104)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-B Centertel Czarny (center) (0508103)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-B Centertel Bezowy (center) (0508102)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C Swisscom (swiss) (0508176)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C Swisscom (swiss) (0508177)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C Swisscom (swiss) (0508178)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C Tutch (tutch) (0508170)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C BT Cellnet (BTCELBL) (0508203)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C TMN Beige (0508296)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C Vodafone (0508297)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C Mobilkom (mobiko) (0508446)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C Mobilkom (mobiko) (0508445)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C Mobilkom (mobiko) (0508444)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-B ERA BM (0508041)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C E-Plus (0508040)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-C Vodafone Ireland (0508862)

    New Operator Variant for Europe:
    NPE-4 6310 EURO-D Pannon Black (0508861)

- Additional labels (npe_4lbl.ini modified):
    DPM06471.pcx Omnitel (additional OPI)
    DPM06598.pcx Israel without BT sign

- Flash update package 02.04.000 (FPS-8/FLS-4 prommer software update)
    - Just installing Phone Data Package is enough for updating FLS-4
    - Update FPS-8 software after installing Phone Data Package:
        1. Make sure that FPS-8 box is connected
        2. Open Phoenix
        3. Select Flashing - FPS-8/FPS-8C Maintenance
        4. Answer OK to dialog that asks if you want to update the 
           new prommer software
           (4.1 If dialog does not appear for some reason:
                4.1.1 Push Update button
                4.1.2 Select file Phoenix\Flash\fps8upd.ini)
        5. Wait until update is completed


This installation package includes
  - MCU software release 4.31
  - Language packages (PPM) for MCU software 4.31
  - NPE_4.ini file, that includes
      - names of flash files
      - options used in flashing
      - list of settings that can be saved from customer's phone when
        updating software
  - <product code>.ini files, that define
      - language packages that belong to each product
      - default settings for each product
  - Default SW setting files (Product profiles, user profiles, WAP bookmarks etc.)
  - User interface configuration file for Product Profile tool 
  - NPE-4en.val includes product type specific module information for Faultlogger
  - readme.txt (this file)

Known limitations/problems:
  - All settings are not yet included in NPE_4.INI, because saving them does not work
    yet or causes some problems.
  - Reading/writing some settings may show an Error, but should not cause failing of
    the whole flashing procedure.


Date: 25-Jul-2002

Copyright (c) Nokia Corporation. All rights reserved.
