/*	 Automatically generated from i_pp_data_def.h : "Oct 22 2008"  */
/*	
 * "RM247" Product Profile File
 *
 * Copyright (c) Nokia Mobile Phones. All rights reserved.
 *
 * File creation date : "Oct 22 2008"
 */
PRODUCT_PROFILE_PHONE_SETTINGS_V.2.0
PP_IDS_FREEZE_ON
PHONE
  TYPE
    Model = "RM247"
  SETS
    Count = 1
  FEATURES
4 "CSP" STATIC CHECKBOX;
9 "Parallel product" STATIC COMBOBOX
 0 "Lumiere"
        1 "Devlon4"
        2 "Lumiere_nam"
    ;
220 "Vodafone menu browser cache" STATIC COMBOBOX
0 "OFF"
1 "256kb reservation"
2 "512kb reservation"
3 "1024kb reservation"
;
56 "AutoSMS( R&D )" STATIC CHECKBOX;
61 "Enhanced network selection" STATIC CHECKBOX;
219 "Windows DRM Media" STATIC CHECKBOX;
73 "BT Chip Type" STATIC COMBOBOX
    0 "CSR_BC02"
    1 "CSR_BC03"
        2 "CSR_BC04"
    3 "TI_BRF6150"
    ;
135 "TracFone Pre-paid billing" STATIC CHECKBOX;
264 "S60 WLAN control" STATIC CHECKBOX;
156 "Camera on Phone" STATIC CHECKBOX;
35 "PoC Supported" STATIC CHECKBOX;
157 "Send extended cell ID when requested by SIM card" STATIC CHECKBOX;
158 "SIM card MO SM Control" STATIC CHECKBOX;
166 "NOS warnings that should cause a reset" STATIC EDITFIELD 0 7;
183 "Send terminal profile after 3G session refresh" STATIC CHECKBOX;
205 "FBUS as default media" STATIC CHECKBOX;
217 "Controls the strength of ABE" STATIC EDITFIELD 0 32767;
228 "Multimedia application shall comply to EN-50332" STATIC CHECKBOX;
281 "Show Bootlogo at phone startup" STATIC CHECKBOX;
285 "Nokia radios filter time" STATIC COMBOBOX
    0 "50 us"
    1 "75 us"
    ;
288 "Location methods" STATIC EDITFIELD 0 127;
289 "Location communication channel" STATIC EDITFIELD 0 15;
299 "ATK cmd:Set Up Event List for ZuHause appl of Vodafone" STATIC CHECKBOX;
306 "ISIM appl start on USIM at power-on" STATIC CHECKBOX;
314 "H264 video decoding supported" STATIC CHECKBOX;
319 "Old SIM polling interval" STATIC CHECKBOX;
323 "Audio Variant Tuning" STATIC COMBOBOX
    0 "Standard"
    1 "Variant 1"
    2 "Variant 2"
    ;
5469 "2G GAN report threshold" STATIC EDITFIELD 1 0x77;
5498 "3G PS Quick Release" STATIC CHECKBOX;
130 "GSM( A5/1 - A5/7) ciphering algorithms support" STATIC EDITFIELD 1 0x7F;
100 "Advanced HPLMN recognition" STATIC CHECKBOX;
1 "Alternate Line Service (ALS)" STATIC CHECKBOX;
147 "Set always to auto network selection mode after power cycle" STATIC CHECKBOX;
71 "TX power reduction switching" STATIC CHECKBOX;
34 "Cell Info Display Enabled" STATIC CHECKBOX;
0 "Codec order" STATIC EDITFIELD 0 0x7F;
271 "Codec order 2" STATIC EDITFIELD 0 0x06;
296 "Crossband operation" STATIC CHECKBOX;
212 "Opening a dial-up connection to restricted access points is prevented." STATIC CHECKBOX;
5464 "DTM-EGPRS multislot class" STATIC EDITFIELD 0 45;
5463 "DTM-GPRS multislot class" STATIC EDITFIELD 0 45;
211 "PCO is sent to network with FOMA identifier" STATIC CHECKBOX;
79 "Dual Transfer Mode" STATIC CHECKBOX;
5462 "EGPRS multislot class" STATIC EDITFIELD 0 45;
69 "EDGE Support" STATIC CHECKBOX;
214 "EONS feature" STATIC EDITFIELD 0 3;
317 "Fido sim cards standby time improvement in Rogers nw" STATIC CHECKBOX;
5465 "FDN GPRS Control" STATIC CHECKBOX;
320 "GSM preferred ECPM handling" STATIC COMBOBOX
    0 "Always try first GSM"
    1 "Try GSM if GSM is camping on VPLMN or on HPLMN"
    2 "Try GSM only if GSM is camping on HPLMN"
    ;
206 "GAN pref mode" STATIC EDITFIELD 0 3;
131 "Supported GEA encryption algorithms" STATIC EDITFIELD 1 0x7F;
284 "MCU-DSP Interface version check support" STATIC CHECKBOX;
5461 "GPRS multislot class" STATIC EDITFIELD 0 45;
146 "H3G always-on PDP context func supported" STATIC CHECKBOX;
177 "CS call interrupts streaming PS connections" STATIC CHECKBOX;
145 "Limitation for H3G QoS parameters" STATIC CHECKBOX;
168 "H3G specific bit rate mapping of streaming QoS PDP context related RAB" STATIC CHECKBOX;
139 "Selection b/w dynamic and permanent ms tx power level reduction" STATIC CHECKBOX;
138 "FCC requirements of HAC on GSM band basis" STATIC EDITFIELD 0 0x0F;
5490 "Delay Ecall attempt with HSxPA" STATIC EDITFIELD 0 0x0F;
309 "HSxPA UI Menu settings" STATIC COMBOBOX
    0x00 "HSxPA menu not shown, user setting initially disabled"
    0x01 "HSxPA menu not shown, user setting initially enabled"
    0x10 "HSxPA menu shown, user setting initially disabled"
    0x11 "HSxPA menu shown, user setting initially enabled"
    ;
78 "JATE" STATIC COMBOBOX
    0x00 "OFF"
    0x01 "JATE ON"
    0x10 "DOCOMO CHECK ON"
    0x11 "JATE AND DOCOMO CHECK ON"
    ;
5500 "Enable handling for SKT and KTF operators emergency setup in Korea" STATIC CHECKBOX;
202 "Maximum Amount of PDP Contexts" STATIC EDITFIELD 1 11;
5501 "Support for +CGCMOD AT command" STATIC CHECKBOX;
2 "Multislot class = HSCSD class" STATIC EDITFIELD 0 6;
270 "Network Mode Setting" STATIC COMBOBOX
    0 "Dual"
    1 "GSM only"
    2 "WCDMA only"
    ;
5468 "No REL5 QOS Extensions" STATIC CHECKBOX;
5504 "Non 3GPP HPLMN search" STATIC CHECKBOX;
5478 "Nokia Test Mobile Customer ID" STATIC EDITFIELD 0 255;
7 "GPRS PCCCH support" STATIC CHECKBOX;
66 "Read Preferred RAT" STATIC CHECKBOX;
65 "Read Preferred startup RAT" STATIC CHECKBOX;
5475 "Primary Power-on WCDMA Band" STATIC COMBOBOX
    0 "No primary power-on band"
    1 "Op Band I    : WCDMA2100"
    2 "Op Band II   : WCDMA1900"
    3 "Op Band III  : WCDMA1800"
    4 "Op Band IV   : WCDMA1700/2100"
    5 "Op Band V    : WCDMA850"
    6 "Op Band VI   : WCDMA800"
    7 "Op Band VII  : WCDMA2600"
    8 "Op Band VIII : WCDMA900"
    9 "Op Band IX   : WCDMA1700"
    ;
70 "HPLMN Scans: R99(0), R97(1)" STATIC CHECKBOX;
5466 "Repeated ACCH" STATIC COMBOBOX
    0x00 "No Repeated SACCH/DL FACCH support"
    0x01 "Repeated DL FACCH supported"
    0x03 "Repeated SACCH and DL FACCH supported"
    ;
165 "P-CSCF address discovery using PCO IE during PDP context activation" STATIC CHECKBOX;
5481 "Selected WCDMA bands (subset of supported bands)" STATIC EDITFIELD 0 0xFFFF;
310 "No SMS FDN SMSC check" STATIC CHECKBOX;
5492 "Softbank signalling connection release indication" STATIC CHECKBOX;
307 "UMA customer operator" STATIC COMBOBOX
    0 "None"
    1 "TIM, Italy"
    2 "Orange"
    3 "British Telecom"
    4 "China Mobile"
    5 "T-Mobile = TMO"
    ;
294 "Disable HSDPA and/or HSUPA" STATIC COMBOBOX
    0 "AS_CATEGORY_CONFIGURED"
    1 "HSUPA_DISABLED"
    2 "HSDPA_HSUPA_DISABLED"
    ;
5471 "WLAN Mobility High Hysteresis" STATIC EDITFIELD 0 100;
5472 "WLAN Mobility High Threshold" STATIC EDITFIELD 0 100;
5473 "WLAN Mobility Low Hysteresis" STATIC EDITFIELD 0 100;
5474 "WLAN Mobility Low Threshold" STATIC EDITFIELD 0 100;
