-=UBOOTLOADER v.1.5 FOR SYMBIAN (SX1 FW15 ONLY)=-
11.11.06
[SERRGE,VoVan888]
[www.oslik.ru (C) 2006]

Changes:
v.1.5
1. Different clean-ups

v.1.4
1. Added: Creating file s60boot.lck on mmc, as is flag for kernel linux, for not starting init EGold;

v1.3:
1. Resolved problem witch LCD. Now worked fine!

v1.1:
1. Uboot File name for loading, rename to "u-boot.bin"
2. Loading Kernel (uImage.bin) in memory and send var. to u-boot for 
loading kernel linux witchout PC.
_______________________________________
-------------------------------------------------------

Instructions:

1. Unpack archive to mmc card in next struct:
E:\Load_uboot.exe
E:\System\libs\uboot.ldd

2. Download last u-boot and kernel linux for sx1.
Put files to root MMC card:
E:\u-boot.bin
E:\uImage.bin

________________________________________

Best Regards!

[Russia.Kemerovo]
[Stepkin Sergey aka SERRGE]
