How to use gdfs scripts for smartphones.

*NOTE* 

Before writing a script, BACKUP your GDFS with XS++ "GDFS BACKUP"!!!

1. Selecting your script

We have prepared a number of various scripts for you to use which will update/downdate your smartphone versions. The scripts are named in the following format:

MODEL_PHONE_CCPU_ORGANIZER_CDA_REGIONX_REVISION.gdfs

For example:

P990i_R9F011_R5A01_R5A17_CDA162007_1_R5A13.gdfs

 Phone software version: CXC162037 R9F011
 Processing Unit: CXC162087 R5A03
 Organizer: CXC162036 R5A17
 CDA: CDA162007/1 R5A13

2. Drag  & Drop or select from the file browse dialog your selected script.

3. Press the 'Write Script' button and XS++ with run the script.

4. When XS++ has notified you of a successful operation, disconnect the cable from phone and turn on the phone.

5. Reconnect and boot the smartphone with XS++ and you will see your verison details should now have been updated/downdated.

*NOTE* 

Now that your versions have ben modified you can use SEUS to debrand/update your smartphone.

ADDITIONAL STEP

6. You may now update your smartphone with SEUS. It Will be recognised with whatever verisons you filled it with. 


*NOTE*

In the system menu, you may have 2 strings of the versions. Update with SEUS and your should have just the one. 

DO NOT change any of the bytes in the script!
