*-*-*-*-*-*-*-*-*-*-*-
    SMAF/HV Sample
-*-*-*-*-*-*-*-*-*-*-*

<Creating Procedure>

  1) Prepare SMF file. Input the meta-event of HV pronunciation channel specification. 
       Data should be saved as Format 0.
        ( "SMAFHVSample.MID" )

  2) Open [Preference] of AuthoringTool and put a checkmark to [HV] box.

  3) Open required Voice File (.vm3, .vm5) into Authoring Tool.
        ( Open "SMAFHVSample.vm5" by [Open Voice File...]. )

  4) Import prepared SMF to Authoring Tool.
        ( Open "SMAFHVSample.MID" by [Import from SMF...]. )

  5) Open [HV Extend Voice Map] and create voice data.
       Here, please use the extended voice file which is prepared beforehand.
        ( Right-click "SMAFHVSample.hvp" on the line of [Pch#][VoiceName]
           and open it by [Import from HV Extend Voice File...]. )

  6) Open [HV-Script Assign Map] and write HV-Script.
       Here, please use the HV-Script which is prepared beforehand.
        (Right-click "SMAFHVSample.hs5" on the line of [HV-Script name][HV-Script]
          and open it by [Import from Multi HV-Script File...]. )

  7) Put check marks into the channel which synchronize with VS and LED if needed.
        ( Set VS: 2ch and LED: HVch. )

  8) Play it and confirm whether it plays correctly.

  9) Save the file.
        ( "SMAFHVSample.mmf" )
