---------------------------------------------------------
Release Note

Tool Name		:  ATS-SMAFPhraseL2

---------------------------------------------------------
/////////////////////////////////////////////////////////

Ver.1.3.4.1

- User's Manual was updated to Ver.1.3.4.1.


/////////////////////////////////////////////////////////

Ver.1.3.4

- Newly Released

 * SMAF-Phrase (.spf), which multi-file can be played back
   simultaneously in an application such as JAVA, BREW etc.,
   can be created.

   SMAF-Phrase can play up to four files, such as BGM, explosion,
   and/or shooting sound, simultaneously on an optional time.
   SMAF-Phrase (*.spf) is one of effective format to interactive
   application such as games.

 * Both PhraseL1 and PharseL2 can be created in this Authoring
   Tool since the mode-change function has been adapted.
   In addition to FM voices, PCM voices (WT) can be used in
   PhraseL2 (By the correspondence after MA-5).

 Note: The file, created by PhraseL1 (MA-3) mode of this tool,
       can not be played back on MA-2 audio LSI.
       Please use "ATS-SMAFPhraseL1" to create the SMAF-Phrase file
       for MA-2 audio LSI.

/////////////////////////////////////////////////////////
