---------------------------------------------------------
       Release Note

  Tool Name     :  WSD (Wave Sound Decorator)

---------------------------------------------------------
/////////////////////////////////////////////////////////

Ver1.1.0

- New function was added

  * SMAF/MA7 is available.

    SMAF/MA7 can be created.

    - SMAF/MA7 Mode: Mono|up to 48kHz, Stereo|up to 24kHz  : Playable on mobile phone MA-7 or later.

---------------------------------------------------------

Ver1.0.0 

- Newly released. 

  * Long-awaited WSD debut

    Well-reputed WSC-MA2 that has so far been released on SMAF-GLOBAL.
    This WSD (Wave Sound Decorator) supports SMAF-MA3 and SMAF-MA5 as well as SMAF-MA2.
    The WSD can create high-quality SMAF with higher sampling frequency in addition to the previous WSC-MA2 functions.
    - SMAF-MA2 Mode: Mono|4, 8kHz                           : Playable on mobile phone MA-2 or later.
    - SMAF-MA3 Mode: Mono|up to 16kHz                       : Playable on mobile phone MA-3 or later.
    - SMAF-MA5 Mode: Mono|up to 24kHz, Stereo|up to 12kHz  : Playable on mobile phone MA-5 or later.

  * Implementation of converters for Channel and Sampling rate.

    Converters for channel and sampling rate are implemented in the WSD.
    Desired conversion to sound quality, size, and SMAF mode can be freely performed. 

  * Implementation for Waveform Editing Function 

    Read function for WAV/AIFF file up to 48kHz and waveform display function are implemented.
    In addition, since edit functions such as Trimming, Fade, Normalize and Partial Playback function are implemented,
    flexible WAVE-to-SMAF conversion can be realized.


---------------------------------------------------------
/////////////////////////////////////////////////////////
